Altium Designer Pick and Place Locations
C:\Subversion\Boards\Boards_RFOC\B2416_STM32WW611_board_interface\Trunk\02-Manufacturing\B2416A_PCB\Assembly\B2416A_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       27/01/25
Time:       08:04
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator  Comment                        Layer       Footprint                                 Center-X(mm) Center-Y(mm) Rotation Description                                                                   
TP5         Test_Point_PTH_1mm_2mm         TopLayer    TP_PTH_1MM_1P4MM                          10.1200      1.2700       90       "Test Point trought hole 1mm/1.4mm"                                           
TP4         Test_Point_PTH_1mm_2mm         TopLayer    TP_PTH_1MM_1P4MM                          38.7919      1.3270       90       "Test Point trought hole 1mm/1.4mm"                                           
JP4         "Jumper_Header1.27 2x1 Fitted" TopLayer    CON_WP_707-2-02-2-20-00                   32.7393      1.8424       0        "Header, 2x1, 1.27mm, RA, TH, T=3.05mm/2.29mm"                                
JP3         "Jumper_Header1.27 2x1 Fitted" TopLayer    CON_WP_707-2-02-2-20-00                   19.1230      1.8793       0        "Header, 2x1, 1.27mm, RA, TH, T=3.05mm/2.29mm"                                
JP2         "Jumper_Header1.27 2x1 Fitted" TopLayer    CON_WP_707-2-02-2-20-00                   28.3602      1.9575       0        "Header, 2x1, 1.27mm, RA, TH, T=3.05mm/2.29mm"                                
SB14        SB_OFF                         BottomLayer SOLDER-BRIDGE_R0402-0R                    32.0968      3.7514       90       "Solder Bridge 0402 OFF"                                                      
SB11        SB_OFF                         BottomLayer SOLDER-BRIDGE_R0402-0R                    18.5039      3.7862       90       "Solder Bridge 0402 OFF"                                                      
SB8         SB_OFF                         BottomLayer SOLDER-BRIDGE_R0402-0R                    27.7292      3.7533       90       "Solder Bridge 0402 OFF"                                                      
SB10        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                    19.8206      3.7862       90       "Resistor, 0R, SB0402, 5%, 0.063W"                                            
HW4         STICKER_PRODUCT                TopLayer    STICKER_PRODUCT_25X5                      -275.4530    -237.3752    90       "Sticker product 25x5 mm"                                                     
Designator1 Comment                        TopLayer    PCB_SPECIFICATIONS                        -275.4530    -237.3752    0        ""                                                                            
HW5         STICKER_BOARD                  TopLayer    STICKER_BOARD_25X5                        -275.4530    -237.3752    90       "Sticker product 25x5 mm"                                                     
CART-1      Comment                        TopLayer    Sheetbox_6L2S                             44.9274      -27.0590     0        ""                                                                            
U3          ESD-TRANSIL                    TopLayer    ESD_ST0201                                14.1870      13.5342      0        "ESD protection 6V1"                                                          
U2          LD39050PU33R                   BottomLayer ICC_DFN6-EPAD_3X3_P095                    13.2336      3.2446       0        "Low quiescent current and low noise voltage regulators"                      
U1          MB2248                         TopLayer    MB2248_STAMP_FOOTPRINT                    21.2823      32.2489      0        ""                                                                            
R11         ""                             TopLayer    R0603                                     30.2593      13.7083      0        Resistor,47K,0603,1%,1/10W                                                    
R10         ""                             TopLayer    R0603                                     32.5761      13.7028      180      Resistor,100K,0603,1%,1/10W                                                   
R2          ""                             TopLayer    R0603                                     8.9811       7.8881       90       Resistor,100K,0603,1%,1/10W                                                   
R1          ""                             TopLayer    R0603                                     8.9700       10.3374      270      Resistor,330R,0603,1%,1/10W                                                   
LD1         LED_red                        TopLayer    LED_0603_OSRAM_LS-Q976-NR-1_RED_1A2K_H0P8 31.5901      7.6101       90       "LED, Red, 2V, 20mA, 0603"                                                    
C7          Capacitor                      BottomLayer C0402                                     34.1426      24.2601      0        "Capacitor, MLCC, 10uF, 10V, X5R, +/-20%, 0402, T=0.5mm"                      
C6          Capacitor                      BottomLayer C0402                                     16.1064      2.4868       270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
C4          Capacitor                      BottomLayer C0402                                     12.2712      1.0066       180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
C3          Capacitor                      BottomLayer C0402                                     12.7400      5.3327       180      "Capacitor, MLCC, 1uF, 6.3V, X5R, +/- 10%, 0402, T=0.5mm"                     
C2          ""                             TopLayer    C0402                                     14.0764      14.2645      180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                        
C1          Capacitor                      BottomLayer C0402                                     8.7630       4.6990       270      "Capacitor, MLCC, 10uF, 10V, X5R, +/-20%, 0402, T=0.5mm"                      
SB12        SB_OFF                         BottomLayer SOLDER-BRIDGE_R0402-0R                    36.8481      37.3813      90       "Solder Bridge 0402 OFF"                                                      
SB5         SB_OFF                         BottomLayer SOLDER-BRIDGE_R0402-0R                    23.1663      3.7589       90       "Solder Bridge 0402 OFF"                                                      
SB7         SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                    29.0122      3.7606       90       "Resistor, 0R, SB0402, 5%, 0.063W"                                            
SB2         SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                    16.6258      0.6969       0        "Resistor, 0R, SB0402, 5%, 0.063W"                                            
SB1         SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                    15.4003      6.3784       180      "Resistor, 0R, SB0402, 5%, 0.063W"                                            
U4          ""                             TopLayer    ESD_ST0201                                10.1634      8.3270       270      "ESD protection 6V1"                                                          
R7          Resistor                       TopLayer    R0402                                     26.4577      5.0567       180      Resistor,47R,0402,1%,1/16W                                                    
Q1          ""                             TopLayer    NPN_SOT23                                 31.5780      10.9708      180      "NPN Bipolar Transistor"                                                      
B2          SW-PUSH-CMS_EVQP2_BLACK        TopLayer    SWI_PANASONIC_EVQP2F02K                   12.5975      9.6360       90       "EVQP2 - 4.7mm x 3.5 mm SMD Light Touch Switch"                               
SB13        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                    33.3621      3.7562       90       "Resistor, 0R, SB0402, 5%, 0.063W"                                            
SB9         SB_OFF                         BottomLayer SOLDER-BRIDGE_R0402-0R                    9.0614       14.7525      0        "Solder Bridge 0402 OFF"                                                      
SB3         SB_OFF                         BottomLayer SOLDER-BRIDGE_R0402-0R                    9.2883       3.3168       0        "Solder Bridge 0402 OFF"                                                      
TP3         Test_Point_PTH_1mm_2mm         TopLayer    TP_PTH_1MM_1P4MM                          5.0400       1.2700       90       "Test Point trought hole 1mm/1.4mm"                                           
TP2         Test_Point_PTH_1mm_2mm         TopLayer    TP_PTH_1MM_1P4MM                          7.5800       1.2700       90       "Test Point trought hole 1mm/1.4mm"                                           
TP1         Test_Point_PTH_1mm_2mm         TopLayer    TP_PTH_1MM_1P4MM                          2.5000       1.2700       90       "Test Point trought hole 1mm/1.4mm"                                           
SB6         SB_OFF                         BottomLayer SOLDER-BRIDGE_R0402-0R                    34.5719      22.9484      270      "Solder Bridge 0402 OFF"                                                      
SB4         SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                    24.4145      3.7500       90       "Resistor, 0R, SB0402, 5%, 0.063W"                                            
R9          ""                             TopLayer    R0603                                     31.5742      5.0989       90       Resistor,1K,0603,1%,1/10W                                                     
R8          Resistor                       TopLayer    R0402                                     26.4754      13.1945      0        Resistor,47R,0402,1%,1/16W                                                    
R6          Resistor                       TopLayer    R0402                                     24.2751      13.1948      180      Resistor,47R,0402,1%,1/16W                                                    
R5          Resistor                       TopLayer    R0402                                     24.2912      5.0493       0        Resistor,47R,0402,1%,1/16W                                                    
R4          Resistor                       TopLayer    R0402                                     21.3793      13.1863      0        Resistor,47R,0402,1%,1/16W                                                    
R3          Resistor                       TopLayer    R0402                                     19.1865      13.1883      180      Resistor,47R,0402,1%,1/16W                                                    
JP1         "Jumper_Header1.27 2x1 Fitted" TopLayer    CON_WP_707-2-02-2-20-00                   23.7277      1.8588       0        "Header, 2x1, 1.27mm, RA, TH, T=3.05mm/2.29mm"                                
CN3         "Header 7x2"                   TopLayer    CON_SAMTEC_FTSH-107-01-L-DV-K-A           22.2075      9.1267       0        "Header, 7x2, 1.27mm, VR, T=5.97mm, FTSH series STDC14 without Alignment Pin" 
C11         ""                             TopLayer    C0402                                     10.1284      10.6507      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                        
C10         Capacitor                      TopLayer    C0603                                     21.1888      4.8973       180      "Capacitor, MLCC, 1uF, 16V, X5R, 10%, 0603, T=0,8mm"                          
C9          Capacitor                      BottomLayer C0402                                     37.2701      36.0012      0        "Capacitor, MLCC, 10uF, 10V, X5R, +/-20%, 0402, T=0.5mm"                      
C8          Capacitor                      BottomLayer C0402                                     8.5643       13.3811      270      "Capacitor, MLCC, 10uF, 10V, X5R, +/-20%, 0402, T=0.5mm"                      
C5          Capacitor                      BottomLayer C0402                                     15.2914      2.5110       270      "Capacitor, MLCC, 1uF, 6.3V, X5R, +/- 10%, 0402, T=0.5mm"                     
CN2         FTSH-125-02-L-DV               BottomLayer FTSH-125-02-L-DV                          38.6560      18.5480      180      "Header, 25x2, 12.7mm, VR, SMD, T=4.83mm"                                     
CN1         FTSH-125-02-L-DV               BottomLayer FTSH-125-02-L-DV                          4.3660       18.5480      180      "Header, 25x2, 12.7mm, VR, SMD, T=4.83mm"                                     
B1          SW-PUSH-CMS_EVQP2_BLACK        TopLayer    SWI_PANASONIC_EVQP2F02K                   6.2604       9.6362       90       "EVQP2 - 4.7mm x 3.5 mm SMD Light Touch Switch"                               
