Altium Designer Pick and Place Locations
C:\Subversion\MB1035-STM32F3-Sunfish512K-446-Disco\Trunk\02-Manufacturing\MB1035E_PCB\Assembly\MB1035E_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       21/04/20
Time:       14:04
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator Comment            Layer       Footprint               Center-X(mm) Center-Y(mm) Rotation Description                                                                         
C19        100nF              TopLayer    0603C                   58.4271      68.0079      90       Capacitor                                                                           
R49        10K                TopLayer    0402R                   36.7101      36.0039      270      Resistor                                                                            
C39        Capacitor          TopLayer    C0603                   36.7101      34.3529      360      "Capacitor, MLCC, 470nF, 16V, X7R, 10%, 0603, T=0.8mm"                              
C18        10uF               TopLayer    0603C                   56.5221      68.0330      90       Capacitor                                                                           
X3         MC306-G-06Q-32.768 TopLayer    MC306-CRYSTAL           46.3350      63.9800      0        ""                                                                                  
R38        330                TopLayer    0402R                   20.3000      35.8749      0        Resistor                                                                            
C20        1uF                TopLayer    TAN-B                   19.6650      60.6399      180      "Polarized Capacitor (Radial)"                                                      
R35        510                TopLayer    0402R                   45.0650      49.8449      0        Resistor                                                                            
C13        100nF              TopLayer    0402C                   36.1750      72.7049      0        Capacitor                                                                           
C23        20pF               TopLayer    0603C                   33.7620      61.0209      90       Capacitor                                                                           
R27        10K                TopLayer    0402R                   60.7131      67.2459      90       Resistor                                                                            
C32        100nF              TopLayer    0603C                   43.7950      39.1769      270      Capacitor                                                                           
SB19       "Circuit Breaker"  BottomLayer JP2_SMD                 41.9400      50.4799      360      "Circuit Breaker"                                                                   
R26        100                TopLayer    0402R                   37.4450      72.7049      0        Resistor                                                                            
SB11       "Circuit Breaker"  BottomLayer JP2_SMD                 23.6020      71.6119      90       "Circuit Breaker"                                                                   
R5         100                TopLayer    0402R                   19.6650      88.9609      180      Resistor                                                                            
C27        100nF              TopLayer    0603C                   17.7600      54.4550      270      Capacitor                                                                           
SB14       "Circuit Breaker"  BottomLayer JP2_SMD                 39.9350      65.8469      180      "Circuit Breaker"                                                                   
SB10       "Circuit Breaker"  BottomLayer JP2_SMD                 26.6500      71.3849      270      "Circuit Breaker"                                                                   
R2         0                  TopLayer    0402R                   17.5060      92.5169      0        Resistor                                                                            
R33        0                  TopLayer    0402R                   32.1110      60.8939      180      Resistor                                                                            
R32        220                TopLayer    0402R                   29.9520      60.8939      180      Resistor                                                                            
R34        0                  TopLayer    0402R                   38.4610      60.6399      180      Resistor                                                                            
R6         100                TopLayer    0402R                   20.9360      88.9549      180      Resistor                                                                            
R24        4K7                TopLayer    0402R                   22.9670      71.6889      180      Resistor                                                                            
C10        100nF              TopLayer    0402C                   23.4750      76.1339      0        Capacitor                                                                           
C22        20pF               TopLayer    0603C                   28.3010      61.0209      90       Capacitor                                                                           
SB4        "Circuit Breaker"  BottomLayer JP2_SMD                 39.9350      77.3150      180      "Circuit Breaker"                                                                   
R25        4K7                TopLayer    0402R                   24.2370      71.6889      180      Resistor                                                                            
R47        680                TopLayer    0603R                   36.5921      10.0578      135      Resistor                                                                            
R46        680                TopLayer    0603R                   33.0000      8.5699       90       Resistor                                                                            
R45        680                TopLayer    0603R                   29.4079      10.0578      45       Resistor                                                                            
R44        510                TopLayer    0603R                   38.0800      13.6499      180      Resistor                                                                            
LD7        Green              TopLayer    0603D                   41.8900      13.6499      0        "Typical RED, GREEN, YELLOW, AMBER GaAs LED"                                        
R40        680                TopLayer    0603R                   29.4079      17.2420      315      Resistor                                                                            
R43        510                TopLayer    0603R                   27.9200      13.6499      0        Resistor                                                                            
LD10       Red                TopLayer    0603D                   33.0000      4.7599       270      "Typical RED, GREEN, YELLOW, AMBER GaAs LED"                                        
LD6        Green              TopLayer    0603D                   24.1100      13.6499      180      "Typical RED, GREEN, YELLOW, AMBER GaAs LED"                                        
C7         20pF               TopLayer    0402C                   15.8550      80.9599      180      Capacitor                                                                           
LD8        Orange             TopLayer    0603D                   26.7138      7.3638       225      "Typical RED, GREEN, YELLOW, AMBER GaAs LED"                                        
LD4        Blue               TopLayer    0603D                   26.7138      19.9361      135      "Typical RED, GREEN, YELLOW, AMBER GaAs LED"                                        
LD9        Blue               TopLayer    0603D                   39.2862      7.3638       315      "Typical RED, GREEN, YELLOW, AMBER GaAs LED"                                        
R42        680                TopLayer    0603R                   36.5921      17.2420      225      Resistor                                                                            
LD5        Orange             TopLayer    0603D                   39.2862      19.9361      45       "Typical RED, GREEN, YELLOW, AMBER GaAs LED"                                        
R41        680                TopLayer    0603R                   33.0000      18.7299      270      Resistor                                                                            
LD3        Red                TopLayer    0603D                   33.0000      22.5399      90       "Typical RED, GREEN, YELLOW, AMBER GaAs LED"                                        
L1         fcm1608-0603       TopLayer    0603L                   13.9500      63.1799      270      Inductor                                                                            
LD2        LD_BICOLOR_CMS     TopLayer    HSMF-A201               20.3000      92.7709      270      "Bicolor Led"                                                                       
CN2        5075BMR-05-SM      TopLayer    USB-MINI-B-SMD          56.4923      93.2999      0        ""                                                                                  
SB21       "Circuit Breaker"  BottomLayer JP2_SMD                 46.9700      34.5549      270      "Circuit Breaker"                                                                   
SB23       "Circuit Breaker"  BottomLayer JP2_SMD                 38.1300      34.6049      360      "Circuit Breaker"                                                                   
C38        20pF               BottomLayer 0402C                   31.0442      75.9307      360      Capacitor                                                                           
R48        100                BottomLayer 0402R                   32.2888      75.9180      180      Resistor                                                                            
C5         100nF              TopLayer    0402C                   27.2850      83.6650      270      Capacitor                                                                           
C33        100nF              TopLayer    0603C                   18.3950      35.8749      90       Capacitor                                                                           
X1         8MHz               TopLayer    XTAL1                   19.6700      79.2108      90       "Crystal Oscillator"                                                                
SB8        "Circuit Breaker"  BottomLayer JP2_SMD                 55.8460      72.1960      180      "Circuit Breaker"                                                                   
R21        22                 TopLayer    0402R                   10.1400      75.8799      90       Resistor                                                                            
R9         10K                TopLayer    0402R                   27.9200      86.2050      0        Resistor                                                                            
SB2        "Circuit Breaker"  BottomLayer JP2_SMD                 39.9350      79.8550      180      "Circuit Breaker"                                                                   
SB6        "Circuit Breaker"  BottomLayer JP2_SMD                 39.9350      74.7750      180      "Circuit Breaker"                                                                   
JP1        ""                 TopLayer    SIP2/2.54               6.3300       92.3899      270      ""                                                                                  
SB5        "Circuit Breaker"  BottomLayer JP2_SMD                 55.8100      74.7750      180      "Circuit Breaker"                                                                   
SB9        "Circuit Breaker"  BottomLayer JP2_SMD                 39.9350      72.2350      180      "Circuit Breaker"                                                                   
SB1        "Circuit Breaker"  BottomLayer JP2_SMD                 55.8100      79.8550      180      "Circuit Breaker"                                                                   
R14        0                  TopLayer    0402R                   34.2700      86.2050      0        Resistor                                                                            
SB13       "Circuit Breaker"  BottomLayer JP2_SMD                 10.7250      69.5299      180      "Circuit Breaker"                                                                   
R8         10K                TopLayer    0402R                   26.6500      86.2050      0        Resistor                                                                            
C34        10uF               TopLayer    0603C                   30.6141      35.2419      270      Capacitor                                                                           
C9         20pF               TopLayer    0402C                   15.8550      77.1499      0        Capacitor                                                                           
R13        0                  TopLayer    0402R                   33.0000      86.2050      0        Resistor                                                                            
SB15       "Circuit Breaker"  BottomLayer JP2_SMD                 10.7250      66.9899      180      "Circuit Breaker"                                                                   
R20        22                 TopLayer    0402R                   10.1400      78.4199      90       Resistor                                                                            
R28        10K                TopLayer    0402R                   60.7131      68.6429      90       Resistor                                                                            
C8         100nF              TopLayer    0402C                   36.8100      79.8550      0        Capacitor                                                                           
R39        100K               TopLayer    0402R                   43.7950      36.0400      180      Resistor                                                                            
JP3        ""                 TopLayer    SIP2/2.54               15.2200      71.4349      0        ""                                                                                  
C14        6.8pF              TopLayer    0603C                   44.4300      67.7900      0        Capacitor                                                                           
R19        22                 TopLayer    0402R                   10.1400      83.4999      90       Resistor                                                                            
C24        1uF                TopLayer    0603C                   36.8100      60.8939      90       Capacitor                                                                           
C16        1uF                TopLayer    TAN-B                   19.6650      64.4499      180      "Polarized Capacitor (Radial)"                                                      
R11        100K               TopLayer    0402R                   30.4600      86.2050      0        Resistor                                                                            
R12        1K5                TopLayer    0402R                   31.7300      86.2050      0        Resistor                                                                            
R29        0                  TopLayer    0402R                   39.9850      65.8850      90       Resistor                                                                            
R10        100K               TopLayer    0402R                   29.1900      86.2050      0        Resistor                                                                            
R22        22                 TopLayer    0402R                   10.1400      73.3399      90       Resistor                                                                            
SB7        "Circuit Breaker"  BottomLayer JP2_SMD                 10.0900      74.6099      180      "Circuit Breaker"                                                                   
C31        100nF              TopLayer    0603C                   41.8900      39.2150      270      Capacitor                                                                           
LD1        RED                TopLayer    0603D                   12.0450      92.5550      90       ""                                                                                  
R3         10K                TopLayer    0402R                   11.4100      89.3800      90       Resistor                                                                            
D1         BAT60JFILM         TopLayer    SOD323/A                11.4100      86.0399      180      BAT60JFILM                                                                          
R31        0                  TopLayer    0402R                   15.8550      63.1799      0        Resistor                                                                            
R37        100                TopLayer    0402R                   18.3950      39.6849      180      Resistor                                                                            
C28        100nF              TopLayer    0603C                   19.6650      54.4169      270      Capacitor                                                                           
U3         LSM303AGR          TopLayer    ICC_LGA12_2X2_P050      58.6540      71.4349      180      "3D accelerometer and 3D magnetometer"                                              
R7         100                TopLayer    0402R                   14.5850      86.0399      90       Resistor                                                                            
SB16       "Circuit Breaker"  BottomLayer JP2_SMD                 39.9350      64.4499      180      "Circuit Breaker"                                                                   
C37        100nF              TopLayer    0603C                   41.8900      36.0400      270      Capacitor                                                                           
P1         "Header 25X2"      TopLayer    HEAD25X2/2.54           7.6000       32.6999      270      "Header, 25-Pin, Dual row"                                                          
C17        100nF              TopLayer    0603C                   24.7450      64.4499      270      Capacitor                                                                           
CN4        "Header 4"         TopLayer    HEADER_4                47.6050      76.0450      270      "Header, 4-Pin"                                                                     
U2         STM32F103CBT6      TopLayer    ICC_LQFP48_7X7_P050     30.4600      77.3150      270      "Medium-density performance line ARM-based 32-bit MCU with 128KB Flash"             
JP4        JP2                TopLayer    SIP2/2.54               6.3300       68.2599      90       ""                                                                                  
C11        100nF              TopLayer    0603C                   55.6331      70.6749      180      Capacitor                                                                           
C21        100nF              TopLayer    0603C                   24.7450      60.6399      270      Capacitor                                                                           
U5         I3G4250D           TopLayer    ICC_LGA16_4X4_P065_H1P1 33.6963      30.5246      0        "MEMS motion sensor: 3-axis digital output gyroscope LG4-16 4x4mm"                  
R1         1K                 TopLayer    0402R                   13.9530      92.5550      180      Resistor                                                                            
SB20       "Circuit Breaker"  BottomLayer JP2_SMD                 18.5220      37.7299      270      "Circuit Breaker"                                                                   
P2         "Header 25X2"      TopLayer    HEAD25X2/2.54           58.4000      32.6999      270      "Header, 25-Pin, Dual row"                                                          
U4         STM32F303VCT6      TopLayer    ICC_LQFP100_14X14_P050  32.6889      48.5522      180      "STM32F303VCT6 (Manta-Edge)"                                                        
JP2        ""                 TopLayer    SIP2/2.54               59.6700      79.6899      270      ""                                                                                  
C6         1µF_X5R_0603       TopLayer    0603C                   43.1510      84.7669      0        "0603  X5R 1µF"                                                                     
CN3        "Header 6"         TopLayer    HDR1X6                  6.3300       79.6899      270      "Header, 6-Pin"                                                                     
U1         LD3985M33R         TopLayer    SOT-23-5L               43.1510      91.7559      180      "Ultra low drop-low noise BiCMOS voltage, regulators low ESR capacitors compatible" 
C2         100nF              TopLayer    0603C                   43.1510      89.2119      180      Capacitor                                                                           
C4         100nF              TopLayer    0603C                   48.8750      91.1199      270      Capacitor                                                                           
C1         10nF_X7R_0603      TopLayer    0603C                   43.1510      94.2999      180      "0603  X7R 10NF"                                                                    
C3         1µF_X5R_0603       TopLayer    0603C                   46.9670      91.1199      270      "0603  X5R 1µF"                                                                     
D3         BAT60JFILM         TopLayer    SOD323/A                44.4230      87.3039      180      BAT60JFILM                                                                          
R15        100K               TopLayer    0402R                   53.3200      86.6749      0        Resistor                                                                            
R16        1K5                TopLayer    0402R                   54.5900      86.6749      0        Resistor                                                                            
R18        22                 TopLayer    0402R                   57.1300      86.6749      0        Resistor                                                                            
R17        22                 TopLayer    0402R                   55.8600      86.6749      0        Resistor                                                                            
C25        100nF              TopLayer    0603C                   40.4930      60.8939      270      Capacitor                                                                           
CN1        5075BMR-05-SM      TopLayer    USB-MINI-B-SMD          32.9973      93.2999      0        ""                                                                                  
D4         BAT60JFILM         TopLayer    SOD323/A                59.0350      86.0399      90       BAT60JFILM                                                                          
SB3        "Circuit Breaker"  BottomLayer JP2_SMD                 55.8100      77.1499      180      "Circuit Breaker"                                                                   
D2         BAT60JFILM         TopLayer    SOD323/A                38.0800      86.6749      180      BAT60JFILM                                                                          
D5         BAT60JFILM         TopLayer    SOD323/A                60.9400      86.0399      270      BAT60JFILM                                                                          
B2         SW-PUSH-CMS        TopLayer    BP1CMS                  45.7000      30.1599      270      "Non-Open Push-Button 0.1A 24V"                                                     
B1         SW-PUSH-CMS        TopLayer    BP1CMS                  20.3000      30.1599      90       "Non-Open Push-Button 0.1A 24V"                                                     
C30        100nF              TopLayer    0603C                   22.4590      41.7169      270      Capacitor                                                                           
SB12       "Circuit Breaker"  BottomLayer JP2_SMD                 32.3650      68.8449      270      "Circuit Breaker"                                                                   
C26        6.8pF              TopLayer    0603C                   44.4300      60.0049      0        Capacitor                                                                           
C15        220nF              TopLayer    0603C                   58.6811      73.9769      360      Capacitor                                                                           
X2         8MHz               TopLayer    XTAL1                   31.7208      65.0799      0        "Crystal Oscillator"                                                                
C36        10nF/25V           TopLayer    0603C                   34.5511      35.2419      270      Capacitor                                                                           
R30        0                  TopLayer    0402R                   39.9850      63.5609      90       Resistor                                                                            
C12        100nF              TopLayer    0402C                   20.9350      71.4349      180      Capacitor                                                                           
SB17       "Circuit Breaker"  BottomLayer JP2_SMD                 35.4900      61.9099      180      "Circuit Breaker"                                                                   
SB18       "Circuit Breaker"  BottomLayer JP2_SMD                 35.4900      59.8779      180      "Circuit Breaker"                                                                   
C29        100nF              TopLayer    0603C                   20.5540      41.7169      270      Capacitor                                                                           
R4         220K               TopLayer    0603R                   14.5850      88.5799      270      Resistor                                                                            
R23        100K               TopLayer    0402R                   19.6650      71.4349      0        Resistor                                                                            
R36        10K                TopLayer    0402R                   46.3350      49.8449      0        Resistor                                                                            
C35        100nF              TopLayer    0603C                   32.5191      35.2419      270      Capacitor                                                                           
SB22       "Circuit Breaker"  BottomLayer JP2_SMD                 45.0921      34.6569      90       "Circuit Breaker"                                                                   
