Altium Designer Pick and Place Locations
C:\work\maintenance\mb1115\RevD\02-Manufacturing\MB1115D_PCB\Assembly\MB1115D_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       26/05/20
Time:       15:45
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator Comment           Layer       Footprint                Center-X(mm) Center-Y(mm) Rotation Description                                                                         
M1         Comment           TopLayer    SMDPAD-T_(PRIMARY)       45.1920      94.2060      0        ""                                                                                  
R68        10K               BottomLayer 0402R_(Primary)          15.8496      12.6238      180      Resistor                                                                            
C68        100nF             BottomLayer 0402C_(Primary)          15.9100      19.1770      270      Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                              
C69        Capacitor         BottomLayer 0603C_(Primary)          15.8496      15.6718      270      "Capacitor, MLCC, 470nF, 16V, X7R, 10%, 0603, T=0.8mm"                              
CN5        USB-MICRO-AB      TopLayer    USB-MICRO-AB_(PRIMARY)   36.8100      3.5125       90       "USB-MICRO-AB, 47590-0001, SMT, MOLEX"                                              
U9         EMIF02-USB03F2    TopLayer    FLIP_CHIP_(PRIMARY)      42.6500      15.4750      90       "2-line IPAD, EMI filter including ESD protection"                                  
X2         8MHz              TopLayer    XTAL1_(Primary)          30.5308      63.4450      0        "Crystal Oscillator,8Mhz,20PF,20PPM,-10-70 degree,DIP,HC-49S"                       
C22        1uF               TopLayer    TAN-A_(Primary)          23.5000      62.7000      270      "Polarized Capacitor,1uF,16V,10%,typeA,AVX"                                         
C46        100nF             TopLayer    0402C_(Primary)          29.2500      25.4500      0        Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                              
R6         100K              TopLayer    0402R_(Primary)          30.7000      85.3000      0        Resistor                                                                            
R10        22                TopLayer    0402R_(Primary)          9.5000       83.2000      90       Resistor                                                                            
U7         I3G4250D          TopLayer    ICC_LGA16_4X4_P065_H1P1  16.7500      20.7000      270      "MEMS motion sensor: 3-axis digital output gyroscope LG4-16 4x4mm"                  
R62        [NA]              TopLayer    0402R_(Primary)          44.5000      7.7000       0        Resistor,[NA],0402                                                                  
R3         100               TopLayer    0402R_(Primary)          15.5000      85.7000      180      Resistor                                                                            
SB7        "Circuit Breaker" BottomLayer JP2_SMD_(PRIMARY)        55.6490      75.0409      180      "Circuit Breaker"                                                                   
CN2        "Header 6"        TopLayer    HDR1X6_(PRIMARY)         6.3300       79.3500      270      "Header, 6-Pin"                                                                     
U8         CS43L22           TopLayer    QFN40_6X6_(PRIMARY)      27.7500      20.2000      0        "Low Power, Stereo DAC w/Headphone & Speaker Amps"                                  
R41        10K               TopLayer    0402R_(Primary)          42.2000      26.3000      0        Resistor                                                                            
C2         100nF             TopLayer    0402C_(Primary)          46.0000      87.4500      180      Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                              
C66        100nF             TopLayer    0402C_(Primary)          50.7500      8.7000       180      Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                              
B2         SW-PUSH-CMS_BLACK TopLayer    BP1CMS_(Primary)         45.0396      31.7728      270      "Non-Open Push-Button 0.1A 24V"                                                     
R51        100               TopLayer    0402R_(Primary)          33.0000      17.7000      270      Resistor                                                                            
C47        1uF               TopLayer    0603C_(Primary)          35.2000      23.2000      0        Capacitor,1uF,16V,X5R,10%,0603,YAGEO                                                
R33        [NA]              TopLayer    0402R_(Primary)          43.7000      39.7000      180      Resistor,[NA],0402                                                                  
C8         100nF             TopLayer    0402C_(Primary)          35.6000      81.9000      0        Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                              
C51        150pF             TopLayer    0603C_(Primary)          33.0000      21.2000      180      Capacitor,150pF,50V,NPO,5%,0603,YAGEO                                               
C44        100nF             TopLayer    0402C_(Primary)          26.7500      25.4500      0        Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                              
R57        0                 TopLayer    0402R_(Primary)          40.5500      12.2000      0        Resistor,0,0402                                                                     
C39        100nF             TopLayer    0402C_(Primary)          46.4500      36.8000      270      Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                              
SB4        "Circuit Breaker" BottomLayer JP2_SMD_(PRIMARY)        39.8489      77.5809      180      "Circuit Breaker"                                                                   
JP4        ""                BottomLayer SIP2/2.54_(PRIMARY)      59.6700      92.3900      90       ""                                                                                  
C11        100nF             TopLayer    0402C_(Primary)          23.5000      71.4500      180      Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                              
SB17       "Circuit Breaker" BottomLayer JP2_SMD_(PRIMARY)        37.6500      65.1000      360      "Circuit Breaker"                                                                   
LD6        "LED, blue"       TopLayer    0603D_(Primary)          33.4000      27.1000      180      "LED, blue, 0603"                                                                   
R24        220               TopLayer    0402R_(Primary)          30.0000      59.7000      0        Resistor                                                                            
U4         STM32F411VET6U    TopLayer    TQFP100_14X14_(PRIMARY)  32.6635      48.4619      180      "STM32 Tiny Manta (STM32F401VCT6U)"                                                 
P1         "Header 25X2"     TopLayer    HDR2X25_(PRIMARY)        7.6000       32.7000      270      "Header, 25-Pin, Dual row"                                                          
T1         9013-SOT23        TopLayer    SOT23_(Primary)          37.9500      11.1500      90       "NPN Bipolar Transistor"                                                            
C28        6.8pF             TopLayer    0402C_(Primary)          42.2500      59.7000      90       Capacitor,6.8pF,50V,NPO,4%,0402,AVX                                                 
R17        22                TopLayer    0402R_(Primary)          9.5000       72.9500      90       Resistor                                                                            
CN1        USB-MINI-typeB    TopLayer    USB-MINI-B-SMD_(Primary) 33.3563      93.0260      0        "USB-MINI-typeB connector"                                                          
SB10       "Circuit Breaker" BottomLayer JP2_SMD_(PRIMARY)        8.9500       72.2000      360      "Circuit Breaker"                                                                   
B1         SW-PUSH-CMS_BLUE  TopLayer    BP1CMS_(Primary)         20.9604      31.7728      90       "Non-Open Push-Button 0.1A 24V"                                                     
SB6        "Circuit Breaker" BottomLayer JP2_SMD_(PRIMARY)        39.8489      75.0409      180      "Circuit Breaker"                                                                   
R8         0                 TopLayer    0402R_(Primary)          33.2000      85.3000      0        Resistor,0,0402                                                                     
C55        100nF             TopLayer    0402C_(Primary)          16.9164      16.3322      90       Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                              
R53        0                 TopLayer    0402R_(Primary)          38.6000      15.7000      90       Resistor,0,0402                                                                     
SB11       "Circuit Breaker" BottomLayer JP2_SMD_(PRIMARY)        8.9500       70.8000      360      "Circuit Breaker"                                                                   
LD4        "LED, green"      TopLayer    0603D_(Primary)          29.0000      31.0000      0        "LED, green, 0603"                                                                  
SB5        "Circuit Breaker" BottomLayer JP2_SMD_(PRIMARY)        55.6490      77.5809      180      "Circuit Breaker"                                                                   
LD8        "LED, red"        TopLayer    0603D_(Primary)          45.0000      2.4500       90       "LED, red, 0603"                                                                    
R21        0                 TopLayer    0402R_(Primary)          37.6000      65.1000      90       Resistor,0,0402                                                                     
R35        220K              TopLayer    0402R_(Primary)          22.7500      36.9500      0        Resistor                                                                            
C34        100nF             TopLayer    0402C_(Primary)          23.7500      40.4500      180      Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                              
R28        510               TopLayer    0402R_(Primary)          45.4000      50.7000      0        Resistor                                                                            
R58        22                TopLayer    0402R_(Primary)          43.7500      12.0000      90       Resistor                                                                            
LD7        "LED, green"      TopLayer    0603D_(Primary)          29.2500      2.4500       90       "LED, green, 0603"                                                                  
R64        330               TopLayer    0603R_(Primary)          27.2500      2.4500       90       Resistor                                                                            
C18        20pF              TopLayer    0402C_(Primary)          29.2000      66.7000      270      Capacitor,20pF,50V,NPO,5%,0402,YAGEO                                                
SB13       "Circuit Breaker" BottomLayer JP2_SMD_(PRIMARY)        29.7500      69.9000      270      "Circuit Breaker"                                                                   
SB14       "Circuit Breaker" BottomLayer JP2_SMD_(PRIMARY)        33.8000      68.2000      360      "Circuit Breaker"                                                                   
JP1        JP2               TopLayer    SIP2/2.54_(PRIMARY)      6.3300       68.1075      90       ""                                                                                  
CN4        ST-225-02         TopLayer    JACK-ST-225_(Primary)    17.7600      5.5600       90       "Connector Jack 35mm"                                                               
X3         XTAL_32K_20PPM    TopLayer    MC306-CRYSTAL_(Primary)  44.2000      63.5000      0        "Crystal oscillator for clock,32.768K,6PF,20PPM,-40~85 degree,SMT"                  
LD2        "LED, red"        TopLayer    0603D_(Primary)          41.5000      84.7000      90       "LED, red, 0603"                                                                    
R34        330               TopLayer    0402R_(Primary)          20.0000      37.9500      90       Resistor                                                                            
C23        100nF             TopLayer    0402C_(Primary)          15.5000      60.7000      0        Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                              
SB20       "Circuit Breaker" BottomLayer JP2_SMD_(PRIMARY)        20.3000      47.1500      90       "Circuit Breaker"                                                                   
SB19       "Circuit Breaker" BottomLayer JP2_SMD_(PRIMARY)        43.7500      52.7000      360      "Circuit Breaker"                                                                   
C58        10nF              TopLayer    0603C_(Primary)          39.3000      17.7000      0        Capacitor,10nF,50V,X7R,10%,0603,YAGEO                                               
C12        100nF             TopLayer    0402C_(Primary)          36.0000      72.1000      0        Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                              
R19        4K7               TopLayer    0402R_(Primary)          25.5000      71.4500      180      Resistor                                                                            
SB1        "Circuit Breaker" TopLayer    JP2_SMD_(PRIMARY)        46.7430      39.2711      180      "Circuit Breaker"                                                                   
R55        [NA]              TopLayer    0402R_(Primary)          37.9000      13.7000      270      Resistor,[NA],0402                                                                  
C42        100nF             TopLayer    0402C_(Primary)          30.0200      29.2100      90       Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                              
SB16       "Circuit Breaker" BottomLayer JP2_SMD_(PRIMARY)        33.8000      66.7000      360      "Circuit Breaker"                                                                   
LD1        LD_BICOLOR_CMS    TopLayer    HSMF-A201_(Primary)      16.2360      89.3800      270      "Bicolor Led"                                                                       
C65        1uF               TopLayer    0603C_(Primary)          47.7500      12.4500      0        Capacitor,1uF,16V,X5R,10%,0603,YAGEO                                                
R61        0                 TopLayer    0402R_(Primary)          43.2500      7.7000       180      Resistor,0,0402                                                                     
R9         0                 TopLayer    0402R_(Primary)          34.4000      85.3000      0        Resistor,0,0402                                                                     
C38        2.2uF             TopLayer    TAN-A_(Primary)          40.5000      36.7000      180      "Capacitor,2.2uF,16V, X7R,10%,0805,YAGEO"                                           
R52        1.2K              TopLayer    0402R_(Primary)          36.2000      15.7000      90       Resistor                                                                            
C45        100nF             TopLayer    0402C_(Primary)          28.0000      25.4500      0        Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                              
C48        10nF              TopLayer    0603C_(Primary)          20.5000      21.4500      270      Capacitor,10nF,50V,X7R,10%,0603,YAGEO                                               
C59        100nF             TopLayer    0402C_(Primary)          20.5000      15.4500      90       Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                              
R37        100               TopLayer    0402R_(Primary)          17.0000      36.2000      270      Resistor                                                                            
R39        1K                TopLayer    0402R_(Primary)          37.7000      29.3000      270      Resistor                                                                            
R13        1K                TopLayer    0402R_(Primary)          41.5000      81.9500      0        Resistor                                                                            
C7         100nF             TopLayer    0402C_(Primary)          26.6000      82.4000      0        Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                              
SB15       "Circuit Breaker" BottomLayer JP2_SMD_(PRIMARY)        37.2500      69.4000      270      "Circuit Breaker"                                                                   
SB8        "Circuit Breaker" BottomLayer JP2_SMD_(PRIMARY)        39.8489      72.5009      180      "Circuit Breaker"                                                                   
R45        100               TopLayer    0402R_(Primary)          32.4000      23.1500      270      Resistor                                                                            
R31        510               TopLayer    0402R_(Primary)          19.4000      47.0000      180      Resistor                                                                            
C15        100nF             TopLayer    0402C_(Primary)          11.0000      66.4500      0        Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                              
SB12       "Circuit Breaker" BottomLayer JP2_SMD_(PRIMARY)        22.2500      71.2500      90       "Circuit Breaker"                                                                   
C35        100nF             TopLayer    0402C_(Primary)          40.7500      39.7000      0        Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                              
C31        100nF             TopLayer    0402C_(Primary)          19.5000      53.2000      0        Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                              
L1         Ferrite           TopLayer    0603L_(Primary)          19.8067      60.6602      270      Bead,600R,350mA,0603,FCM1608KF-601T03,Tai-tech                                      
R22        0                 TopLayer    0402R_(Primary)          37.6000      63.3000      90       Resistor,0,0402                                                                     
C32        100nF             TopLayer    0402C_(Primary)          21.6000      53.2000      0        Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                              
R14        10K               TopLayer    0402R_(Primary)          14.7500      81.2000      0        Resistor                                                                            
C14        1uF               TopLayer    0603C_(Primary)          9.2500       66.4500      90       Capacitor,1uF,16V,X5R,10%,0603,YAGEO                                                
C64        1uF               TopLayer    TAN-A_(Primary)          29.5000      11.9500      90       "Polarized Capacitor,1uF,16V,10%,typeA,AVX"                                         
C5         10nF              TopLayer    0603C_(Primary)          45.0000      84.4500      0        Capacitor,10nF,50V,X7R,10%,0603,YAGEO                                               
C20        6.8pF             TopLayer    0402C_(Primary)          42.0000      67.2000      90       Capacitor,6.8pF,50V,NPO,4%,0402,AVX                                                 
C40        100nF             TopLayer    0402C_(Primary)          29.6000      34.1000      90       Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                              
C9         20pF              TopLayer    0402C_(Primary)          16.0000      77.3000      0        Capacitor,20pF,50V,NPO,5%,0402,YAGEO                                                
C17        1uF               TopLayer    0603C_(Primary)          19.3000      67.4000      270      Capacitor,1uF,16V,X5R,10%,0603,YAGEO                                                
C16        100nF             TopLayer    0402C_(Primary)          17.7600      67.0280      0        Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                              
C21        100nF             TopLayer    0402C_(Primary)          21.5000      64.0000      0        Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                              
SB18       "Circuit Breaker" BottomLayer JP2_SMD_(PRIMARY)        37.6500      63.3000      360      "Circuit Breaker"                                                                   
R15        22                TopLayer    0402R_(Primary)          9.2500       77.9500      90       Resistor                                                                            
R50        100K              TopLayer    0402R_(Primary)          36.4000      19.9000      270      Resistor                                                                            
C1         1uF               TopLayer    0603C_(Primary)          43.8000      87.5000      90       Capacitor,1uF,16V,X5R,10%,0603,YAGEO                                                
C36        [NA]              TopLayer    0402C_(Primary)          20.0000      36.2000      270      Capacitor,NA,0402                                                                   
C26        100nF             TopLayer    0402C_(Primary)          34.4605      60.1700      90       Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                              
R49        47K               TopLayer    0402R_(Primary)          46.0000      21.7000      0        Resistor                                                                            
C41        220nF             TopLayer    0603C_(Primary)          36.5982      33.7820      270      Capacitor,220nF,16V,X7R,10%,0603,YAGEO                                              
R29        [NA]              TopLayer    0402R_(Primary)          46.8000      50.7000      0        Resistor,[NA],0402                                                                  
D3         BAT60JFILM        TopLayer    SOD323/A_(Primary)       53.2000      83.8000      90       BAT60JFILM                                                                          
SB21       "Circuit Breaker" BottomLayer JP2_SMD_(PRIMARY)        19.5000      40.6500      270      "Circuit Breaker"                                                                   
C50        100nF             TopLayer    0402C_(Primary)          22.6000      20.4500      90       Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                              
R26        0                 TopLayer    0402R_(Primary)          37.7500      59.7000      0        Resistor,0,0402                                                                     
R20        4K7               TopLayer    0402R_(Primary)          26.7500      71.4500      180      Resistor                                                                            
C63        1uF               TopLayer    0603C_(Primary)          33.4500      14.2000      90       Capacitor,1uF,16V,X5R,10%,0603,YAGEO                                                
U10        IMP34DT05TR       TopLayer    MIC_HCLGA_3X4X1_4LD      47.6830      7.8860       180      "MEMS audio sensor omnidirectional digital microphone for industrial applications"  
R25        0                 TopLayer    0402R_(Primary)          32.2500      59.7000      180      Resistor,0,0402                                                                     
C3         100nF             TopLayer    0402C_(Primary)          51.3000      87.3000      0        Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                              
R5         100K              TopLayer    0402R_(Primary)          29.4000      85.3000      0        Resistor                                                                            
C37        10uF              TopLayer    0603C_(Primary)          29.5000      35.6000      0        Capacitor,10uF,6.3V,X5R,20%,0603,YAGEO                                              
CN3        "Header 4"        TopLayer    HEADER_4_(PRIMARY)       47.2989      76.3109      270      "Header, 4-Pin"                                                                     
R4         100               TopLayer    0402R_(Primary)          17.0000      85.7000      180      Resistor                                                                            
R7         1K5               TopLayer    0402R_(Primary)          32.0000      85.3000      0        Resistor                                                                            
R40        510               TopLayer    0402R_(Primary)          36.4000      27.2000      90       Resistor                                                                            
C56        1uF               TopLayer    0603C_(Primary)          22.5000      16.9500      180      Capacitor,1uF,16V,X5R,10%,0603,YAGEO                                                
C54        4.7uF             TopLayer    TAN-A_(Primary)          44.0000      18.4500      180      "Polarized Capacitor,4.7uF,16V,10%,typeA,AVX"                                       
R56        22                TopLayer    0402R_(Primary)          43.7500      13.2000      90       Resistor                                                                            
C67        20pF              BottomLayer 0402C_(Primary)          33.2500      71.7000      180      Capacitor,20pF,50V,NPO,5%,0402,YAGEO                                                
SB2        "Circuit Breaker" BottomLayer JP2_SMD_(PRIMARY)        39.8489      80.1209      180      "Circuit Breaker"                                                                   
C10        100nF             TopLayer    0402C_(Primary)          24.5000      75.4500      0        Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                              
R18        100K              TopLayer    0402R_(Primary)          22.2500      71.4500      0        Resistor                                                                            
C13        10nF              TopLayer    0603C_(Primary)          10.0000      69.2000      0        Capacitor,10nF,50V,X7R,10%,0603,YAGEO                                               
R59        51                TopLayer    0402R_(Primary)          25.2500      10.7000      0        Resistor                                                                            
R36        1K                TopLayer    0402R_(Primary)          31.2000      37.7000      270      Resistor                                                                            
U2         STM32F103C8T6     TopLayer    LQFP48_(Primary)         31.3000      77.1000      0        "Medium-density performance line ARM-based 32-bit MCU with 64KB Flash"              
R66        100               BottomLayer 0402R_(Primary)          33.2500      74.1500      180      Resistor                                                                            
C33        2.2uF             TopLayer    TAN-A_(Primary)          19.7500      39.9500      0        "Capacitor,2.2uF,16V, X7R,10%,0805,YAGEO"                                           
R42        0                 TopLayer    0402R_(Primary)          44.0000      26.3000      0        Resistor,0,0402                                                                     
R12        10K               TopLayer    0402R_(Primary)          24.9000      82.4000      0        Resistor                                                                            
D2         BAT60JFILM        TopLayer    SOD323/A_(Primary)       9.0000       86.7000      270      BAT60JFILM                                                                          
U5         LSM303AGR         TopLayer    ICC_LGA12_2X2_P050       33.4558      32.6639      90       "3D accelerometer and 3D magnetometer"                                              
C29        100nF             TopLayer    0402C_(Primary)          42.0000      56.9500      0        Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                              
R54        47K               TopLayer    0402R_(Primary)          40.7000      15.6000      180      Resistor                                                                            
R27        4.7K              TopLayer    0402R_(Primary)          49.0000      52.4500      180      Resistor                                                                            
R30        10K               TopLayer    0402R_(Primary)          17.7500      46.9500      0        Resistor                                                                            
JP2        ""                TopLayer    SIP2/2.54_(PRIMARY)      17.2500      54.4300      270      ""                                                                                  
R38        330               TopLayer    0402R_(Primary)          28.3000      32.7000      270      Resistor                                                                            
C52        1uF               TopLayer    0603C_(Primary)          22.5000      18.9500      180      Capacitor,1uF,16V,X5R,10%,0603,YAGEO                                                
R48        0                 TopLayer    0402R_(Primary)          44.7000      21.7000      180      Resistor,0,0402                                                                     
C62        1uF               TopLayer    0603C_(Primary)          31.7000      14.2000      90       Capacitor,1uF,16V,X5R,10%,0603,YAGEO                                                
R23        47                TopLayer    0402R_(Primary)          21.5000      60.7000      0        Resistor                                                                            
R60        51                TopLayer    0402R_(Primary)          27.2500      10.7000      180      Resistor                                                                            
C4         1uF               TopLayer    0603C_(Primary)          53.2000      87.3000      90       Capacitor,1uF,16V,X5R,10%,0603,YAGEO                                                
R11        [NA]              TopLayer    0402R_(Primary)          23.7000      82.4000      0        Resistor,[NA],0402                                                                  
C6         20pF              TopLayer    0402C_(Primary)          16.0000      81.2000      180      Capacitor,20pF,50V,NPO,5%,0402,YAGEO                                                
R2         [NA]              TopLayer    0402R_(Primary)          10.5000      86.7000      0        Resistor,[NA],0402                                                                  
C53        150pF             TopLayer    0603C_(Primary)          33.0000      19.4500      180      Capacitor,150pF,50V,NPO,5%,0603,YAGEO                                               
R63        0                 TopLayer    0402R_(Primary)          24.7500      2.2000       0        Resistor,0,0402                                                                     
D1         BAT60JFILM        TopLayer    SOD323/A_(Primary)       41.6000      88.5000      270      BAT60JFILM                                                                          
JP3        ""                BottomLayer SIP2/2.54_(PRIMARY)      6.3300       92.3900      90       ""                                                                                  
LD3        "LED, orange"     TopLayer    0603D_(Primary)          33.4000      35.6000      0        "LED, orange, 0603"                                                                 
C27        1uF               TopLayer    0603C_(Primary)          39.5000      60.0000      90       Capacitor,1uF,16V,X5R,10%,0603,YAGEO                                                
LD5        "LED, red"        TopLayer    0603D_(Primary)          37.6000      31.0000      0        "LED, red, 0603"                                                                    
C30        100nF             TopLayer    0402C_(Primary)          44.0000      56.9500      0        Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                              
R16        22                TopLayer    0402R_(Primary)          9.5000       75.4500      90       Resistor                                                                            
R43        10K               TopLayer    0402R_(Primary)          32.5000      24.9000      90       Resistor                                                                            
X1         8MHz              TopLayer    XTAL1_(Primary)          20.1050      79.2308      90       "Crystal Oscillator,8Mhz,20PF,20PPM,-10-70 degree,DIP,HC-49S"                       
U3         LD3985M25R        TopLayer    SOT-23-5L_(Primary)      14.4000      66.9000      180      "Ultra low drop-low noise BiCMOS voltage, regulators low ESR capacitors compatible" 
P2         "Header 25X2"     TopLayer    HDR2X25_(PRIMARY)        58.4000      32.7000      270      "Header, 25-Pin, Dual row"                                                          
R44        100K              TopLayer    0402R_(Primary)          36.9000      24.9000      90       Resistor                                                                            
R46        [NA]              TopLayer    0402R_(Primary)          38.0000      23.2000      90       Resistor,[NA],0402                                                                  
U6         STMPS2141STR      TopLayer    SOT23-5L_(PRIMARY)       41.2500      22.7000      0        "Enhanced single channel power switches"                                            
R1         0                 TopLayer    0402R_(Primary)          16.5000      92.7000      90       Resistor,0,0402                                                                     
R67        100               BottomLayer 0402R_(Primary)          35.5000      75.2000      360      Resistor                                                                            
C60        22nF              TopLayer    0603C_(Primary)          25.2500      14.2000      270      Capacitor,22nF,50V,X7R,10%,0603,YAGEO                                               
C57        1uF               TopLayer    0603C_(Primary)          36.1500      17.7000      0        Capacitor,1uF,16V,X5R,10%,0603,YAGEO                                                
C43        10uF              TopLayer    0603C_(Primary)          17.8500      25.3500      270      Capacitor,10uF,6.3V,X5R,20%,0603,YAGEO                                              
C24        1uF               TopLayer    TAN-A_(Primary)          17.7500      61.2000      270      "Polarized Capacitor,1uF,16V,10%,typeA,AVX"                                         
SB9        "Circuit Breaker" BottomLayer JP2_SMD_(PRIMARY)        55.6490      72.5009      180      "Circuit Breaker"                                                                   
C49        100nF             TopLayer    0402C_(Primary)          22.6000      21.7000      270      Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                              
C19        20pF              TopLayer    0402C_(Primary)          33.7500      66.7000      90       Capacitor,20pF,50V,NPO,5%,0402,YAGEO                                                
C25        100nF             TopLayer    0402C_(Primary)          27.2500      60.2000      90       Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                              
U1         LD3985M33R        TopLayer    SOT-23-5L_(Primary)      48.5990      86.7210      270      "Ultra low drop-low noise BiCMOS voltage, regulators low ESR capacitors compatible" 
SB3        "Circuit Breaker" BottomLayer JP2_SMD_(PRIMARY)        55.6490      80.1209      180      "Circuit Breaker"                                                                   
R32        4.7K              TopLayer    0402R_(Primary)          46.7000      47.9000      270      Resistor                                                                            
C61        22nF              TopLayer    0603C_(Primary)          27.2500      14.2000      270      Capacitor,22nF,50V,X7R,10%,0603,YAGEO                                               
R47        [NA]              TopLayer    0402R_(Primary)          36.4000      21.2000      270      Resistor,[NA],0402                                                                  
R65        620               TopLayer    0603R_(Primary)          47.0000      2.4500       90       Resistor                                                                            
