Altium Designer Pick and Place Locations
C:\Subversion\Boards\EOL-2020\STM32F469I-DISCO\MB1189-STM32F4-Dragon2M-434-Disco\Trunk\02-Manufacturing\MB1189C_PCB\Assembly\MB1189C_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       15/03/22
Time:       10:52
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator Comment                        Layer       Footprint              Center-X(mm) Center-Y(mm) Rotation Description                                                                         
HW4        STICKER_QR_CODE                BottomLayer STICKER_QR_CODE_8X8    -300.0000    -300.0000    180      ""                                                                                  
HW3        STICKER_BOARD_CPN              BottomLayer STICKER_BOARD-CPN_13X3 -300.0000    -300.0000    180      ""                                                                                  
U11        "ISSI IS42S32400F-6BL"         BottomLayer ICC_VFBGA90_8X13_P080  36.1950      55.6260      90       "SDRAM 128MBit 166MHZ 90BGA"                                                        
U3         "STLINK V2-1"                  BottomLayer LQFP48_0R5_9X9         26.1620      104.9020     90       ""                                                                                  
CN9        PJS008-2003-1                  BottomLayer MSD_PJS008_            8.4925       35.2903      90       "MicroSD Card Conn, Reversed-Type, Mnt Push-Push, Positionning holes"               
CN11       F206A-2*04MGF-A                BottomLayer SSM-104-L-DH           7.6200       19.0500      270      "Header, 4-Pin, Dual row"                                                           
U4         ST890CDR                       BottomLayer SOIC8_1R27_4R9X6       43.9420      93.8530      90       ""                                                                                  
U2         IMP34DT05TR                    TopLayer    MIC_HCLGA_3X4X1_4LD_   28.8300      5.6150       270      "MEMS audio sensor omnidirectional digital microphone for industrial applications"  
U1         IMP34DT05TR                    TopLayer    MIC_HCLGA_3X4X1_4LD_   12.8269      123.5961     270      "MEMS audio sensor omnidirectional digital microphone for industrial applications"  
U6         IMP34DT05TR                    TopLayer    MIC_HCLGA_3X4X1_4LD_   49.8309      5.6131       270      "MEMS audio sensor omnidirectional digital microphone for industrial applications"  
R55        10K                            BottomLayer 0402R                  9.1440       46.3550      360      Resistor                                                                            
R39        51                             BottomLayer 0402R                  15.7480      93.8530      90       Resistor                                                                            
R40        51                             BottomLayer 0402R                  14.3510      93.8530      90       Resistor                                                                            
R152       10K                            BottomLayer 0402R                  13.0810      12.1920      270      Resistor                                                                            
R9         10K                            BottomLayer 0402R                  26.7970      116.8400     360      Resistor                                                                            
R38        10K                            BottomLayer 0402R                  39.3700      93.9800      90       Resistor                                                                            
R28        10K                            BottomLayer 0402R                  30.4800      97.5360      90       Resistor                                                                            
R122       10K                            BottomLayer 0402R                  20.7010      33.7820      270      Resistor                                                                            
R149       10K                            BottomLayer 0402R                  29.7180      13.8430      270      Resistor                                                                            
R34        100K                           BottomLayer 0402R                  56.6420      96.9010      90       Resistor                                                                            
R13        0                              BottomLayer 0603R                  28.9560      114.6810     270      Resistor                                                                            
R29        [N/A]                          BottomLayer 0603R                  29.2100      97.5360      90       "Resistor 0402 / 0603 / 0805"                                                       
R20        100                            BottomLayer 0603R                  19.5580      109.6010     360      Resistor                                                                            
R116       47K                            BottomLayer 0603R                  18.0340      36.8300      360      Resistor                                                                            
R3         680                            TopLayer    0603R                  21.9710      120.9040     90       Resistor                                                                            
R6         100K                           BottomLayer 0603R                  16.5100      117.6020     90       Resistor                                                                            
R14        0                              BottomLayer 0603R                  27.6860      114.6810     270      Resistor                                                                            
R11        100                            BottomLayer 0603R                  56.7690      115.3160     360      Resistor                                                                            
R12        1K5                            BottomLayer 0603R                  30.2260      114.6810     270      Resistor                                                                            
R16        36K                            BottomLayer 0603R                  24.8920      114.6810     90       Resistor                                                                            
R150       [N/A]                          BottomLayer 0603R                  31.1150      13.7160      270      Resistor                                                                            
R19        220K                           BottomLayer 0603R                  14.4780      113.0300     270      Resistor                                                                            
R18        330                            BottomLayer 0603R                  16.1290      113.0300     270      Resistor                                                                            
R7         820                            BottomLayer 0603R                  43.0530      117.4750     360      Resistor                                                                            
R2         510                            TopLayer    0603R                  17.2720      120.9040     90       Resistor                                                                            
R5         680                            TopLayer    0603R                  31.3690      120.9040     90       Resistor                                                                            
R117       0                              BottomLayer 0603R                  54.7370      35.8140      270      Resistor                                                                            
R24        0                              BottomLayer 0603R                  3.3020       108.4580     360      Resistor                                                                            
R114       47K                            BottomLayer 0603R                  18.0340      39.7510      360      Resistor                                                                            
R10        100                            BottomLayer 0603R                  18.6690      115.4430     360      Resistor                                                                            
R86        47K                            BottomLayer 0603R                  18.0340      41.1480      360      Resistor                                                                            
R57        0                              BottomLayer 0603R                  5.7150       44.9580      360      Resistor                                                                            
R4         680                            TopLayer    0603R                  26.6700      120.9040     90       Resistor                                                                            
R120       47K                            BottomLayer 0603R                  18.0340      35.5600      360      Resistor                                                                            
R115       47K                            BottomLayer 0603R                  18.0340      38.2270      360      Resistor                                                                            
R132       0                              BottomLayer 0603R                  23.3680      20.0660      360      Resistor                                                                            
R133       0                              BottomLayer 0603R                  23.3680      21.5900      360      Resistor                                                                            
R58        10                             BottomLayer 0603R                  56.3880      44.1960      270      Resistor                                                                            
R22        2K7                            BottomLayer 0603R                  32.1310      111.5060     270      Resistor                                                                            
R36        4K7                            BottomLayer 0603R                  53.5940      96.9010      90       Resistor                                                                            
R118       4K7                            BottomLayer 0603R                  53.2130      35.8140      270      Resistor                                                                            
R32        4K7                            BottomLayer 0603R                  19.9390      97.5360      90       "Resistor 0402 / 0603 / 0805"                                                       
R33        4K7                            BottomLayer 0603R                  18.6690      97.5360      90       "Resistor 0402 / 0603 / 0805"                                                       
R37        2K7                            BottomLayer 0603R                  49.5300      95.7580      360      "Resistor 0402 / 0603 / 0805"                                                       
R25        4K7                            BottomLayer 0603R                  32.2580      107.6960     90       Resistor                                                                            
R155       47K                            BottomLayer 0603R                  19.3040      11.9380      270      Resistor                                                                            
R157       47K                            BottomLayer 0603R                  10.0330      9.3980       270      Resistor                                                                            
R48        47K                            BottomLayer 0603R                  18.1610      80.0100      90       Resistor                                                                            
R47        47K                            BottomLayer 0603R                  19.5580      80.0100      270      Resistor                                                                            
R124       2K2                            BottomLayer 0603R                  18.0340      32.8930      360      Resistor                                                                            
R121       2K2                            BottomLayer 0603R                  18.0340      34.1630      360      Resistor                                                                            
R142       1K5                            BottomLayer 0603R                  33.7820      17.0180      90       Resistor                                                                            
R140       1K5                            BottomLayer 0603R                  36.0680      17.0180      90       Resistor                                                                            
R154       10K                            BottomLayer 0603R                  20.8280      11.9380      270      Resistor                                                                            
R35        100                            BottomLayer 0603R                  23.8760      111.6330     90       "Resistor 0402 / 0603 / 0805"                                                       
R119       [N/A]                          BottomLayer 0603R                  51.6890      35.8140      270      Resistor                                                                            
R31        [N/A]                          BottomLayer 0603R                  21.2090      97.5360      90       "Resistor 0402 / 0603 / 0805"                                                       
R144       [N/A]                          BottomLayer 0603R                  29.5910      17.0180      270      Resistor                                                                            
R59        100K                           BottomLayer 0603R                  54.3560      44.1960      90       Resistor                                                                            
R8         100K                           BottomLayer 0603R                  38.7350      117.4750     360      Resistor                                                                            
R26        100K                           BottomLayer 0603R                  19.1770      105.6640     360      "Resistor 0402 / 0603 / 0805"                                                       
R42        100K                           BottomLayer 0603R                  43.9420      90.4240      360      Resistor                                                                            
R30        100K                           BottomLayer 0603R                  22.4790      97.5360      270      "Resistor 0402 / 0603 / 0805"                                                       
R27        100K                           BottomLayer 0603R                  32.2580      104.6480     270      "Resistor 0402 / 0603 / 0805"                                                       
R1         10K                            TopLayer    0603R                  10.0330      121.0310     0        Resistor                                                                            
R153       330                            BottomLayer 0603R                  27.6860      11.9380      270      Resistor                                                                            
R158       680                            BottomLayer 0603R                  8.5090       9.3980       90       Resistor                                                                            
R161       0                              BottomLayer 0603R                  24.8920      6.9850       270      Resistor                                                                            
R46        0                              BottomLayer 0603R                  20.9550      80.0100      270      Resistor                                                                            
R49        510                            BottomLayer 0603R                  11.4300      80.0100      360      Resistor                                                                            
R143       510                            BottomLayer 0603R                  31.1150      17.0180      270      Resistor                                                                            
R15        100                            BottomLayer 0603R                  26.2890      114.6810     270      "Resistor 0402 / 0603 / 0805"                                                       
R17        100                            BottomLayer 0603R                  54.2290      114.5540     270      Resistor                                                                            
R41        0                              BottomLayer 0603R                  10.2870      91.4400      270      Resistor                                                                            
R159       0                              BottomLayer 0603R                  22.8600      9.0170       360      Resistor                                                                            
R160       0                              BottomLayer 0603R                  19.9390      9.0170       360      Resistor                                                                            
R151       0                              BottomLayer 0603R                  11.5570      12.4968      90       Resistor                                                                            
R156       0                              BottomLayer 0603R                  11.5570      9.3980       270      Resistor                                                                            
R23        0                              BottomLayer 0603R                  6.8580       108.4580     360      Resistor                                                                            
R21        0                              BottomLayer 0603R                  54.2290      111.5060     270      Resistor                                                                            
R123       0                              BottomLayer 0603R                  21.9710      33.6550      270      Resistor                                                                            
R131       0                              BottomLayer 0603R                  23.3680      24.8920      360      Resistor                                                                            
R135       0                              BottomLayer 0603R                  42.4180      17.0180      270      Resistor                                                                            
R87        0                              BottomLayer 0603R                  47.4980      40.1320      90       Resistor                                                                            
R43        [N/A]                          BottomLayer 0603R                  10.0330      12.4968      270      Resistor                                                                            
C18        1uF                            BottomLayer 0603C                  11.6840      91.3130      270      Capacitor                                                                           
C38        1uF                            BottomLayer 0603C                  34.4170      66.0400      360      Capacitor                                                                           
C33        1uF                            BottomLayer 0603C                  36.7030      72.5170      270      Capacitor                                                                           
C31        1uF                            BottomLayer 0603C                  15.2400      80.1370      270      Capacitor                                                                           
C11        10pF                           BottomLayer 0603C                  26.1620      97.5360      270      "Capacitor 0402 / 0603 / 0805"                                                      
C39        10nF                           BottomLayer 0603C                  36.8300      65.2780      90       "0603  X7R 10NF"                                                                    
C21        22nF                           BottomLayer 0603C                  14.3510      91.1860      90       Capacitor,22nF,50V,X7R,10%,0603,YAGEO                                               
C27        150pF_NPO_5%_0603              BottomLayer 0603C                  21.7170      83.9470      360      Capacitor,150pF,50V,NPO,5%,0603,YAGEO                                               
C4         [N/A]                          BottomLayer 0603C                  15.2400      115.4430     360      Capacitor                                                                           
C24        150pF_NPO_5%_0603              BottomLayer 0603C                  21.7170      85.3440      360      Capacitor,150pF,50V,NPO,5%,0603,YAGEO                                               
C63        10nF                           BottomLayer 0603C                  48.6410      44.8310      360      Capacitor                                                                           
C66        10nF                           BottomLayer 0603C                  57.0230      36.5760      360      Capacitor                                                                           
C20        22nF                           BottomLayer 0603C                  15.7480      91.1860      90       Capacitor,22nF,50V,X7R,10%,0603,YAGEO                                               
C94        3.0pF                          BottomLayer 0603C                  20.9550      22.3520      90       Capacitor                                                                           
C93        3.0pF                          BottomLayer 0603C                  20.9550      19.3040      270      Capacitor                                                                           
C19        1uF                            BottomLayer 0603C                  20.8280      91.1860      270      Capacitor                                                                           
C22        1uF                            BottomLayer 0603C                  10.9220      88.5190      360      Capacitor                                                                           
C10        10pF                           BottomLayer 0603C                  27.6860      97.5360      270      "Capacitor 0402 / 0603 / 0805"                                                      
C83        8.2pF                          BottomLayer 0603C                  23.3680      27.8130      360      Capacitor                                                                           
C85        8.2pF                          BottomLayer 0603C                  23.3680      26.2890      360      Capacitor                                                                           
C13        [N/A]                          BottomLayer 0603C                  11.0490      94.1070      360      Capacitor                                                                           
C26        20pF                           BottomLayer 0603C                  22.6060      111.6330     270      Capacitor,20pF,50V,NPO,5%,0402,YAGEO                                                
C96        2.2uF                          BottomLayer 1206C                  46.2280      18.1610      270      Capacitor                                                                           
C76        2.2uF                          BottomLayer 1206C                  47.1170      35.8140      90       Capacitor                                                                           
C61        4.7uF/10V                      BottomLayer 1206C                  47.8790      46.7360      360      "Polarized Capacitor (Radial)"                                                      
C79        4.7uF/50V                      BottomLayer 1206C                  56.6420      32.3850      360      Capacitor                                                                           
C81        2.2uF                          BottomLayer 1206C                  47.1170      30.8610      90       Capacitor                                                                           
C60        4.7uF                          BottomLayer CPOL_TAJ-A_1206_H180   23.3680      48.1330      270      "Capacitor, Tantalum, 4.7uF, 16V, 10%, 4ohms, pkg Type_A (3216 metric), T=1.6mm"    
C35        10uF                           BottomLayer CPOL_TAJ-A_1206_H180   42.1640      71.5010      360      "Capacitor, Tantalum, 10uF, 16V, 10%, 3Ohms, pkg Type_A (3216 metric), T=1.6mm"     
C32        10uF                           BottomLayer CPOL_TAJ-A_1206_H180   12.9540      75.1840      360      "Capacitor, Tantalum, 10uF, 16V, 10%, 3Ohms, pkg Type_A (3216 metric), T=1.6mm"     
C29        10uF                           BottomLayer CPOL_TAJ-A_1206_H180   26.5430      82.2960      180      "Capacitor, Tantalum, 10uF, 16V, 10%, 3Ohms, pkg Type_A (3216 metric), T=1.6mm"     
C37        10uF                           BottomLayer CPOL_TAJ-A_1206_H180   21.5900      71.6280      90       "Capacitor, Tantalum, 10uF, 16V, 10%, 3Ohms, pkg Type_A (3216 metric), T=1.6mm"     
C65        1uF                            BottomLayer CPOL_TAJ-A_1206_H180   25.4000      36.9570      180      "Capacitor, Tantalum, 1uF, 16V, 10%, 11Ohms, pkg Type_A (3216 metric), T=1.6mm"     
C82        "4.7uF 16V"                    BottomLayer CPOL_TAJ-A_1206_H180   54.1020      28.0670      360      "Capacitor, Tantalum, 4.7uF, 16V, 10%, 4ohms, pkg Type_A (3216 metric), T=1.6mm"    
C101       "4.7uF 16V"                    BottomLayer CPOL_TAJ-A_1206_H180   16.8910      8.7630       90       "Capacitor, Tantalum, 4.7uF, 16V, 10%, 4ohms, pkg Type_A (3216 metric), T=1.6mm"    
C86        1uF                            BottomLayer CPOL_TAJ-A_1206_H180   46.9800      25.6950      270      "Capacitor, Tantalum, 1uF, 16V, 10%, 11Ohms, pkg Type_A (3216 metric), T=1.6mm"     
C80        1uF                            BottomLayer CPOL_TAJ-A_1206_H180   25.4000      31.6230      180      "Capacitor, Tantalum, 1uF, 16V, 10%, 11Ohms, pkg Type_A (3216 metric), T=1.6mm"     
C56        10uF                           BottomLayer CPOL_TAJ-A_1206_H180   47.8790      49.1490      180      "Capacitor, Tantalum, 10uF, 16V, 10%, 3Ohms, pkg Type_A (3216 metric), T=1.6mm"     
C15        10uF                           BottomLayer CPOL_TAJ-A_1206_H180   19.0000      92.2000      90       "Capacitor, Tantalum, 10uF, 16V, 10%, 3Ohms, pkg Type_A (3216 metric), T=1.6mm"     
C98        4.7uF                          BottomLayer CPOL_TAJ-A_1206_H180   26.9240      15.8750      270      "Capacitor, Tantalum, 4.7uF, 16V, 10%, 4ohms, pkg Type_A (3216 metric), T=1.6mm"    
C41        100nF                          BottomLayer 0402C                  16.6370      66.2940      360      Capacitor                                                                           
C3         100nF                          BottomLayer 0402C                  14.9860      117.8560     90       Capacitor                                                                           
C2         100nF                          TopLayer    0402C                  28.7020      3.3020       180      Capacitor                                                                           
C77        100nF                          BottomLayer 0402C                  25.4000      35.1790      360      Capacitor                                                                           
C67        100nF                          BottomLayer 0402C                  44.0690      36.5760      90       Capacitor                                                                           
C72        100nF                          BottomLayer 0402C                  31.3690      36.5760      90       Capacitor                                                                           
C88        100nF                          BottomLayer 0402C                  26.7970      25.2730      360      Capacitor                                                                           
C90        100nF                          BottomLayer 0402C                  26.7970      22.7330      360      Capacitor                                                                           
C87        100nF                          BottomLayer 0402C                  49.0220      25.4000      90       Capacitor                                                                           
C68        100nF                          BottomLayer 0402C                  41.4020      36.5760      90       Capacitor                                                                           
C91        100nF                          BottomLayer 0402C                  26.7970      21.5900      360      Capacitor                                                                           
C73        100nF                          BottomLayer 0402C                  30.3530      36.5760      90       Capacitor                                                                           
C92        100nF                          BottomLayer 0402C                  26.7970      20.3200      360      Capacitor                                                                           
C70        100nF                          BottomLayer 0402C                  36.4490      36.5760      90       Capacitor                                                                           
C46        100nF                          BottomLayer 0402C                  32.6390      62.1030      90       Capacitor                                                                           
C43        100nF                          BottomLayer 0402C                  39.3700      62.1030      90       Capacitor                                                                           
C45        100nF                          BottomLayer 0402C                  34.1630      62.1030      90       Capacitor                                                                           
C59        100nF                          BottomLayer 0402C                  33.0200      49.5300      360      Capacitor                                                                           
C51        100nF                          BottomLayer 0402C                  45.4660      56.5150      360      Capacitor                                                                           
C44        100nF                          BottomLayer 0402C                  37.5920      62.1030      90       Capacitor                                                                           
C58        100nF                          BottomLayer 0402C                  39.1160      49.0220      270      Capacitor                                                                           
C42        100nF                          BottomLayer 0402C                  40.5130      62.1030      90       Capacitor                                                                           
C7         100nF                          BottomLayer 0402C                  19.3040      107.6960     360      "Capacitor 0402 / 0603 / 0805"                                                      
C5         100nF                          BottomLayer 0402C                  29.0830      110.7440     360      "Capacitor 0402 / 0603 / 0805"                                                      
C8         100nF                          BottomLayer 0402C                  32.2580      101.9810     270      "Capacitor 0402 / 0603 / 0805"                                                      
C9         100nF                          BottomLayer 0402C                  31.6230      97.5360      90       "Capacitor 0402 / 0603 / 0805"                                                      
C40        100nF                          BottomLayer 0402C                  34.5440      64.3890      360      "Capacitor 0402 / 0603 / 0805"                                                      
C14        100nF                          BottomLayer 0402C                  48.6410      93.0910      90       "Capacitor 0402 / 0603 / 0805"                                                      
C12        100nF                          BottomLayer 0402C                  25.0190      97.5360      90       "Capacitor 0402 / 0603 / 0805"                                                      
C17        100nF                          BottomLayer 0402C                  13.0810      91.3130      90       Capacitor                                                                           
C16        100nF                          BottomLayer 0402C                  17.0180      91.3130      90       Capacitor                                                                           
C30        100nF                          BottomLayer 0402C                  16.5100      80.3910      270      Capacitor                                                                           
C1         100nF                          TopLayer    0402C                  12.7000      121.1580     180      Capacitor                                                                           
C6         100nF                          BottomLayer 0402C                  58.1660      107.9500     270      Capacitor                                                                           
C62        100nF                          BottomLayer 0402C                  20.8280      46.3550      360      Capacitor                                                                           
C53        100nF                          BottomLayer 0402C                  23.3680      52.7050      360      Capacitor                                                                           
C55        100nF                          BottomLayer 0402C                  47.7520      51.0540      360      Capacitor                                                                           
C97        100nF                          BottomLayer 0402C                  49.9110      17.6530      360      Capacitor                                                                           
C64        100nF                          BottomLayer 0402C                  48.6410      43.4340      360      Capacitor                                                                           
C25        100nF                          BottomLayer 0402C                  10.9220      85.3440      360      Capacitor                                                                           
C23        100nF                          BottomLayer 0402C                  10.9220      86.8680      360      Capacitor                                                                           
C34        100nF                          BottomLayer 0402C                  34.9250      72.2630      270      "Capacitor 0402 / 0603 / 0805"                                                      
C49        100nF                          BottomLayer 0402C                  45.4660      57.6580      360      Capacitor                                                                           
C57        100nF                          BottomLayer 0402C                  42.5450      49.0220      270      Capacitor                                                                           
C52        100nF                          BottomLayer 0402C                  27.0510      53.9750      360      Capacitor                                                                           
C48        100nF                          BottomLayer 0402C                  27.0510      57.9120      360      Capacitor                                                                           
C47        100nF                          BottomLayer 0402C                  30.8610      62.1030      90       Capacitor                                                                           
C50        100nF                          BottomLayer 0402C                  27.0510      56.6420      360      Capacitor                                                                           
C89        100nF                          BottomLayer 0402C                  26.7970      24.0030      360      Capacitor                                                                           
C95        100nF                          BottomLayer 0402C                  26.7970      19.0536      360      Capacitor                                                                           
C69        100nF                          BottomLayer 0402C                  38.7350      36.5760      90       Capacitor                                                                           
C74        100nF                          BottomLayer 0402C                  28.8290      36.5760      90       Capacitor                                                                           
C78        100nF                          BottomLayer 0402C                  25.4000      33.6550      360      Capacitor                                                                           
C75        100nF                          BottomLayer 0402C                  20.5740      36.5760      270      Capacitor                                                                           
C71        100nF                          BottomLayer 0402C                  34.0360      36.5760      90       Capacitor                                                                           
C84        100nF                          BottomLayer 0402C                  26.7970      26.5430      360      Capacitor                                                                           
C54        100nF                          BottomLayer 0402C                  23.3680      51.5620      360      Capacitor                                                                           
B1         CTSM-644N-V-T/R                BottomLayer PB10                   19.4310      122.3010     360      "Push-Button BLACK"                                                                 
B2         CTSM-644B-V-T/R                BottomLayer PB10                   7.2390       113.2840     360      "Push-Button BLUE"                                                                  
SB1        "Closed by default"            BottomLayer SB_0603                18.7960      118.3640     360      "Circuit Breaker"                                                                   
SB2        "Closed by default"            BottomLayer SB_0603                18.7960      116.8400     180      "Circuit Breaker"                                                                   
SB3        "Closed by default"            BottomLayer SB_0603                25.7810      111.6330     270      "Circuit Breaker"                                                                   
SB6        "Closed by default"            BottomLayer SB_0603                38.9890      17.0180      90       "Circuit Breaker"                                                                   
SB12       "Closed by default"            BottomLayer SB_0603                48.1330      56.3880      180      "Circuit Breaker"                                                                   
SB10       "Closed by default"            BottomLayer SB_0603                48.1330      59.5630      180      "Circuit Breaker"                                                                   
SB5        "Closed by default"            BottomLayer SB_0603                11.4300      81.4070      360      "Circuit Breaker"                                                                   
SB14       "Closed by default"            BottomLayer SB_0603                49.1490      28.1940      270      "Circuit Breaker"                                                                   
SB15       "Closed by default"            BottomLayer SB_0603                32.5120      17.0180      90       "Circuit Breaker"                                                                   
SB13       "Open by default"              BottomLayer SB_0603                50.0380      53.2130      90       "Circuit Breaker"                                                                   
SB7        "Open by default"              BottomLayer SB_0603                38.9890      13.9700      270      "Circuit Breaker"                                                                   
SB11       "Open by default"              BottomLayer SB_0603                48.1330      57.9120      180      "Circuit Breaker"                                                                   
SB9        "Open by default"              BottomLayer SB_0603                48.1330      61.2140      180      "Circuit Breaker"                                                                   
SB4        "Open by default"              BottomLayer SB_0603                23.7490      97.5360      270      "Circuit Breaker"                                                                   
SB8        "Closed by default"            BottomLayer SB_0603                16.6370      64.5160      360      "Circuit Breaker"                                                                   
SB16       "Open by default"              BottomLayer SB_0603                30.8610      111.5060     90       "Circuit Breaker"                                                                   
SB18       "Closed by default"            TopLayer    SB_0603                45.3390      5.8420       270      "Circuit Breaker"                                                                   
SB19       "Open by default"              BottomLayer SB_0603                23.3680      18.5420      180      "Circuit Breaker"                                                                   
SB17       "opened by default"            TopLayer    SB_0603                9.1440       124.8410     0        "Circuit Breaker"                                                                   
C36        10uF(25V)                      BottomLayer CPOL_TAJ-B_1210_H210   48.5140      66.6750      90       "Capacitor, Tantalum, 10uF, 25V, 10%, 2.5ohms, pkg Type_B (3528 metric), T=1.9mm"   
U10        LD1117S50TR                    BottomLayer SOT-223                42.2910      66.8020      270      ""                                                                                  
U8         LD1117S18TR                    BottomLayer SOT-223                13.7160      70.4850      270      ""                                                                                  
U7         LD1117S33TR                    BottomLayer SOT-223                27.0510      74.2950      360      "LOW DROP FIXED AND ADJUSTABLE POSITIVE VOLTAGE REGULATORS (3.3 Volts)"             
LD6        67-22sursygc-s530-a2-tr8       BottomLayer LED2_3528              56.8046      112.2670     360      ""                                                                                  
LD2        Orange                         TopLayer    0603D                  21.9710      124.2060     270      "Typical RED, GREEN, YELLOW, AMBER GaAs LED"                                        
LD5        red                            BottomLayer 0603D                  46.1010      117.4750     360      "Typical RED, GREEN, YELLOW, AMBER GaAs LED"                                        
LD4        Blue                           TopLayer    0603D                  31.3690      124.2060     270      "Typical RED, GREEN, YELLOW, AMBER GaAs LED"                                        
LD9        Red                            BottomLayer 0603D                  9.2710       7.1120       360      "Typical RED, GREEN, YELLOW, AMBER GaAs LED"                                        
LD3        Red                            TopLayer    0603D                  26.6700      124.2060     270      "Typical RED, GREEN, YELLOW, AMBER GaAs LED"                                        
LD8        Green                          TopLayer    0603D                  24.8920      7.7470       270      "Typical RED, GREEN, YELLOW, AMBER GaAs LED"                                        
LD7        Green                          BottomLayer 0603D                  11.4300      78.6130      360      "Typical RED, GREEN, YELLOW, AMBER GaAs LED"                                        
LD1        Green                          TopLayer    0603D                  17.2720      124.2060     270      "Typical RED, GREEN, YELLOW, AMBER GaAs LED"                                        
L4         4.7uH(1A)                      BottomLayer 1210L                  51.0540      40.1320      270      Inductor                                                                            
X3         NX3215SA-32.768K               BottomLayer XTAL_2SM_3R2X1R5       18.5420      20.9550      90       "Crystal 32.768kHz, 6pF, -+20PPM, R=50K, SMD"                                       
Z1         STPS1L40M                      BottomLayer DO-216AA               50.9270      32.3850      360      "Schottky Diode"                                                                    
L3         BEAD                           BottomLayer 0603L                  51.3080      47.4980      270      Inductor                                                                            
L5         BEAD(FCM1608KF-601T03)         BottomLayer 0603L                  21.9710      36.8300      270      Inductor                                                                            
L1         BEAD(FCM1608KF-601T03)         BottomLayer 0603L                  48.5140      53.2130      270      Inductor                                                                            
L2         BEAD(FCM1608KF-601T03)         BottomLayer 0603L                  46.7360      53.2130      270      Inductor                                                                            
D1         BAT60JFILM                     BottomLayer SOD-323                32.1310      114.6810     270      BAT60JFILM                                                                          
D4         BAT60JFILM                     BottomLayer SOD-323                43.6880      87.5030      270      BAT60JFILM                                                                          
D2         BAT60JFILM                     BottomLayer SOD-323                47.7520      87.5030      270      BAT60JFILM                                                                          
D3         BAT60JFILM                     BottomLayer SOD-323                45.7200      87.5030      270      BAT60JFILM                                                                          
CN12       TSM-108-01-X-DV                BottomLayer TSM-108-01-X-DV        38.6080      5.5880       360      "Header, 8-Pin, Dual row"                                                           
CN4        [N/A]                          BottomLayer HDR_2X3-1_2R54-6       34.0360      86.1060      360      "Header, 3-Pin, Dual row"                                                           
CN1        USB-MINI-typeB                 BottomLayer MINIUSB_AB_5SM_RA      31.3180      122.0260     360      "USB-MINI-typeB connector"                                                          
CN6        SSW-108-22-X-S-VS              BottomLayer SSW-108-22-X-S-VS      54.1020      76.5810      270      "Header, 8-Pin, Single row,female"                                                  
CN7        SSW-108-22-X-S-VS              BottomLayer SSW-108-22-X-S-VS      5.8420       58.8010      90       "Header, 8-Pin, Single row,female"                                                  
CN8        "SAMTEC SSW-106-22-x-S-VS"     BottomLayer SSW-106-22-X-S-VS      54.1020      56.2610      270      "Header, 6-Pin, Single row,female SMD"                                              
CN2        FH19C-6S-05SH                  BottomLayer FH19C-6S-0R5SH_FPC_CPT 56.2724      103.7588     90       "ZIF connector placed bottom side"                                                  
CN13       475900001                      BottomLayer MOLEX_47590001         21.7170      2.8702       360      ""                                                                                  
JP5        TSM-102-01-X-SV                BottomLayer TSM-102-01-X-SV        11.8110      3.6830       270      ""                                                                                  
JP1        TSM-102-01-X-SV                BottomLayer TSM-102-01-X-SV        10.5410      122.3010     360      ""                                                                                  
U5         CS43L22                        BottomLayer QFN40_0R5_6X6          16.1290      85.5980      360      "Low Power, Stereo DAC w/Headphone & Speaker Amps"                                  
CN10       FH26-25S-0.3SHW                BottomLayer FPC25_FPC03025-1420    53.6250      21.7168      270      "ZIF connector placed bottom side"                                                  
D5         EMIF02-USB03F2                 BottomLayer BGA11_0R5_1R57X2R07    21.8948      7.2390       90       "2-line IPAD, EMI filter including ESD protection"                                  
CN5        SSW-110-22-X-S-VS              BottomLayer SSW-110-22-X-S-VS      5.8420       83.1850      90       "Header, 10-Pin, Single row,female"                                                 
U13        STLD40DPUR                     BottomLayer SON8_0R65_3X3          55.1180      40.2590      360      ""                                                                                  
U12        "MICRON MT25QL128ABA1EW9-0SIT" BottomLayer ICC_W-PDFN-8_8X6_P127  15.1250      48.2550      360      "128Mb, 3V, Multiple I/O Serial Flash Memory, Quad/Dual"                            
CN3        PJ3028B-3                      BottomLayer PJ3028B                9.1280       102.1080     360      ""                                                                                  
JP2        TSM-103-01-X-DV                BottomLayer TSM-103-01-X-DV        44.7040      122.1740     270      "Header, 3-Pin, Dual row"                                                           
U9         LD3985M33R                     BottomLayer SOT23-5                35.8140      69.0880      360      "Ultra low drop-low noise BiCMOS voltage, regulators low ESR capacitors compatible" 
U16        STMPS2151STR                   BottomLayer SOT23-5                13.9700      8.7630       360      ""                                                                                  
T3         9013                           BottomLayer SOT-23                 23.4950      12.0650      90       "NPN Bipolar Transistor"                                                            
T1         9013                           BottomLayer SOT-23                 22.2250      114.9350     270      "NPN Bipolar Transistor"                                                            
H3         "POSITION HOLE"                TopLayer    HOLE_C5R5D3            4.1910       4.1910       0        ""                                                                                  
H4         "POSITION HOLE"                TopLayer    HOLE_C5R5D3            55.8089      4.1910       0        ""                                                                                  
H2         "POSITION HOLE"                TopLayer    HOLE_C5R5D3            55.8089      122.8088     0        ""                                                                                  
H1         "POSITION HOLE"                TopLayer    HOLE_C5R5D3            4.1910       122.8088     0        ""                                                                                  
U14        STM32F469NIH6                  BottomLayer BGA216_0R8_13X13       36.4490      27.0510      360      ""                                                                                  
TP3        TP                             BottomLayer TP_C40                 30.9880      39.8780      270      ""                                                                                  
TP4        TP                             BottomLayer TP_C40                 26.9240      59.6900      270      ""                                                                                  
TP1        TP                             BottomLayer TP_C40                 33.0200      39.8780      270      ""                                                                                  
TP2        TP                             BottomLayer TP_C40                 19.9390      43.1800      270      ""                                                                                  
TP5        TP                             BottomLayer TP_C40                 20.9550      48.5140      270      ""                                                                                  
TP6        TP                             BottomLayer TP_C40                 20.9550      50.5460      270      ""                                                                                  
TP7        TP                             BottomLayer TP_C40                 8.7630       48.0060      270      ""                                                                                  
X2         NX3225GD-8.00M                 BottomLayer XTAL_2SM_3R2X2R5_H1    18.2880      26.0350      270      "Crystal 8Mhz, 8pF, -+50PPM, SMD"                                                   
X1         NX3225GD-8.00M                 BottomLayer XTAL_2SM_3R2X2R5_H1    27.6860      93.9800      360      "Crystal 8Mhz, 8pF, -+50PPM, SMD"                                                   
