BOARD : 720p x 1280 DSI 2 lanes LCD
NUMBER : MB1230
REV. : C
BE TECH 07/12/2017 

PHOTOPLOT IN RS274-X FORMAT

  GERBER PARAMETERS:
	ASCII CODE
	UNITS : MILLIMETERS
	ABSOLUTE COORDINATES
	5 INTEGER DIGITS
	5 DECIMAL DIGITS
	LEADING ZERO SUPPRESSION
 
  MB1230C-FC.GBR       ---> TOP SIDE GERBER FILE (1)
  MB1230C-F2.GBR       ---> LAYER 2 GERBER FILE 
  MB1230C-F3.GBR       ---> LAYER 3 GERBER FILE
  MB1230C-FS.GBR       ---> BOTTOM SIDE GERBER FILE   (4)
  MB1230C-VEC.GBR      ---> TOP SIDE SOLDER MASK GERBER FILE
  MB1230C-VES.GBR      ---> BOTTOM SIDE SOLDER MASK GERBER FILE
  MB1230C-BOARD.GBR    ---> BOARD OUTLINE GERBER FILE
  MB1230C-SERC.GBR     ---> TOP SIDE SILK SCREEN GERBER FILE	
  MB1230C-SERS.GBR     ---> BOTTOM SIDE SILK SCREEN GERBER FILE	
  MB1230C-PSTC.GBR     ---> TOP SIDE SOLDER PASTE GERBER FILE
  MB1230C-PSTS.GBR     ---> BOTTOM SIDE SOLDER PASTE GERBER FILE
  MB1230C-USI.GBR      ---> DRILL DRAWING GERBER FILE

 ADDITIONAL NON FUNCTIONAL COPPER POUR (Copper Balance) IS NOT ALLOWED  (copper pouring in prohibited areas may occur).
 IN CASE OF PARTICULAR REQUEST ABOUT COPPER FILLING , PLEASE CONTACT US BEFORE PROCESSING  

  INTERNAL LAYERS TEAR DROPS WILL BE ADDED OR OPTIMIZED BY BOARD MANUFACTURER

  STANDARD COMPONENTS SOLDER PASTE OPENINGS ARE DEFINED WITH SAME DIMENSIONS AS RELATED COPPER PADS.
  THEY ARE REDUCED FOR SPECIFIC CASES SUCH AS QFN THERMAL PADS (ABOUT 70%) AND WIDE PADS (SEGMENTED PASTE SLOTS)
  
  INTERNAL LAYERS UNUSED PADS CAN BE SUPPRESSED.


DRILL 

  DRILL FILE PARAMETERS :
	TYPE : EXCELLON
	ASCII CODE
	UNITS : MILLIMETERS
	ABSOLUTE COORDINATES
	5 INTEGER DIGITS
	4 DECIMAL DIGITS
	LEADING ZERO SUPPRESSION

  MB1230C-PLATED.DRL    ---> PLATED THROUGH HOLES DRILL FILE
  MB1230C-UNPLATED.DRL  ---> UN-PLATED THROUGH HOLES DRILL FILE
  MB1230C-DRILL.DDR     ---> DRILL REPORT


