BOARD : 720p x 1280 DSI 2 lanes LCD
NUMBER : MB1230
REV. : C
BE TECH 07/12/2017 

PHOTOPLOT IN RS274-X FORMAT

  GERBER PARAMETERS:
	ASCII CODE
	UNITS : MILLIMETERS
	ABSOLUTE COORDINATES
	5 INTEGER DIGITS
	5 DECIMAL DIGITS
	LEADING ZERO SUPPRESSION
 
  MB1230C-PSTC.GBR     ---> TOP SIDE SOLDER PASTE GERBER FILE
  MB1230C-PSTS.GBR     ---> BOTTOM SIDE SOLDER PASTE GERBER FILE


  STANDARD COMPONENTS SOLDER PASTE OPENINGS ARE DEFINED WITH SAME DIMENSIONS AS RELATED COPPER PADS.
  THEY ARE REDUCED FOR SPECIFIC CASES SUCH AS QFN THERMAL PADS (ABOUT 70%) AND WIDE PADS (SEGMENTED PASTE SLOTS)
  

ASSEMBLY 


  MB1230C-ASMC.PDF          ---> TOP SIDE ASSEMBLY DRAWING
  MB1230C-ASMS.PDF          ---> BOTTOM SIDE ASSEMBLY DRAWING
  

  MB1230C-CADIF.PAF      ---> CADIF DATABASE EXTRACT

  mb1230 bom_C01.XLSX        ---> BILL OF MATERIAL

  MB1230C-PLACE_TOP.LOC     ---> TOP SIDE SMT DEVICES COORD./ORIENT.
  MB1230C-PLACE_BOT.LOC     ---> BOTTOM SIDE SMT DEVICES COORD./ORIENT.

