Altium Designer Pick and Place Locations
D:\Virgil\Altium\STM\Projets\MB1274E\BASE\MB1274E\.\Generate Files\Pick Place for MB1274E.txt

========================================================================================================================
File Design Information:

Date:       08/04/17
Time:       04:13
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator     Comment       Layer       Footprint                                            Center-X(mm) Center-Y(mm) Rotation Description                                                                       
U21            U21           BottomLayer ESD_QFN2_1P6X1_P125                                  41.225       6.400        180      High power transient voltage suppressor, 7V breakdown                             
CARTOUCHE-BOT1 CARTOUCHE-BOT TopLayer    CARTOUCHE_STM_BOTTOM                                 -50.800      -66.200      0                                                                                          
CARTOUCHE-TOP1 CARTOUCHE-TOP TopLayer    CARTOUCHE_STM_TOP                                    -50.800      -66.200      0                                                                                          
U11            .Designator   TopLayer    ICC_W-CSP-BGA72_4P511X4P023_P050                     15.650       68.350       270      Multi-Channel Audio Hub CODEC for Smartphones                                     
CN11           .Designator   BottomLayer CON_TAG-C_TC2050-IDC-NL                              63.100       72.500       180      Tag_Connector Header, 10-Pin, Dual row No legs                                    
R76            R76           TopLayer    R0402                                                26.825       3.925        90       Resistor,10K,0402,1%,YAGEO                                                        
R75            R75           TopLayer    R0402                                                22.200       3.925        90       Resistor,10K,0402,1%,YAGEO                                                        
R77            R77           TopLayer    R0402                                                28.050       3.925        270      Resistor,10K,0402,1%,YAGEO                                                        
R78            R78           TopLayer    R0402                                                29.500       3.925        270      Resistor,10K,0402,1%,YAGEO                                                        
CN13           CN13          BottomLayer CON_SAMTEC_TSW-102-07-G-S                            53.555       52.500       180      Header 2 pins                                                                     
CN4            CN4           TopLayer    CON_SAMTEC_TSW-102-07-G-S                            3.500        86.950       360      Header 2 pins                                                                     
CN3            CN3           TopLayer    CON_SAMTEC_TSW-102-07-G-S                            3.500        90.200       360      Header 2 pins                                                                     
X1             .Designator   TopLayer    CRY_NX3225GD_2P                                      50.075       77.700       180      Crystal 8Mhz, 8pF, -+50PPM, SMD                                                   
X2             .Designator   TopLayer    CRY_NX3225GD_2P                                      28.450       60.550       180      Crystal 8Mhz, 8pF, -+50PPM, SMD                                                   
X3             .Designator   TopLayer    CRY_NX3215SA_2P                                      35.950       59.350       180      Crystal 32.768kHz, 6pF, -+20PPM, R=50K, SMD                                       
U8             .Designator   TopLayer    ICC_TSSOP16_5P1X4P5_P065                             27.200       81.500       180      SPDT analog switch 4-Channel 2:1 bidirectional                                    
U20            .Designator   BottomLayer ESD_ST0201                                           46.175       5.875        360      Dual Transil array for ESD protection                                             
U4             .Designator   TopLayer    REG_SOT223-TAB                                       43.575       96.675       180      LOW DROP FIXED AND ADJUSTABLE POSITIVE VOLTAGE REGULATORS (3.3 Volts)             
U3             .Designator   TopLayer    REG_SOT223-TAB                                       36.050       96.675       180      IC REG LDO 5V 0.8A SOT223                                                         
U10            .Designator   TopLayer    ICC_SO8_5X4_P127                                     46.050       69.875       90       1.2 A current limited high-side power switch with thermal shutdown                
U7             .Designator   TopLayer    REG_SOT23-5L                                         35.925       84.150       270      Ultra low drop-low noise BiCMOS voltage, regulators low ESR capacitors compatible 
U6             .Designator   TopLayer    ICC_LQFP48_7X7_P050                                  50.575       85.200       360      Medium-density performance line ARM-based 32-bit MCU with 128KB Flash             
U19            U19           BottomLayer ESD_SOT666                                           43.950       6.950        0        USB ESD protection                                                                
U15            .Designator   TopLayer    MOS_SOT23-5L                                         50.525       14.000       90       Enhanced single channel power switches                                            
U18            .Designator   BottomLayer ICC_QFN8-EPAD_3X3_P065                               63.300       28.000       180      White LED power supply for large display backlight, QFN8                          
U12            .Designator   TopLayer    REG_SOT23-5L                                         8.800        61.200       270      Ultra low drop-low noise BiCMOS voltage, regulators low ESR capacitors compatible 
U9             .Designator   TopLayer    ICC_V-PDFN-8_8X6_P127                                32.950       72.325       180      128Mb, 3V, Multiple I/O Serial Flash Memory, Quad/Dual                            
U14            U14           TopLayer    ICC_MINI-BGA48_6X8_P075                              20.600       24.050       270      IC SRAM 8MBIT 55NS 48MINIBGA 6mm x 8mm                                            
U13            U13           TopLayer    ICC_LQFP144_20X20_P050                               30.950       44.300       270      STM32 Tiny Manta 1M5 LQFP144 (STM32F413ZHT6U)                                     
TP21           TP21          TopLayer    TP_SMD_2MM                                           30.980       12.365       270      Test Point                                                                        
TP6            .Designator   TopLayer    TP_SMD_1MM                                           38.400       70.500       90       Test Point                                                                        
TP3            .Designator   TopLayer    TP_SMD_1MM                                           26.825       75.950       90       Test Point                                                                        
TP4            .Designator   TopLayer    TP_SMD_1MM                                           25.050       73.475       90       Test Point                                                                        
T1             .Designator   TopLayer    NPN_SOT23                                            61.425       94.650       270      NPN Bipolar Transistor                                                            
T3             .Designator   TopLayer    NPN_SOT23                                            53.975       9.350        270      NPN Bipolar Transistor                                                            
SB1            .Designator   TopLayer    SOLDER-BRIDGE_R0603-0R                               45.375       102.625      90       Solder Bridge ON                                                                  
SB13           .Designator   BottomLayer SOLDER-BRIDGE_R0603-0R                               26.200       87.350       270      Solder Bridge OFF                                                                 
SB4            .Designator   TopLayer    SOLDER-BRIDGE_R0603-0R                               46.050       73.500       180      Solder Bridge OFF                                                                 
SB22           .Designator   BottomLayer SOLDER-BRIDGE_R0603-0R                               51.675       21.100       270      Solder Bridge ON                                                                  
SB23           .Designator   BottomLayer SOLDER-BRIDGE_R0603-0R                               50.125       21.100       270      Solder Bridge OFF                                                                 
SB2            .Designator   TopLayer    SOLDER-BRIDGE_R0603-0R                               33.025       87.300       270      Solder Bridge ON                                                                  
SB3            .Designator   TopLayer    SOLDER-BRIDGE_R0603-0R                               54.875       77.900       90       Solder Bridge OFF                                                                 
SB16           .Designator   BottomLayer SOLDER-BRIDGE_R0603-0R                               65.625       80.825       270      Solder Bridge ON                                                                  
SB17           .Designator   BottomLayer SOLDER-BRIDGE_R0603-0R                               60.575       80.825       270      Solder Bridge ON                                                                  
SB18           .Designator   BottomLayer SOLDER-BRIDGE_R0603-0R                               58.725       80.825       270      Solder Bridge ON                                                                  
SB15           .Designator   BottomLayer SOLDER-BRIDGE_R0603-0R                               67.425       80.825       270      Solder Bridge ON                                                                  
SB24           .Designator   BottomLayer SOLDER-BRIDGE_R0603-0R                               7.450        21.300       360      Solder Bridge OFF                                                                 
SB21           .Designator   BottomLayer SOLDER-BRIDGE_R0603-0R                               7.450        22.650       360      Solder Bridge ON                                                                  
SB19           .Designator   BottomLayer SOLDER-BRIDGE_R0603-0R                               7.450        25.400       360      Solder Bridge ON                                                                  
SB20           .Designator   BottomLayer SOLDER-BRIDGE_R0603-0R                               7.450        24.050       360      Solder Bridge OFF                                                                 
SB5            .Designator   TopLayer    SOLDER-BRIDGE_R0603-0R                               63.000       59.100       90       Solder Bridge ON                                                                  
SB6            .Designator   TopLayer    SOLDER-BRIDGE_R0603-0R                               48.850       54.450       270      Solder Bridge ON                                                                  
SB7            .Designator   TopLayer    SOLDER-BRIDGE_R0603-0R                               16.075       52.725       270      Solder Bridge ON                                                                  
SB14           .Designator   BottomLayer SOLDER-BRIDGE_R0603-0R                               24.400       87.350       270      Solder Bridge ON                                                                  
R46            .Designator   TopLayer    R0402                                                33.000       58.050       90       Resistor,0R,0402,5%,YAGEO                                                         
R62            .Designator   TopLayer    R0402                                                24.550       20.075       360      Resistor,10K,0402,1%,YAGEO                                                        
R58            .Designator   TopLayer    R0603                                                31.475       27.825       90       Resistor,0R,0603,5%,YAGEO                                                         
R43            .Designator   TopLayer    R0603                                                40.050       58.400       90       Resistor,0R,0603,5%,YAGEO                                                         
R73            .Designator   TopLayer    R0402                                                56.375       4.000        270      Resistor,1K,0402,1%,YAGEO                                                         
R106           .Designator   BottomLayer R0402                                                68.325       17.350       180      Resistor,1K,0402,1%,YAGEO                                                         
R50            .Designator   TopLayer    R0402                                                29.300       57.400       360      Resistor,0R,0402,5%,YAGEO                                                         
R95            .Designator   BottomLayer R0603                                                7.850        57.700       360      Resistor,1K,0603,1%,YAGEO                                                         
R53            .Designator   TopLayer    R0402                                                44.750       51.950       90       Resistor,10K,0402,1%,YAGEO                                                        
R97            .Designator   BottomLayer R0402                                                65.500       87.850       360      Resistor,330R,0402,1%,YAGEO                                                       
R5             .Designator   TopLayer    R0402                                                61.200       98.125       180      Resistor,36K,0402,1%,YAGEO                                                        
R3             .Designator   TopLayer    R0402                                                56.050       98.700       90       Resistor,100K,0402,1%,YAGEO                                                       
R24            .Designator   TopLayer    R0402                                                42.025       72.225       270      Resistor,2K2,0402,1%,YAGEO                                                        
R4             .Designator   TopLayer    R0402                                                57.150       98.700       270      Resistor,1K5,0402,1%,YAGEO                                                        
R6             .Designator   TopLayer    R0402                                                61.200       97.050       360      Resistor,100R,0402,1%,YAGEO                                                       
R36            .Designator   TopLayer    R0402                                                43.500       66.425       180      Resistor,100K,0402,1%,YAGEO                                                       
R37            .Designator   TopLayer    R0402                                                48.600       66.425       360      Resistor,1K,0402,1%,YAGEO                                                         
R27            .Designator   TopLayer    R0402                                                50.200       70.075       270      Resistor,10K,0402,1%,YAGEO                                                        
R34            .Designator   TopLayer    R0402                                                65.725       67.500       180      Resistor,330R,0402,1%,YAGEO                                                       
R2             .Designator   TopLayer    R0402                                                60.300       99.200       360      Resistor,10K,0402,1%,YAGEO                                                        
R38            .Designator   TopLayer    R0402                                                65.725       66.000       180      Resistor,330R,0402,1%,YAGEO                                                       
R15            .Designator   TopLayer    R0603                                                56.875       82.450       180      Resistor,0R,0603,5%,YAGEO                                                         
R19            .Designator   TopLayer    R0603                                                56.325       78.050       90       Resistor,0R,0603,5%,YAGEO                                                         
R86            .Designator   BottomLayer R0402                                                52.575       81.100       270      Resistor,4K7,0402,1%,YAGEO                                                        
R87            .Designator   BottomLayer R0402                                                51.475       81.100       270      Resistor,4K7,0402,1%,YAGEO                                                        
R8             .Designator   TopLayer    R0402                                                52.825       90.900       360      Resistor,100R,0402,1%,YAGEO                                                       
R7             .Designator   TopLayer    R0402                                                51.275       91.200       90       Resistor,56R,0402,1%,YAGEO                                                        
R18            .Designator   TopLayer    R0402                                                53.625       78.400       270      Resistor,100K,0402,1%,YAGEO                                                       
R91            .Designator   BottomLayer R0603                                                60.575       78.025       90       Resistor,22R,0603,1%,Yageo                                                        
R92            .Designator   BottomLayer R0603                                                58.725       78.025       90       Resistor,22R,0603,1%,Yageo                                                        
R90            .Designator   BottomLayer R0603                                                65.625       78.025       90       Resistor,22R,0603,1%,Yageo                                                        
R89            .Designator   BottomLayer R0603                                                67.425       78.025       90       Resistor,22R,0603,1%,Yageo                                                        
R17            .Designator   TopLayer    R0402                                                47.475       78.400       270      Resistor,10K,0402,1%,YAGEO                                                        
R16            .Designator   TopLayer    R0402                                                46.425       78.400       270      Resistor,10K,0402,1%,YAGEO                                                        
R14            .Designator   TopLayer    R0402                                                44.125       84.450       360      Resistor,100K,0402,1%,YAGEO                                                       
R11            .Designator   TopLayer    R0402                                                44.125       85.500       180      Resistor,0R,0402,5%,YAGEO                                                         
R10            .Designator   TopLayer    R0402                                                44.125       86.550       180      Resistor,2K7,0402,1%,YAGEO                                                        
R9             .Designator   TopLayer    R0402                                                44.125       87.600       360      Resistor,4K7,0402,1%,YAGEO                                                        
R40            .Designator   TopLayer    R0402                                                62.425       63.025       360      Resistor,0R,0402,5%,YAGEO                                                         
R96            .Designator   BottomLayer R0402                                                65.500       56.700       180      Resistor,510R,0402,1%,YAGEO                                                       
R85            .Designator   BottomLayer R0402                                                11.825       92.150       90       Resistor,47K,0402,1%,YAGEO                                                        
R84            .Designator   BottomLayer R0402                                                12.925       92.150       90       Resistor,47K,0402,1%,YAGEO                                                        
R83            .Designator   BottomLayer R0402                                                17.350       92.150       90       Resistor,47K,0402,1%,YAGEO                                                        
R82            .Designator   BottomLayer R0402                                                18.450       92.150       90       Resistor,47K,0402,1%,YAGEO                                                        
R81            .Designator   BottomLayer R0402                                                19.550       92.150       90       Resistor,47K,0402,1%,YAGEO                                                        
R93            .Designator   BottomLayer R0402                                                65.500       59.675       360      Resistor,330R,0402,1%,YAGEO                                                       
R79            .Designator   BottomLayer R0603                                                10.200       98.900       90       Resistor,0R,0603,5%,YAGEO                                                         
R94            .Designator   BottomLayer R0402                                                65.500       58.175       180      Resistor,1K,0402,1%,YAGEO                                                         
R109           .Designator   BottomLayer R0402                                                65.150       9.025        360      Resistor,100K,0402,1%,YAGEO                                                       
R72            .Designator   TopLayer    R0402                                                61.850       8.575        360      Resistor,10K,0402,1%,YAGEO                                                        
R13            .Designator   TopLayer    R0402                                                30.050       84.850       360      Resistor,10K,0402,1%,YAGEO                                                        
R74            .Designator   TopLayer    R0402                                                20.750       3.925        90       Resistor,10K,0402,1%,YAGEO                                                        
R71            .Designator   TopLayer    R0402                                                37.575       11.350       180      Resistor,10K,0402,1%,YAGEO                                                        
R63            .Designator   TopLayer    R0402                                                49.425       16.625       360      Resistor,0R,0402,5%,YAGEO                                                         
R64            .Designator   TopLayer    R0402                                                51.275       16.625       360      Resistor,47K,0402,1%,YAGEO                                                        
R67            .Designator   TopLayer    R0603                                                53.675       14.150       360      Resistor,0R,0603,5%,YAGEO                                                         
R70            .Designator   TopLayer    R0402                                                55.075       11.600       180      Resistor,100K,0402,1%,YAGEO                                                       
R65            .Designator   TopLayer    R0402                                                53.325       16.425       180      Resistor,0R,0402,5%,YAGEO                                                         
R69            .Designator   TopLayer    R0402                                                53.375       11.600       360      Resistor,47K,0402,1%,YAGEO                                                        
R66            .Designator   TopLayer    R0402                                                53.325       15.350       360      Resistor,47K,0402,1%,YAGEO                                                        
R107           .Designator   BottomLayer R0402                                                48.150       10.000       90       Resistor,330R,0402,1%,YAGEO                                                       
R108           .Designator   BottomLayer R0402                                                46.200       10.000       270      Resistor,1K,0402,1%,YAGEO                                                         
R98            .Designator   BottomLayer R0402                                                66.700       32.150       180      Resistor,100K,0402,1%,YAGEO                                                       
R100           .Designator   BottomLayer R0402                                                64.100       25.200       90       Resistor,100K,0402,1%,YAGEO                                                       
R101           .Designator   BottomLayer R0603                                                62.400       25.300       180      Resistor,10R,0603,1%,ROHM,1/4W                                                    
R99            .Designator   BottomLayer R0402                                                66.700       31.100       0        Resistor,100K,0402,1%,YAGEO                                                       
R88            .Designator   BottomLayer R0402                                                19.450       79.850       360      Resistor,100K,0402,1%,YAGEO                                                       
R103           .Designator   BottomLayer R0402                                                47.575       21.550       90       Resistor,100K,0402,1%,YAGEO                                                       
R105           .Designator   BottomLayer R0402                                                42.850       17.150       90       Resistor,100K,0402,1%,YAGEO                                                       
R80            .Designator   BottomLayer R0402                                                31.250       96.100       270      Resistor,10K,0402,1%,YAGEO                                                        
R1             R1            TopLayer    R0402                                                26.500       103.425      270      Resistor,10K,0402,1%,YAGEO                                                        
R35            .Designator   TopLayer    R0402                                                9.650        67.200       360      Resistor,20R,0402,1%,YAGEO                                                        
R32            .Designator   TopLayer    R0402                                                9.650        68.250       360      Resistor,20R,0402,1%,YAGEO                                                        
R12            .Designator   TopLayer    R0603                                                8.125        84.425       90       Resistor,0R,0603,5%,YAGEO                                                         
R29            .Designator   TopLayer    R0603                                                11.050       69.450       360      Resistor,0R,0603,5%,YAGEO                                                         
R39            .Designator   TopLayer    R0402                                                20.225       64.450       270      Resistor,2K2,0402,1%,YAGEO                                                        
R22            .Designator   TopLayer    R0603                                                12.000       72.700       270      Resistor,0R,0603,5%,YAGEO                                                         
R33            .Designator   TopLayer    R0603                                                20.150       68.050       180      Resistor,0R,0603,5%,YAGEO                                                         
R28            .Designator   TopLayer    R0603                                                22.850       69.500       180      Resistor,0R,0603,5%,YAGEO                                                         
R23            .Designator   TopLayer    R0603                                                13.400       72.700       270      Resistor,0R,0603,5%,YAGEO                                                         
R26            .Designator   TopLayer    R0603                                                20.150       70.425       360      Resistor,0R,0603,5%,YAGEO                                                         
R25            .Designator   TopLayer    R0603                                                11.050       70.850       180      Resistor,0R,0603,5%,YAGEO                                                         
R30            .Designator   TopLayer    R0402                                                19.825       69.225       180      Resistor,10K,0402,1%,YAGEO                                                        
R31            .Designator   TopLayer    R0402                                                36.100       68.425       180      Resistor,10K,0402,1%,YAGEO                                                        
R20            .Designator   TopLayer    R0402                                                26.700       73.425       90       Resistor,10K,0402,1%,YAGEO                                                        
R21            .Designator   TopLayer    R0402                                                27.850       73.425       90       Resistor,10K,0402,1%,YAGEO                                                        
R61            .Designator   TopLayer    R0402                                                17.675       20.175       360      Resistor,0R,0402,5%,YAGEO                                                         
R59            .Designator   TopLayer    R0402                                                25.900       22.300       180      Resistor,0R,0402,5%,YAGEO                                                         
R60            .Designator   TopLayer    R0402                                                25.900       21.250       360      Resistor,10K,0402,1%,YAGEO                                                        
R57            .Designator   TopLayer    R0402                                                34.750       30.900       270      Resistor,2K7,0402,1%,YAGEO                                                        
R56            .Designator   TopLayer    R0402                                                33.700       30.900       270      Resistor,2K7,0402,1%,YAGEO                                                        
R102           .Designator   BottomLayer R0402                                                4.950        24.050       180      Resistor,2K7,0402,1%,YAGEO                                                        
R104           .Designator   BottomLayer R0402                                                4.950        21.200       180      Resistor,2K7,0402,1%,YAGEO                                                        
R51            .Designator   TopLayer    R0402                                                23.600       56.600       180      Resistor,56R,0402,1%,YAGEO                                                        
R52            .Designator   TopLayer    R0402                                                43.650       51.950       270      Resistor,10K,0402,1%,YAGEO                                                        
R55            .Designator   TopLayer    R0402                                                44.750       49.600       90       Resistor,10K,0402,1%,YAGEO                                                        
R44            .Designator   TopLayer    R0402                                                27.600       58.450       180      Resistor,0R,0402,5%,YAGEO                                                         
R54            .Designator   TopLayer    R0402                                                43.650       49.600       90       Resistor,10K,0402,1%,YAGEO                                                        
R45            .Designator   TopLayer    R0402                                                29.300       58.450       360      Resistor,0R,0402,5%,YAGEO                                                         
R47            .Designator   TopLayer    R0402                                                35.100       57.700       180      Resistor,0R,0402,5%,YAGEO                                                         
R48            .Designator   TopLayer    R0402                                                36.800       57.700       360      Resistor,0R,0402,5%,YAGEO                                                         
LD6            LD6           BottomLayer LED_0603_GREEN                                       67.800       87.850       360      LED, Green, 0603                                                                  
LD1            .Designator   TopLayer    LED_0603_RED                                         46.000       66.425       180      LED, Red, 0603                                                                    
LD2            LD2           BottomLayer LED_BI-GR_HSMF-A201-A00J1                            66.850       66.750       90       Bicolor Led                                                                       
LD5            .Designator   BottomLayer LED_0603_GREEN                                       67.800       56.700       360      LED, Green, 0603                                                                  
LD3            LD3           BottomLayer LED_0603_GREEN                                       67.800       59.675       360      LED, Green, 0603                                                                  
LD4            .Designator   BottomLayer LED_0603_RED                                         67.800       58.175       360      LED, Red, 0603                                                                    
LD7            .Designator   BottomLayer LED_0603_GREEN                                       48.150       7.850        270      LED, Green, 0603                                                                  
LD8            .Designator   BottomLayer LED_0603_RED                                         46.200       7.850        270      LED, Red, 0603                                                                    
L2             .Designator   BottomLayer L0603                                                66.400       34.250       270      Bead,600R,350mA,0603                                                              
L5             .Designator   BottomLayer L0603                                                62.400       23.650       0        Bead,600R,350mA,0603                                                              
L3             .Designator   BottomLayer L0603                                                64.200       34.400       180      Bead,600R,350mA,0603                                                              
L4             .Designator   BottomLayer L1210_LQH                                            67.150       28.000       90       FIXED IND 4.7UH 1A 180 MOHM 30% SMD                                               
L7             .Designator   BottomLayer L0603                                                67.200       20.850       0        Bead,600R,350mA,0603                                                              
L6             .Designator   BottomLayer L0603                                                62.400       22.150       0        Bead,600R,350mA,0603                                                              
L8             .Designator   BottomLayer L0603                                                62.400       20.650       0        Bead,600R,350mA,0603                                                              
L1             .Designator   TopLayer    L0603                                                16.950       57.900       270      Bead,600R,350mA,0603                                                              
JP1            .Designator   TopLayer    CON_SAMTEC_TSW-102-07-G-S                            66.650       94.600       180      Connector jumper 1 position                                                       
JP2            .Designator   TopLayer    CON_SAMTEC_TSW-102-07-G-S                            66.650       91.150       180      Connector jumper 1 position                                                       
JP3            .Designator   TopLayer    CON_SAMTEC_TSM-104-01-X-DV                           65.275       83.750       270      Header, 4-Pins, Double row Vertical, SMD, 2.54                                    
D3             .Designator   TopLayer    DIO_SOD323                                           38.625       88.900       270      BAT60JFILM                                                                        
D2             .Designator   TopLayer    DIO_SOD323                                           36.725       88.900       270      BAT60JFILM                                                                        
D1             .Designator   TopLayer    DIO_SOD323                                           34.825       88.900       270      BAT60JFILM                                                                        
D4             .Designator   TopLayer    DIO_SOD323                                           42.100       85.525       90       BAT60JFILM                                                                        
D5             .Designator   BottomLayer DIO_DO216-AA                                         64.835       36.650       0        Low Drop power Schottky rectifier(1A, 40V, 0.4V)                                  
CN2            CN2           TopLayer    CON_USBMICROB_MOLEX_105017-0001_H2P90                57.140       102.200      180      USB-MICRO-B, 1050170001, SMT, MOLEX                                               
CN12           CN12          BottomLayer CON_FCI_20021311-XXX20XXLF_MOD-MB1299                4.325        65.975       270      20 Position Receptacle Connector 0.050" (1.27mm) Through Hole Vertical Mount      
CN9            .Designator   TopLayer    CON_FISCHER_BL1-6-G                                  10.620       28.500       270      Header, 6-Pins, Single row, female THT, 2.54                                      
CN8            .Designator   TopLayer    CON_FISCHER_BL1-8-G                                  58.880       31.040       90       Header, 8-Pins, Single row, female, THT, 2.54                                     
CN7            .Designator   TopLayer    CON_FISCHER_BL1-8-G                                  10.620       48.820       270      Header, 8-Pins, Single row, female, THT, 2.54                                     
CN6            CN6           TopLayer    CON_FISCHER_BL1-10-G                                 58.880       55.420       90       Header, 10-Pin, Single row, female, THT, 2.54                                     
CN1            CN1           TopLayer    CON_MICROSD_YAMAICHI_PJS008-2003-1                   16.950       95.975       90       Memory Card Connectors MicroSD Card Conn Revrs Mnt Push-Push                      
CN17           CN17          BottomLayer CON_USBMICROAB_MOLEX_47590-0001_H3                   44.275       2.625        180      USB-MICRO-AB, 47590-0001, SMT, MOLEX                                              
CN16           .Designator   BottomLayer CON_HRS_FH26-29S-03SHW                               40.760       20.063       0        29pins FPC connector                                                              
CN15           .Designator   BottomLayer CON_SAMTEC_TMMH-113-01-F-DV                          52.800       37.000       270      26 Position Receptacle Connector 0.079" (2.00mm) Surface Mount                    
C16            .Designator   TopLayer    C0603                                                22.600       81.150       90       Capacitor,1uF,16V,X5R,10%,0603,YAGEO                                              
C78            .Designator   TopLayer    C0402                                                57.500       4.000        270      Capacitor,10pF,50V,NPO,5%,0402,YAGEO                                              
C90            .Designator   BottomLayer C0402                                                67.050       9.025        180      Capacitor,10pF,50V,NPO,5%,0402,YAGEO                                              
C50            .Designator   TopLayer    C0402                                                38.900       58.050       270      Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C7             .Designator   TopLayer    C0402                                                46.625       102.725      90       Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C6             .Designator   TopLayer    C0805                                                43.575       102.625      270      Capacitor,10uF,25V,X5R,10%,0805,YAGEO                                             
C5             .Designator   TopLayer    C0805                                                41.275       102.625      270      Capacitor,10uF,25V,X5R,10%,0805,YAGEO                                             
C4             .Designator   TopLayer    C0805                                                36.050       102.625      270      Capacitor,10uF,25V,X5R,10%,0805,YAGEO                                             
C3             .Designator   TopLayer    C0805                                                33.750       102.625      270      Capacitor,10uF,25V,X5R,10%,0805,YAGEO                                             
C27            .Designator   TopLayer    C0402                                                41.950       68.775       90       Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C30            .Designator   TopLayer    C0603                                                50.250       67.275       90       Capacitor,1uF,16V,X5R,10%,0603,YAGEO                                              
C19            .Designator   TopLayer    C0402                                                45.425       78.400       90       Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C15            .Designator   TopLayer    C0402                                                44.625       82.500       270      Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C9             .Designator   TopLayer    C0402                                                47.875       90.775       180      Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C10            .Designator   TopLayer    C0402                                                56.375       87.900       90       Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C14            .Designator   TopLayer    C0603                                                38.575       82.200       90       Capacitor,10nF,50V,X7R,10%,0603,YAGEO                                             
C11            .Designator   TopLayer    C0402                                                35.275       86.400       180      Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C12            .Designator   TopLayer    C0402                                                38.125       86.400       360      Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C13            .Designator   TopLayer    C0603                                                38.575       84.750       90       Capacitor,1uF,16V,X5R,10%,0603,YAGEO                                              
C17            .Designator   TopLayer    C0603                                                35.525       81.650       180      Capacitor,1uF,16V,X5R,10%,0603,YAGEO                                              
C18            .Designator   TopLayer    C0402                                                52.625       78.400       90       Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C8             .Designator   TopLayer    C0402                                                52.825       91.875       180      Capacitor,20pF,50V,NPO,5%,0402,YAGEO                                              
C20            .Designator   TopLayer    C0402                                                49.125       75.750       360      Capacitor,10pF,50V,NPO,5%,0402,YAGEO                                              
C21            .Designator   TopLayer    C0402                                                51.025       75.750       180      Capacitor,10pF,50V,NPO,5%,0402,YAGEO                                              
C42            .Designator   TopLayer    C0402                                                64.425       63.025       180      Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C58            .Designator   TopLayer    C0402                                                48.850       52.225       90       Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C57            .Designator   TopLayer    C0402                                                14.825       52.625       270      Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C76            .Designator   TopLayer    C0603                                                53.675       12.800       180      Capacitor,4.7uF,16V, X5R,10%,0603,YAGEO                                           
C85            .Designator   BottomLayer CPOL_TAJ-A_1206_H180                                 66.850       24.600       180      Polarized Capacitor,4.7uF,16V,10%,typeA,AVX                                       
C86            .Designator   BottomLayer C0402                                                67.550       22.950       0        Capacitor,10nF,16V,X7R,10%,0402,YAGEO                                             
C89            .Designator   BottomLayer C0402                                                67.550       22.050       0        Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C87            .Designator   BottomLayer C0402                                                66.250       22.500       270      Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C88            .Designator   BottomLayer C0805                                                64.800       21.700       270      Capacitor,10uF,25V,X5R,10%,0805,YAGEO                                             
C83            .Designator   BottomLayer C0402                                                64.550       33.200       0        Capacitor,10nF,16V,X7R,10%,0402,YAGEO                                             
C84            .Designator   BottomLayer C1206                                                63.600       31.650       0        Capacitor,4.7uF,50V, X7R,10%,1206,AVX                                             
C81            C81           BottomLayer C0402                                                19.450       86.850       180      Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C79            .Designator   BottomLayer C0402                                                52.100       98.000       90       Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C2             .Designator   TopLayer    C0402                                                51.800       103.350      90       Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C80            .Designator   BottomLayer C0402                                                31.250       98.000       90       Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C1             .Designator   TopLayer    C0402                                                30.850       103.375      90       Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C33            .Designator   TopLayer    C0603                                                11.050       65.900       180      Capacitor,2.2uF,10V, X5R,10%,0603,YAGEO                                           
C40            .Designator   TopLayer    C0603                                                11.050       64.475       180      Capacitor,2.2uF,10V, X5R,10%,0603,YAGEO                                           
C36            .Designator   TopLayer    C0603                                                13.050       64.100       270      Capacitor,2.2uF,10V, X5R,10%,0603,YAGEO                                           
C34            .Designator   TopLayer    C0603                                                21.500       64.700       90       Capacitor,1uF,16V,X5R,10%,0603,YAGEO                                              
C31            .Designator   TopLayer    C0402                                                11.350       67.200       360      Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C29            .Designator   TopLayer    C0402                                                11.350       68.250       360      Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C32            .Designator   TopLayer    C0603                                                20.150       66.700       180      Capacitor,4.7uF,16V, X5R,10%,0603,YAGEO                                           
C39            .Designator   TopLayer    C0603                                                18.825       64.100       90       Capacitor,4.7uF,16V, X5R,10%,0603,YAGEO                                           
C41            .Designator   TopLayer    C0603                                                16.125       62.575       90       Capacitor,1uF,16V,X5R,10%,0603,YAGEO                                              
C26            .Designator   TopLayer    C0402                                                16.300       72.025       180      Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C37            .Designator   TopLayer    C0603                                                14.400       64.100       90       Capacitor,4.7uF,16V, X5R,10%,0603,YAGEO                                           
C82            .Designator   BottomLayer C0402                                                12.750       63.800       90       Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C23            .Designator   TopLayer    C0603                                                17.875       72.700       270      Capacitor,1uF,16V,X5R,10%,0603,YAGEO                                              
C25            .Designator   TopLayer    C0402                                                18.975       72.450       270      Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C24            .Designator   TopLayer    C0603                                                20.075       72.700       270      Capacitor,4.7uF,16V, X5R,10%,0603,YAGEO                                           
C35            .Designator   TopLayer    C0402                                                15.950       64.825       180      Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C45            .Designator   TopLayer    C0402                                                11.200       60.700       270      Capacitor,10nF,16V,X7R,10%,0402,YAGEO                                             
C22            .Designator   TopLayer    C0603                                                14.750       72.700       270      Capacitor,1uF,16V,X5R,10%,0603,YAGEO                                              
C38            .Designator   TopLayer    C0603                                                17.500       64.100       90       Capacitor,4.7uF,16V, X5R,10%,0603,YAGEO                                           
C28            .Designator   TopLayer    C0402                                                29.800       68.525       180      Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C71            .Designator   TopLayer    C0402                                                20.125       27.875       180      Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C72            .Designator   TopLayer    C0402                                                21.000       19.750       90       Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C56            .Designator   TopLayer    C0402                                                43.450       53.250       180      Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C60            .Designator   TopLayer    C0402                                                43.450       46.975       180      Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C62            .Designator   TopLayer    C0402                                                43.800       41.550       180      Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C66            .Designator   TopLayer    C0402                                                39.825       32.225       360      Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C67            .Designator   TopLayer    C0402                                                27.250       32.175       360      Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C69            .Designator   TopLayer    C1206                                                39.725       29.400       90       Capacitor,2.2uF,16V, X7R,10%,1206,YAGEO                                           
C64            .Designator   TopLayer    C1206                                                15.800       34.650       90       Capacitor,2.2uF,16V, X7R,10%,1206,YAGEO                                           
C65            .Designator   TopLayer    C0402                                                18.450       35.350       360      Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C63            .Designator   TopLayer    C0402                                                18.325       41.050       360      Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C61            .Designator   TopLayer    C0402                                                18.450       45.550       360      Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C59            .Designator   TopLayer    C0402                                                18.450       52.050       360      Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C53            .Designator   TopLayer    C0402                                                24.900       56.800       270      Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C54            .Designator   TopLayer    C0402                                                31.475       56.800       270      Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C55            .Designator   TopLayer    CPOL_TAJ-A_1206_H180                                 46.675       51.600       270      Polarized Capacitor,4.7uF,16V,10%,typeA,AVX                                       
C68            .Designator   TopLayer    C0402                                                32.700       30.900       90       Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C70            .Designator   TopLayer    CPOL_TAJ-A_1206_H180                                 33.450       27.375       270      Polarized Capacitor,1uF,16V,10%,typeA,AVX                                         
C51            .Designator   TopLayer    C0402                                                24.000       58.000       270      Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C48            .Designator   TopLayer    CPOL_TAJ-A_1206_H180                                 22.350       59.250       90       Polarized Capacitor,1uF,16V,10%,typeA,AVX                                         
C52            .Designator   TopLayer    C0402                                                20.600       57.050       270      Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C49            .Designator   TopLayer    CPOL_TAJ-A_1206_H180                                 18.950       58.250       90       Polarized Capacitor,1uF,16V,10%,typeA,AVX                                         
C43            .Designator   TopLayer    C0402                                                27.600       62.550       360      Capacitor,8.2pF,50V,NPO,4%,0402,AVX                                               
C44            .Designator   TopLayer    C0402                                                29.300       62.550       180      Capacitor,8.2pF,50V,NPO,4%,0402,AVX                                               
C46            .Designator   TopLayer    C0402                                                35.100       60.900       360      Capacitor, 5.1pF, 50V, NPO, -+0.25pF, 0402, YAGEO                                 
C47            .Designator   TopLayer    C0402                                                36.800       60.900       180      Capacitor, 5.1pF, 50V, NPO, -+0.25pF, 0402, YAGEO                                 
CN14           CN14          BottomLayer CON_SAMTEC_TSW-104-07-G-S                            67.700       47.000       270      Header, 4-Pin                                                                     
H3             .Designator   TopLayer    PTH_M1261-3005-N_3P5X6_M3_H14                        4.250        4.250        0                                                                                          
H1             .Designator   TopLayer    PTH_M1261-3005-N_3P5X6_M3_H14                        4.250        100.750      0                                                                                          
H2             .Designator   TopLayer    PTH_M1261-3005-N_3P5X6_M3_H14                        65.750       100.750      0                                                                                          
H4             .Designator   TopLayer    PTH_M1261-3005-N_3P5X6_M3_H14                        65.750       4.250        0                                                                                          
CN10           CN10          BottomLayer CON_HRS_DF37NB-10DS-04V                              18.550       83.400       90       Header, 5-Pin, Dual row                                                           
B2             B2            BottomLayer SWI_C&K_KSC321GLFS_BLACK                             55.675       4.000        360      Tactile_switch_CMS_BLACK_2N                                                       
B1             B1            BottomLayer SWI_C&K_KSC721GLFS_BLUE                              63.000       13.175       180      Tactile_switch_CMS_BLUE_2.25N                                                     
U1             .Designator   TopLayer    MIC_STM_MP23DB01MMTR                                 28.700       102.421      0        MEMS audio sensor, omnidirectional digital microphone                             
U2             .Designator   TopLayer    MIC_STM_MP23DB01MMTR                                 49.700       102.421      0        MEMS audio sensor, omnidirectional digital microphone                             
U17            .Designator   BottomLayer MIC_HCLGA_3X4X1_4LD                                  28.700       97.000       360      MEMS audio sensor, omnidirectional digital microphone                             
U16            .Designator   BottomLayer MIC_HCLGA_3X4X1_4LD                                  49.700       97.000       360      MEMS audio sensor, omnidirectional digital microphone                             
MIRE1          MIRE1         TopLayer    MIRE_PLACE_SMD_0P8MM                                 6.775        96.075       0                                                                                          
MIRE2          MIRE2         TopLayer    MIRE_PLACE_SMD_0P8MM                                 2.000        18.600       0                                                                                          
MIRE3          MIRE3         TopLayer    MIRE_PLACE_SMD_0P8MM                                 58.600       8.675        0                                                                                          
MIRE6          MIRE6         BottomLayer MIRE_PLACE_SMD_0P8MM                                 58.600       8.675        180                                                                                        
MIRE4          MIRE4         BottomLayer MIRE_PLACE_SMD_0P8MM                                 4.325        95.750       180                                                                                        
MIRE5          MIRE5         BottomLayer MIRE_PLACE_SMD_0P8MM                                 7.875        19.150       180                                                                                        
C73            C73           TopLayer    C0603                                                19.675       16.075       270      Capacitor,2.2uF,10V, X5R,10%,0603,YAGEO                                           
C75            C75           TopLayer    C0402                                                18.425       15.825       90       Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
C74            C74           TopLayer    C0603                                                38.925       15.925       90       Capacitor,2.2uF,10V, X5R,10%,0603,YAGEO                                           
C77            C77           TopLayer    C0402                                                40.350       12.775       360      Capacitor,100nF,16V,X7R,10%,0402,YAGEO                                            
M1             M1            BottomLayer MOD_WIFI_INVENTEK-SYSTEMS_ISM43362-M3G-L44-E-SPI-CXX 28.032       8.500        180      WIFI Module ISM43362-M3G-L44-E: IEEE802.11 b/g/n integrated Antenna               
R68            R68           TopLayer    R0402                                                33.925       13.500       90       Resistor,47K,0402,1%,YAGEO                                                        
R49            R49           TopLayer    R0402                                                27.600       57.400       180      Resistor,0R,0402,5%,YAGEO                                                         
R42            R42           TopLayer    R0402                                                67.150       60.450       360      Resistor,47K,0402,1%,YAGEO                                                        
R41            R41           TopLayer    R0402                                                67.150       61.600       360      Resistor,100K,0402,1%,YAGEO                                                       
SB8            SB8           TopLayer    SOLDER-BRIDGE_R0603-0R                               35.325       14.500       90       Solder Bridge ON                                                                  
SB9            SB9           TopLayer    SOLDER-BRIDGE_R0603-0R                               36.800       14.500       90       Solder Bridge ON                                                                  
SB11           SB11          TopLayer    SOLDER-BRIDGE_R0603-0R                               37.100       4.250        360      Solder Bridge OFF                                                                 
SB12           SB12          TopLayer    SOLDER-BRIDGE_R0603-0R                               37.100       2.825        360      Solder Bridge OFF                                                                 
SB10           SB10          TopLayer    SOLDER-BRIDGE_R0603-0R                               21.475       6.925        270      Solder Bridge OFF                                                                 
T2             T2            TopLayer    NPN_SOT23                                            66.650       57.675       180      NPN Bipolar Transistor                                                            
TP1            TP1           TopLayer    TP_SMD_1MM                                           27.625       85.275       180      Test Point                                                                        
TP16           TP16          TopLayer    TP_SMD_1MM                                           29.900       23.850       180      Test Point                                                                        
TP10           TP10          TopLayer    TP_SMD_1MM                                           14.775       57.075       180      Test Point                                                                        
TP11           TP11          TopLayer    TP_SMD_1MM                                           48.800       49.525       180      Test Point                                                                        
TP14           TP14          TopLayer    TP_SMD_1MM                                           47.950       41.850       180      Test Point                                                                        
TP7            TP7           TopLayer    TP_SMD_1MM                                           24.450       67.859       180      Test Point                                                                        
TP5            TP5           TopLayer    TP_SMD_1MM                                           9.925        73.400       180      Test Point                                                                        
TP8            TP8           TopLayer    TP_SMD_1MM                                           8.025        65.575       180      Test Point                                                                        
TP2            TP2           TopLayer    TP_SMD_1MM                                           34.625       77.275       180      Test Point                                                                        
TP13           TP13          TopLayer    TP_SMD_1MM                                           44.950       43.100       180      Test Point                                                                        
TP12           TP12          TopLayer    TP_SMD_1MM                                           17.825       49.425       90       Test Point                                                                        
TP15           TP15          TopLayer    TP_SMD_1MM                                           46.325       39.950       180      Test Point                                                                        
TP18           TP18          TopLayer    TP_SMD_2MM                                           23.360       12.365       360      Test Point                                                                        
TP9            TP9           TopLayer    TP_SMD_1MM                                           34.450       63.950       90       Test Point                                                                        
TP17           TP17          TopLayer    TP_SMD_2MM                                           20.820       12.365       360      Test Point                                                                        
TP19           TP19          TopLayer    TP_SMD_2MM                                           25.900       12.365       360      Test Point                                                                        
TP20           TP20          TopLayer    TP_SMD_2MM                                           28.440       12.365       360      Test Point                                                                        
TP22           TP22          TopLayer    TP_SMD_1MM                                           24.275       3.925        270      Test Point                                                                        
U5             U5            TopLayer    ESD_SOT666                                           58.325       95.875       180      USB ESD protection                                                                
CN5            CN5           TopLayer    CON_PHONE-JACK-3P5_HY_PJ3028B                        9.250        79.650       360      Connector Jack Stereo 3.5mm, female SMT, 4 PIN                                    
LCD1           Comment       BottomLayer LCD_DRAWING_PROJET-MB1274                            -50.800      -66.200      180                                                                                        
