Altium Designer Pick and Place Locations
C:\Users\tguilhot\Documents\_SubVersion\HW_Boards\MB1355-Nucleo68-IntSMPS\02-Manufacturing\MB1355D_PCB\Assembly\MB1355D_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       07/01/21
Time:       19:31
Revision:   6
Variant:    No variations
Units used: mm

Designator Comment                          Layer       Footprint                                 Center-X(mm) Center-Y(mm) Rotation Description                                                             
L5         Inductor                         TopLayer    IND_0402_MURATA_LQW15AN_H0P5              18.9121      44.3019      360      "inductor, 10nH +-2%, 100mA max,1.3 ohm DC max, Q min = 13,0402"        
SB27       Open                             BottomLayer SB-tiny                                   35.6262      36.3484      360      "Solder Jumper"                                                         
U13        ESD-TRANSIL                      BottomLayer ESD_QFN2_1P6X1_P125                       54.2196      8.7909       90       "High power transient voltage suppressor, 7V breakdown"                 
U12        MLPF-WB55-01E3                   TopLayer    ST_CSP650x58P2x3_160x100x42               23.0953      50.3420      0        "2.4 GHz low pass filter matched to STM32WBx5Cx/Rx"                     
U11        ESD-TRANSIL                      BottomLayer ESD_QFN2_1P6X1_P125                       42.8755      6.6797       90       "High power transient voltage suppressor, 7V breakdown"                 
SW5        SW_MECA_1K2                      BottomLayer SWI_SPDT-RA_TE-CONNECTIVITY_MLL1200S_1P2T 34.7550      22.6413      90       "SPDT RA SMT SLIDE SWITCH"                                              
R13        nc                               TopLayer    0402_RES                                  30.7589      53.7837      360      Resistor                                                                
JP6        HEADER_1X2                       TopLayer    Header_M_1x2x2.54_TH_V                    12.2961      45.7930      90       ""                                                                      
JMP12      "Jumper 2.54mm"                  TopLayer    Jumper_2.54mm_BLACK                       -113.0380    -152.3930    90       "Jumper 2.54mm"                                                         
Q1         2N2222                           TopLayer    SOT23-3                                   50.4320      9.8040       180      2N2222_SOT23                                                            
SB39       Close                            TopLayer    SB-tiny                                   38.5141      21.6960      360      "Solder Jumper"                                                         
C32        100nF                            BottomLayer 0402_CAP_NPOL                             31.2301      45.6890      360      "Capacitor_not polarized"                                               
SB45       Open                             BottomLayer SB-tiny                                   31.0291      40.6980      360      "Solder Jumper"                                                         
SB46       Open                             BottomLayer SB-tiny                                   31.0391      42.1470      360      "Solder Jumper"                                                         
U1         STM32WBxx_QFN68                  TopLayer    VFQFPN68_8x8x0.1_p0.4                     24.8314      44.2520      180      ""                                                                      
SC4        "Shield Clip_A 3.9x1.1x1.28"     TopLayer    Shield_Clip_A_3.9x1.1x1.28                23.3291      52.7520      180      "Harwin S0951-46R"                                                      
SC3        "Shield Clip_A 3.9x1.1x1.28"     TopLayer    Shield_Clip_A_3.9x1.1x1.28                31.8291      44.2520      90       "Harwin S0951-46R"                                                      
SC2        "Shield Clip_A 3.9x1.1x1.28"     TopLayer    Shield_Clip_A_3.9x1.1x1.28                23.3291      35.7520      180      "Harwin S0951-46R"                                                      
SC1        "Shield Clip_A 3.9x1.1x1.28"     TopLayer    Shield_Clip_A_3.9x1.1x1.28                14.8291      44.2520      90       "Harwin S0951-46R"                                                      
SW3        "User PB"                        TopLayer    SW-PB_SMD_KMR2                            27.1769      1.9666       0        "Push-button SMD"                                                       
SW2        "User PB"                        TopLayer    SW-PB_SMD_KMR2                            21.6143      1.9666       0        "Push-button SMD"                                                       
SW1        "User PB"                        TopLayer    SW-PB_SMD_KMR2                            16.1801      1.9666       0        "Push-button SMD"                                                       
JP5        HEADER_2X8                       TopLayer    Header_M_2x8x2.54_TH_V                    25.5171      16.2170      270      ""                                                                      
LED6       HSMF-A201-A00J1/KAA-3528SURKCGKC TopLayer    HSMF-A201                                 46.6701      4.5140       90       "Bicolor Led"                                                           
LED1       "LED BLUE"                       TopLayer    0603_LED_Blue                             31.1501      1.9740       90       "Light-Emitting Diode"                                                  
LED3       "LED RED"                        TopLayer    0603_LED_RED                              35.2801      1.9440       90       "Light-Emitting Diode"                                                  
CN5        HEADER_1X10                      TopLayer    Header_F_1x10x2.54_TH_V                   59.1301      38.3140      90       ""                                                                      
CN6        HEADER_1X8_F                     TopLayer    Header_F_1x8x2.54_TH_V                    10.8700      31.7100      270      ""                                                                      
CN7        HEADER_2X19_M                    TopLayer    Header_M_2x19x2.54_TH_M_top_+_M_bottom    4.5836       27.9000      270      ""                                                                      
CN10       HEADER_2X19_M                    TopLayer    Header_M_2x19x2.54_TH_M_top_+_M_bottom    65.5436      27.9000      270      ""                                                                      
CN9        HEADER_1X8_F                     TopLayer    Header_F_1x8x2.54_TH_V                    59.1301      13.9300      90       ""                                                                      
CN8        HEADER_1X6                       TopLayer    Header_F_1x6x2.54_TH_V                    10.8700      11.3900      270      ""                                                                      
LED2       "LED GREEN"                      TopLayer    0603_LED_GREEN                            33.2201      1.9440       90       "Light-Emitting Diode"                                                  
SW4        "Reset PB"                       TopLayer    SW-PB_SMD_KMR2                            40.4357      1.8650       0        "Push-button SMD"                                                       
C9         10uF/25V                         TopLayer    1210_CAP_POL                              41.1421      41.6840      180      Condensateur_polarise                                                   
C10        10uF/25V                         TopLayer    1210_CAP_POL                              43.2601      31.5040      360      Condensateur_polarise                                                   
C11        4.7uF/10V                        TopLayer    1210_CAP_POL                              50.9301      31.2840      180      Condensateur_polarise                                                   
CN3        HEADER_1X5                       TopLayer    Header_NF_1x5x2.54_TH                     9.1461       49.5870      90       ""                                                                      
CN4        HEADER_1X2                       TopLayer    Header_NF_1x2x2.54_TH                     32.4331      29.7140      180      ""                                                                      
CN11       HEADER_1X2                       TopLayer    Header_M_1x2x2.54_TH_V                    4.5201       54.6970      180      ""                                                                      
CN12       HEADER_1X2                       TopLayer    Header_M_1x2x2.54_TH_V                    65.4800      54.1998      180      ""                                                                      
CN13       HEADER_1X6                       TopLayer    Header_NF_1x6x2.54_TH                     53.3301      54.2040      360      ""                                                                      
D2         BAT60JFILM                       BottomLayer SOD-323                                   56.8701      18.7340      270      "Default Diode"                                                         
U10        74LVC1G07                        TopLayer    SOT353-1                                  40.3328      18.8360      180      ""                                                                      
U9         ECMF02-2AMX6                     BottomLayer ESD_QFN-6L_1P7X1P5_P050                   52.3516      8.7361       360      "Common mode filter with ESD protection for USB 2.0 interface"          
JP1        HEADER_2X4                       TopLayer    Header_M_2x4x2.54_TH_V                    46.0551      46.2350      360      ""                                                                      
JP3        HEADER_1X2                       TopLayer    Header_M_1x2x2.54_TH_V                    25.4921      29.7230      360      ""                                                                      
JP4        HEADER_1X2                       TopLayer    Header_M_1x2x2.54_TH_V                    12.2891      51.5860      270      ""                                                                      
LED5       "LED RED"                        TopLayer    0603_LED_RED                              53.5929      3.7700       90       "Light-Emitting Diode"                                                  
R25        100/2K7                          TopLayer    0402_RES                                  45.9301      8.1740       90       Resistor                                                                
R27        100/100                          TopLayer    0402_RES                                  47.4101      8.1740       90       Resistor                                                                
U5         LD3985M33R                       BottomLayer SOT23-5                                   33.7501      14.6840      360      "3.3V low drop voltage regulator"                                       
U6         ECMF02-2AMX6                     BottomLayer ESD_QFN-6L_1P7X1P5_P050                   40.9857      6.6299       360      "Common mode filter with ESD protection for USB 2.0 interface"          
CN1        1050170001                       BottomLayer USBMICROB_MOLEX_105017-0001_H2P90         40.3595      2.7854       180      "USB-MICRO-B, 1050170001, SMT, MOLEX"                                   
CN15       1050170001                       BottomLayer USBMICROB_MOLEX_105017-0001_H2P90         52.9071      4.8000       180      "USB-MICRO-B, 1050170001, SMT, MOLEX"                                   
J2         SMA                              TopLayer    SMA_T_9.52_NF                             38.2981      54.9095      90       ""                                                                      
U7         TXS0108EPW                       TopLayer    TSSOP20                                   33.6751      21.5060      360      "TXS0108E Bi-directional Level Shifter TSSOP20"                         
U8         STM32F103CBT6                    TopLayer    LQFP48_7X7_P050                           47.2101      17.8460      180      "Medium-density performance line ARM-based 32-bit MCU with 128KB Flash" 
X3         XTAL_2_PINS                      TopLayer    CRY_NX3225GD_2P                           50.1099      25.5174      90       "Crystal 8MHz, 8pF, +-20ppm, 500ohms max,  SMD"                         
LED4       "LED RED"                        TopLayer    0603_LED_RED                              52.0689      3.7700       90       "Light-Emitting Diode"                                                  
U2         LD1117S50TR                      TopLayer    SOT223_SC73_A                             42.3001      36.5840      270      "IC REG LDO 5V 0.8A SOT223"                                             
U3         LD39050PU33R                     TopLayer    DFN6_3x3mm                                54.0309      46.5663      360      "3.3V voltage regulator 500mA"                                          
U4         TPS2041C                         TopLayer    MOS_SOT23-5L                              51.2750      35.2321      270      "5V Power Switch, 0.85A, RDSon 130mOhm max, with active low enable pin" 
R31        10                               BottomLayer 0402_RES                                  60.3261      52.2330      360      Resistor                                                                
R32        100K                             TopLayer    0402_RES                                  40.4001      20.5060      180      Resistor                                                                
JMP1       "Jumper 2.54mm"                  TopLayer    Jumper_2.54mm_BLACK                       -113.0380    -152.3930    270      "Jumper 2.54mm"                                                         
JMP2       "Jumper 2.54mm"                  TopLayer    Jumper_2.54mm_BLACK                       -113.0380    -152.3930    90       "Jumper 2.54mm"                                                         
JMP3       "Jumper 2.54mm"                  TopLayer    Jumper_2.54mm_BLACK                       -113.0380    -152.3930    360      "Jumper 2.54mm"                                                         
JMP4       "Jumper 2.54mm"                  TopLayer    Jumper_2.54mm_BLACK                       -113.0380    -152.3930    270      "Jumper 2.54mm"                                                         
JMP5       "Jumper 2.54mm"                  TopLayer    Jumper_2.54mm_BLACK                       -113.0380    -152.3930    180      "Jumper 2.54mm"                                                         
JMP6       "Jumper 2.54mm"                  TopLayer    Jumper_2.54mm_BLACK                       -113.0380    -152.3930    180      "Jumper 2.54mm"                                                         
JMP7       "Jumper 2.54mm"                  TopLayer    Jumper_2.54mm_BLACK                       -113.0380    -152.3930    180      "Jumper 2.54mm"                                                         
JMP8       "Jumper 2.54mm"                  TopLayer    Jumper_2.54mm_BLACK                       -113.0380    -152.3930    180      "Jumper 2.54mm"                                                         
JMP9       "Jumper 2.54mm"                  TopLayer    Jumper_2.54mm_BLACK                       -113.0380    -152.3930    180      "Jumper 2.54mm"                                                         
JMP10      "Jumper 2.54mm"                  TopLayer    Jumper_2.54mm_BLACK                       -113.0380    -152.3930    180      "Jumper 2.54mm"                                                         
JMP11      "Jumper 2.54mm"                  TopLayer    Jumper_2.54mm_BLACK                       -113.0380    -152.3930    180      "Jumper 2.54mm"                                                         
C1         Capacitor                        BottomLayer C0402                                     44.0540      6.5197       270      "Capacitor, MLCC, 100pF, 50V, NPO, 5%, 0402, T=0,5mm"                   
C2         Capacitor                        BottomLayer C0402                                     55.4124      8.4693       90       "Capacitor, MLCC, 100pF, 50V, NPO, 5%, 0402, T=0,5mm"                   
C3         100nF                            BottomLayer 0402_CAP_NPOL                             15.2941      45.9980      360      "Capacitor_not polarized"                                               
C6         10pF                             TopLayer    0402_CAP_NPOL                             30.3871      39.5560      270      "Capacitor_not polarized"                                               
C7         10pF                             TopLayer    0402_CAP_NPOL                             30.4961      44.5350      90       "Capacitor_not polarized"                                               
C8         100nF/25V                        TopLayer    0402_CAP_NPOL                             39.4801      31.8940      270      "Capacitor_not polarized"                                               
C12        100nF                            TopLayer    0402_CAP_NPOL                             48.0570      35.6640      270      "Capacitor_not polarized"                                               
C13        1uF/X5R                          TopLayer    0603_CAP_NPOL                             56.4601      44.1980      270      "Capacitor_not polarized"                                               
C14        100nF                            TopLayer    0402_CAP_NPOL                             53.8521      49.5050      90       "Capacitor_not polarized"                                               
C15        1uF/X5R                          TopLayer    0603_CAP_NPOL                             52.5071      49.7310      90       "Capacitor_not polarized"                                               
C16        100nF                            TopLayer    0402_CAP_NPOL                             54.1191      43.1610      180      "Capacitor_not polarized"                                               
C17        100nF                            TopLayer    0402_CAP_NPOL                             28.9851      29.7320      270      "Capacitor_not polarized"                                               
C18        100nF                            TopLayer    0402_CAP_NPOL                             27.3443      38.2030      270      "Capacitor_not polarized"                                               
C19        100nF                            BottomLayer 0402_CAP_NPOL                             23.3921      46.2765      270      "Capacitor_not polarized"                                               
C20        100nF                            BottomLayer 0402_CAP_NPOL                             22.5643      46.2724      270      "Capacitor_not polarized"                                               
C21        1uF/X5R                          BottomLayer 0603_CAP_NPOL                             33.3801      11.2740      360      "Capacitor_not polarized"                                               
C22        1uF/X5R                          BottomLayer 0603_CAP_NPOL                             35.7101      11.8040      270      "Capacitor_not polarized"                                               
C23        4.7uF                            TopLayer    0402_CAP_NPOL                             17.1961      42.5351      180      "Capacitor_not polarized"                                               
C24        100nF                            TopLayer    0402_CAP_NPOL                             18.8445      42.6027      90       "Capacitor_not polarized"                                               
C25        100nF                            BottomLayer 0402_CAP_NPOL                             33.4900      12.5940      360      "Capacitor_not polarized"                                               
C26        100nF                            BottomLayer 0402_CAP_NPOL                             33.9900      16.6740      180      "Capacitor_not polarized"                                               
C27        100nF                            BottomLayer 0402_CAP_NPOL                             36.9201      12.1140      270      "Capacitor_not polarized"                                               
C28        100nF                            TopLayer    0402_CAP_NPOL                             28.4100      38.2120      270      "Capacitor_not polarized"                                               
C29        4.7uF                            TopLayer    0402_CAP_NPOL                             18.4076      46.1589      270      "Capacitor_not polarized"                                               
C31        100nF                            TopLayer    0402_CAP_NPOL                             26.4091      38.1630      270      "Capacitor_not polarized"                                               
C33        100nF                            BottomLayer 0402_CAP_NPOL                             20.8283      48.2049      90       "Capacitor_not polarized"                                               
C34        100pF                            BottomLayer 0402_CAP_NPOL                             21.6106      48.1998      90       "Capacitor_not polarized"                                               
C36        ""                               TopLayer    0402_CAP_NPOL                             22.8631      55.5510      270      "Capacitor_not polarized"                                               
C37        1.2pF                            TopLayer    0402_CAP_NPOL                             19.5661      55.5780      90       "Capacitor_not polarized"                                               
C39        ""                               TopLayer    0402_CAP_NPOL                             34.9571      50.6300      90       "Capacitor_not polarized"                                               
C40        ""                               TopLayer    0402_CAP_NPOL                             38.9240      51.2562      180      "Capacitor_not polarized"                                               
C41        100nF                            TopLayer    0402_CAP_NPOL                             38.0111      24.3650      90       "Capacitor_not polarized"                                               
C42        100nF                            TopLayer    0402_CAP_NPOL                             29.4781      23.1310      90       "Capacitor_not polarized"                                               
C43        100nF                            TopLayer    0402_CAP_NPOL                             40.3101      17.1460      360      "Capacitor_not polarized"                                               
C44        20pF                             TopLayer    0402_CAP_NPOL                             48.1201      25.4560      270      "Capacitor_not polarized"                                               
C45        20pF                             TopLayer    0402_CAP_NPOL                             52.0641      25.5320      270      "Capacitor_not polarized"                                               
C46        100nF                            TopLayer    0402_CAP_NPOL                             47.1701      25.4660      270      "Capacitor_not polarized"                                               
C47        100nF                            TopLayer    0402_CAP_NPOL                             45.2601      25.4560      90       "Capacitor_not polarized"                                               
C48        100nF                            TopLayer    0402_CAP_NPOL                             40.3101      15.0760      180      "Capacitor_not polarized"                                               
C49        100nF                            TopLayer    0402_CAP_NPOL                             51.4141      12.8860      360      "Capacitor_not polarized"                                               
C50        100nF                            TopLayer    0402_CAP_NPOL                             53.4201      20.6360      360      "Capacitor_not polarized"                                               
D1         BAT54KFILM                       BottomLayer SOD523                                    15.2701      46.9980      180      "Schottky Diode"                                                        
L1         10uH                             TopLayer    0805_COIL                                 16.9797      45.2344      270      "Coil Wurtz 10uH ref: 74479777310A"                                     
L2         FCM1608KF-601T03                 BottomLayer 0603_COIL                                 31.9651      43.8520      180      ""                                                                      
L3         3.6nH                            TopLayer    0402_COIL                                 21.2010      56.1730      180      ""                                                                      
L4         0R                               TopLayer    0402_COIL                                 36.5707      51.2260      0        ""                                                                      
Label_4    LOGO_STM32                       TopLayer    LOGO_STM32                                -113.0380    -152.3930    0        ""                                                                      
R1         100K                             BottomLayer 0402_RES                                  36.6271      5.6600       270      Resistor                                                                
R2         680                              BottomLayer 0402_RES                                  31.1754      4.6640       270      Resistor                                                                
R3         680                              BottomLayer 0402_RES                                  33.2054      4.6340       270      Resistor                                                                
R4         680                              BottomLayer 0402_RES                                  35.2755      4.6340       270      Resistor                                                                
R5         0R                               TopLayer    0402_RES                                  29.5260      53.7952      180      Resistor                                                                
R6         10K                              BottomLayer 0402_RES                                  30.7811      39.6290      360      Resistor                                                                
R7         1K                               BottomLayer 0402_RES                                  17.1241      2.4780       90       Resistor                                                                
R8         1K                               BottomLayer 0402_RES                                  22.6461      2.4960       90       Resistor                                                                
R9         1K                               BottomLayer 0402_RES                                  28.2031      2.5040       90       Resistor                                                                
R10        1K                               TopLayer    0402_RES                                  53.8631      6.4760       270      Resistor                                                                
R11        10K                              TopLayer    0402_RES                                  54.0341      35.0210      270      Resistor                                                                
R12        1K                               TopLayer    0402_RES                                  52.2901      6.4950       270      Resistor                                                                
R14        2K7                              TopLayer    0402_RES                                  53.4101      16.5660      180      Resistor                                                                
R15        4K7                              TopLayer    0402_RES                                  53.4201      17.5460      360      Resistor                                                                
R16        10K                              TopLayer    0402_RES                                  53.8261      12.8860      360      Resistor                                                                
R17        100                              TopLayer    0402_RES                                  53.8561      14.8890      360      Resistor                                                                
R18        10K                              TopLayer    0402_RES                                  54.2141      25.5120      90       Resistor                                                                
R19        100K                             TopLayer    0402_RES                                  53.4001      18.6060      180      Resistor                                                                
R20        36K                              TopLayer    0402_RES                                  53.8161      13.9330      180      Resistor                                                                
R21        1K5                              BottomLayer 0402_RES                                  51.2321      10.3894      180      Resistor                                                                
R22        10K                              TopLayer    0402_RES                                  53.1941      25.5220      90       Resistor                                                                
R23        100K                             BottomLayer 0402_RES                                  50.3901      8.5840       270      Resistor                                                                
R24        100K                             TopLayer    0402_RES                                  46.2400      25.4660      90       Resistor                                                                
R26        4K7                              TopLayer    0402_RES                                  43.2801      25.4660      90       Resistor                                                                
R28        4K7                              TopLayer    0402_RES                                  44.2601      25.4560      90       Resistor                                                                
R29        100                              TopLayer    0402_RES                                  44.9101      12.1260      180      Resistor                                                                
R30        ""                               TopLayer    0402_RES                                  40.2901      16.1260      360      Resistor                                                                
SB1        Close                            BottomLayer SB-tiny                                   56.3901      34.9380      90       "Solder Jumper"                                                         
SB2        Open                             BottomLayer SB-tiny                                   22.2144      35.5618      360      "Solder Jumper"                                                         
SB3        Open                             BottomLayer SB-tiny                                   56.3811      32.2770      270      "Solder Jumper"                                                         
SB4        Open                             BottomLayer SB-tiny                                   20.4229      35.5752      180      "Solder Jumper"                                                         
SB5        Close                            BottomLayer SB-tiny                                   54.5501      37.2380      90       "Solder Jumper"                                                         
SB6        Open                             BottomLayer SB-tiny                                   54.5701      39.0980      90       "Solder Jumper"                                                         
SB7        Open                             BottomLayer SB-tiny                                   25.3441      32.6330      360      "Solder Jumper"                                                         
SB8        Close                            BottomLayer SB-tiny                                   56.0901      28.9080      90       "Solder Jumper"                                                         
SB9        Close                            BottomLayer SB-tiny                                   25.3441      33.9370      360      "Solder Jumper"                                                         
SB10       Open                             BottomLayer SB-tiny                                   25.2560      35.3910      270      "Solder Jumper"                                                         
SB11       Close                            BottomLayer SB-tiny                                   56.5711      12.6730      90       "Solder Jumper"                                                         
SB12       Close                            BottomLayer SB-tiny                                   28.5651      33.7670      0        "Solder Jumper"                                                         
SB13       Open                             BottomLayer SB-tiny                                   28.5617      35.2882      0        "Solder Jumper"                                                         
SB14       Close                            BottomLayer SB-tiny                                   13.0157      13.4726      90       "Solder Jumper"                                                         
SB15       Close                            BottomLayer SB-tiny                                   56.5041      8.3880       90       "Solder Jumper"                                                         
SB16       Open                             BottomLayer SB-tiny                                   12.9624      10.9222      270      "Solder Jumper"                                                         
SB17       Close                            BottomLayer SB-tiny                                   56.5561      10.9090      90       "Solder Jumper"                                                         
SB18       Open                             BottomLayer SB-tiny                                   20.9051      32.1750      90       "Solder Jumper"                                                         
SB22       Open                             BottomLayer SB-tiny                                   14.8154      48.7243      180      "Solder Jumper"                                                         
SB23       Open                             BottomLayer SB-tiny                                   12.3171      55.2870      180      "Solder Jumper"                                                         
SB24       Open                             BottomLayer SB-tiny                                   35.6011      33.5000      360      "Solder Jumper"                                                         
SB25       Open                             TopLayer    SB-tiny                                   51.3351      38.1100      360      "Solder Jumper"                                                         
SB26       Close                            BottomLayer SB-tiny                                   35.4895      37.7368      180      "Solder Jumper"                                                         
SB28       Open                             BottomLayer SB-tiny                                   35.6231      34.9080      360      "Solder Jumper"                                                         
SB30       Open                             BottomLayer SB-tiny                                   30.2801      37.6480      180      "Solder Jumper"                                                         
SB32       Close                            BottomLayer SB-tiny                                   27.8921      38.3580      180      "Solder Jumper"                                                         
SB34       Open                             BottomLayer SB-tiny                                   26.3881      38.3520      360      "Solder Jumper"                                                         
SB35       Close                            BottomLayer SB-tiny                                   32.9941      42.0350      270      "Solder Jumper"                                                         
SB36       Close                            BottomLayer SB-tiny                                   56.0191      16.0670      180      "Solder Jumper"                                                         
SB37       Open                             BottomLayer SB-tiny                                   56.0071      14.7390      180      "Solder Jumper"                                                         
SB40       Open                             TopLayer    SB-tiny                                   36.4930      15.9640      90       "Solder Jumper"                                                         
SB41       Close                            BottomLayer SB-tiny                                   55.9401      37.1000      270      "Solder Jumper"                                                         
X1         NX2016_32M                       TopLayer    NX2016_4P                                 19.5067      48.9141      0        "Crystal NDK 2.0x1.6mm  32 MHz"                                         
X2         NX2012_32K768                    TopLayer    NX2012_2P                                 30.5911      42.0570      90       "Crystal NDK 2.0x1.2mm  32.768 KHz"                                     
SK_BT1     CR2032-SCK1B                     BottomLayer CR2032-SCK1                               45.1201      26.5740      90       ""                                                                      
SB38       Close                            TopLayer    SB-tiny                                   41.7801      24.0720      270      "Solder Jumper"                                                         
Label_6    LOGO_CE                          BottomLayer LOGO_CE                                   -113.0380    -152.3930    180      ""                                                                      
Label_7    LOGO_ESD                         BottomLayer LOGO_ESD                                  -113.0380    -152.3930    180      ""                                                                      
Label_8    LOGO_StickerArea_W21x6           BottomLayer LOGO_StickerArea_Border                   -113.0380    -152.3930    90       ""                                                                      
SB47       Close                            BottomLayer SB-tiny                                   14.5052      2.7627       90       "Solder Jumper"                                                         
SB48       Open                             BottomLayer SB-tiny                                   18.8206      2.8270       90       "Solder Jumper"                                                         
SB49       Open                             BottomLayer SB-tiny                                   34.0139      35.2812      270      "Solder Jumper"                                                         
SB50       Close                            BottomLayer SB-tiny                                   33.1641      33.7610      0        "Solder Jumper"                                                         
SB51       Open                             BottomLayer SB-tiny                                   33.1596      32.4292      360      "Solder Jumper"                                                         
SB33       Close                            BottomLayer SB-tiny                                   18.4311      38.5050      180      "Solder Jumper"                                                         
SB31       Open                             BottomLayer SB-tiny                                   18.0060      42.5060      360      "Solder Jumper"                                                         
CN14       HEADER_1X2                       TopLayer    Header_NF_1x2x2.54_TH                     40.1281      12.5090      180      ""                                                                      
JP2        HEADER_1X2                       TopLayer    Header_M_1x2x2.54_TH_V                    37.8671      46.2160      90       ""                                                                      
SB42       Open                             BottomLayer SB-tiny                                   56.1701      38.9720      270      "Solder Jumper"                                                         
Label_1    LOGO_ST                          TopLayer    LOGO_ST_Size3                             -113.0380    -152.3930    360      ""                                                                      
Label_3    LOGO_Nucleo_www                  TopLayer    LOGO_Nucleo_www                           -113.0380    -152.3930    90       ""                                                                      
R33        1K                               TopLayer    0402_RES                                  37.5931      36.9950      90       Resistor                                                                
SH1        "Shield 17.2x17.2x3"             TopLayer    Shield_17.2x17.2x3                        -113.0380    -152.3930    0        Shield                                                                  
STICKER_1  FCC_ID_Sticker_16x5              TopLayer    Sticker_FCC_ID_16x5mm                     -113.0380    -152.3930    360      "Sticker for FCC_ID 16x5mm"                                             
STICKER_2  Sticker_BrdRef_21x5              BottomLayer Sticker_BrdRef_21x5mm                     -113.0380    -152.3930    90       "Sticker_BrdRef 21x5mm"                                                 
STICKER_3  "Sticker_CPN_FG 16x5"            BottomLayer Sticker_CPN_FG_16x5mm                     -113.0380    -152.3930    180      "Sticker for CPN_FG 16x5mm"                                             
