Altium Designer Pick and Place Locations
C:\VIRGIL\AAA__JOB\ALTIUM\STM\Projets\MB1370B\BASE\MB1370B\03-Manufacturing\MB1370B_PCB\Assembly\MB1370-B01_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       19/09/19
Time:       00:08
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator   Comment              Layer       Footprint                          Center-X(mm) Center-Y(mm) Rotation Description                                                                                                                                           
CN2          "Header 5x2 Generic" BottomLayer CON_SAMTEC_FTSH-105-01-L-DV-K      143.7500     52.0000      90       "Surface mount, vertical male connector. Double row of 5 pins, 1.27mm pitch, 3.05mm lead. Mates with FFSD connector"                                  
C25          Capacitor            BottomLayer C0402                              89.2000      52.0750      180      "Capacitor, MLCC, 10pF, 50V, NPO, 5%, 0402, T=0,5mm"                                                                                                  
C24          Capacitor            BottomLayer C0402                              89.2000      52.9750      180      "Capacitor, MLCC, 10pF, 50V, NPO, 5%, 0402, T=0,5mm"                                                                                                  
CN1          FH52E-40S-0.5SH      BottomLayer CON_HRS_FH52E-40S-05SH             81.5400      64.8000      180      "FFC et FPC connector 0.5MM 40P LNG MTL FITNG SMT VERT MNT"                                                                                           
MIRE-PLACE-9 MIRE-PLACE-3         BottomLayer MIRE_PLACE_SMD_0P8MM               161.0000     5.0000       180      ""                                                                                                                                                    
MIRE-PLACE-8 MIRE-PLACE-3         TopLayer    MIRE_PLACE_SMD_0P8MM               161.0000     5.0000       0        ""                                                                                                                                                    
MIRE-PLACE-7 MIRE-PLACE-3         TopLayer    MIRE_PLACE_SMD_0P8MM               161.0000     112.0000     0        ""                                                                                                                                                    
MIRE-PLACE-6 MIRE-PLACE-3         BottomLayer MIRE_PLACE_SMD_0P8MM               161.0000     112.0000     180      ""                                                                                                                                                    
MIRE-PLACE-5 MIRE-PLACE-3         BottomLayer MIRE_PLACE_SMD_0P8MM               5.0000       5.0000       180      ""                                                                                                                                                    
MIRE-PLACE-4 MIRE-PLACE-3         TopLayer    MIRE_PLACE_SMD_0P8MM               5.0000       5.0000       0        ""                                                                                                                                                    
R7           Resistor             BottomLayer R0402                              96.4000      54.2500      360      Resistor,10K,0402,1%,1/16W                                                                                                                            
R10          Resistor             BottomLayer R0402                              96.4000      52.2500      360      Resistor,10K,0402,1%,1/16W                                                                                                                            
R6           Resistor             BottomLayer R0603                              74.8000      69.1750      90       Resistor,0R,0603,5%,1/10W                                                                                                                             
R1           Resistor             BottomLayer R0603                              138.6500     54.5250      180      Resistor,0R,0603,5%,1/10W                                                                                                                             
R3           Resistor             BottomLayer R0402                              87.8250      52.5250      270      Resistor,0R,0402,5%,1/16W                                                                                                                             
R17          Inductor             BottomLayer IND_0603_H0P8                      62.7000      47.8500      180      "Ferrite bead, 600R @ 100MHz,  1.3A, 150mOhm, 0603"                                                                                                   
C4           Capacitor            BottomLayer C0402                              149.8500     51.2250      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                
C3           Capacitor            BottomLayer C0805                              148.4000     51.6250      270      "Capacitor, MLCC, 10uF, 25V, X5R, 10%, 0805, T=0,85mm"                                                                                                
C2           Capacitor            BottomLayer C0805                              52.9500      52.9640      180      "Capacitor, MLCC, 4.7uF, 16V, 0805, X5R, 10%, T=1,25mm"                                                                                               
C16          Capacitor            BottomLayer C1206_H1P15                        44.3500      41.7140      360      "Capacitor, MLCC, 1uF, 50V, 1206, X7R, 10%, T=1mm"                                                                                                    
C1           Capacitor            BottomLayer C0402                              46.7000      57.1640      270      "Capacitor, MLCC, 220nF, 16V, 0402, X7R, 10%, T=0,5mm"                                                                                                
C5           Capacitor            BottomLayer C0603                              70.1500      49.0890      270      "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                                                                                                
C6           Capacitor            BottomLayer C0402                              71.4000      48.8390      270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                
C22          Capacitor            BottomLayer C1210                              118.7000     34.6840      360      "Capacitor, MLCC, 22uF, 16V, 1210, X7R, 20%, T=2,5mm, ESR 2mohm@410KHz"                                                                               
C17          Capacitor            BottomLayer C1210                              104.7250     40.2090      90       "Capacitor, MLCC, 22uF, 16V, 1210, X7R, 20%, T=2,5mm, ESR 2mohm@410KHz"                                                                               
C23          Capacitor            BottomLayer C0402                              113.7500     34.4840      180      "Capacitor, MLCC, 22pF, 50V, C0G, 5%, 0402, T=0,5mm"                                                                                                  
C21          Capacitor            BottomLayer C0402                              123.0750     36.9590      360      "Capacitor, MLCC, 1nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                  
C7           Capacitor            BottomLayer C0402                              111.3500     47.1090      360      "Capacitor, MLCC, 1nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                  
C15          Capacitor            BottomLayer C0402                              122.4000     42.4340      270      "Capacitor, MLCC, 220nF, 16V, 0402, X7R, 10%, T=0,5mm"                                                                                                
C18          Capacitor            BottomLayer C0402                              122.8250     41.0090      360      "Capacitor, MLCC, 220nF, 16V, 0402, X7R, 10%, T=0,5mm"                                                                                                
C20          Capacitor            BottomLayer C0402                              122.4250     39.7340      270      "Capacitor, MLCC, 22nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                 
C19          Capacitor            BottomLayer C0402                              123.8750     40.1750      360      "Capacitor, MLCC, 220nF, 16V, 0402, X7R, 10%, T=0,5mm"                                                                                                
C8           Capacitor            BottomLayer C0402                              120.1750     45.5590      270      "Capacitor, MLCC, 220nF, 16V, 0402, X7R, 10%, T=0,5mm"                                                                                                
C9           Capacitor            BottomLayer C1206_H1P15                        109.9250     44.4340      360      "Capacitor, MLCC, 1uF, 50V, 1206, X7R, 10%, T=1mm"                                                                                                    
C12          Capacitor            BottomLayer C0402                              145.5500     42.4350      270      "Capacitor, MLCC, 1nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                  
C10          Capacitor            BottomLayer C0402                              144.3750     42.4600      270      "Capacitor, MLCC, 1nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                  
C13          Capacitor            BottomLayer C0402                              143.2250     42.4350      270      "Capacitor, MLCC, 1nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                  
C14          Capacitor            BottomLayer C0402                              142.0250     42.4350      270      "Capacitor, MLCC, 1nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                  
C11          Capacitor            BottomLayer C0402                              140.8500     42.4600      270      "Capacitor, MLCC, 1nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                  
D1           SCHOTTKY_1A_2K       BottomLayer DIO_SMA_1A_2K                      45.7000      45.9640      90       "Low Drop power Schottky rectifier(1A, 40V, 0.37 V)"                                                                                                  
D2           SCHOTTKY_1A_2K       BottomLayer DIO_SMA_1A_2K                      109.2500     41.6340      360      "Low Drop power Schottky rectifier(1A, 40V, 0.37 V)"                                                                                                  
D3           DIODE_3P_DUAL_SERIES BottomLayer DIO_SOT323                         126.4000     41.2340      180      "Dual surface mount small signal schotky diode in series"                                                                                             
HW3          LCD_RK070ER9427L     TopLayer    LCD_DRAWING_ROCKTEK_RK070ER9427-CT -865.8550    -823.8600    360      "Display (TFT LCD) - 7-inch LCD Module 800x480 (RGB 24-bit) with integrated capacitive touch panel"                                                   
J2           CONN_FH12S-6S-05SH   BottomLayer CON_FCI_SFW6R-1STE9LF              143.7500     38.1850      180      "6-pin 1mm Pitch SMT connector for FPC/FFC lower contact type"                                                                                        
L1           INDUCTOR_POWER       BottomLayer IND_TDK_CLF7045T-100M-D            51.7000      48.2140      360      "Magnetic shield type wound inductor for power circuits 10uH 38mOhms 2.7A 20%"                                                                        
L2           INDUCTOR_POWER       BottomLayer IND_TDK_VLS4012ET-4R7M             110.0500     37.6840      90       "Surface mount Wound Magnetically shielded Power inductor. 4.7uH +/-20%; DCres:95mohm; 1.32A(-30% from initial value); 1.57A(+40°C temperature rise)" 
R8           Resistor             BottomLayer R0805                              49.9500      52.9640      180      Resistor,0R,0805,5%                                                                                                                                   
R4           Resistor             BottomLayer R0805                              48.2000      57.8390      270      "Resistor, 1R, 0805, 1%, 1/8W"                                                                                                                        
R15          Resistor             BottomLayer R0402                              72.4000      48.8390      270      Resistor,10K,0402,1%,1/16W                                                                                                                            
R13          Resistor             BottomLayer R0402                              72.4000      50.5390      270      Resistor,10K,0402,1%,1/16W                                                                                                                            
R14          Resistor             BottomLayer R0402                              96.4000      49.3750      180      Resistor,10K,0402,1%,1/16W                                                                                                                            
R9           Resistor             BottomLayer R0402                              96.4000      53.2500      360      Resistor,10K,0402,1%,1/16W                                                                                                                            
R12          Resistor             BottomLayer R0402                              96.4000      51.2500      360      Resistor,10K,0402,1%,1/16W                                                                                                                            
R27          Resistor             BottomLayer R0805                              122.4000     34.0590      180      Resistor,0R,0805,5%                                                                                                                                   
R22          Resistor             BottomLayer R0805                              104.5500     43.4590      180      Resistor,0R,0805,5%                                                                                                                                   
R28          Resistor             BottomLayer R0402                              113.7500     33.4840      180      Resistor,130K,0402,1%,1/16W                                                                                                                           
R26          Resistor             BottomLayer R0402                              123.0500     35.9890      360      Resistor,15K,0402,5%,1/16W                                                                                                                            
R16          Resistor             BottomLayer R0402                              111.3500     48.0590      360      Resistor,750K,0402,1%,1/16W                                                                                                                           
R18          Resistor             BottomLayer R0402                              111.3500     46.1590      360      Resistor,402K,0402,1%,1/16W                                                                                                                           
R29          Resistor             BottomLayer R0402                              113.7500     32.4340      360      Resistor,16K,0402,1%,1/16W                                                                                                                            
R23          Resistor             BottomLayer R0805                              129.4250     40.0840      180      Resistor,0R,0805,5%                                                                                                                                   
R21          Resistor             BottomLayer R0805                              122.3750     44.5590      360      Resistor,0R,0805,5%                                                                                                                                   
R20          Resistor             BottomLayer R0402                              118.8750     45.0840      360      Resistor,1M,0402,1%,1/16W                                                                                                                             
R25          Resistor             BottomLayer R0402                              124.4250     38.7590      270      Resistor,750K,0402,1%,1/16W                                                                                                                           
R24          Resistor             BottomLayer R0402                              123.3000     38.8340      90       Resistor,130K,0402,1%,1/16W                                                                                                                           
R19          Resistor             BottomLayer R0402                              118.8750     46.0840      180      Resistor,82K,0402,1%,1/16W                                                                                                                            
U1           TPS61165             BottomLayer MOS_SOT23-6L                       46.6500      54.1140      180      "High-Brightness White LED Driver in SOT-23 Package"                                                                                                  
U6           TPS65100             BottomLayer ICC_HTSSOP24-EPAD_7P8X4P4_P065     117.1500     40.3590      90       "Triple-Output LCD Supply With Linear Regulator and VCOM Buffer"                                                                                      
U5           FIL_EMIF_ESD_8L      BottomLayer ESD_UQFN16L-EPAD_3P3X1P35_P040     75.1250      49.6990      360      "8-line L-C EMI filter and ESD protection for LCD application"                                                                                        
U4           FIL_EMIF_ESD_8L      BottomLayer ESD_UQFN16L-EPAD_3P3X1P35_P040     79.0583      49.6990      360      "8-line L-C EMI filter and ESD protection for LCD application"                                                                                        
U3           FIL_EMIF_ESD_8L      BottomLayer ESD_UQFN16L-EPAD_3P3X1P35_P040     82.9917      49.6990      360      "8-line L-C EMI filter and ESD protection for LCD application"                                                                                        
U2           FIL_EMIF_ESD_8L      BottomLayer ESD_UQFN16L-EPAD_3P3X1P35_P040     86.9250      49.6990      360      "8-line L-C EMI filter and ESD protection for LCD application"                                                                                        
J1           CONN_FH12S-50S-05SH  BottomLayer CON_HRS_FH12A-50S-05SH             81.5400      45.2640      360      "50-pin 05mm Pitch connector for FPC/FFC top contact version"                                                                                         
