Altium Designer Pick and Place Locations
C:\Users\tguilhot\Documents\_SubVersion\HW_Boards\MB1454-STM32G0-OraZero64K-466-Disco\02-Manufacturing\MB1454B_PCB\Assembly\MB1454-B02_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       25-06-19
Time:       09:36
Revision:   7
Variant:    No variations
Units used: mm

Designator Comment                    Layer       Footprint                             Center-X(mm) Center-Y(mm) Rotation Description                                                                   
R8         Resistor                   TopLayer    R0402                                 1.4580       35.6874      360      Resistor,100R,0402,1%,1/16W                                                   
R7         Resistor                   TopLayer    R0402                                 1.5000       37.5000      180      Resistor,36K,0402,1%,1/16W                                                    
R5         Resistor                   TopLayer    R0402                                 6.2500       39.5000      180      Resistor,10K,0402,1%,1/16W                                                    
R2         Resistor                   TopLayer    R0402                                 7.5000       44.5000      180      Resistor,1K5,0402,1%,1/16W                                                    
Q1         9013-SOT23                 TopLayer    NPN_SOT23                             6.0000       42.0000      270      "NPN Bipolar Transistor"                                                      
CN7        "Jumper_Header 2x1 Fitted" BottomLayer CON_SAMTEC_TSW-102-07-G-S             15.7500      -0.7500      360      "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm - Shunt Fitted by default" 
CN5        "Jumper_Header 2x1 Fitted" BottomLayer CON_SAMTEC_TSW-102-07-G-S             15.7500      50.0000      360      "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm - Shunt Fitted by default" 
CN8        "Jumper_Header 2x1 Fitted" BottomLayer CON_SAMTEC_TSW-102-07-G-S             2.7500       -0.7500      180      "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm - Shunt Fitted by default" 
CN6        "Jumper_Header 2x1 Fitted" BottomLayer CON_SAMTEC_TSW-102-07-G-S             2.7500       50.0000      180      "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm - Shunt Fitted by default" 
M1         Comment                    TopLayer    MIRE-1.27mm                           14.7750      46.8750      0        ""                                                                            
M2         Comment                    TopLayer    MIRE-1.27mm                           1.7132       2.4000       0        ""                                                                            
A1         Comment                    TopLayer    ATTACHE                               9.2750       -3.5000      0        ""                                                                            
CN4        DIL8-LYCONN-7.40X1.83      TopLayer    CON_LYCONN_DIL8_7P40X1P83_P254        9.2750       -10.7500     0        "PCB socket DIL 8-pin"                                                        
B1         SW-PUSH-CMS_BLUE           TopLayer    SWI_WEALTHMETAL_TD-0341_4P_BLUE       9.2750       4.6640       270      "Non-Open Push-Button 0.1A 24V BLUE"                                          
C14        Capacitor                  TopLayer    C0402                                 9.2500       -15.0000     180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                        
C13        Capacitor                  TopLayer    C0402                                 2.2500       4.7500       90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                        
C7         Capacitor                  TopLayer    C0402                                 17.2500      34.5000      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                        
C4         Capacitor                  TopLayer    C0402                                 13.5000      34.5000      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                        
C3         Capacitor                  TopLayer    C0402                                 4.9000       37.8000      180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                        
C12        Capacitor                  TopLayer    C0402                                 9.7250       23.5000      90       "Capacitor, MLCC, 10pF, 50V, NPO, 5%, 0402, T=0,5mm"                          
C11        Capacitor                  TopLayer    C0402                                 4.7250       23.5000      90       "Capacitor, MLCC, 10pF, 50V, NPO, 5%, 0402, T=0,5mm"                          
C8         Capacitor                  TopLayer    C0402                                 1.7250       29.5000      270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                        
C10        Capacitor                  TopLayer    C0402                                 8.7500       26.0000      360      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                        
C5         Capacitor                  TopLayer    C0402                                 14.7500      34.5000      90       "Capacitor, MLCC, 10nF, 16V, X7R, 10%, 0402, T=0.5mm"                         
C2         Capacitor                  TopLayer    C0402                                 17.0000      40.0000      360      "Capacitor, MLCC, 1uF, 6V3, X5R, 10%, 0402, T=0,5mm"                          
C1         Capacitor                  TopLayer    C0402                                 15.0000      40.0000      180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                        
C9         Capacitor                  TopLayer    C0402                                 15.4500      29.2500      180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                        
C6         Capacitor                  TopLayer    C0402                                 16.0000      34.5000      90       "Capacitor, MLCC, 1uF, 6V3, X5R, 10%, 0402, T=0,5mm"                          
C15        Capacitor                  TopLayer    C0402                                 9.2500       -16.2500     180      "Capacitor, MLCC, 4.7uF, 6V3, X5R, 20%, 0402, T=0,5mm"                        
CN1        USB_uB_105017.0001         TopLayer    CON_USBMICROB_MOLEX_105017-0001_H2P90 9.2270       48.7020      180      "USB-MICRO-B, 0.65mm, RA, SMT, Bottom Mount,"                                 
CN2        "Header STLINK"            TopLayer    HDR_1x5_2R54_V_M                      16.1040      44.6040      90       "Header 5 pads for ST-LINK prog. Not fitted"                                  
JP1        "Jumper_Header 2x1 Fitted" TopLayer    CON_SAMTEC_TSW-102-07-G-S             1.9000       15.2489      90       "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm - Shunt Fitted by default" 
LD1        LD_BICOLOR_CMS             TopLayer    LED_BI-GR_HSMF-A201-A00J1             1.9050       44.8330      180      "LED Bicolor"                                                                 
LD2        LED_green                  TopLayer    LED_0603_GREEN                        17.0000      4.7500       270      "LED, Green, 0603"                                                            
R13        Resistor                   TopLayer    R0402                                 11.2250      24.7500      90       Resistor,4K7,0402,1%,1/16W                                                    
R14        Resistor                   TopLayer    R0402                                 12.4750      24.7500      90       Resistor,4K7,0402,1%,1/16W                                                    
R15        Resistor                   TopLayer    R0402                                 17.0000      7.5000       270      Resistor,510R,0402,1%,1/16W                                                   
R1         Resistor                   TopLayer    R0402                                 7.5000       45.7500      360      Resistor,100K,0402,1%,1/16W                                                   
R6         Resistor                   TopLayer    R0402                                 12.7500      38.7500      90       Resistor,100R,0402,1%,1/16W                                                   
R11        Resistor                   TopLayer    R0402                                 1.7250       24.7500      90       Resistor,10K,0402,1%,1/16W                                                    
R10        Resistor                   TopLayer    R0402                                 1.5000       31.2500      360      Resistor,100K,0402,1%,1/16W                                                   
R9         Resistor                   TopLayer    R0402                                 1.5000       33.7500      180      Resistor,4K7,0402,1%,1/16W                                                    
R3         Resistor                   TopLayer    R0402                                 1.2500       40.7500      90       Resistor,330R,0402,1%,1/16W                                                   
R12        Resistor                   TopLayer    R0402                                 3.1650       24.7500      90       Resistor,10K,0402,1%,1/16W                                                    
R4         Resistor                   TopLayer    R0402                                 2.7500       40.7500      90       Resistor,330R,0402,1%,1/16W                                                   
SB1        SB_OFF                     TopLayer    SOLDER-BRIDGE_R0603-0R                15.4500      27.0000      180      "Solder Bridge OFF"                                                           
U2         LDK120M33R                 TopLayer    REG_SOT23-5L                          16.0000      37.5000      180      "200 mA low quiescent current very low noise LDO"                             
U5         STM32G031J6M6              TopLayer    ICC_SO8_5X4_P127                      9.2750       -10.7500     360      "STM32G031Jx, SO8N package"                                                   
U4         ESD-TRANSIL                TopLayer    ESD_ST0201                            1.0000       4.7500       270      "ESD protection 6V1"                                                          
U3         STM32F103CBT6              TopLayer    ICC_LQFP48_7X7_P050                   7.7500       32.0000      360      "Medium-density performance line ARM-based 32-bit MCU with 128KB Flash"       
U1         USBLC6-2P6                 TopLayer    ESD_SOT666                            9.4850       43.7400      180      "USB OTG FS ESD protection"                                                   
X1         XTAL_8M_NX3225GD           TopLayer    CRY_NX3225GD_2P                       7.2500       23.7500      360      "Crystal 8Mhz, 8pF, -+50PPM, SMD"                                             
CN3        STM8-MODULE-DIL8-SOCKET    TopLayer    DIP8                                  9.5000       15.7500      0        STM8-MODULE-DIL8-                                                             
