Altium Designer Pick and Place Locations
C:\Users\tguilhot\Documents\_SubVersion\HW_Boards\MB1641-Nucleo64-IntSMPS\02-Manufacturing\MB1641C_PCB\Assembly\MB1641C_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       15/01/21
Time:       08:10
Revision:   9
Variant:    No variations
Units used: mm

Designator Comment                    Layer       Footprint                                                Center-X(mm) Center-Y(mm) Rotation Description                                                                                                           
U13        MLPF-WB55-01E3             TopLayer    ICC_BUMPLESS-CSP6_AN2348-FLIP-CHIP_1X1P60_P050-P0587     22.5891      50.1740      0        "2.4 GHz low pass filter matched to STM32WBx5Cx/Rx"                                                                   
R13        Resistor                   TopLayer    R0402                                                    37.4857      51.1001      360      Resistor,0R,0402,5%,1/16W                                                                                             
R5         Resistor                   TopLayer    R0402                                                    30.9147      54.2134      360      Resistor,0R,0402,5%,1/16W                                                                                             
R1         Resistor                   TopLayer    R0402                                                    30.0095      54.2118      180      Resistor,0R,0402,5%,1/16W                                                                                             
CN2        "BATTERY HOLDER"           BottomLayer BAT_RENATA-SMTU2032-LF_KEYSTONE-1769533_CR2032_SMD_2P_DI 45.3700      27.0340      270      "Battery Coin Cell holder, CR2032_20mm, Height 5.4mm"                                                                 
C17        Capacitor                  TopLayer    C0402                                                    28.0416      39.8847      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                             
C50        Capacitor                  TopLayer    C0402                                                    44.8700      23.0000      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                             
CN6        "Socket 8x1"               TopLayer    CON_SAMTEC_SSW-108-01-X-S                                11.1200      32.1700      270      "Socket 8x1, 2.54mm, VR, TH, height 8.51/2.64mm"                                                                      
CN8        "Socket 6x1"               TopLayer    CON_SAMTEC_SSW-106-01-X-S                                11.1200      11.8500      270      "Socket 6x1, 2.54mm, VR, TH, height 8.51/2.64mm"                                                                      
CN15       USB_uB_105017.0001         BottomLayer CON_USBMICROB_MOLEX_105017-0001_H2P90                    53.0450      5.3248       180      "USB-MICRO-B, 0.65mm, RA, SMT, Bottom Mount,"                                                                         
U2         LD1117S50TR                TopLayer    REG_SOT223-TAB                                           42.3750      35.8000      270      "IC REG LDO 5V 0.8A SOT223"                                                                                           
LD6        LD_BICOLOR_CMS             TopLayer    LED_BI-GR_HSMF-A201-A00J1                                46.5200      5.5000       360      "LED Bicolor"                                                                                                         
LD5        LED_green                  TopLayer    LED_0603_VISHAY_VLMTG1300-GS08_GREEN_1A2K_H0P8           56.9000      47.5500      270      "LED Green, 0603 SMD, Fw Voltage = 2.8V - 3.6V"                                                                       
LD4        LED_red                    TopLayer    LED_0603_VISHAY_VLMS1300-GS08_RED_1A2K_H0P8              48.2241      37.9981      90       "LED Red, 0603 SMD, 2V Forward Voltage"                                                                               
LD3        LED_red                    TopLayer    LED_0603_VISHAY_VLMS1300-GS08_RED_1A2K_H0P8              43.1240      2.5000       270      "LED Red, 0603 SMD, 2V Forward Voltage"                                                                               
LD2        LED_green                  TopLayer    LED_0603_VISHAY_VLMTG1300-GS08_GREEN_1A2K_H0P8           41.6310      2.5000       270      "LED Green, 0603 SMD, Fw Voltage = 2.8V - 3.6V"                                                                       
LD1        LED_blue                   TopLayer    LED_0603_VISHAY_VLMB1300-GS08_BLUE_1A2K_H0P8             40.0040      2.5000       270      "LED Blue, 0603 SMD, 3.3 V Forward Voltage"                                                                           
B4         SW-PUSH-CMS_KMR2_BLACK     TopLayer    SWI_C&K_Y78B23110FP__ITT_KMR231GLFS                      35.5040      2.5000       180      "Microminiature Tact Switch for SMT - KMR 2 Series - 1.9 mm height"                                                   
B3         SW-PUSH-CMS_KMR2_BLACK     TopLayer    SWI_C&K_Y78B23110FP__ITT_KMR231GLFS                      29.5785      2.5000       180      "Microminiature Tact Switch for SMT - KMR 2 Series - 1.9 mm height"                                                   
B2         SW-PUSH-CMS_KMR2_BLACK     TopLayer    SWI_C&K_Y78B23110FP__ITT_KMR231GLFS                      23.7225      2.5000       180      "Microminiature Tact Switch for SMT - KMR 2 Series - 1.9 mm height"                                                   
B1         SW-PUSH-CMS_KMR2_BLACK     TopLayer    SWI_C&K_Y78B23110FP__ITT_KMR231GLFS                      17.8100      2.5000       180      "Microminiature Tact Switch for SMT - KMR 2 Series - 1.9 mm height"                                                   
SB16       SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                                   34.6375      28.2000      360      "Solder Bridge 0402 ON"                                                                                               
SB14       SB_ON                      TopLayer    SOLDER-BRIDGE_R0402-0R                                   54.6788      41.2161      180      "Solder Bridge 0402 ON"                                                                                               
SB6        SB_ON                      TopLayer    SOLDER-BRIDGE_R0402-0R                                   17.2857      46.3799      180      "Solder Bridge 0402 ON"                                                                                               
SB5        SB_ON                      TopLayer    SOLDER-BRIDGE_R0402-0R                                   17.2765      47.3691      180      "Solder Bridge 0402 ON"                                                                                               
U12        ESD-TRANSIL                TopLayer    ESD_QFN2_1P6X1_P125                                      53.1500      5.7000       270      "High power transient voltage suppressor, 7V breakdown"                                                               
L4         Inductor                   TopLayer    IND_0805_WURTH_74479777310A                              17.1137      44.1843      270      "PMI Series 10 µH ±20% Multilayer SMD Inductor, 0805 25MHz 650mA dc 500mO Rdc"                                        
C51        Capacitor                  TopLayer    C0402                                                    54.2300      5.7000       270      Capacitor,MLCC,100pF,50V,NPO,+/-5%,0402,T=0,5mm                                                                       
JP6        "Jumper_Header 2x1 Fitted" TopLayer    CON_SAMTEC_TSW-102-07-G-S                                12.9924      46.1644      90       "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm - Shunt Fitted by default"                                         
Q1         9013-SOT23                 TopLayer    NPN_SOT23                                                54.1000      12.7000      180      "NPN Bipolar Transistor"                                                                                              
SB31       SB_ON                      TopLayer    SOLDER-BRIDGE_R0402-0R                                   39.9375      19.4941      360      "Solder Bridge 0402 ON"                                                                                               
C32        Capacitor                  TopLayer    C0402                                                    30.1290      46.0620      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                             
SB10       SB_ON                      TopLayer    SOLDER-BRIDGE_R0402-0R                                   31.5520      41.3786      90       "Solder Bridge 0402 ON"                                                                                               
SB12       SB_ON                      TopLayer    SOLDER-BRIDGE_R0402-0R                                   31.5520      43.1915      270      "Solder Bridge 0402 ON"                                                                                               
U1         STM32WB15_QFN48            TopLayer    ICC_UFQFPN48-EPAD_7X7_H0P55_P050                         23.5891      44.7120      180      "Multiprotocol wireless 32-bit MCU ARM®-based Cortex®-M4 with FPU, Bluetooth® Low-Energy and 802.15.4 radio solution" 
L5         Inductor                   TopLayer    IND_0402_MURATA_LQW15AN_H0P5                             18.8630      43.4366      360      "inductor, 10nH +-2%, 100mA max,1.3 ohm DC max, Q min = 13,0402"                                                      
JP5        "Header 8x2"               TopLayer    CON_SAMTEC_TSW-108-07-X-D                                25.7670      16.6770      270      "Header, 8x2, 2,54mm, VR, TH, Height 5.84mm/2.54mm"                                                                   
CN9        "Socket 8x1"               TopLayer    CON_SAMTEC_SSW-108-01-X-S                                59.3800      14.3900      90       "Socket 8x1, 2.54mm, VR, TH, height 8.51/2.64mm"                                                                      
C9         Capacitor                  TopLayer    C0805                                                    41.6700      30.1769      270      "Capacitor, MLCC, 10uF, 25V, X5R, +/-10%, 0805, T=0,85mm"                                                             
C10        Capacitor                  TopLayer    C0805                                                    42.5000      40.6000      180      "Capacitor, MLCC, 10uF, 25V, X5R, +/-10%, 0805, T=0,85mm"                                                             
C11        Cap_POL_TANA               TopLayer    CPOL_TAJ-A_1206_H180                                     52.6295      35.0478      360      "Capacitor, Tantalum, 4.7uF, 16V, 4ohms, +/-10%, pkg Type_A (3216 metric), T=1.6mm"                                   
CN3        "Header 5x1"               TopLayer    CON_SAMTEC_TSW-105-07-X-S                                9.5960       50.0507      270      "Header, 5x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm"                                                                   
CN4        "Header 2x1"               TopLayer    CON_SAMTEC_TSW-102-07-G-S                                32.5320      30.1830      180      "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm"                                                                   
CN11       "Jumper_Header 2x1 Fitted" TopLayer    CON_SAMTEC_TSW-102-07-G-S                                4.7700       54.6640      180      "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm - Shunt Fitted by default"                                         
CN12       "Jumper_Header 2x1 Fitted" TopLayer    CON_SAMTEC_TSW-102-07-G-S                                65.7300      54.6640      180      "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm - Shunt Fitted by default"                                         
CN13       "Header 6x1"               TopLayer    CON_SAMTEC_TSW-106-07-X-S                                53.5641      54.6640      360      "Header, 6x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm"                                                                   
D2         BAT60JFILM                 TopLayer    DIO_SOD323                                               53.7000      20.7000      270      BAT60JFILM                                                                                                            
U10        74LVC1G07GW-Q100           TopLayer    ICC_TSSOP5_SOT353-1_2P05X1P25_P065                       38.8000      17.5400      90       "Buffer/Driver 1-CH Non-Inverting Open Drain CMOS Automotive 5-Pin TSSOP T/R"                                         
U9         ECMF02-2AMX6               BottomLayer ESD_QFN-6L_1P7X1P5_P050                                  53.5740      9.2000       360      "Common mode filter with ESD protection for USB 2.0 interface"                                                        
JP1        "Jumper_Header 4x2"        TopLayer    CON_SAMTEC_TSW-104-07-X-D                                47.1130      46.0000      360      "Header, 4x2, 2,54mm, VR, TH, Height 5.84mm/2.54mm"                                                                   
JP3        "Jumper_Header 2x1 Fitted" TopLayer    CON_SAMTEC_TSW-102-07-G-S                                25.7725      30.1830      360      "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm - Shunt Fitted by default"                                         
JP4        "Jumper_Header 2x1 Fitted" TopLayer    CON_SAMTEC_TSW-102-07-G-S                                12.9924      52.2490      270      "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm - Shunt Fitted by default"                                         
R25        Resistor                   TopLayer    R0402                                                    46.0950      10.1383      270      Resistor,100R,0402,1%,1/16W                                                                                           
R27        Resistor                   TopLayer    R0402                                                    47.0450      10.1383      270      Resistor,100R,0402,1%,1/16W                                                                                           
U5         LD3985M33R                 BottomLayer REG_SOT23-5L                                             33.0100      15.8000      90       "Ultra low drop-low noise BiCMOS voltage, regulators low ESR capacitors compatible"                                   
U7         TXS0108EPWR                TopLayer    ICC_TSSOP20_6P50X4P40_P065                               34.3520      23.0000      270      "8bits_bidirectionnal level shifter, Delay 312ns/1V8"                                                                 
U8         STM32F103CBT6              TopLayer    ICC_LQFP48_7X7_P050                                      46.5950      16.2941      180      "Medium-density performance line ARM-based 32-bit MCU with 128KB Flash"                                               
X3         XTAL_2_PINS                TopLayer    CRY_NX3225GD_2P                                          48.7850      25.5285      360      "Crystal 8MHz, 8pF, +-20ppm, 500ohms max,  SMD"                                                                       
U3         LD39050PU33R               TopLayer    ICC_DFN6-EPAD_3X3_P095                                   54.6000      44.4299      360      "Low quiescent current and low noise voltage regulators"                                                              
U4         TPS2041C                   TopLayer    MOS_SOT23-5L                                             50.7641      37.9543      180      "5V Power Switch, 0.85A, RDSon 130mOhm max, with active low enable pin"                                               
R31        Resistor                   TopLayer    R0402                                                    56.2804      12.7691      270      Resistor,10R,0402,1%,1/16W                                                                                            
R32        Resistor                   TopLayer    R0402                                                    40.7000      17.1000      270      Resistor,100K,0402,1%,1/16W                                                                                           
C3         Capacitor                  BottomLayer C0402                                                    29.5625      44.9707      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                             
C6         Capacitor                  TopLayer    C0402                                                    30.7125      41.5780      90       "Capacitor, MLCC, 10pF, 50V, NPO, +/-5%, 0402, T=0,5mm"                                                               
C7         Capacitor                  TopLayer    C0402                                                    30.7125      43.2831      270      "Capacitor, MLCC, 10pF, 50V, NPO, +/-5%, 0402, T=0,5mm"                                                               
C8         Capacitor                  TopLayer    C0603                                                    43.4700      30.3394      90       "Capacitor, MLCC, 100nF, 50V, X7R, +/-10%, 0603, T=0.8mm"                                                             
C12        Capacitor                  TopLayer    C0402                                                    53.3731      39.6290      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                             
C13        Capacitor                  TopLayer    C0603                                                    56.2804      41.0853      90       "Capacitor, MLCC, 1uF, 16V, X5R, +/-10%, 0603, T=0,8mm"                                                               
C14        Capacitor                  TopLayer    C0402                                                    54.6720      47.4000      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                             
C15        Capacitor                  TopLayer    C0603                                                    53.6000      47.5107      270      "Capacitor, MLCC, 1uF, 16V, X5R, +/-10%, 0603, T=0,8mm"                                                               
C16        Capacitor                  TopLayer    C0402                                                    57.2959      41.1353      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                             
C18        Capacitor                  BottomLayer C0402                                                    20.1237      42.1705      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                             
C19        Capacitor                  BottomLayer C0402                                                    23.3391      48.0870      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                             
C20        Capacitor                  TopLayer    C0402                                                    27.3000      39.8847      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                             
C21        Capacitor                  BottomLayer C0603                                                    29.5625      15.7270      270      "Capacitor, MLCC, 1uF, 16V, X5R, +/-10%, 0603, T=0,8mm"                                                               
C22        Capacitor                  BottomLayer C0603                                                    36.0900      13.4500      90       "Capacitor, MLCC, 1uF, 16V, X5R, +/-10%, 0603, T=0,8mm"                                                               
C23        Capacitor                  TopLayer    C0402                                                    17.4640      41.5630      360      "Capacitor, MLCC, 4.7uF, 6V3, X5R, +/-20%, 0402, T=0,5mm"                                                             
C24        Capacitor                  TopLayer    C0402                                                    18.8190      41.9641      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                             
C25        Capacitor                  BottomLayer C0402                                                    30.5790      15.6225      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                             
C26        Capacitor                  BottomLayer C0402                                                    35.5487      16.0000      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                             
C27        Capacitor                  BottomLayer C0402                                                    34.8125      13.3700      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                             
C28        Capacitor                  BottomLayer C0402                                                    28.7180      39.9530      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                             
C29        Capacitor                  TopLayer    C0402                                                    18.3796      44.8243      90       "Capacitor, MLCC, 4.7uF, 6V3, X5R, +/-20%, 0402, T=0,5mm"                                                             
C31        Capacitor                  TopLayer    C0402                                                    22.6891      39.0331      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                             
C33        Capacitor                  BottomLayer C0402                                                    20.8140      49.5758      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                             
C34        Capacitor                  BottomLayer C0402                                                    20.8097      50.3434      180      Capacitor,MLCC,100pF,50V,NPO,+/-5%,0402,T=0,5mm                                                                       
C36        Capacitor                  TopLayer    C0402                                                    22.8000      56.0380      90       "Capacitor, High Q type for high frequency and high power, SMD, 1.2pF, 50V, 0,05pf, 0402"                             
C37        Capacitor                  TopLayer    C0402                                                    19.8160      56.0380      90       "Capacitor, High Q type for high frequency and high power, SMD, 1.2pF, 50V, 0,05pf, 0402"                             
C39        Capacitor                  TopLayer    C0402                                                    35.4000      50.6640      90       "Capacitor, High Q type for high frequency and high power, SMD, 1.2pF, 50V, 0,05pf, 0402"                             
C40        Capacitor                  TopLayer    C0402                                                    39.4733      50.6096      90       "Capacitor, High Q type for high frequency and high power, SMD, 1.2pF, 50V, 0,05pf, 0402"                             
C41        Capacitor                  TopLayer    C0402                                                    39.2125      25.2750      360      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                             
C42        Capacitor                  TopLayer    C0402                                                    30.0123      24.9000      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                             
C43        Capacitor                  TopLayer    C0402                                                    37.0000      17.5200      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                             
C44        Capacitor                  TopLayer    C0402                                                    47.8270      27.5605      180      "Capacitor, MLCC, 20pF, 50V, NPO, +/- 5%, 0402, T=0,5mm"                                                              
C45        Capacitor                  TopLayer    C0402                                                    49.7808      27.5605      360      "Capacitor, MLCC, 20pF, 50V, NPO, +/- 5%, 0402, T=0,5mm"                                                              
C46        Capacitor                  TopLayer    C0402                                                    47.3000      23.0000      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                             
C47        Capacitor                  TopLayer    C0402                                                    49.1000      10.5909      360      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                             
C48        Capacitor                  TopLayer    C0402                                                    40.7700      13.4000      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                             
C49        Capacitor                  TopLayer    C0402                                                    52.3000      19.1000      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                             
D1         SCHOTTKY_1A_2K             BottomLayer DIO_SOD523_1A_2K                                         31.0945      45.4207      360      "Small signal Schottky diodes"                                                                                        
L6         BEAD                       TopLayer    L0603                                                    30.4790      47.1138      180      "SMD Chip ferrite bead, 600R@100MHz +/-25%, 350mA, 500mohm DC, 0603, T=0.8mm"                                         
L1         Inductor                   TopLayer    IND_0402_MURATA_LGQ15HS02_H0P5                           21.2750      56.4880      180      "Inductor, LQG15H, 3.6nH, +-0.3nH 0402"                                                                               
R2         Resistor                   BottomLayer R0402                                                    40.0000      5.4891       270      Resistor,680R,0402,1%,1/16W                                                                                           
R3         Resistor                   BottomLayer R0402                                                    41.6310      5.4891       270      Resistor,680R,0402,1%,1/16W                                                                                           
R4         Resistor                   BottomLayer R0402                                                    43.1240      5.4891       270      Resistor,680R,0402,1%,1/16W                                                                                           
R6         Resistor                   BottomLayer R0402                                                    29.0180      42.6530      90       Resistor,10K,0402,1%,1/16W                                                                                            
R7         Resistor                   BottomLayer R0402                                                    19.4400      3.0900       180      Resistor,1K,0402,1%,1/16W                                                                                             
R8         Resistor                   BottomLayer R0402                                                    24.6000      4.0125       180      Resistor,1K,0402,1%,1/16W                                                                                             
R9         Resistor                   BottomLayer R0402                                                    30.5260      3.0289       180      Resistor,1K,0402,1%,1/16W                                                                                             
R10        Resistor                   TopLayer    R0402                                                    55.7304      47.4000      270      Resistor,270R,0402,1%,1/16W                                                                                           
R11        Resistor                   TopLayer    R0402                                                    49.6150      35.0478      360      Resistor,10K,0402,1%,1/16W                                                                                            
R12        Resistor                   TopLayer    R0402                                                    48.2241      35.7478      270      Resistor,1K,0402,1%,1/16W                                                                                             
R14        Resistor                   TopLayer    R0402                                                    55.1977      17.3094      270      Resistor,2K7,0402,1%,1/16W                                                                                            
R15        Resistor                   TopLayer    R0402                                                    54.3255      17.3094      90       Resistor,4K7,0402,1%,1/16W                                                                                            
R16        Resistor                   TopLayer    R0402                                                    55.1397      16.0441      360      Resistor,10K,0402,1%,1/16W                                                                                            
R17        Resistor                   TopLayer    R0402                                                    53.3000      15.1590      360      Resistor,100R,0402,1%,1/16W                                                                                           
R18        Resistor                   TopLayer    R0402                                                    50.9130      22.8875      90       Resistor,10K,0402,1%,1/16W                                                                                            
R19        Resistor                   TopLayer    R0402                                                    52.2941      17.5000      90       Resistor,100K,0402,1%,1/16W                                                                                           
R20        Resistor                   TopLayer    R0402                                                    55.1397      15.1590      180      Resistor,36K,0402,1%,1/16W                                                                                            
R21        Resistor                   BottomLayer R0402                                                    52.4750      10.7000      180      Resistor,1K5,0402,1%,1/16W                                                                                            
R22        Resistor                   TopLayer    R0402                                                    49.9130      22.8875      90       Resistor,10K,0402,1%,1/16W                                                                                            
R23        Resistor                   TopLayer    R0402                                                    52.1000      5.7000       90       Resistor,100K,0402,1%,1/16W                                                                                           
R24        Resistor                   TopLayer    R0402                                                    46.5000      23.0000      90       Resistor,100K,0402,1%,1/16W                                                                                           
R26        Resistor                   TopLayer    R0402                                                    43.2000      23.0000      270      Resistor,4K7,0402,1%,1/16W                                                                                            
R28        Resistor                   TopLayer    R0402                                                    44.0700      23.0000      270      Resistor,4K7,0402,1%,1/16W                                                                                            
R29        Resistor                   TopLayer    R0402                                                    44.3450      10.5760      180      Resistor,100R,0402,1%,1/16W                                                                                           
R30        Resistor                   TopLayer    R0402                                                    39.6625      14.6000      360      Resistor,10K,0402,1%,1/16W                                                                                            
SB13       SB_ON                      TopLayer    SOLDER-BRIDGE_R0402-0R                                   39.9900      30.4175      90       "Solder Bridge 0402 ON"                                                                                               
SB15       SB_ON                      TopLayer    SOLDER-BRIDGE_R0402-0R                                   53.0961      37.7793      90       "Solder Bridge 0402 ON"                                                                                               
SB17       SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                                   36.3325      42.2435      360      "Solder Bridge 0402 ON"                                                                                               
SB19       SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                                   39.3900      41.8245      90       "Solder Bridge 0402 ON"                                                                                               
SB20       SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                                   29.6000      39.9530      90       "Solder Bridge 0402 ON"                                                                                               
SB22       SB_ON                      TopLayer    SOLDER-BRIDGE_R0402-0R                                   21.8100      38.4375      90       "Solder Bridge 0402 ON"                                                                                               
SB24       SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                                   30.7125      49.0000      360      "Solder Bridge 0402 ON"                                                                                               
SB28       SB_ON                      TopLayer    SOLDER-BRIDGE_R0402-0R                                   55.1977      19.5816      270      "Solder Bridge 0402 ON"                                                                                               
SB29       SB_ON                      TopLayer    SOLDER-BRIDGE_R0402-0R                                   53.3231      16.7469      270      "Solder Bridge 0402 ON"                                                                                               
SB32       SB_ON                      TopLayer    SOLDER-BRIDGE_R0402-0R                                   39.6625      15.6600      180      "Solder Bridge 0402 ON"                                                                                               
X1         XTAL_4_PINS                TopLayer    CRY_NX2016SA_4P                                          18.3266      50.0036      360      "Crystal 32MHz, 8pF, +-10ppm, 60ohms max, SMD"                                                                        
X2         XTAL_2_PINS                TopLayer    CRY_NX2012SA_2P                                          29.3469      42.4790      90       "Crystal 32.768kHz, 7pF, +-20ppm, 80Kohms max, SMD"                                                                   
SB30       SB_ON                      TopLayer    SOLDER-BRIDGE_R0402-0R                                   42.1000      22.8625      270      "Solder Bridge 0402 ON"                                                                                               
SB25       SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                                   30.1625      47.4000      180      "Solder Bridge 0402 ON"                                                                                               
SB26       SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                                   33.3200      46.8625      270      "Solder Bridge 0402 ON"                                                                                               
SB27       SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                                   32.2000      47.8875      90       "Solder Bridge 0402 ON"                                                                                               
SB21       SB_ON                      TopLayer    SOLDER-BRIDGE_R0402-0R                                   20.8391      38.4375      90       "Solder Bridge 0402 ON"                                                                                               
SB23       SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                                   16.9125      44.9707      180      "Solder Bridge 0402 ON"                                                                                               
CN14       "Header 2x1"               TopLayer    CON_SAMTEC_TSW-102-07-G-S                                39.0600      10.5760      180      "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm"                                                                   
JP2        "Jumper_Header 2x1 Fitted" TopLayer    CON_SAMTEC_TSW-102-07-G-S                                38.9250      46.0000      90       "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm - Shunt Fitted by default"                                         
R33        Resistor                   BottomLayer R0402                                                    14.3500      41.0600      360      Resistor,1K,0402,1%,1/16W                                                                                             
SB11       SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                                   17.5625      3.0900       180      "Solder Bridge 0402 ON"                                                                                               
CN10       "Header 19x2"              TopLayer    CON_SAMTEC_TSW-119-09-X-D                                65.7300      28.3600      270      "Header, 19x2, 2,54mm, VR, TH, Height 5.84mm/10.16mm"                                                                 
CN7        "Header 19x2"              TopLayer    CON_SAMTEC_TSW-119-09-X-D                                4.7700       28.3600      270      "Header, 19x2, 2,54mm, VR, TH, Height 5.84mm/10.16mm"                                                                 
CN5        "Socket 10x1"              TopLayer    CON_SAMTEC_SSW-110-01-X-S                                59.3800      38.7740      90       "Socket 10x1, 2.54mm, VR, TH, height 8.51/2.64mm"                                                                     
SW5        SW_MECA                    BottomLayer SWI_SPDT-RA_TE-CONNECTIVITY_MLL1200S_1P2T                34.7270      22.8150      90       "SPDT RA SMT SLIDE SWITCH"                                                                                            
J2         SMA-J-P-H-ST-EM1           TopLayer    CON_SMA-RF_CINCH_142-0701-851                            39.4728      55.3953      360      "RF SMA connector PCB edge"                                                                                           
SC1        Shield-clip_S0951-46R      TopLayer    CLIP_HARWIN_S0951-46R                                    15.8391      41.7200      90       "shield clip Harwin S0951-46R to fix RF shielded cavity"                                                              
SC2        Shield-clip_S0951-46R      TopLayer    CLIP_HARWIN_S0951-46R                                    20.6900      53.2200      180      "shield clip Harwin S0951-46R to fix RF shielded cavity"                                                              
SC3        Shield-clip_S0951-46R      TopLayer    CLIP_HARWIN_S0951-46R                                    24.3400      36.2200      180      "shield clip Harwin S0951-46R to fix RF shielded cavity"                                                              
SC4        Shield-clip_S0951-46R      TopLayer    CLIP_HARWIN_S0951-46R                                    32.8400      41.8700      90       "shield clip Harwin S0951-46R to fix RF shielded cavity"                                                              
HW20       Daughter_Board             TopLayer    SHIELD_RF_ST-CUSTOM_17P2X17P2_H3                         -244.5936    -206.1699    90       "RF shield (17,2x17,2x3mm), Brass with Sn finishing, Sheet tickness : 0,2mm"                                          
HW18       STICKER_PRODUCT            BottomLayer STICKER_PRODUCT_25X9                                     -244.5936    -206.1699    360      "Sticker product 25x9 mm"                                                                                             
HW16       STICKER_BOARD              BottomLayer STICKER_BOARD_25X9                                       -244.5936    -206.1699    270      "Sticker Board 25x9 mm"                                                                                               
