Altium Designer Pick and Place Locations
C:\Subversion\MB1684-STM32C0-Spider32K-443-DK\Trunk\02-Manufacturing\MB1684A_PCB\Assembly\MB1684A_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       25/06/21
Time:       15:21
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator Comment                    Layer       Footprint                                                          Center-X(mm) Center-Y(mm) Rotation Description                                                                                                  
M1         MARK                       TopLayer    MARK                                                               69.0000      20.5000      0        ""                                                                                                           
C11        Capacitor                  TopLayer    C0402                                                              9.5028       10.1249      270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                                                       
U5         USBLC6-2P6                 TopLayer    ESD_SOT666                                                         7.5438       11.8250      270      "USB OTG FS ESD protection"                                                                                  
HW2        STICKER_BOARD              BottomLayer STICKER_Board_15X5                                                 -254.5784    -223.6391    180      "Sticker board 15x5 mm"                                                                                      
C2         Capacitor                  TopLayer    C0402                                                              11.8238      18.6079      360      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                                                       
CN1        "Header 2x2"               TopLayer    CON_SAMTEC_TSW-102-09-G-D                                          3.7000       19.8000      90       "Header, 2x2, 2.54mm, VR, TH, T=5.84mm/10.16mm"                                                              
U2         ESD-TRANSIL                TopLayer    ESD_ST0201                                                         15.8020      18.8064      360      "ESD protection 6V1"                                                                                         
SB1        SB_ON                      TopLayer    SOLDER-BRIDGE_R0402-0R                                             19.2007      18.6500      180      "Solder Bridge 0402 ON"                                                                                      
SB2        SB_ON                      TopLayer    SOLDER-BRIDGE_R0402-0R                                             21.5265      18.6500      180      "Solder Bridge 0402 ON"                                                                                      
CN4        "Header 4x1"               TopLayer    CON_988-JIUBABA_A2006LF-04A                                        64.5000      4.1750       360      "Header 4x1, 2mm, VR, SMT"                                                                                   
X1         XTAL_8M_NX3225GD           TopLayer    CRY_NX3225GD_2P                                                    24.0853      11.5603      90       "Crystal 8Mhz, 8pF, -+50PPM, SMD"                                                                            
U4         STM32F103CBT6              TopLayer    ICC_LQFP48_7X7_P050                                                15.2580      12.8249      90       "Medium-density performance line ARM-based 32-bit MCU with 128KB Flash"                                      
U6         LDK120M33R                 BottomLayer REG_SOT23-5L                                                       9.4319       17.3887      90       "200 mA low quiescent current very low noise LDO"                                                            
SB3        SB_OFF                     TopLayer    SOLDER-BRIDGE_R0603-0R                                             24.7857      15.7020      180      "Solder Bridge OFF"                                                                                          
R4         Resistor                   TopLayer    R0402                                                              60.6623      16.7988      45       Resistor,5K1,0402,1%,1/16W                                                                                   
R5         Resistor                   TopLayer    R0402                                                              21.3830      16.7566      180      Resistor,4K7,0402,1%,1/16W                                                                                   
R6         Resistor                   TopLayer    R0402                                                              21.3830      15.6377      180      Resistor,4K7,0402,1%,1/16W                                                                                   
R15        Resistor                   TopLayer    R0402                                                              21.0831      7.2783       90       Resistor,10K,0402,1%,1/16W                                                                                   
R14        Resistor                   TopLayer    R0402                                                              20.0331      7.2783       90       Resistor,10K,0402,1%,1/16W                                                                                   
R17        Resistor                   TopLayer    R0402                                                              15.5806      6.9227       360      Resistor,100K,0402,1%,1/16W                                                                                  
R16        Resistor                   TopLayer    R0402                                                              13.7238      6.9227       360      Resistor,4K7,0402,1%,1/16W                                                                                   
R21        Resistor                   BottomLayer R0402                                                              10.8618      8.2761       90       Resistor,100R,0402,1%,1/16W                                                                                  
R18        Resistor                   BottomLayer R0402                                                              6.8424       10.7113      360      Resistor,36K,0402,1%,1/16W                                                                                   
R7         Resistor                   TopLayer    R0402                                                              9.5028       15.0773      270      Resistor,100R,0402,1%,1/16W                                                                                  
R19        Resistor                   BottomLayer R0402                                                              8.6424       10.7113      360      Resistor,10K,0402,1%,1/16W                                                                                   
R1         Resistor                   TopLayer    R0402                                                              7.7238       18.2248      90       Resistor,330R,0402,1%,1/16W                                                                                  
R2         Resistor                   TopLayer    R0402                                                              8.8238       18.2000      90       Resistor,330R,0402,1%,1/16W                                                                                  
R20        Resistor                   BottomLayer R0402                                                              10.8744      10.0314      270      Resistor,1K5,0402,1%,1/16W                                                                                   
R11        Resistor                   TopLayer    R0402                                                              6.2320       9.5096       90       Resistor,100K,0402,1%,1/16W                                                                                  
Q1         9013-SOT23                 BottomLayer NPN_SOT23                                                          8.3800       8.2955       360      "NPN Bipolar Transistor"                                                                                     
LD3        LED_green                  TopLayer    LED_0402_EVERLIGHT_16-213SYGC/S530-E3-TR8 _YELLOW-GREEN_1A2K_H0P45 56.8300      12.6150      270      "LED, Yellow Green, 2V, 25mA, 0402, 0.45mm"                                                                  
LD1        LD_BICOLOR_CMS             TopLayer    LED_BI-GR_HSMF-A201-A00J1                                          9.7000       20.8998      90       "LED Bicolor"                                                                                                
HW1        STICKER_PRODUCT            BottomLayer STICKER_PRODUCT_15X5                                               -254.5784    -223.6391    180      "Sticker product 15x5 mm"                                                                                    
CN3        USB_uB_105017.0001         TopLayer    CON_USBMICROB_MOLEX_105017-0001_H2P90                              3.0000       11.5000      270      "USB-MICRO-B, 0.65mm, RA, SMT, Bottom Mount,"                                                                
C1         Capacitor                  TopLayer    C0402                                                              13.6238      18.6500      360      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                    
C9         Capacitor                  TopLayer    C0402                                                              22.0633      12.5768      270      "Capacitor, MLCC, 10pF, 50V, NPO, 5%, 0402, T=0,5mm"                                                         
C10        Capacitor                  TopLayer    C0402                                                              22.0633      10.6868      90       "Capacitor, MLCC, 10pF, 50V, NPO, 5%, 0402, T=0,5mm"                                                         
C8         Capacitor                  TopLayer    C0402                                                              23.2537      14.3903      180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                                                       
C7         Capacitor                  TopLayer    C0402                                                              21.3830      14.4566      180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                                                       
C20        Capacitor                  BottomLayer C0402                                                              10.4500      14.2899      360      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                                                       
C18        Capacitor                  BottomLayer C0402                                                              10.4500      15.1789      360      "Capacitor, MLCC, 1uF, 6V3, X5R, 10%, 0402, T=0,5mm"                                                         
C17        Capacitor                  BottomLayer C0402                                                              11.7126      17.8628      90       "Capacitor, MLCC, 10nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                        
C14        Capacitor                  TopLayer    C0402                                                              17.6331      6.9227       360      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                                                       
C21        Capacitor                  BottomLayer C0402                                                              8.5569       14.2899      180      "Capacitor, MLCC, 1uF, 6V3, X5R, 10%, 0402, T=0,5mm"                                                         
C19        Capacitor                  BottomLayer C0402                                                              8.5569       15.1789      180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                                                       
CN5        "Header 19x2"              TopLayer    CON_SAMTEC_TSW-119-09-X-D                                          32.7000      3.5000       360      "Header, 19x2, 2,54mm, VR, TH, Height 5.84mm/10.16mm"                                                        
CN2        "Socket 10x2_DIP20"        TopLayer    CON_FCI_DILB20P-223TLF                                             40.3600      12.5896      180      "Socket_IC, 20 (2 x 10) Pos DIP, 0.3" (7.62mm) Row Spacing Socket Tin Through Hole"                          
CN6        "Header STLINK"            TopLayer    HDR_1x5_2R54_V_M                                                   4.0600       3.5300       180      "Header 5 pads for ST-LINK prog. Not fitted"                                                                 
U1         NHD-C0216CZ-FSW-FBW-3V3    TopLayer    LCD_NHD_C0216CZ_FSW_FBW_3V3                                        44.9999      20.5749      360      "Character LCD Display Module Transflective 5 x 8 Dots FSTN - Film Super-Twisted Nematic LED - White Serial" 
SB4        SB_OFF                     TopLayer    SOLDER-BRIDGE_R0603-0R                                             23.6500      7.0848       180      "Solder Bridge OFF"                                                                                          
R10        Resistor                   TopLayer    R0402                                                              58.2050      10.3446      270      Resistor,680R,0402,1%,1/16W                                                                                  
R9         Resistor                   TopLayer    R0402                                                              56.8300      10.3446      270      Resistor,680R,0402,1%,1/16W                                                                                  
R12        Resistor                   TopLayer    R0402                                                              69.1303      9.0946       90       Resistor,2K,0402,1%,1/16W                                                                                    
R13        Resistor                   TopLayer    R0402                                                              70.1250      9.0946       90       Resistor,510R,0402,1%,1/16W                                                                                  
R8         Resistor                   TopLayer    R0402                                                              70.1250      10.8101      90       Resistor,820R,0402,1%,1/16W                                                                                  
R3         Resistor                   TopLayer    R0402                                                              69.6175      17.2128      135      Resistor,1K8,0402,1%,1/16W                                                                                   
LD2        LED_red                    TopLayer    LED_0402_KINGBRIGHT_KPHHS-1005SURCK_HYPER-RED_1A2K_H0P5            58.2050      12.6010      90       "LED 0402 Red"                                                                                               
CN7        "Header 10x1"              BottomLayer CON_SAMTEC_TSW-110-14-G-S                                          88.0574      20.4313      360      "Header 10x1, 2,54mm height  10.67mm"                                                                        
CN8        "Header 10x1"              BottomLayer CON_SAMTEC_TSW-110-14-G-S                                          88.0574      12.8114      360      "Header 10x1, 2,54mm height  10.67mm"                                                                        
C13        Capacitor                  TopLayer    C0402                                                              23.8792      8.2481       360      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                    
C12        Capacitor                  TopLayer    C0402                                                              68.1603      9.0946       90       "Capacitor, MLCC, 10nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                     
C5         Capacitor                  TopLayer    C0603                                                              82.2284      16.1835      90       "Capacitor, MLCC, 2.2uF, 16V, X5R,+/-10%, 0603, T=0.8mm"                                                     
C6         Capacitor                  TopLayer    C0402                                                              83.3946      16.4347      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                    
C16        Capacitor                  BottomLayer C0603                                                              33.9775      19.7000      180      "Capacitor, MLCC, 1uF, 25V, X5R, +/-10%, 0603, T=0,8mm"                                                      
C15        Capacitor                  BottomLayer C0603                                                              34.0775      21.2500      360      "Capacitor, MLCC, 1uF, 25V, X5R, +/-10%, 0603, T=0,8mm"                                                      
C3         Capacitor                  TopLayer    C0603                                                              55.5600      17.2500      270      "Capacitor, MLCC, 1uF, 25V, X5R, +/-10%, 0603, T=0,8mm"                                                      
B1         SW-PUSH-CMS_KMR2_BLACK     TopLayer    SWI_C&K_Y78B23110FP__ITT_KMR231GLFS                                15.2500      20.9498      180      "Microminiature Tact Switch for SMT - KMR 2 Series - 1.9 mm height"                                          
U3         STM32C011F6U6              TopLayer    ICC_UFQFPN20_3X3_P050                                              86.4179      16.5714      360      "MCU, ARM?-based 32-bit MCU Cortex-M0+, 32KB Flash, 6KB SRAM"                                                
JP1        "Jumper_Header 2x1 Fitted" TopLayer    CON_SAMTEC_TSW-102-07-G-S                                          20.8020      21.2500      360      "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm - Shunt Fitted by default"                                
C4         Capacitor                  TopLayer    C0402                                                              54.4602      17.3407      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                    
B2         "Joystick MT-008A_M"       TopLayer    SWI_XIEJIA_MT-008A_6P                                              65.2000      13.5680      135      "Joystick, 4 dir, 1 OK"                                                                                      
