Altium Designer Pick and Place Locations
C:\Subversion\MB1717-Nucleo64-LQFP48\Trunk\02-Manufacturing\MB1717B_PCB\Assembly\MB1717B_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       05/01/21
Time:       15:43
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator Comment                        Layer       Footprint                               Center-X(mm) Center-Y(mm) Rotation Description                                                                   
SB30       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                  17.7300      19.6850      180      "Solder Bridge ON"                                                            
SB33       SB_OFF                         TopLayer    SOLDER-BRIDGE_R0603-0R                  12.1150      9.3980       360      "Solder Bridge OFF"                                                           
SB32       SB_ON                          TopLayer    SOLDER-BRIDGE_R0603-0R                  8.4670       9.3980       180      "Solder Bridge ON"                                                            
SB31       SB_OFF                         TopLayer    SOLDER-BRIDGE_R0603-0R                  12.1150      10.7950      360      "Solder Bridge OFF"                                                           
SB29       SB_OFF                         TopLayer    SOLDER-BRIDGE_R0603-0R                  15.8250      20.4470      180      "Solder Bridge OFF"                                                           
R31        Resistor                       TopLayer    R0402                                   15.8750      22.8600      360      Resistor,0R,0402,5%,1/16W                                                     
HW1        STICKER_PRODUCT                TopLayer    STICKER_PRODUCT_25X9                    -230.0000    -190.0000    360      "Sticker product 25x9 mm"                                                     
HW2        STICKER_BOARD                  BottomLayer STICKER_BOARD_25X9                      -230.0000    -190.0000    180      "Sticker Board 25x9 mm"                                                       
D1         BAT60JFILM                     TopLayer    DIO_SOD323                              29.4386      68.8086      270      BAT60JFILM                                                                    
SB17       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                  14.8852      67.3100      180      "Solder Bridge ON"                                                            
U3         STMPS2141STR                   TopLayer    MOS_SOT23-5L                            52.8320      60.1472      0        "Enhanced single channel power switches with active low enable pin"           
R22        Resistor                       TopLayer    R0603                                   56.1340      60.5282      270      Resistor,47K,0603,1%,1/10W                                                    
R16        Resistor                       TopLayer    R0603                                   53.6194      64.3382      270      Resistor,1K,0603,1%,1/10W                                                     
LD2        LED_red                        TopLayer    LED_0603_RED                            55.1942      64.2874      270      "LED, Red, 0603"                                                              
C14        Capacitor                      TopLayer    C0603                                   51.8922      56.5912      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0603, T=0,8mm"                     
C6         Capacitor                      TopLayer    C0603                                   49.9872      60.5536      90       "Capacitor, MLCC, 1uF, 16V, X5R, +/-10%, 0603, T=0,8mm"                       
R5         Resistor                       TopLayer    R0603                                   23.1394      68.8086      270      Resistor,100K,0603,1%,1/10W                                                   
R6         Resistor                       TopLayer    R0603                                   25.9080      68.8086      90       Resistor,4K7,0603,1%,1/10W                                                    
R7         Resistor                       TopLayer    R0603                                   27.4574      68.8086      270      Resistor,2K7,0603,1%,1/10W                                                    
T2         BSN20                          BottomLayer MOS_SOT23                               42.4102      33.8176      270      "Transistor, N-channel enhancement mode field-effect transistor"              
U5         LD1117S50TR                    TopLayer    REG_SOT223-TAB                          10.9220      38.4810      0        "IC REG LDO 5V 0.8A SOT223"                                                   
X2         XTAL_2_PINS                    TopLayer    CRY_NX2012SA_2P                         13.3350      22.2250      90       "Crystal 32.768kHz, 6pF, -+20ppm, 80Kohm max, SMD"                            
X3         XTAL_4_PINS                    TopLayer    CRY_NX1612SA_4P                         12.7000      17.1450      270      "Crystal 48MHz, 7pF, +-20 ppm, 80ohm max, SMD"                                
LD1        LD_BICOLOR_CMS                 TopLayer    LED_BI-GR_HSMF-A201-A00J1               49.5554      72.8218      180      "LED Bicolor"                                                                 
X1         XTAL_2_PINS                    TopLayer    CRY_NX3225GD_2P                         16.2560      62.4332      90       "Crystal 8MHz, 8pF, +-20ppm, 500ohms max,  SMD"                               
T1         9013-SOT23                     TopLayer    NPN_SOT23                               45.2374      73.1774      0        "NPN Bipolar Transistor"                                                      
U1         USBLC6-2SC6                    TopLayer    ESD_SOT23-6L                            36.4998      69.2150      180      "Very low capacitance ESD protection"                                         
CN10       "Header 19x2"                  TopLayer    CON_SAMTEC_TSW-119-09-X-D               54.6100      22.8600      270      "Header, 19x2, 2,54mm, VR, TH, Height 5.84mm/10.16mm"                         
CN7        "Header 19x2"                  TopLayer    CON_SAMTEC_TSW-119-09-X-D               -6.3500      22.8600      270      "Header, 19x2, 2,54mm, VR, TH, Height 5.84mm/10.16mm"                         
CN8        "Socket 6x1"                   TopLayer    CON_SAMTEC_SSW-106-03-X-S               0.0000       6.3500       270      "Socket, 6x1, 2.54mm, VR, TH, Height 8.51mm/10mm"                             
CN9        "Socket 8x1"                   TopLayer    CON_SAMTEC_SSW-108-03-X-S               48.2600      8.8900       90       "Socket, 8x1, 2.54mm, VR, TH, Height 8.51mm/10mm"                             
CN6        "Socket 8x1"                   TopLayer    CON_SAMTEC_SSW-108-03-X-S               0.0000       26.6700      270      "Socket, 8x1, 2.54mm, VR, TH, Height 8.51mm/10mm"                             
CN5        "Socket 10x1"                  TopLayer    CON_SAMTEC_SSW-110-03-X-S               48.2600      33.2740      90       "Socket, 10x1, 2.54mm, VR, TH, Height 8.51mm/10mm"                            
B1         SW-PUSH-CMS                    TopLayer    SWI_WEALTHMETAL_TD-0341_4P_BLUE         15.8750      48.2600      270      "Non-Open Push-Button 0.1A 24V"                                               
B2         SW-PUSH-CMS                    TopLayer    SWI_WEALTHMETAL_TD-0341_4P_BLACK        32.3850      48.2600      90       "Non-Open Push-Button 0.1A 24V BLACK"                                         
CN2        "Header 4x1"                   TopLayer    CON_988-JIUBABA_PHFS25-11-04-G0B115-T-1 11.4300      71.1200      90       "Header, 4x1, 2.54mm, VR, TH, Height 6mm/3mm"                                 
JP6        "Jumper_Header 2x1 Fitted"     TopLayer    CON_SAMTEC_TSW-102-07-G-S               23.4950      37.4650      360      "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm - Shunt Fitted by default" 
JP3        "Jumper_Header 2x1"            TopLayer    CON_SAMTEC_TSW-102-09-X-S               55.8800      72.3900      90       "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/10.16mm"                          
JP2        "Jumper_Header 2x1"            TopLayer    CON_SAMTEC_TSW-102-09-X-S               -7.6200      72.3900      90       "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/10.16mm"                          
JP4        "Jumper_Header 2x1"            TopLayer    CON_SAMTEC_TSW-102-07-G-S               2.5400       57.1500      90       "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm"                           
D3         BAT60JFILM                     TopLayer    DIO_SOD323                              37.3126      61.2140      360      BAT60JFILM                                                                    
D2         BAT60JFILM                     TopLayer    DIO_SOD323                              2.0066       68.5800      360      BAT60JFILM                                                                    
U4         LDK120M33R                     TopLayer    REG_SOT23-5L                            41.7577      60.2996      270      "200 mA low quiescent current very low noise LDO"                             
CN1        USB_uB_105017.0001             TopLayer    CON_USBMICROB_MOLEX_105017-0001_H2P90   36.1950      74.6544      180      "USB-MICRO-B, 0.65mm, RA, SMT, Bottom Mount,"                                 
C15        Capacitor                      TopLayer    C0603                                   26.9240      55.1434      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0603, T=0,8mm"                     
C11        Capacitor                      TopLayer    C0603                                   39.8748      56.6421      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0603, T=0,8mm"                     
C4         Capacitor                      TopLayer    C0603                                   12.8270      63.3984      0        "Capacitor, MLCC, 10pF, 50V, NPO, +/-5%, 0603, T=0,8mm"                       
C10        Capacitor                      TopLayer    C0603                                   16.8910      58.9280      360      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0603, T=0,8mm"                     
C12        Capacitor                      TopLayer    C0603                                   41.3988      56.6420      90       "Capacitor, MLCC, 1uF, 16V, X5R, +/-10%, 0603, T=0,8mm"                       
C27        Capacitor                      BottomLayer C0603                                   22.0726      63.2714      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0603, T=0,8mm"                     
C3         Capacitor                      TopLayer    C0603                                   30.9880      65.4222      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0603, T=0,8mm"                     
C5         Capacitor                      TopLayer    C0603                                   12.8270      61.4934      0        "Capacitor, MLCC, 10pF, 50V, NPO, +/-5%, 0603, T=0,8mm"                       
C13        Capacitor                      TopLayer    C0603                                   42.8974      56.6404      90       "Capacitor, MLCC, 10nF, 50V, X7R, +/-10%, 0603, T=0.8mm"                      
C9         Capacitor                      TopLayer    C0603                                   30.9880      59.7154      180      "Capacitor, MLCC, 20pF, 50V, NPO, +/-5%, 0603, T=0,8mm"                       
C1         Capacitor                      TopLayer    C0603                                   21.3868      68.8086      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0603, T=0,8mm"                     
C8         Capacitor                      TopLayer    C0603                                   46.2030      60.5520      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0603, T=0,8mm"                     
C7         Capacitor                      TopLayer    C0603                                   44.6790      60.5520      90       "Capacitor, MLCC, 1uF, 16V, X5R, +/-10%, 0603, T=0,8mm"                       
C28        Capacitor                      BottomLayer C0603                                   25.3746      49.7833      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0603, T=0,8mm"                     
C16        Capacitor                      TopLayer    C0603                                   8.7630       46.6344      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0603, T=0,8mm"                     
C18        Capacitor                      TopLayer    C0805                                   16.5100      36.1950      270      "Capacitor, MLCC, 10uF, 25V, X5R, +/-10%, 0805, T=0,85mm"                     
C17        Capacitor                      TopLayer    C0805                                   5.3340       40.7670      90       "Capacitor, MLCC, 10uF, 25V, X5R, +/-10%, 0805, T=0,85mm"                     
C20        Capacitor                      TopLayer    C0603                                   31.1150      34.7646      90       "Capacitor, MLCC, 1uF, 16V, X5R, +/-10%, 0603, T=0,8mm"                       
C19        Capacitor                      TopLayer    C0603                                   29.5910      34.7646      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0603, T=0,8mm"                     
C21        Capacitor                      TopLayer    C0603                                   36.7284      34.6376      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0603, T=0,8mm"                     
C22        Capacitor                      TopLayer    C0603                                   38.2524      34.6376      270      "Capacitor, MLCC, 1uF, 16V, X5R, +/-10%, 0603, T=0,8mm"                       
C32        Capacitor                      BottomLayer C0603                                   17.7800      18.4150      360      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0603, T=0,8mm"                     
C31        Capacitor                      BottomLayer C0603                                   17.7800      20.9550      360      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0603, T=0,8mm"                     
C23        Capacitor                      TopLayer    C0402                                   11.4300      22.8600      360      "Capacitor, MLCC, 8.2pF, 50V, NPO, +/- 0.25pF, 0402, T=0,5mm"                 
C24        Capacitor                      TopLayer    C0402                                   11.4300      21.5900      360      "Capacitor, MLCC, 8.2pF, 50V, NPO, +/- 0.25pF, 0402, T=0,5mm"                 
C25        Capacitor                      TopLayer    C0402                                   10.7950      17.1450      90       "Capacitor, MLCC, 4.3pF, 50V, NPO, +/-0.25pF, 0402, T=0,5mm"                  
C26        Capacitor                      TopLayer    C0402                                   12.7000      15.2400      360      "Capacitor, MLCC, 4.3pF, 50V, NPO, +/-0.25pF, 0402, T=0,5mm"                  
C2         Capacitor                      TopLayer    C0603                                   41.2750      68.8086      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0603, T=0,8mm"                     
CN3        "Header 6x1"                   TopLayer    CON_988-JIUBABA_PHFS25-11-06-G0B115-T-1 -2.5400      62.2300      90       "Header, 6x1, 2.54mm, VR, TH, Height 6mm/3mm"                                 
L1         BEAD                           BottomLayer L0603                                   14.6050      19.6850      180      "SMD Chip ferrite bead, 600R@100MHz +/-25%, 350mA, 500mohm DC, 0603, T=0.8mm" 
LD4        LED_green                      TopLayer    LED_0603_GREEN                          44.6532      49.6824      90       "LED, Green, 0603"                                                            
LD3        LED_green                      TopLayer    LED_0603_GREEN                          41.3004      49.7002      90       "LED, Green, 0603"                                                            
R1         Resistor                       TopLayer    R0603                                   1.3970       73.4060      0        Resistor,10K,0603,1%,1/10W                                                    
R3         Resistor                       TopLayer    R0603                                   18.3134      68.8086      270      Resistor,10K,0603,1%,1/10W                                                    
R4         Resistor                       TopLayer    R0603                                   19.8120      68.8086      270      Resistor,10K,0603,1%,1/10W                                                    
R15        Resistor                       TopLayer    R0603                                   1.3971       66.0401      360      Resistor,22R,0603,1%,1/10W                                                    
R18        Resistor                       TopLayer    R0603                                   1.3971       64.5415      360      Resistor,22R,0603,1%,1/10W                                                    
R2         Resistor                       TopLayer    R0603                                   1.3970       71.8820      180      Resistor,22R,0603,1%,1/10W                                                    
R19        Resistor                       TopLayer    R0603                                   1.3971       63.0429      360      Resistor,22R,0603,1%,1/10W                                                    
R8         Resistor                       TopLayer    R0603                                   33.7820      68.8086      90       Resistor,1K5,0603,1%,1/10W                                                    
R13        Resistor                       TopLayer    R0603                                   32.2580      68.8086      270      Resistor,100K,0603,1%,1/10W                                                   
R14        Resistor                       TopLayer    R0603                                   42.7736      68.8086      270      Resistor,10K,0603,1%,1/10W                                                    
R9         Resistor                       TopLayer    R0603                                   44.2976      68.8086      90       Resistor,36K,0603,1%,1/10W                                                    
R11        Resistor                       TopLayer    R0603                                   48.7934      68.8086      90       Resistor,330R,0603,1%,1/10W                                                   
R12        Resistor                       TopLayer    R0603                                   50.2920      68.8086      90       Resistor,330R,0603,1%,1/10W                                                   
R20        Resistor                       TopLayer    R0603                                   1.3971       61.5443      360      Resistor,22R,0603,1%,1/10W                                                    
R24        Resistor                       TopLayer    R0603                                   21.1836      55.1434      90       Resistor,4K7,0603,1%,1/10W                                                    
R25        Resistor                       TopLayer    R0603                                   28.4226      55.1434      270      Resistor,100R,0603,1%,1/10W                                                   
R21        Resistor                       TopLayer    R0603                                   30.9880      61.2394      360      Resistor,100R,0603,1%,1/10W                                                   
R23        Resistor                       TopLayer    R0603                                   19.6596      55.1434      90       Resistor,4K7,0603,1%,1/10W                                                    
R26        Resistor                       TopLayer    R0603                                   8.7630       49.7840      270      Resistor,100R,0603,1%,1/10W                                                   
R27        Resistor                       TopLayer    R0603                                   44.6278      46.7690      270      Resistor,510R,0603,1%,1/10W                                                   
R28        Resistor                       TopLayer    R0603                                   41.3004      46.7614      90       Resistor,1K,0603,1%,1/10W                                                     
R32        Resistor                       TopLayer    R0402                                   15.8750      21.5900      360      Resistor,0R,0402,5%,1/16W                                                     
R33        Resistor                       TopLayer    R0402                                   15.8750      17.7800      360      Resistor,0R,0402,5%,1/16W                                                     
R34        Resistor                       TopLayer    R0402                                   15.8750      16.5100      360      Resistor,0R,0402,5%,1/16W                                                     
R29        Resistor                       TopLayer    R0603                                   7.2644       46.6344      90       Resistor,4K7,0603,1%,1/10W                                                    
R35        Resistor                       BottomLayer R0603                                   43.6372      36.8204      90       Resistor,1M,0603,1%,1/10W                                                     
R10        Resistor                       TopLayer    R0603                                   45.7962      68.8086      270      Resistor,100R,0603,1%,1/10W                                                   
SB2        SB_ON                          TopLayer    SOLDER-BRIDGE_R0603-0R                  28.0670      34.7146      270      "Solder Bridge ON"                                                            
SB12       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                  7.3414       74.9300      180      "Solder Bridge OFF"                                                           
SB11       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                  14.8852      74.9300      180      "Solder Bridge ON"                                                            
SB14       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                  7.3414       72.3900      180      "Solder Bridge OFF"                                                           
SB13       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                  14.8852      72.3900      180      "Solder Bridge ON"                                                            
SB16       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                  7.3414       69.8500      180      "Solder Bridge OFF"                                                           
SB15       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                  14.8852      69.8500      180      "Solder Bridge ON"                                                            
SB18       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                  7.3414       67.3100      180      "Solder Bridge OFF"                                                           
SB1        SB_OFF                         TopLayer    SOLDER-BRIDGE_R0603-0R                  24.5110      68.9800      270      "Solder Bridge OFF"                                                           
SB23       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                  23.9014      55.0934      270      "Solder Bridge ON"                                                            
SB22       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                  6.5540       55.8800      180      "Solder Bridge ON"                                                            
SB21       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                  6.5540       58.4200      180      "Solder Bridge ON"                                                            
SB19       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                  30.9579      62.1984      360      "Solder Bridge ON"                                                            
SB20       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                  30.8618      58.8772      180      "Solder Bridge OFF"                                                           
SB24       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                  23.7264      46.8114      90       "Solder Bridge ON"                                                            
SB26       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                  45.2374      34.2050      270      "Solder Bridge ON"                                                            
SB27       SB_ON                          TopLayer    SOLDER-BRIDGE_R0603-0R                  8.4590       10.7950      180      "Solder Bridge ON"                                                            
SB9        SB_ON                          TopLayer    SOLDER-BRIDGE_R0603-0R                  6.6302       1.9304       180      "Solder Bridge ON"                                                            
SB7        SB_OFF                         TopLayer    SOLDER-BRIDGE_R0603-0R                  6.7302       5.0292       360      "Solder Bridge OFF"                                                           
SB8        SB_ON                          TopLayer    SOLDER-BRIDGE_R0603-0R                  6.6302       3.4544       180      "Solder Bridge ON"                                                            
SB10       SB_OFF                         TopLayer    SOLDER-BRIDGE_R0603-0R                  6.7302       0.4064       360      "Solder Bridge OFF"                                                           
SB28       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                  17.8300      22.2250      360      "Solder Bridge ON"                                                            
U7         STM32C031C6T6                  TopLayer    ICC_LQFP48_7X7_P050                     24.1300      19.5580      270      "MCU, ARM™-based 32-bit MCU Cortex-M0+, 32KB Flash, 6KB SRAM"                 
SB4        SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                  21.5900      23.7910      270      "Solder Bridge OFF"                                                           
SB3        SB_OFF                         TopLayer    SOLDER-BRIDGE_R0603-0R                  15.8250      24.1300      180      "Solder Bridge OFF"                                                           
SB6        SB_ON                          TopLayer    SOLDER-BRIDGE_R0603-0R                  15.2250      15.2400      180      "Solder Bridge ON"                                                            
SB5        SB_ON                          TopLayer    SOLDER-BRIDGE_R0603-0R                  15.8250      19.0500      180      "Solder Bridge ON"                                                            
U2         STM32F103CBT6                  TopLayer    ICC_LQFP48_7X7_P050                     24.1300      61.9760      270      "Medium-density performance line ARM-based 32-bit MCU with 128KB Flash"       
R30        Resistor                       TopLayer    R0603                                   3.1750       40.6400      270      Resistor,1K,0603,1%,1/10W                                                     
C33        Capacitor                      BottomLayer C0603                                   17.7800      17.1450      360      "Capacitor, MLCC, 4.7uF, 16V, X5R, +/-10%, 0603, T=0.8mm"                     
C29        Capacitor                      BottomLayer C0603                                   43.6626      40.3114      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0603, T=0,8mm"                     
SB25       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                  45.2374      40.4630      90       "Solder Bridge OFF"                                                           
U6         LDL112PV33R                    TopLayer    ICC_DFN6-EPAD_3X3_P095                  33.9090      34.6376      90       "1.2 A low quiescent current LDO with reverse current protection"             
D5         BAT60JFILM                     TopLayer    DIO_SOD323                              37.3126      57.3278      360      BAT60JFILM                                                                    
D4         BAT60JFILM                     TopLayer    DIO_SOD323                              37.3126      59.2836      360      BAT60JFILM                                                                    
JP1        "Jumper_Header 2x1"            TopLayer    CON_SAMTEC_TSW-102-07-G-S               23.4950      74.9300      180      "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm"                           
JP5        "Jumper_Header 4x2 Fitted 1-2" TopLayer    CON_SAMTEC_TSW-104-07-X-D               35.5600      39.3700      180      "Header, 4x2, 2,54mm, VR, TH, Height 5.84mm/2.54mm - Shunt Fitted 1-2"        
R17        Resistor                       TopLayer    R0603                                   56.7090      64.3382      90       Resistor,47K,0603,1%,1/10W                                                    
