Altium Designer Pick and Place Locations
C:\Data\Project\BEE_boards\MB1792 - STM32WL-QFN48-4Layers-WMBUS169MHz_RefBoard\02-Manufacturing\MB1792A_PCB\Assembly\MB1792A_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       31/03/22
Time:       09:44
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator   Comment          Layer       Footprint                            Center-X(mm) Center-Y(mm) Rotation Description                                                                          
Designator16 Comment          TopLayer    IMPEDANCE_TABLE                      -228.7116    -209.0572    0        ""                                                                                   
Designator1  Comment          TopLayer    Sheetbox_4L2S                        57.3847      -40.7560     0        ""                                                                                   
Designator1  Comment          TopLayer    PCB_SPECIFICATIONS                   -228.7116    -209.0572    0        ""                                                                                   
J1           HEADER_1X2_L     TopLayer    CO_MOLEX_22-03-2021                  17.7925      -7.9848      0        "Header 1x2 Through hole 2.54mm"                                                     
X2           ""               TopLayer    OSC_NDK_NX2016SA                     33.4397      8.2074       270      "Crystal 32 MHz, 8pF, -+10 PPM, R=60O, SMD"                                          
X1           XTAL_2_PINS      TopLayer    OSC_NDK_NX2012SA                     28.7633      1.8321       0        "Crystal 32.768kHz, 6pF, -+20PPM, R=80K, SMD"                                        
U2           ""               BottomLayer DIOM0603X03N                         42.5675      -5.2825      180      "ESD protection 6V1"                                                                 
R3           ""               TopLayer    RESC1005X04N                         57.3301      4.6764       90       Resistor,100R,0402,1%,1/16W                                                          
R2           ""               TopLayer    RESC1005X04N                         58.5804      -5.2437      270      Resistor,100R,0402,1%,1/16W                                                          
R1           ""               BottomLayer RESC1608X05N                         42.8517      0.7478       270      Resistor,10K,0603,1%,1/10W                                                           
L2           ""               BottomLayer INDC2012X13N                         32.1925      -7.1108      0        "MLZ2012 Multilayer Shielded Inductor 15µH, ±5%"                                     
L1           ""               BottomLayer INDC1608X95N                         27.0370      -4.2388      90       "SMD Chip ferrite bead, 600R@100MHz +/-25%, 350mA, 500mohm DC, 0603, T=0.8mm"        
SB11         Close            BottomLayer GC_0402                              42.8421      -1.6149      270      "Solder Jumper - Close"                                                              
J4           SMA_T_9.52_NF    TopLayer    CO_SAMTEC_SMA-J-P-ST-EMI             70.0300      0.0250       90       "SMA Jack, Edge Mount, 50 Ohms"                                                      
J2           HEADER_1X2_L     TopLayer    CO_MOLEX_22-03-2021                  17.7925      -4.6096      0        "Header 1x2 Through hole 2.54mm"                                                     
CN2          CON20            BottomLayer CO_SAMTEC_TSW-120-07-X-S             40.4301      -13.9996     180      "Connector right-angle, pitch 2.54mm, 20 contacts"                                   
CN1          CON20            BottomLayer CO_SAMTEC_TSW-120-07-X-S             40.4301      14.0004      180      "Connector right-angle, pitch 2.54mm, 20 contacts"                                   
C34          ""               TopLayer    0201                                 38.4885      2.5599       270      "Capacitor, MLCC, 33pF, 50V, NPO, 2%, 0402, T=0,5mm"                                 
C33          ""               TopLayer    0201                                 41.4315      1.9948       180      "Capacitor, MLCC, 33pF, 50V, NPO, 2%, 0402, T=0,5mm"                                 
C31          N/C              TopLayer    CAPC1005X06N                         33.4397      6.3574       180      "Not fitted"                                                                         
C30          ""               TopLayer    CAPC1005X06N                         46.1147      -1.3997      180      "Condensateurs céramique multicouches MLCC - CMS 0402 2.7pF 50Volts C0G +/-0.1pF"    
C29          ""               TopLayer    CAPC1005X06N_-_DUPLICATE_-_DUPLICATE 61.5722      -0.5000      270      "Condensateurs céramique multicouches MLCC - CMS 0402 3.3pF 50Volts C0G +/-0.05pF"   
C28          ""               TopLayer    CAPC1005X06N_-_DUPLICATE_-_DUPLICATE 64.7587      -0.5000      270      "Condensateurs céramique multicouches MLCC - CMS 0402 3.3pF 50Volts C0G +/-0.05pF"   
C27          NC               TopLayer    CAPC1005X06N                         47.6317      -2.2230      270      "Not connected [0402]"                                                               
C25          ""               TopLayer    CAPC1005X06N                         60.0551      0.0254       0        "Multilayer Ceramic Capacitors MLCC - SMD/SMT 0402 68pF 50volts C0G 5%"              
C24          ""               TopLayer    CAPC1005X06N                         46.1147      -2.6984      0        "Condensateurs céramique multicouches MLCC - CMS 0402 3.6pF 50Volts C0G +/-0.05pF"   
C23          ""               TopLayer    CAPC1005X06N                         56.9301      2.9261       0        "Capacitor, MLCC, 1nF, 16V, X7R, 10%, 0402, T=0.5mm"                                 
C22          ""               TopLayer    CAPC1005X06N                         56.0432      0.8292       270      "Condensateurs céramique multicouches MLCC - CMS 0402 2.7 pF 50Volts C0G +/-0.25pF"  
C21          ""               TopLayer    CAPC1005X06N_-_DUPLICATE_-_DUPLICATE 50.9228      -0.1700      90       "Condensateurs céramique multicouches MLCC - CMS 0402 3.3pF 50Volts C0G +/-0.05pF"   
C20          ""               TopLayer    CAPC1005X06N_-_DUPLICATE_-_DUPLICATE 47.7363      -0.1700      270      N/C                                                                                  
C19          ""               TopLayer    CAPC1005X06N                         54.5261      0.3540       180      "Multilayer Ceramic Capacitors MLCC - SMD/SMT 0402 68pF 50volts C0G 5%"              
C18          ""               TopLayer    0201                                 45.1689      2.4591       90       "Capacitor, MLCC,68pF, 50V, C0G, 1%, 0402, T=0.5mm"                                  
C17          ""               TopLayer    CAPC1005X06N                         49.3300      1.5044       0        "Condensateurs céramique multicouches MLCC - CMS 0402 2.7pF 50Volts C0G +/-0.1pF"    
C15          ""               TopLayer    0201                                 44.4794      2.4594       270      "Capacitor, MLCC,47nF, 16V, X7R, 10%, 0402, T=0.5mm"                                 
C14          ""               BottomLayer CAPC1608X09N                         33.0585      -2.8338      90       "Capacitor, MLCC, 4.7 uF, 16V, X5R, 10%, 0603, T=0.8mm"                              
C13          ""               TopLayer    CAPC1005X06N                         58.9210      -3.4701      180      "Capacitor, MLCC, 1nF, 16V, X7R, 10%, 0402, T=0.5mm"                                 
C12          ""               BottomLayer CAPC1005X06N                         42.3997      -4.0323      180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                               
C11          ""               TopLayer    CAPC1005X06N                         31.8793      -7.4772      270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                               
C10          ""               TopLayer    CAPC1608X09N                         30.3790      -7.7790      270      "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                               
C9           Capacitor        TopLayer    CAPC1005X06N                         27.7383      3.5073       0        "Capacitor, MLCC, 6.8pF, 50V, NPO, +-0.1pF, 0402, T=0.5mm"                           
C8           Capacitor        TopLayer    CAPC1005X06N                         29.7386      3.5073       180      "Capacitor, MLCC, 6.8pF, 50V, NPO, +-0.1pF, 0402, T=0.5mm"                           
C7           ""               TopLayer    CAPC1005X06N                         30.1792      -2.3872      270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                               
C6           ""               TopLayer    CAPC1608X09N                         28.6789      -3.1385      270      "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                               
C5           ""               TopLayer    CAPC1005X06N                         33.6807      0.9504       270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                               
C3           ""               TopLayer    CAPC1005X06N                         42.3230      -8.3399      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                               
C2           ""               TopLayer    CAPC1005X06N                         40.9227      -8.3399      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                               
C1           ""               TopLayer    CAPC1608X09N                         31.8301      1.1754       270      "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                               
U3           BGS12SN6         TopLayer    SON40P70X40-6N                       57.8301      0.1004       0        "DC switch - Ultra-Low  SPDT analog switch"                                          
SB14         Close            TopLayer    SB_0402                              35.4397      7.3074       180      "Solder Bridge 0R [0402] (Populated with 0 Ohm)"                                     
SB13         Close            TopLayer    SB_0402                              39.1408      7.3657       180      "Solder Bridge 0R [0402] (Populated with 0 Ohm)"                                     
SB10         SB_3Pads         TopLayer    SB3PADS_0402                         43.6364      0.2671       90       "Solder Bridge"                                                                      
SB6          Close            TopLayer    SB_0402                              55.6299      5.1504       0        "Solder Bridge 0R [0402] (Populated with 0 Ohm)"                                     
SB7          Open             TopLayer    SB_0402                              44.5677      6.3407       0        "Solder Bridge Open [0402] (Unpopulated)"                                            
SB9          Open             TopLayer    SB_0402                              55.6299      6.5507       0        "Solder Bridge Open [0402] (Unpopulated)"                                            
SB5          Open             TopLayer    SB_0402                              56.8801      -8.5496      0        "Solder Bridge Open [0402] (Unpopulated)"                                            
SB4          Open             TopLayer    SB_0402                              56.8801      -5.9005      0        "Solder Bridge Open [0402] (Unpopulated)"                                            
SB3          Close            TopLayer    SB_0402                              56.8801      -7.2008      0        "Solder Bridge 0R [0402] (Populated with 0 Ohm)"                                     
SB2          Close            TopLayer    SB_0402                              28.0883      -0.2929      90       "Solder Bridge 0R [0402] (Populated with 0 Ohm)"                                     
SB1          Close            TopLayer    SB_0402                              29.4886      -0.2929      90       "Solder Bridge 0R [0402] (Populated with 0 Ohm)"                                     
U4           STM32WLxx_QFN48  TopLayer    STM32WLXX_QFN48                      38.3697      -2.4787      90       "STM32WL ARM MCU Multiprotocol LPWAN 32-bit Arm Cortex-M4 MCUs LoRa (G)FSK-MSK BPSK" 
C32          ""               TopLayer    0201                                 39.1625      3.5642       0        "Capacitor, MLCC, 33pF, 50V, NPO, 2%, 0402, T=0,5mm"                                 
SB8          Close            TopLayer    SB_0402                              44.5678      4.9404       180      "Solder Bridge 0R [0402] (Populated with 0 Ohm)"                                     
C4           ""               TopLayer    CAPC1005X06N                         31.2503      -5.3787      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                               
C35          ""               TopLayer    CAPC1608X09N                         61.2269      -7.8799      0        "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                               
SB15         Open             TopLayer    SB_0402                              46.8946      3.8487       180      "Solder Bridge Open [0402] (Unpopulated)"                                            
SB18         Open             TopLayer    SB_0402                              27.9188      -7.3478      90       "Solder Bridge Open [0402] (Unpopulated)"                                            
C39          ""               TopLayer    CAPC1005X06N                         60.7470      -12.2740     180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                               
C40          MCD-00277        TopLayer    0201                                 41.4310      2.6780       0        "Capacitor, MLCC, 33pF, 50V, NPO, 2%, 0402, T=0,5mm"                                 
C26          N/C              TopLayer    CAPC1005X06N                         31.3153      8.3618       270      "Not fitted"                                                                         
C38          Capa_0402        TopLayer    CAPC1005X06N                         59.3114      -1.7022      180      "10pF ±1% 50V Ceramic Capacitor C0G, NP0 0402 (1005 Metric)"                         
C41          Capa_0402        TopLayer    CAPC1005X06N                         59.0262      2.7715       180      "10pF ±1% 50V Ceramic Capacitor C0G, NP0 0402 (1005 Metric)"                         
L3           "MURATA LQW18AN" TopLayer    LQW18AN                              46.2425      2.1055       270      ""                                                                                   
L4           "MURATA LQW18AN" TopLayer    LQW18AN                              49.3296      0.3542       0        ""                                                                                   
L5           "MURATA LQW18AN" TopLayer    LQW18AN                              52.5160      0.3540       0        ""                                                                                   
L6           "MURATA LQW18AN" TopLayer    LQW18AN                              45.9760      0.3542       0        ""                                                                                   
L7           "MURATA LQW18AN" TopLayer    LQW18AN                              63.1654      0.0250       180      ""                                                                                   
L8           "MURATA LQW18AN" TopLayer    LQW18AN                              44.5476      -1.9774      90       ""                                                                                   
