Altium Designer Pick and Place Locations
C:\Subversion\__Boards\MB1801-Nucleo64-MiniBoard\Trunk\02-Manufacturing\MB1801D_PCB\Assembly\MB1801D_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       14/02/24
Time:       07:52
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator Comment                    Layer       Footprint                                      Center-X(mm) Center-Y(mm) Rotation Description                                                                                
U19        ESD-TRANSIL                TopLayer    ESD_ST0201                                     -24.2500     -49.0000     270      "ESD protection 6V1"                                                                       
U18        ESD-TRANSIL                TopLayer    ESD_ST0201                                     -37.5000     -45.6500     180      "ESD protection 6V1"                                                                       
U17        ESD-TRANSIL                TopLayer    ESD_ST0201                                     -39.5000     -45.5000     180      "ESD protection 6V1"                                                                       
U16        ESD-TRANSIL                TopLayer    ESD_ST0201                                     -49.7500     -45.5000     180      "ESD protection 6V1"                                                                       
SB33       SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                         -42.2875     -39.0000     180      "Solder Bridge 0402 ON"                                                                    
SB30       SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                         -40.9625     -6.5000      0        "Solder Bridge 0402 ON"                                                                    
SB29       SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                         -40.9625     -7.7500      0        "Solder Bridge 0402 ON"                                                                    
C62        Capacitor                  TopLayer    C0402                                          -24.2500     -47.5000     90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                     
1          Comment                    TopLayer    Sheetbox_2L2S                                  -137.3800    -47.5058     0        ""                                                                                         
""         Comment                    TopLayer    PCB_SPECIFICATIONS                             -295.5350    -249.5710    0        ""                                                                                         
MIRE6      Comment                    TopLayer    MIRE_PLACE_SMD_0P8MM                           -62.7500     -47.5000     0        ""                                                                                         
MIRE5      Comment                    TopLayer    MIRE_PLACE_SMD_0P8MM                           4.7500       2.5000       0        ""                                                                                         
MIRE3      Comment                    BottomLayer MIRE_PLACE_SMD_0P8MM                           -62.2500     2.0000       0        ""                                                                                         
MIRE2      Comment                    BottomLayer MIRE_PLACE_SMD_0P8MM                           3.5000       2.0000       0        ""                                                                                         
MIRE4      Comment                    TopLayer    MIRE_PLACE_SMD_0P8MM                           3.2500       -47.7500     0        ""                                                                                         
MIRE1      Comment                    BottomLayer MIRE_PLACE_SMD_0P8MM                           -62.5000     -47.2500     0        ""                                                                                         
HW1        PCB_MB1801                 BottomLayer STICKER_PRODUCT_25X5                           -295.5350    -249.5710    270      "PCB 2L2S of NUCLEO64 for MiniBoard"                                                       
U15        74AVC4TD245BQ              BottomLayer ICC_DHVQFN16-EPAD_SOT763-1_2P5X3P5_H0P85_P050  -49.0000     -24.2500     90       "4-bit dual supply translating transceiver with configurable voltage translation; 3-state" 
SB26       SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                         -45.0375     -21.0000     180      "Solder Bridge 0402 ON"                                                                    
SB25       SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                         -14.7875     -20.2500     180      "Solder Bridge 0402 ON"                                                                    
SB24       SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                         -14.7875     -14.5000     180      "Solder Bridge 0402 ON"                                                                    
SB8        SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                         -14.7875     -26.7500     180      "Solder Bridge 0402 ON"                                                                    
SB7        SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                         -14.7875     -28.0000     180      "Solder Bridge 0402 ON"                                                                    
R67        Resistor                   BottomLayer R0402                                          -50.5000     -20.5000     90       Resistor,100K,0402,1%,1/16W                                                                
R66        Resistor                   BottomLayer R0402                                          -49.2500     -20.5000     90       Resistor,100K,0402,1%,1/16W                                                                
R65        Resistor                   BottomLayer R0402                                          -48.0000     -20.5000     90       Resistor,100K,0402,1%,1/16W                                                                
R64        Resistor                   BottomLayer R0402                                          -50.8250     -27.7500     270      Resistor,100K,0402,1%,1/16W                                                                
R63        Resistor                   BottomLayer R0402                                          -49.4500     -27.7500     270      Resistor,100K,0402,1%,1/16W                                                                
R62        Resistor                   BottomLayer R0402                                          -48.4750     -27.7500     270      Resistor,100K,0402,1%,1/16W                                                                
R61        Resistor                   BottomLayer R0402                                          -47.1000     -27.7500     270      Resistor,100K,0402,1%,1/16W                                                                
C61        Capacitor                  BottomLayer C0402                                          -45.7500     -23.0000     90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                     
C60        Capacitor                  BottomLayer C0402                                          -45.7500     -25.5000     90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                     
SB3        SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                         -44.9625     -29.2500     0        "Solder Bridge 0402 ON"                                                                    
SB22       SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                         -46.5375     -43.5000     180      "Solder Bridge 0402 ON"                                                                    
SB21       SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                         -42.2125     -40.2500     0        "Solder Bridge 0402 ON"                                                                    
SB28       SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                         -40.9625     -5.2500      0        "Solder Bridge 0402 ON"                                                                    
X1         XTAL_4_PINS                BottomLayer CRY_NX2016SA_4P                                -26.7500     -16.7500     0        "Crystal, 24MHz, 6pF, +/-20ppm, 80R, 2x1.6mm"                                              
U14        ESDALC6V1W5                BottomLayer ESD_SOT323-5L                                  -44.7500     0.5000       0        "Dual Transil array for ESD protection"                                                    
U13        ESDALC6V1W5                BottomLayer ESD_SOT323-5L                                  -43.7500     -3.7500      0        "Dual Transil array for ESD protection"                                                    
U12        STMPS2151STR               BottomLayer MOS_SOT23-5L                                   -38.5000     -38.0000     0        "500mA, Enhanced single channel power switches with active high enable pin"                
U11        ST730M33R                  BottomLayer ICC_SOT23-5L_H1P45                             -19.7500     -36.5000     270      "LDO, 3.3V, 300mA, High input voltage: 2.5V to 28V, SOT23-5L"                              
U10        TPS259535DSG               BottomLayer ICC_WSON8-EPAD_2X2_P050                        -37.7503     -31.5000     180      "eFuse with Fast Overvoltage Protection 2.7V to 18V 4A 34mOhm 8-Pin WSON"                  
U9         74AVC4TD245BQ              BottomLayer ICC_DHVQFN16-EPAD_SOT763-1_2P5X3P5_H0P85_P050  -38.5000     -16.5000     180      "4-bit dual supply translating transceiver with configurable voltage translation; 3-state" 
U8         ECMF02-2AMX6               BottomLayer ESD_QFN-6L_1P7X1P5_P050                        -27.7500     -40.2500     180      "Common mode filter with ESD protection for USB 2.0 interface"                             
TP1        "Test Point"               BottomLayer TP_SMD_1MM                                     -29.5500     -34.0000     180      "Test Point 1mm"                                                                           
SB14       SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                         -7.4625      -10.0000     0        "Solder Bridge 0402 ON"                                                                    
SB12       SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                         -13.5375     -6.5000      180      "Solder Bridge 0402 ON"                                                                    
SB27       SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                         -44.9625     -14.0000     0        "Solder Bridge 0402 ON"                                                                    
SB23       SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                         -40.9625     -4.0000      0        "Solder Bridge 0402 ON"                                                                    
R60        Resistor                   BottomLayer R0402                                          -41.2500     -23.5000     90       Resistor,100K,0402,1%,1/16W                                                                
R59        Resistor                   BottomLayer R0402                                          -35.7500     -23.5000     270      Resistor,100K,0402,1%,1/16W                                                                
R58        Resistor                   BottomLayer R0402                                          -33.0000     -29.7500     180      "Resistor, 33R, 0402, +/-1%, 1/16W"                                                        
R57        Resistor                   BottomLayer R0402                                          -19.5000     -29.3500     0        "Resistor, 0R, 0402, +/-5%, 1/16W"                                                         
R56        Resistor                   BottomLayer R0402                                          -33.0000     -23.7500     180      "Resistor, 33R, 0402, +/-1%, 1/16W"                                                        
R55        Resistor                   BottomLayer R0402                                          -33.0000     -27.7500     180      "Resistor, 0R, 0402, +/-5%, 1/16W"                                                         
R54        Resistor                   BottomLayer R0402                                          -55.5000     0.2500       0        "Resistor, 100R, 0402, +/-1%, 1/16W"                                                       
R53        Resistor                   BottomLayer R0402                                          -35.2500     -39.0000     180      "Resistor, 100K, 0402, +/-1%, 1/16W"                                                       
R52        Resistor                   BottomLayer R0402                                          -35.2500     -37.0000     180      "Resistor, 100K, 0402, +/-1%, 1/16W"                                                       
R51        Resistor                   TopLayer    R0402                                          -10.5000     -34.5000     270      "Resistor, 330R, 0402, +/-1%, 1/16W"                                                       
R50        Resistor                   TopLayer    R0402                                          -14.0000     -34.5000     90       "Resistor, 330R, 0402, +/-1%, 1/16W"                                                       
R49        Resistor                   TopLayer    R0402                                          -12.0000     -34.5000     90       "Resistor, 1K, 0402, +/-0.1%, 1/16W, +/-25ppm/°C"                                          
R48        Resistor                   TopLayer    R0402                                          -15.5000     -34.4500     90       "Resistor, 1K, 0402, +/-0.1%, 1/16W, +/-25ppm/°C"                                          
R47        Resistor                   TopLayer    R0402                                          -22.5000     -12.5000     90       "Resistor, 100K, 0402, +/-1%, 1/16W"                                                       
R46        Resistor                   BottomLayer R0402                                          -34.7500     -30.2500     270      "Resistor, 100K, 0402, +/-1%, 1/16W"                                                       
R45        Resistor                   BottomLayer R0402                                          -41.7500     -30.2500     90       "Resistor, 3K9, 0402, +/-1%, 1/16W, +/-100ppm/°C"                                          
R44        Resistor                   BottomLayer R0402                                          -40.7500     -30.2500     90       "Resistor, 1K3, 0402, +/-1%, 1/16W"                                                        
R43        Resistor                   BottomLayer R0402                                          -39.7500     -30.2500     90       "Resistor, 1K8, 0402, +/-1%, 1/16W"                                                        
R42        Resistor                   BottomLayer R0402                                          -41.7500     -32.7500     90       "Resistor, 5K1, 0402, +/-1%, 1/16W"                                                        
R41        Resistor                   BottomLayer R0402                                          -41.2500     -18.0000     90       Resistor,100K,0402,1%,1/16W                                                                
R40        Resistor                   BottomLayer R0402                                          -40.7500     -32.7500     90       "Resistor, 3K, 0402, +/-1%, 1/16W"                                                         
R39        Resistor                   BottomLayer R0402                                          -33.0000     -21.8750     180      Resistor,10K,0402,1%,1/16W                                                                 
R38        Resistor                   BottomLayer R0402                                          -19.5000     -24.0000     0        Resistor,10K,0402,1%,1/16W                                                                 
R37        Resistor                   BottomLayer R0402                                          -42.2500     -18.0000     270      Resistor,47R,0402,1%,1/16W                                                                 
R36        Resistor                   BottomLayer R0402                                          -19.5000     -23.0000     0        "Resistor, 5K1, 0402, +/-1%, 1/16W"                                                        
R35        Resistor                   BottomLayer R0402                                          -43.2500     -18.0000     270      Resistor,47R,0402,1%,1/16W                                                                 
R34        Resistor                   BottomLayer R0402                                          -42.2500     -15.0000     90       Resistor,47R,0402,1%,1/16W                                                                 
R33        Resistor                   BottomLayer R0402                                          -20.0000     -18.7500     90       Resistor,10K,0402,1%,1/16W                                                                 
R32        Resistor                   BottomLayer R0402                                          -41.2500     -15.0000     90       Resistor,47R,0402,1%,1/16W                                                                 
LD6        LED_BICOLOR                TopLayer    LED_BI-GR_WE-150141SV73110                     -11.2500     -38.0000     0        "LED Bicolor, Green/Red, 2V, 20mA,  4-PLCC"                                                
LD5        LED_BICOLOR                TopLayer    LED_BI-GR_WE-150141SV73110                     -14.7500     -38.0000     0        "LED Bicolor, Green/Red, 2V, 20mA,  4-PLCC"                                                
JP4        "Jumper_Header 2x1"        BottomLayer CON_SAMTEC_TSW-102-07-G-S                      -20.2500     -12.5000     90       "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm"                                        
JP3        "Jumper_Header 2x1"        BottomLayer CON_SAMTEC_TSW-102-07-G-S                      -41.5000     3.7500       180      "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm"                                        
D1         SCHOTTKY_1A_2K             BottomLayer DIO_SOD523_1A_2K                               -21.0000     -39.5000     0        "Small signal Schottky diodes"                                                             
CN17       "Header 7x2"               BottomLayer CON_STDC14_Receiver_MEDIUM_WITH_MIPI10_3D      -50.5000     -2.2500      90       "Header, 5x2, 1.27mm, VR, SMD, T=5.97mm/3.05mm"                                            
CN16       "Header 4x1"               BottomLayer CON_SAMTEC_TSW-104-07-G-S                      -33.0000     3.7500       180      "Header, 4x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm"                                        
CN15       USB_TYPE_C_Receptacle      BottomLayer CON_USB-TYPEC_AMPHENOL_12401826E412A           -27.7600     -45.5700     180      "USB_TypeC, 24 pins, RA, SMD, T=2.96mm"                                                    
CN9        USB_TYPE_C_Receptacle      BottomLayer CON_USB-TYPEC_AMPHENOL_12401826E412A           -12.7400     -45.5700     180      "USB_TypeC, 24 pins, RA, SMD, T=2.96mm"                                                    
C59        Capacitor                  BottomLayer C0603                                          -39.0000     -35.2500     180      "Capacitor, MLCC, 10uF, 10V, X5R, +/-10%, 0603, T=0.8mm"                                   
C58        Capacitor                  BottomLayer C0402                                          -38.5000     -41.0000     180      "Capacitor, MLCC, 100nF, 25V, X7R, +/-10%, 0402, T=0.5mm"                                  
C57        Capacitor                  BottomLayer C0402                                          -30.5000     -32.5000     90       "Capacitor, MLCC, 2.2uF, 6.3V, X5R, +/-10%, 0402, T=0.5mm"                                 
C56        Capacitor                  BottomLayer C0402                                          -19.5000     -28.4000     180      "Capacitor, MLCC, 2.2uF, 6.3V, X5R, +/-10%, 0402, T=0.5mm"                                 
C55        Capacitor                  BottomLayer C0603                                          -17.0000     -36.0000     90       "Capacitor, MLCC, 10uF, 10V, X5R, +/-10%, 0603, T=0.8mm"                                   
C54        Capacitor                  BottomLayer C0805                                          -17.7500     -39.5000     180      "Capacitor, MLCC, 2.2uF, 25V, X7R, +/-10%, 0805, T=1,25mm"                                 
C53        Capacitor                  BottomLayer C0402                                          -33.0000     -26.8000     180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                     
C52        Capacitor                  BottomLayer C0402                                          -33.0000     -25.5500     180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                     
C51        Capacitor                  BottomLayer C0402                                          -33.0000     -24.7500     180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                     
C50        Capacitor                  BottomLayer C0402                                          -33.0000     -22.7500     180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                     
C49        Capacitor                  BottomLayer C0402                                          -30.6000     -18.7500     90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                     
C48        Capacitor                  BottomLayer C0402                                          -29.3750     -18.7500     90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                     
C47        Capacitor                  BottomLayer C0402                                          -28.1250     -18.7500     90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                     
C46        Capacitor                  BottomLayer C0402                                          -25.0000     -18.7500     90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                     
C45        Capacitor                  BottomLayer C0402                                          -22.5000     -18.7500     90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                     
C44        Capacitor                  BottomLayer C0402                                          -21.5000     -18.7500     90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                     
C43        Capacitor                  BottomLayer C0402                                          -19.5000     -25.2500     0        "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                     
C42        Capacitor                  BottomLayer C0402                                          -19.5000     -26.1000     0        "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                     
C41        Capacitor                  BottomLayer C0402                                          -19.5000     -27.2500     0        "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                     
C40        Capacitor                  BottomLayer C0402                                          -28.2500     -32.5000     270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                     
C39        Capacitor                  BottomLayer C0402                                          -27.0000     -32.5000     270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                     
C38        Capacitor                  BottomLayer C0402                                          -23.0000     -32.5000     270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                     
C37        Capacitor                  BottomLayer C0402                                          -26.2000     -32.5000     270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                     
C36        Capacitor                  BottomLayer C0402                                          -35.7500     -30.2500     270      "Capacitor, MLCC, 10nF, 50V, X7R, +/-10%, 0402, T=0.5mm"                                   
C35        Capacitor                  BottomLayer C0402                                          -36.7500     -33.7500     0        "Capacitor, MLCC, 100nF, 25V, X7R, +/-10%, 0402, T=0.5mm"                                  
C34        Capacitor                  BottomLayer C0603                                          -39.0000     -33.7500     180      "Capacitor, MLCC, 10uF, 10V, X5R, +/-10%, 0603, T=0.8mm"                                   
C33        Capacitor                  BottomLayer C0402                                          -23.8750     -32.5000     90       "Capacitor, MLCC, 2.2uF, 6.3V, X5R, +/-10%, 0402, T=0.5mm"                                 
C32        Capacitor                  BottomLayer C0402                                          -41.5000     1.5000       0        "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                     
SB20       SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                         -47.5000     -37.4625     90       "Solder Bridge 0402 ON"                                                                    
CN14       "Header 2x1"               TopLayer    CON_SAMTEC_TSW-102-07-G-S                      -20.2500     -47.2500     90       "Header, 2x1, 2.54mm, VR, TH, T=5.84mm/2.54mm"                                             
HW2        STICKER_BOARD              BottomLayer STICKER_BOARD_25X5                             -295.5350    -249.5710    180      "Sticker board 25x5 mm"                                                                    
U7         ESD-TRANSIL                TopLayer    ESD_QFN1610_2N_1K_2A                           -30.0000     -44.2500     270      "High power Transient voltage suppressor:25V/35A EOS and ESD transients protection."       
U6         74AVC4TD245BQ              BottomLayer ICC_DHVQFN16-EPAD_SOT763-1_2P5X3P5_H0P85_P050  -38.5000     -25.0000     180      "4-bit dual supply translating transceiver with configurable voltage translation; 3-state" 
U5         STLINK-V3EC                BottomLayer ICC_UFBGA201_176+25_10X10_P065                 -26.2500     -25.5000     270      "MCU, Arm Cortex-M7 32-bit MCU, 512KB Flash, 276KB RAM, With Crypto"                       
U4         LD39050PU33R               BottomLayer ICC_DFN6-EPAD_3X3_P095                         -34.2500     -6.5000      270      "Low quiescent current and low noise voltage regulators"                                   
U3         LD1117S50TR                BottomLayer REG_SOT223-TAB                                 -25.5000     -6.0000      90       "IC REG LDO 5V 0.8A SOT223"                                                                
U2         ESD-TRANSIL                TopLayer    ESD_QFN1610_2N_1K_2A                           -15.0000     -44.2500     270      "High power Transient voltage suppressor:25V/35A EOS and ESD transients protection."       
U1         ECMF02-2AMX6               BottomLayer ESD_QFN-6L_1P7X1P5_P050                        -12.7500     -40.2500     0        "Common mode filter with ESD protection for USB 2.0 interface"                             
SW1        SW_MECA                    BottomLayer SWI_SPDT-RA_TE-CONNECTIVITY_MLL1200S_1P2T      -46.5996     -48.1088     180      "Slide switch, 3x1, 1.5mm, RA, SMT, T=1.65mm"                                              
SB19       SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                         -44.0375     -43.5000     180      "Solder Bridge 0402 ON"                                                                    
SB17       SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                         -40.9625     -9.0000      0        "Solder Bridge 0402 ON"                                                                    
SB13       SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                         -14.7875     -12.7500     180      "Solder Bridge 0402 ON"                                                                    
SB15       SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                         -40.9625     -10.2500     0        "Solder Bridge 0402 ON"                                                                    
SB11       SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                         -8.0375      -41.5000     180      "Solder Bridge 0402 ON"                                                                    
SB10       SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                         -47.7125     -17.7500     0        "Solder Bridge 0402 ON"                                                                    
SB9        SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                         -13.5375     -5.0000      180      "Solder Bridge 0402 ON"                                                                    
SB6        SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                         -8.0375      -37.0000     180      "Solder Bridge 0402 ON"                                                                    
SB5        SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                         -44.9625     -27.5000     0        "Solder Bridge 0402 ON"                                                                    
SB4        SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                         -8.0375      -34.7500     180      "Solder Bridge 0402 ON"                                                                    
SB2        SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                         -8.0375      -39.2500     180      "Solder Bridge 0402 ON"                                                                    
SB1        SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                         -15.6000     -3.2875      270      "Solder Bridge 0402 ON"                                                                    
SB16       SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                         -7.4625      -9.0000      0        "Solder Bridge 0402 ON"                                                                    
SB18       SB_ON                      BottomLayer SOLDER-BRIDGE_R0402-0R                         -41.2125     -43.5000     0        "Solder Bridge 0402 ON"                                                                    
R31        Resistor                   BottomLayer R0402                                          -19.5000     -20.9000     0        Resistor,10K,0402,1%,1/16W                                                                 
R30        Resistor                   BottomLayer R0402                                          -24.8250     -32.5000     270      Resistor,3K,0402,1%,1/16W                                                                  
R29        Resistor                   BottomLayer R0402                                          -19.5000     -22.0000     0        "Resistor, 0R, 0402, +/-5%, 1/16W"                                                         
R28        Resistor                   BottomLayer R0402                                          -43.2500     -15.0000     90       Resistor,100K,0402,1%,1/16W                                                                
R27        Resistor                   BottomLayer R0402                                          -35.7500     -17.7500     270      Resistor,100K,0402,1%,1/16W                                                                
R26        Resistor                   BottomLayer R0402                                          -34.7500     -17.7500     270      Resistor,100K,0402,1%,1/16W                                                                
R25        Resistor                   BottomLayer R0402                                          -34.7500     -15.0000     90       Resistor,100K,0402,1%,1/16W                                                                
R24        Resistor                   BottomLayer R0402                                          -35.7500     -15.0000     270      Resistor,100K,0402,1%,1/16W                                                                
R23        Resistor                   BottomLayer R0402                                          -29.5000     -40.0000     90       "Resistor, 5K1, 0402, +/-1%, 1/16W"                                                        
R22        Resistor                   BottomLayer R0402                                          -30.5000     -40.0000     90       "Resistor, 100K, 0402, +/-1%, 1/16W"                                                       
R21        Resistor                   BottomLayer R0402                                          -29.5500     -32.5000     270      "Resistor, 0R, 0402, +/-5%, 1/16W"                                                         
R20        Resistor                   BottomLayer R0402                                          -25.0000     -40.0000     90       "Resistor, 100K, 0402, +/-1%, 1/16W"                                                       
R19        Resistor                   BottomLayer R0402                                          -41.7500     -26.2500     270      Resistor,100K,0402,1%,1/16W                                                                
R18        Resistor                   BottomLayer R0402                                          -42.4500     -23.5000     90       Resistor,100K,0402,1%,1/16W                                                                
R17        Resistor                   BottomLayer R0402                                          -35.7500     -26.5000     270      Resistor,100K,0402,1%,1/16W                                                                
R16        Resistor                   BottomLayer R0402                                          -34.7500     -26.5000     270      Resistor,100K,0402,1%,1/16W                                                                
R15        Resistor                   BottomLayer R0402                                          -34.7500     -23.5000     90       Resistor,100K,0402,1%,1/16W                                                                
R14        Resistor                   BottomLayer R0402                                          -26.0000     -40.0000     90       "Resistor, 5K1, 0402, +/-1%, 1/16W"                                                        
R13        Resistor                   TopLayer    R0402                                          -32.0000     -41.5500     270      "Resistor, 1K5, 0402, +/-1%, 1/16W"                                                        
R1         Resistor                   BottomLayer R0402                                          -30.7500     -6.5000      90       "Resistor, 1K, 0402, +/-1%,1/16W"                                                          
R12        Resistor                   BottomLayer R0402                                          -14.5000     -40.2500     270      "Resistor, 5K1, 0402, +/-1%, 1/16W"                                                        
R11        Resistor                   BottomLayer R0402                                          -11.0000     -40.2500     270      "Resistor, 5K1, 0402, +/-1%, 1/16W"                                                        
R8         Resistor                   TopLayer    R0402                                          -11.0000     -47.5000     270      "Resistor, 680R, 0402, +/-1%, 1/16W"                                                       
R7         Resistor                   TopLayer    R0402                                          -13.5000     -47.5000     270      "Resistor, 680R, 0402, +/-1%, 1/16W"                                                       
R6         Resistor                   TopLayer    R0402                                          -16.0000     -47.5000     270      "Resistor, 680R, 0402, +/-1%, 1/16W"                                                       
R2         Resistor                   BottomLayer R0402                                          -32.5000     -19.5000     270      Resistor,100K,0402,1%,1/16W                                                                
LD4        LED_green                  TopLayer    LED_0603_VISHAY_VLMTG1300-GS08_GREEN_1A2K_H0P8 -32.0000     -39.0000     90       "LED Green, 0603 SMD, Fw Voltage = 2.8V - 3.6V"                                            
LD3        LED_red                    TopLayer    LED_0603_VISHAY_VLMS1300-GS08_RED_1A2K_H0P8    -9.7500      -47.0000     90       "LED Red, 0603 SMD, 2V Forward Voltage"                                                    
LD2        LED_green                  TopLayer    LED_0603_VISHAY_VLMTG1300-GS08_GREEN_1A2K_H0P8 -12.2500     -47.0000     90       "LED Green, 0603 SMD, Fw Voltage = 2.8V - 3.6V"                                            
LD1        LED_blue                   TopLayer    LED_0603_VISHAY_VLMB1300-GS08_BLUE_1A2K_H0P8   -14.7500     -47.0000     90       "LED Blue, 0603 SMD, 3.3 V Forward Voltage"                                                
JP2        "Jumper_Header 2x1 Fitted" TopLayer    CON_SAMTEC_TSW-102-07-G-S                      -49.5000     -39.0000     90       "Header, 2x1, 2.54mm, VR, TH, T=5.84mm/2.54mm"                                             
JP1        "Jumper 5 Positions"       TopLayer    CON_SAMTEC_TMM-105-06-T-D-SM                   -38.5000     -40.1250     0        "Header, 10x2, 2,00mm, h=7,04mm, VR, SMD"                                                  
CN13       "Header 2x1"               TopLayer    CON_SAMTEC_TSW-102-07-G-S                      1.2700       3.9370       0        "Header, 2x1, 2.54mm, VR, TH, T=5.84mm/2.54mm"                                             
CN12       "Header 2x1"               TopLayer    CON_SAMTEC_TSW-102-07-G-S                      -59.6900     3.9370       0        "Header, 2x1, 2.54mm, VR, TH, T=5.84mm/2.54mm"                                             
CN11       "Header 2x1"               BottomLayer CON_SAMTEC_TSW-102-07-G-S                      -18.0000     -4.7500      90       "Header, 2x1, 2.54mm, VR, TH, T=5.84mm/2.54mm"                                             
CN10       "Header 2x1"               TopLayer    CON_SAMTEC_TSW-102-07-G-S                      -45.5000     -39.0000     90       "Header, 2x1, 2.54mm, VR, TH, T=5.84mm/2.54mm"                                             
CN8        "Socket 8x1"               TopLayer    CON_SAMTEC_SSW-108-01-X-S                      -5.0800      -36.8300     90       "Socket, 8x1, 2.54mm, VR, TH, T=8.51/2.64mm"                                               
CN7        "Socket 6x1"               TopLayer    CON_SAMTEC_SSW-106-01-X-S                      -53.3400     -39.3700     270      "Socket, 6x1, 2.54mm, VR, TH, T=8.51/2.64mm"                                               
CN6        "Socket 10x1"              TopLayer    CON_SAMTEC_SSW-110-01-X-S                      -5.0800      -12.4460     90       "Socket, 10x1, 2.54mm, VR, TH, T=8.51/2.64mm"                                              
CN5        "Socket 8x1"               TopLayer    CON_SAMTEC_SSW-108-01-X-S                      -53.3400     -19.0500     270      "Socket, 8x1, 2.54mm, VR, TH, T=8.51/2.64mm"                                               
CN4        "Header 19x2"              TopLayer    CON_SAMTEC_TSW-119-09-X-D                      1.2700       -22.8600     270      "Header, 19x2, 2.54mm, VR, TH, T=5.84mm/10.16mm"                                           
CN3        "Header 19x2"              TopLayer    CON_SAMTEC_TSW-119-09-X-D                      -59.6900     -22.8600     270      "Header, 19x2, 2.54mm, VR, TH, T=5.84mm/10.16mm"                                           
CN2        CLP-125-02-F-D             TopLayer    CON_SAMTEC_CLP-125-02-F-D                      -12.0646     -15.2400     0        "Socket, 25x2, 1.27mm, VR, SMD, T=2.29mm"                                                  
CN1        CLP-125-02-F-D             TopLayer    CON_SAMTEC_CLP-125-02-F-D                      -46.3546     -15.2400     0        "Socket, 25x2, 1.27mm, VR, SMD, T=2.29mm"                                                  
C31        Capacitor                  BottomLayer C0402                                          -39.0000     -13.2500     90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                     
C30        Capacitor                  BottomLayer C0402                                          -38.0000     -13.2500     270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                     
C29        Capacitor                  BottomLayer C0402                                          -25.0000     -16.7500     90       "Capacitor, MLCC, 2.7pF, 50V, NPO, +/-0.1pF, 0402, T=0.5mm"                                
C28        Capacitor                  BottomLayer C0402                                          -28.5000     -16.7500     90       "Capacitor, MLCC, 2.7pF, 50V, NPO, +/-0.1pF, 0402, T=0.5mm"                                
C27        Capacitor                  BottomLayer C0402                                          -30.5000     -38.0000     90       "Capacitor, MLCC, 10nF, 50V, X7R, +/-10%, 0402, T=0.5mm"                                   
C26        Capacitor                  BottomLayer C0402                                          -25.0000     -38.0000     90       "Capacitor, MLCC, 10nF, 50V, X7R, +/-10%, 0402, T=0.5mm"                                   
C25        Capacitor                  BottomLayer C0402                                          -39.5000     -21.7500     180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                     
C24        Capacitor                  BottomLayer C0402                                          -37.5000     -21.7500     180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                     
C23        Capacitor                  TopLayer    C0402                                          -25.5000     -44.2500     270      "Capacitor, MLCC, 100pF, 50V, NPO, +/-5%, 0402, T=0.5mm"                                   
C22        Capacitor                  BottomLayer C0402                                          -35.0000     -8.7500      180      "Capacitor, MLCC, 100nF, 25V, X7R, +/-10%, 0402, T=0.5mm"                                  
C21        Capacitor                  BottomLayer C0805_H0P85                                    -34.5000     -10.2500     180      "Capacitor, MLCC, 1uF, 16V, X5R, +/-10%, 0805, T=0.85mm"                                   
C20        Capacitor                  BottomLayer C0402                                          -35.0000     -4.2500      180      "Capacitor, MLCC, 100nF, 25V, X7R, +/-10%, 0402, T=0.5mm"                                  
C19        Capacitor                  BottomLayer C0805_H0P85                                    -34.5000     -2.7500      180      "Capacitor, MLCC, 1uF, 16V, X5R, +/-10%, 0805, T=0.85mm"                                   
C18        Capacitor                  BottomLayer C0402                                          -29.0000     -0.2500      270      "Capacitor, MLCC, 100nF, 25V, X7R, +/-10%, 0402, T=0.5mm"                                  
C17        Cap_POL_TANA               BottomLayer CPOL_TAJ-B_1210_H210                           -25.5000     -11.2500     180      "Capacitor, Tantalum, 10uF, 25V, 2R5, +/-10%, Type_B (3528 metric), T=1.9mm"               
C16        Cap_POL_TANA               BottomLayer CPOL_TAJ-B_1210_H210                           -25.5000     -0.7500      0        "Capacitor, Tantalum, 10uF, 25V, 2R5, +/-10%, Type_B (3528 metric), T=1.9mm"               
C11        Capacitor                  TopLayer    C0402                                          -16.5000     -32.5000     0        "Capacitor, MLCC, 100nF, 25V, X7R, +/-10%, 0402, T=0.5mm"                                  
C10        Capacitor                  TopLayer    C0402                                          -17.0000     -19.0000     0        "Capacitor, MLCC, 100nF, 25V, X7R, +/-10%, 0402, T=0.5mm"                                  
C9         Capacitor                  TopLayer    C0402                                          -16.2500     1.2500       270      "Capacitor, MLCC, 100nF, 25V, X7R, +/-10%, 0402, T=0.5mm"                                  
C8         Capacitor                  TopLayer    C0402                                          -44.7500     -33.0000     90       "Capacitor, MLCC, 100nF, 25V, X7R, +/-10%, 0402, T=0.5mm"                                  
C7         Capacitor                  TopLayer    C0402                                          -43.0000     0.5000       270      "Capacitor, MLCC, 100nF, 25V, X7R, +/-10%, 0402, T=0.5mm"                                  
C6         Capacitor                  TopLayer    C0805_H0P85                                    -13.5000     -32.5000     180      "Capacitor, MLCC, 1uF, 16V, X5R, +/-10%, 0805, T=0.85mm"                                   
C5         Capacitor                  TopLayer    C0805_H0P85                                    -17.2500     -20.5000     0        "Capacitor, MLCC, 1uF, 16V, X5R, +/-10%, 0805, T=0.85mm"                                   
C4         Capacitor                  TopLayer    C0805_H0P85                                    -17.7500     1.2500       270      "Capacitor, MLCC, 1uF, 16V, X5R, +/-10%, 0805, T=0.85mm"                                   
C3         Capacitor                  TopLayer    C0805_H0P85                                    -46.2500     -33.5000     90       "Capacitor, MLCC, 1uF, 16V, X5R, +/-10%, 0805, T=0.85mm"                                   
C2         Capacitor                  TopLayer    C0805_H0P85                                    -40.7500     0.0000       180      "Capacitor, MLCC, 1uF, 16V, X5R, +/-10%, 0805, T=0.85mm"                                   
C1         Capacitor                  TopLayer    C0805_H0P85                                    -20.5000     -4.7500      270      "Capacitor, MLCC, 1uF, 16V, X5R, +/-10%, 0805, T=0.85mm"                                   
C15        Capacitor                  TopLayer    C0402                                          -10.5000     -44.2500     90       "Capacitor, MLCC, 100pF, 50V, NPO, +/-5%, 0402, T=0.5mm"                                   
C14        Capacitor                  TopLayer    C0402                                          -37.5000     -45.0000     0        "Capacitor, MLCC, 10nF, 50V, X7R, +/-10%, 0402, T=0.5mm"                                   
C13        Capacitor                  TopLayer    C0402                                          -39.5000     -44.7500     0        "Capacitor, MLCC, 10nF, 50V, X7R, +/-10%, 0402, T=0.5mm"                                   
C12        Capacitor                  TopLayer    C0402                                          -49.7500     -44.7500     0        "Capacitor, MLCC, 10nF, 50V, X7R, +/-10%, 0402, T=0.5mm"                                   
B4         SW-PUSH-CMS_KMR2_BLACK     TopLayer    SWI_C&K_Y78B23110FP__ITT_KMR231GLFS            -27.5500     -47.8500     0        "Microminiature Tact Switch for SMT - KMR 2 Series - 1.9 mm height"                        
B3         SW-PUSH-CMS_KMR2_BLACK     TopLayer    SWI_C&K_Y78B23110FP__ITT_KMR231GLFS            -35.8000     -47.8500     0        "Microminiature Tact Switch for SMT - KMR 2 Series - 1.9 mm height"                        
B2         SW-PUSH-CMS_KMR2_BLACK     TopLayer    SWI_C&K_Y78B23110FP__ITT_KMR231GLFS            -41.9500     -47.8220     0        "Microminiature Tact Switch for SMT - KMR 2 Series - 1.9 mm height"                        
B1         SW-PUSH-CMS_KMR2_BLACK     TopLayer    SWI_C&K_Y78B23110FP__ITT_KMR231GLFS            -48.2500     -47.8220     0        "Microminiature Tact Switch for SMT - KMR 2 Series - 1.9 mm height"                        
