Altium Designer Pick and Place Locations
C:\Subversion\__Boards\MB1803-MiniBoard-WBA5x-QFN48-SMPS-SingleAntenna\Trunk\02-Manufacturing\MB1803B_PCB\Assembly\MB1803B_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       22/02/24
Time:       11:45
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator   Comment                     Layer       Footprint                        Center-X(mm) Center-Y(mm) Rotation Description                                                                   
CN1          FTSH-125-02-L-DV            BottomLayer FTSH-125-02-L-DV                 4.3664       18.5484      180      "Header, 25x2, 12.7mm, VR, SMD, T=4.83mm"                                     
CN2          FTSH-125-02-L-DV            BottomLayer FTSH-125-02-L-DV                 38.6564      18.5558      180      "Header, 25x2, 12.7mm, VR, SMD, T=4.83mm"                                     
SH1          "RF Shield (22.2x19.2x2mm)" TopLayer    SHIELD_RF_ST-CUSTOM_22P2X19P2_H2 -275.4530    -237.3752    0        "RF Shield (22.2x19.2x2mm)"                                                   
SB43         SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           9.8531       13.8804      180      "Solder Bridge OFF, 0R, 0402"                                                 
C27          Capacitor                   BottomLayer C0402                            10.0289      14.7823      180      "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                       
L7           Inductor                    TopLayer    IND_0603_H0P8                    14.9116      24.6887      90       "Ferrite bead, 47R @ 100MHz, +/-25%, 3.5A, 0R02, 0603, T=0.8mm"               
L5           Inductor                    TopLayer    C0402                            20.5054      25.3126      270      "Inductor, 10nH, +/-2%, 500 mA, 0.26Ohm, 0402, T=0.5mm"                       
SB30         SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           17.6700      17.6761      0        "Solder Bridge 0402 ON"                                                       
SB17         SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           10.8520      8.2208       0        "Solder Bridge 0402 ON"                                                       
SB14         SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           10.8712      7.2048       0        "Solder Bridge OFF, 0R, 0402"                                                 
SB10         SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           31.6001      28.8225      0        "Solder Bridge 0402 ON"                                                       
SB42         SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           29.5452      26.8231      0        "Solder Bridge 0402 ON"                                                       
SB41         SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           15.2234      28.4113      0        "Solder Bridge 0402 ON"                                                       
SB6          SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           13.0840      28.4005      0        "Solder Bridge OFF, 0R, 0402"                                                 
L6           Inductor                    TopLayer    L0805_H0P9                       19.9094      23.5343      180      "Inductor, 2.2uH, +/-20%, 0.7A, 0R156, 0805, T=0.9mm"                         
L4           Inductor                    TopLayer    IND_0603_H0P8                    17.1218      22.4783      180      "Ferrite bead, 47R @ 100MHz, +/-25%, 3.5A, 0R02, 0603, T=0.8mm"               
C26          Capacitor                   TopLayer    C0402                            15.1378      33.0566      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
C25          Capacitor                   TopLayer    C0402                            16.9413      24.3230      90       "Capacitor, MLCC, 2.2uF, 6V3, X5R,+/-10%, 0402, T=0.5mm"                      
C24          Capacitor                   TopLayer    C0402                            15.6516      27.7586      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
C23          Capacitor                   TopLayer    C0402                            17.8253      24.3144      270      "Capacitor, MLCC, 4.7uF, 6V3, X5R, +/-20%, 0402, T=0.5mm"                     
C6           Capacitor                   TopLayer    C0603_H0P8                       18.8370      25.8285      180      "Capacitor, MLCC, 10uF, 10V, X6S, +/-20%, 0603, T=1mm"                        
Designator16 Comment                     TopLayer    IMPEDANCE_TABLE                  -275.4530    -237.3752    0        ""                                                                            
Designator15 Comment                     TopLayer    Sheetbox_4L2S                    96.9858      -7.8310      0        ""                                                                            
Designator14 Comment                     TopLayer    PCB_SPECIFICATIONS               -275.4530    -237.3752    0        ""                                                                            
Label_7      LOGO_ESD                    BottomLayer LOGO_ESD                         -275.4530    -237.3752    180      ""                                                                            
Label_6      LOGO_CE                     BottomLayer LOGO_CE                          -275.4530    -237.3752    180      ""                                                                            
L1           Inductor                    TopLayer    C0402                            17.8360      36.1036      90       "Inductor, 1.8nH, +/-0.3nH, 9500 mA, 0.08Ohm, 0402, T=0.5mm"                  
L2           Inductor                    TopLayer    C0402                            17.8067      38.7920      90       "Inductor, 1.3nH, +/-0.3nH, 1000 mA, 0.07Ohm, 0402, T=0.5mm"                  
Label_2      LOGO_ST                     BottomLayer LOGO_ST_Size3                    -275.4530    -237.3752    180      ""                                                                            
SB4          SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           10.1636      17.1072      180      "Solder Bridge OFF, 0R, 0402"                                                 
SB3          SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           10.7817      24.2954      180      "Solder Bridge OFF, 0R, 0402"                                                 
SB2          SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           10.7263      33.8458      180      "Solder Bridge OFF, 0R, 0402"                                                 
Label_1      LOGO_ST                     TopLayer    LOGO_ST_Size3                    -275.4530    -237.3752    0        ""                                                                            
Label_4      LOGO_STM32                  TopLayer    LOGO_STM32                       -275.4530    -237.3752    0        ""                                                                            
CN3          "Header 7x2"                TopLayer    CON_SAMTEC_FTSH-107-01-L-DV-K-A  22.1014      4.5794       0        "Header, 7x2, 1.27mm, VR, T=5.97mm, FTSH series STDC14 without Alignment Pin" 
U1           STM32WBA55CGU6              TopLayer    ICC_UFQFPN48-EPAD_7X7_H0P55_P050 21.8948      30.6081      90       "MCU,ARM Cortex M33,1MB Flash, 128KB SRAM, Crypto, RF 2.4GHz, BLE, 802.15.4"  
SB5          SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           32.4350      2.3430       0        "Solder Bridge OFF, 0R, 0402"                                                 
SB1          SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           10.8552      22.3294      180      "Solder Bridge OFF, 0R, 0402"                                                 
C19          Capacitor                   TopLayer    C0402                            15.6578      28.5752      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
C18          Capacitor                   TopLayer    C0402                            19.5456      36.2872      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
C17          Capacitor                   TopLayer    C0402                            27.4565      33.0519      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
C16          Capacitor                   TopLayer    C0402                            25.4739      25.8314      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
C15          Capacitor                   TopLayer    C0402                            15.6731      29.3688      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
C5           Capacitor                   BottomLayer C0402                            34.6782      2.8806       90       "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                       
C3           Capacitor                   BottomLayer C0402                            8.7818       24.1515      270      "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                       
C2           Capacitor                   BottomLayer C0402                            8.6490       34.2552      270      "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                       
C1           Capacitor                   BottomLayer C0402                            9.0496       21.8036      90       "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                       
X2           XTAL_4_PINS                 TopLayer    CRY_NX1612SA_4P                  15.0061      30.9636      0        "Crystal, 32MHz, 8pF, +/-10ppm, 40R, 1612(metric), T=0.3mm"                   
X1           XTAL_2_PINS                 TopLayer    CRY_NX1610SE_2P                  26.5812      29.5724      270      "Crystal, 32.768kHz, 6pF, +/-20ppm, 70KR, 1.6x1mm"                            
SC5          Shield-clip_S0951-46R       TopLayer    CLIP_HARWIN_S0951-46R            9.1846       31.0128      90       "shield clip Harwin S0951-46R to fix RF shielded cavity"                      
SC4          Shield-clip_S0951-46R       TopLayer    CLIP_HARWIN_S0951-46R            20.5020      20.7446      180      "shield clip Harwin S0951-46R to fix RF shielded cavity"                      
SC3          Shield-clip_S0951-46R       TopLayer    CLIP_HARWIN_S0951-46R            31.1821      29.9714      90       "shield clip Harwin S0951-46R to fix RF shielded cavity"                      
SC2          Shield-clip_S0951-46R       TopLayer    CLIP_HARWIN_S0951-46R            27.2220      39.7420      180      "shield clip Harwin S0951-46R to fix RF shielded cavity"                      
SC1          Shield-clip_S0951-46R       TopLayer    CLIP_HARWIN_S0951-46R            12.8619      39.7485      180      "shield clip Harwin S0951-46R to fix RF shielded cavity"                      
SB40         SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           14.7474      32.2376      180      "Solder Bridge OFF, 0R, 0402"                                                 
SB39         SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           12.8242      31.1166      180      "Solder Bridge OFF, 0R, 0402"                                                 
SB38         SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           28.4237      28.5688      0        "Solder Bridge OFF, 0R, 0402"                                                 
SB37         SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           28.5742      30.6123      0        "Solder Bridge OFF, 0R, 0402"                                                 
SB36         SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           32.4336      17.9410      0        "Solder Bridge OFF, 0R, 0402"                                                 
SB35         SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           32.3298      21.7226      180      "Solder Bridge OFF, 0R, 0402"                                                 
SB34         SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.3773      5.5556       0        "Solder Bridge 0402 ON"                                                       
SB33         SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.3565      24.7894      180      "Solder Bridge 0402 ON"                                                       
SB32         SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           27.6206      18.6501      180      "Solder Bridge OFF, 0R, 0402"                                                 
SB31         SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.3948      19.9317      0        "Solder Bridge 0402 ON"                                                       
SB29         SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.3895      10.6680      180      "Solder Bridge 0402 ON"                                                       
SB28         SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           29.7946      17.9998      180      "Solder Bridge OFF, 0R, 0402"                                                 
SB27         SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           29.8222      17.0752      180      "Solder Bridge OFF, 0R, 0402"                                                 
SB26         SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.3451      22.7312      180      "Solder Bridge 0402 ON"                                                       
SB25         SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           10.8644      30.0218      180      "Solder Bridge OFF, 0R, 0402"                                                 
SB24         SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.3126      15.1764      180      "Solder Bridge 0402 ON"                                                       
SB23         SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.4425      16.9012      0        "Solder Bridge 0402 ON"                                                       
SB22         SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           29.7783      13.9880      180      "Solder Bridge OFF, 0R, 0402"                                                 
SB21         SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           16.4808      6.0397       90       "Solder Bridge 0402 ON"                                                       
SB20         SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           27.6207      19.5311      180      "Solder Bridge OFF, 0R, 0402"                                                 
SB19         SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           10.8876      9.3366       0        "Solder Bridge OFF, 0R, 0402"                                                 
SB18         SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.4110      7.2742       0        "Solder Bridge 0402 ON"                                                       
SB16         SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.4226      8.3714       0        "Solder Bridge 0402 ON"                                                       
SB15         SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.4020      11.8324      0        "Solder Bridge 0402 ON"                                                       
SB13         SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           31.5858      29.7890      0        "Solder Bridge 0402 ON"                                                       
SB12         SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.3843      9.6978       0        "Solder Bridge 0402 ON"                                                       
SB11         SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.4264      26.7458      0        "Solder Bridge 0402 ON"                                                       
SB9          SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           10.8627      6.2802       0        "Solder Bridge 0402 ON"                                                       
SB8          SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           23.4212      12.0213      90       "Solder Bridge OFF, 0R, 0402"                                                 
SB7          SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.4158      25.7670      0        "Solder Bridge 0402 ON"                                                       
R9           Resistor                    BottomLayer R0402                            27.0237      3.8997       270      Resistor,47R,0402,1%,1/16W                                                    
R8           Resistor                    BottomLayer R0402                            25.9224      9.8779       90       Resistor,47R,0402,1%,1/16W                                                    
R7           Resistor                    BottomLayer R0402                            24.6584      9.8529       90       Resistor,47R,0402,1%,1/16W                                                    
R6           Resistor                    BottomLayer R0402                            24.3864      2.6308       90       Resistor,47R,0402,1%,1/16W                                                    
R5           Resistor                    BottomLayer R0402                            23.3764      9.8779       90       Resistor,47R,0402,1%,1/16W                                                    
R4           Resistor                    BottomLayer R0402                            22.0924      9.8524       90       Resistor,47R,0402,1%,1/16W                                                    
R3           Resistor                    BottomLayer R0402                            20.8874      9.8779       90       Resistor,47R,0402,1%,1/16W                                                    
R2           Resistor                    BottomLayer R0402                            19.6054      9.8779       90       Resistor,47R,0402,1%,1/16W                                                    
R1           Resistor                    TopLayer    R0402                            11.1249      28.3196      270      "Resistor, 100K, 0402, +/-1%, 1/16W"                                          
L3           Inductor                    TopLayer    IND_0603_H0P8                    23.5490      24.0943      90       "Ferrite bead, 47R @ 100MHz, +/-25%, 3.5A, 0R02, 0603, T=0.8mm"               
HW4          STICKER_PRODUCT             TopLayer    STICKER_PRODUCT_25X5             -275.4530    -237.3752    90       "Sticker product 25x5 mm"                                                     
HW3          STICKER_BOARD               TopLayer    STICKER_BOARD_25X5               -275.4530    -237.3752    90       "Sticker board 25x5 mm"                                                       
D1           SCHOTTKY_1A_2K              TopLayer    DIO_SOD523_1A_2K                 12.8790      25.7837      180      "Small signal Schottky diodes"                                                
C22          Capacitor                   BottomLayer C0603                            20.2308      2.5544       90       "Capacitor, MLCC, 1uF, 16V, X5R, 10%, 0603, T=0,8mm"                          
C21          Capacitor                   TopLayer    C0402                            15.1068      22.2215      180      "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                       
C20          Capacitor                   TopLayer    C0402                            25.0201      24.8610      180      "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                       
C10          Capacitor                   TopLayer    C0402                            15.0340      32.2015      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
C14          Capacitor                   TopLayer    C0402_MURATA_GRM155_H0P5         17.3336      40.1764      180      "Capacitor, MLCC, 2.7pF, 50V, +/-0.1pF, 0402, T=0.5mm"                        
C13          Capacitor                   TopLayer    C0402                            17.3551      37.4304      0        "Capacitor, MLCC, 3.9pF, 50V, C0G, +/-0.25pF, 0402, T=0.5mm"                  
C12          Capacitor                   TopLayer    C0402                            17.4325      34.8732      180      "Capacitor, MLCC, 1.5pF, 50V, C0G, +/-0.25pF, 0402, T=0.5mm"                  
C11          Capacitor                   TopLayer    C0603                            15.9748      34.6216      270      "Capacitor, MLCC, 470nF, 16V, X7R, +/-10%, 0603, T=0.8mm"                     
C4           Capacitor                   BottomLayer C0402                            8.5040       16.5807      270      "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                       
C9           Capacitor                   TopLayer    C0402                            28.0528      30.1185      180      "Capacitor, MLCC, 6 pF, 50V, NPO, ±0,25pF, 0402, T=0.5mm"                     
C8           Capacitor                   TopLayer    C0402                            28.0606      28.9956      180      "Capacitor, MLCC, 6 pF, 50V, NPO, ±0,25pF, 0402, T=0.5mm"                     
C7           Capacitor                   TopLayer    C0402                            13.0421      24.7447      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
