Altium Designer Pick and Place Locations
C:\work\MC board\RevB\final\02-Manufacturing\MB1811B_PCB\Assembly\MB1811B_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       24/05/22
Time:       15:27
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator Comment                                Layer       Footprint                                       Center-X(mm) Center-Y(mm) Rotation Description                                                                                                                  
U15        TPS259535DSG                           TopLayer    ICC_WSON8-EPAD_2X2_P050                         55.1150      96.8934      90       "IC, eFuse with Fast Overvoltage Protection 2.7V to 18V 4A 34mOhm 8-Pin WSON"                                                
SB64       SB_OFF                                 TopLayer    SOLDER-BRIDGE_R0603-0R                          6.8547       76.5252      270      "Solder Bridge OFF"                                                                                                          
SB65       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          5.4577       76.5254      270      "Solder Bridge ON"                                                                                                           
SB61       SB_OFF                                 TopLayer    SOLDER-BRIDGE_R0603-0R                          5.5847       61.8913      90       "Solder Bridge OFF"                                                                                                          
SB62       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          8.3820       76.4882      270      "Solder Bridge ON"                                                                                                           
SB63       SB_OFF                                 TopLayer    SOLDER-BRIDGE_R0603-0R                          9.9027       76.5254      270      "Solder Bridge OFF"                                                                                                          
R54        Resistor                               TopLayer    R0402                                           65.5287      93.7185      90       "Resistor, 100K, 0402, +/-1%, 1/16W"                                                                                         
R55        Resistor                               TopLayer    R0402                                           66.6717      93.7183      90       "Resistor, 100K, 0402, +/-1%, 1/16W"                                                                                         
JP3        "Jumper_Header 2x1"                    TopLayer    CON_SAMTEC_TSW-102-07-G-S                       55.4988      104.5213     90       "Header, 2x1, 2.54mm, VR, TH, T=5.84mm/2.54mm"                                                                               
D4         SCHOTTKY_1A_2K                         TopLayer    DIO_SOD323_1A_2K                                33.7788      92.1944      0        "Signal Schottky Diode, If=1A, Ifsm=5A, Vf =0.54V@1A, Vrrm=23V, Ir = 0.65µA@5V, SOD-323"                                     
C44        Capacitor                              TopLayer    C0402                                           63.1157      76.8274      180      "Capacitor, MLCC, 2.7pF, 50V, NPO, +/-0.1pF, 0402, T=0.5mm"                                                                  
C46        Capacitor                              TopLayer    C0402                                           56.1307      94.4805      90       "Capacitor, MLCC, 100nF, 25V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C45        Capacitor                              TopLayer    C0603                                           57.1467      97.5284      90       "Capacitor, MLCC, 10uF, 10V, X5R, +/-10%, 0603, T=0.8mm"                                                                     
C34        Capacitor                              TopLayer    C0402                                           65.5287      90.9244      270      "Capacitor, MLCC, 10nF, 50V, X7R, +/-10%, 0402, T=0.5mm"                                                                     
C33        Capacitor                              TopLayer    C0402                                           61.5917      90.9245      90       "Capacitor, MLCC, 20pF, 50V, NPO, +/- 5%, 0402, T=0.5mm"                                                                     
C32        Capacitor                              TopLayer    C0805                                           36.9537      96.1313      270      "Capacitor, MLCC, 2.2uF, 25V, X7R, +/-10%, 0805, T=1,25mm"                                                                   
CN2        "Header 7x2"                           TopLayer    CON_SAMTEC_FTSH-107-01-L-DV-K-A                 47.7518      104.2031     180      "Header, 7x2, 1.27mm, VR, SMD, T=5.97mm"                                                                                     
X3         XTAL_4_PINS                            TopLayer    CRY_NX2016SA_4P                                 61.9726      75.1764      0        "Crystal, 24MHz, 6pF, +/-20ppm, 80R, 2x1.6mm"                                                                                
X1         OSCILLATOR_4_PINS                      TopLayer    CRY_NZ2016SH_4P                                 30.8606      68.0720      270      "Oscillator, SPXO, 24MHz, +/-50ppm, square wave, 3V3, 2x1.6mm"                                                               
X2         XTAL_2_PINS                            TopLayer    CRY_NX2012SA_2P                                 34.4608      68.8668      0        "Crystal, 32.768kHz, 6pF, +/-20ppm, 80K, 2.05x1.2mm"                                                                         
U9         ESDALC6V1W5                            TopLayer    ESD_SOT323-5L                                   43.5576      95.8774      270      "Dual Transil array for ESD protection"                                                                                      
U10        ESDALC6V1W5                            TopLayer    ESD_SOT323-5L                                   48.5106      95.8774      270      "Dual Transil array for ESD protection"                                                                                      
U6         STMPS2151STR                           TopLayer    MOS_SOT23-5L                                    27.3589      92.6831      270      "500mA, Enhanced single channel power switches with active high enable pin"                                                  
U8         ST730M33R                              TopLayer    ICC_SOT23-5L_H1P45                              38.0968      92.3214      180      "LDO, 3.3V, 300mA, High input voltage: 2.5V to 28V, SOT23-5L"                                                                
U14        ECMF02-2AMX6                           TopLayer    ESD_QFN-6L_1P7X1P5_P050                         63.2172      95.6234      180      "Common mode filter with ESD protection for USB 2.0 interface"                                                               
U13        ESD-TRANSIL                            TopLayer    ESD_QFN1610_2N_1K_2A                            60.8300      95.2424      180      "High power Transient voltage suppressor:25V/35A EOS and ESD transients protection."                                         
U12        STLINK-V3EC                            TopLayer    ICC_UFBGA201_176+25_10X10_P065                  62.6154      83.6705      90       "MCU, Arm Cortex-M7 32-bit MCU, 512KB Flash, 276KB RAM, With Crypto"                                                         
U1         TS461CLT                               TopLayer    AOP_SOT23-5L_H1P45                              8.2010       36.9566      180      "Output rail-to-rail operational amplifiers. Large output swing (+/- 2.4V at VCC  = +/- 2.5V). Operating range: 2.7V to 10V" 
U2         LDL112PV33R                            TopLayer    ICC_DFN6-EPAD_3X3_P095                          18.4149      96.6473      270      "1.2 A low quiescent current LDO with reverse current protection"                                                            
U3         ESD-TRANSIL                            TopLayer    ESD_ST0201                                      17.4059      13.2923      90       "ESD protection 6V1"                                                                                                         
U11        ESD-TRANSIL                            TopLayer    ESD_ST0201                                      52.5778      8.6360       180      "ESD protection 6V1"                                                                                                         
U7         ESD-TRANSIL                            TopLayer    ESD_ST0201                                      35.1788      8.5090       180      "ESD protection 6V1"                                                                                                         
U4         STG4160                                TopLayer    ESD_FLIP-CHIP-BGA8_1P9X0P9_P050                 18.1609      52.5783      270      "Low voltage 0.5 ohm single SPDT switch with break-before-make feature and 15 kV contact ESD protection"                     
U5         STM32G473QET6                          TopLayer    ICC_LQFP128_14X14_P040                          31.1148      53.0784      270      "MCU, Arm Cortex-M4, 32-bit MCU+FPU, up to 512 KB Flash, 128 KB SRAM"                                                        
TP2        "Test Point"                           TopLayer    TP_SMD_1MM                                      15.8717      37.5844      90       "Test Point 1mm"                                                                                                             
TP4        "Test Point"                           TopLayer    TP_SMD_1MM                                      15.4938      93.2183      0        "Test Point 1mm"                                                                                                             
TP3        "Test Point"                           TopLayer    TP_SMD_1MM                                      12.5728      99.5683      0        "Test Point 1mm"                                                                                                             
TP32       "Test Point"                           TopLayer    TP_SMD_1MM                                      68.0718      19.6850      90       "Test Point 1mm"                                                                                                             
TP1        "Test Point"                           TopLayer    TP_SMD_1MM                                      9.1438       99.6950      90       "Test Point 1mm"                                                                                                             
TP41       "Test Point"                           TopLayer    TP_SMD_1MM                                      68.1988      49.9113      90       "Test Point 1mm"                                                                                                             
TP23       "Test Point"                           TopLayer    TP_SMD_1MM                                      64.8968      49.9113      90       "Test Point 1mm"                                                                                                             
TP30       "Test Point"                           TopLayer    TP_SMD_1MM                                      66.5477      41.1483      90       "Test Point 1mm"                                                                                                             
TP20       "Test Point"                           TopLayer    TP_SMD_1MM                                      64.8968      17.1450      90       "Test Point 1mm"                                                                                                             
TP29       "Test Point"                           TopLayer    TP_SMD_1MM                                      65.0238      14.2243      90       "Test Point 1mm"                                                                                                             
TP31       "Test Point"                           TopLayer    TP_SMD_1MM                                      68.0718      15.2400      90       "Test Point 1mm"                                                                                                             
TP10       "Test Point"                           TopLayer    TP_SMD_1MM                                      53.5938      27.1783      90       "Test Point 1mm"                                                                                                             
TP18       "Test Point"                           TopLayer    TP_SMD_1MM                                      63.7538      58.9283      180      "Test Point 1mm"                                                                                                             
TP42       "Test Point"                           TopLayer    TP_SMD_1MM                                      73.9137      81.5343      180      "Test Point 1mm"                                                                                                             
TP25       "Test Point"                           TopLayer    TP_SMD_1MM                                      64.8968      64.2623      180      "Test Point 1mm"                                                                                                             
TP38       "Test Point"                           TopLayer    TP_SMD_1MM                                      68.0718      72.2633      180      "Test Point 1mm"                                                                                                             
TP24       "Test Point"                           TopLayer    TP_SMD_1MM                                      64.8968      61.5953      180      "Test Point 1mm"                                                                                                             
TP28       "Test Point"                           TopLayer    TP_SMD_1MM                                      64.8968      73.4063      180      "Test Point 1mm"                                                                                                             
TP34       "Test Point"                           TopLayer    TP_SMD_1MM                                      68.0718      59.8173      180      "Test Point 1mm"                                                                                                             
TP27       "Test Point"                           TopLayer    TP_SMD_1MM                                      64.8968      70.3583      180      "Test Point 1mm"                                                                                                             
TP36       "Test Point"                           TopLayer    TP_SMD_1MM                                      68.0718      65.5323      180      "Test Point 1mm"                                                                                                             
TP35       "Test Point"                           TopLayer    TP_SMD_1MM                                      68.0718      62.9923      180      "Test Point 1mm"                                                                                                             
TP26       "Test Point"                           TopLayer    TP_SMD_1MM                                      64.8968      67.3103      90       "Test Point 1mm"                                                                                                             
TP37       "Test Point"                           TopLayer    TP_SMD_1MM                                      68.0718      68.5803      90       "Test Point 1mm"                                                                                                             
TP40       "Test Point"                           TopLayer    TP_SMD_1MM                                      68.1988      34.2903      90       "Test Point 1mm"                                                                                                             
TP9        "Test Point"                           TopLayer    TP_SMD_1MM                                      52.7048      45.2123      90       "Test Point 1mm"                                                                                                             
TP17       "Test Point"                           TopLayer    TP_SMD_1MM                                      61.9758      43.6882      90       "Test Point 1mm"                                                                                                             
TP16       "Test Point"                           TopLayer    TP_SMD_1MM                                      61.8488      38.1003      90       "Test Point 1mm"                                                                                                             
TP14       "Test Point"                           TopLayer    TP_SMD_1MM                                      61.2138      34.5443      90       "Test Point 1mm"                                                                                                             
TP39       "Test Point"                           TopLayer    TP_SMD_1MM                                      68.1988      29.0833      90       "Test Point 1mm"                                                                                                             
TP19       "Test Point"                           TopLayer    TP_SMD_1MM                                      64.7698      28.4483      90       "Test Point 1mm"                                                                                                             
TP6        "Test Point"                           TopLayer    TP_SMD_1MM                                      47.1168      30.9883      90       "Test Point 1mm"                                                                                                             
TP13       "Test Point"                           TopLayer    TP_SMD_1MM                                      59.1818      27.1783      90       "Test Point 1mm"                                                                                                             
TP11       "Test Point"                           TopLayer    TP_SMD_1MM                                      53.5938      29.7183      90       "Test Point 1mm"                                                                                                             
TP15       "Test Point"                           TopLayer    TP_SMD_1MM                                      61.3408      29.7183      90       "Test Point 1mm"                                                                                                             
TP5        "Test Point"                           TopLayer    TP_SMD_1MM                                      39.3698      29.7183      90       "Test Point 1mm"                                                                                                             
TP8        "Test Point"                           TopLayer    TP_SMD_1MM                                      51.5618      33.7823      90       "Test Point 1mm"                                                                                                             
TP22       "Test Point"                           TopLayer    TP_SMD_1MM                                      64.8968      25.4003      90       "Test Point 1mm"                                                                                                             
TP7        "Test Point"                           TopLayer    TP_SMD_1MM                                      50.2918      30.9883      90       "Test Point 1mm"                                                                                                             
TP33       "Test Point"                           TopLayer    TP_SMD_1MM                                      68.0718      24.1300      90       "Test Point 1mm"                                                                                                             
TP21       "Test Point"                           TopLayer    TP_SMD_1MM                                      64.8968      21.5900      270      "Test Point 1mm"                                                                                                             
TP12       "Test Point"                           TopLayer    TP_SMD_1MM                                      59.1818      24.1303      90       "Test Point 1mm"                                                                                                             
SB24       SB_OFF                                 TopLayer    SOLDER-BRIDGE_R0603-0R                          19.9347      72.4240      90       "Solder Bridge OFF"                                                                                                          
SB25       SB_OFF                                 TopLayer    SOLDER-BRIDGE_R0603-0R                          21.0779      68.5265      270      "Solder Bridge OFF"                                                                                                          
SB10       SB_OFF                                 TopLayer    SOLDER-BRIDGE_R0603-0R                          16.5098      68.5302      270      "Solder Bridge OFF"                                                                                                          
SB80       SB_OFF                                 BottomLayer SOLDER-BRIDGE_R0603-0R                          28.1658      53.3669      180      "Solder Bridge OFF"                                                                                                          
SB79       SB_ON                                  BottomLayer SOLDER-BRIDGE_R0603-0R                          28.2009      54.7642      180      "Solder Bridge ON"                                                                                                           
SB73       SB_OFF                                 BottomLayer SOLDER-BRIDGE_R0603-0R                          35.5097      53.4670      180      "Solder Bridge OFF"                                                                                                          
SB74       SB_ON                                  BottomLayer SOLDER-BRIDGE_R0603-0R                          35.5097      54.8640      180      "Solder Bridge ON"                                                                                                           
SB77       SB_OFF                                 BottomLayer SOLDER-BRIDGE_R0603-0R                          31.7388      53.3591      180      "Solder Bridge OFF"                                                                                                          
SB78       SB_ON                                  BottomLayer SOLDER-BRIDGE_R0603-0R                          31.7388      54.7561      180      "Solder Bridge ON"                                                                                                           
SB81       SB_ON                                  BottomLayer SOLDER-BRIDGE_R0603-0R                          28.1628      51.8351      180      "Solder Bridge ON"                                                                                                           
SB75       SB_ON                                  BottomLayer SOLDER-BRIDGE_R0603-0R                          35.4098      52.0700      180      "Solder Bridge ON"                                                                                                           
SB76       SB_ON                                  BottomLayer SOLDER-BRIDGE_R0603-0R                          31.7388      51.9621      180      "Solder Bridge ON"                                                                                                           
SB2        SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          11.0488      28.7522      90       "Solder Bridge ON"                                                                                                           
SB3        SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          12.6998      28.7522      90       "Solder Bridge ON"                                                                                                           
SB42       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          38.5308      39.6243      0        "Solder Bridge ON"                                                                                                           
SB1        SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          12.6967      41.2175      270      "Solder Bridge ON"                                                                                                           
SB12       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          18.3650      93.2183      180      "Solder Bridge ON"                                                                                                           
SB83       SB_ON                                  BottomLayer SOLDER-BRIDGE_R0603-0R                          19.8118      54.7872      90       "Solder Bridge ON"                                                                                                           
SB58       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          46.7860      54.8643      0        "Solder Bridge ON"                                                                                                           
SB49       SB_OFF                                 TopLayer    SOLDER-BRIDGE_R0603-0R                          42.7218      54.8643      0        "Solder Bridge OFF"                                                                                                          
SB54       SB_OFF                                 TopLayer    SOLDER-BRIDGE_R0603-0R                          46.5856      50.6733      180      "Solder Bridge OFF"                                                                                                          
SB51       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          42.8137      50.6651      0        "Solder Bridge ON"                                                                                                           
SB56       SB_OFF                                 TopLayer    SOLDER-BRIDGE_R0603-0R                          46.7556      56.7690      0        "Solder Bridge OFF"                                                                                                          
SB68       SB_ON                                  BottomLayer SOLDER-BRIDGE_R0603-0R                          46.7556      56.7690      0        "Solder Bridge ON"                                                                                                           
SB5        SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          15.3439      47.4101      180      "Solder Bridge ON"                                                                                                           
SB59       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          46.9817      52.5701      0        "Solder Bridge ON"                                                                                                           
SB43       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          37.8458      42.1141      270      "Solder Bridge ON"                                                                                                           
SB46       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          40.6398      42.1141      270      "Solder Bridge ON"                                                                                                           
SB15       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          18.8727      59.0553      180      "Solder Bridge ON"                                                                                                           
SB72       SB_ON                                  BottomLayer SOLDER-BRIDGE_R0603-0R                          42.6837      56.8960      0        "Solder Bridge ON"                                                                                                           
SB17       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          18.8730      60.4523      180      "Solder Bridge ON"                                                                                                           
SB57       SB_OFF                                 TopLayer    SOLDER-BRIDGE_R0603-0R                          46.6860      60.5793      180      "Solder Bridge OFF"                                                                                                          
SB30       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          24.8920      65.3280      90       "Solder Bridge ON"                                                                                                           
SB67       SB_ON                                  BottomLayer SOLDER-BRIDGE_R0603-0R                          46.7860      54.8643      0        "Solder Bridge ON"                                                                                                           
SB60       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          50.2148      50.6733      0        "Solder Bridge ON"                                                                                                           
SB50       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          42.6220      60.5793      180      "Solder Bridge ON"                                                                                                           
SB90       SB_ON                                  BottomLayer SOLDER-BRIDGE_R0603-0R                          15.4437      49.0492      180      "Solder Bridge ON"                                                                                                           
SB18       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          18.8944      49.0438      180      "Solder Bridge ON"                                                                                                           
SB91       SB_ON                                  BottomLayer SOLDER-BRIDGE_R0603-0R                          15.4437      60.4789      180      "Solder Bridge ON"                                                                                                           
SB82       SB_ON                                  BottomLayer SOLDER-BRIDGE_R0603-0R                          18.1577      65.5743      90       "Solder Bridge ON"                                                                                                           
SB13       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          18.7731      47.3979      180      "Solder Bridge ON"                                                                                                           
SB34       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          26.2888      65.3284      90       "Solder Bridge ON"                                                                                                           
SB26       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          22.0558      13.2080      0        "Solder Bridge ON"                                                                                                           
SB14       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          28.1178      65.2772      90       "Solder Bridge ON"                                                                                                           
SB44       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          38.6078      65.0742      90       "Solder Bridge ON"                                                                                                           
SB89       SB_ON                                  BottomLayer SOLDER-BRIDGE_R0603-0R                          15.4516      50.6461      180      "Solder Bridge ON"                                                                                                           
SB70       SB_ON                                  BottomLayer SOLDER-BRIDGE_R0603-0R                          42.8488      52.5783      0        "Solder Bridge ON"                                                                                                           
SB53       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          42.9058      46.7444      0        "Solder Bridge ON"                                                                                                           
SB85       SB_ON                                  BottomLayer SOLDER-BRIDGE_R0603-0R                          18.8727      50.6463      180      "Solder Bridge ON"                                                                                                           
SB28       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          23.4917      65.3204      90       "Solder Bridge ON"                                                                                                           
SB33       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          26.4158      68.8844      90       "Solder Bridge ON"                                                                                                           
SB20       SB_OFF                                 TopLayer    SOLDER-BRIDGE_R0603-0R                          18.2837      72.4240      90       "Solder Bridge OFF"                                                                                                          
SB29       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          22.0947      65.3203      90       "Solder Bridge ON"                                                                                                           
SB41       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          37.2108      65.0742      90       "Solder Bridge ON"                                                                                                           
SB27       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          21.4587      72.4320      90       "Solder Bridge ON"                                                                                                           
SB36       SB_ON                                  BottomLayer SOLDER-BRIDGE_R0603-0R                          16.5067      65.5743      90       "Solder Bridge ON"                                                                                                           
SB7        SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          15.4437      60.4792      180      "Solder Bridge ON"                                                                                                           
SB19       SB_OFF                                 TopLayer    SOLDER-BRIDGE_R0603-0R                          18.2837      68.5221      270      "Solder Bridge OFF"                                                                                                          
SB86       SB_ON                                  BottomLayer SOLDER-BRIDGE_R0603-0R                          28.0985      65.3175      90       "Solder Bridge ON"                                                                                                           
SB87       SB_ON                                  BottomLayer SOLDER-BRIDGE_R0603-0R                          18.8727      59.0553      180      "Solder Bridge ON"                                                                                                           
SB55       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          46.7477      59.0550      0        "Solder Bridge ON"                                                                                                           
SB45       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          39.2428      42.1141      270      "Solder Bridge ON"                                                                                                           
SB47       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          42.6837      56.8960      0        "Solder Bridge ON"                                                                                                           
SB71       SB_ON                                  BottomLayer SOLDER-BRIDGE_R0603-0R                          42.8219      54.8643      0        "Solder Bridge ON"                                                                                                           
SB66       SB_ON                                  BottomLayer SOLDER-BRIDGE_R0603-0R                          46.9817      52.5699      0        "Solder Bridge ON"                                                                                                           
SB52       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          42.8488      52.5783      0        "Solder Bridge ON"                                                                                                           
SB16       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          18.8727      50.6463      180      "Solder Bridge ON"                                                                                                           
SB23       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          19.7317      68.5011      270      "Solder Bridge ON"                                                                                                           
SB48       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          42.6837      59.0550      0        "Solder Bridge ON"                                                                                                           
SB92       SB_ON                                  BottomLayer SOLDER-BRIDGE_R0603-0R                          15.3439      47.4101      180      "Solder Bridge ON"                                                                                                           
SB6        SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          15.4437      49.0492      180      "Solder Bridge ON"                                                                                                           
SB88       SB_ON                                  BottomLayer SOLDER-BRIDGE_R0603-0R                          18.7728      47.3982      180      "Solder Bridge ON"                                                                                                           
SB8        SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          15.4518      50.6463      180      "Solder Bridge ON"                                                                                                           
SB39       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          30.6027      35.6371      90       "Solder Bridge ON"                                                                                                           
SB84       SB_ON                                  BottomLayer SOLDER-BRIDGE_R0603-0R                          18.8943      49.0438      180      "Solder Bridge ON"                                                                                                           
SB38       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          29.2098      32.7163      270      "Solder Bridge ON"                                                                                                           
SB40       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          36.4488      42.1143      270      "Solder Bridge ON"                                                                                                           
SB37       SB_OFF                                 TopLayer    SOLDER-BRIDGE_R0603-0R                          29.2057      35.6371      90       "Solder Bridge OFF"                                                                                                          
SB69       SB_ON                                  BottomLayer SOLDER-BRIDGE_R0603-0R                          42.9058      46.7444      0        "Solder Bridge ON"                                                                                                           
SB9        SB_OFF                                 TopLayer    SOLDER-BRIDGE_R0603-0R                          15.1128      68.5302      270      "Solder Bridge OFF"                                                                                                          
SB4        SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          13.7158      68.5303      270      "Solder Bridge ON"                                                                                                           
SB35       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          26.4086      35.6452      90       "Solder Bridge ON"                                                                                                           
SB32       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          24.8918      32.7161      270      "Solder Bridge ON"                                                                                                           
SB31       SB_OFF                                 TopLayer    SOLDER-BRIDGE_R0603-0R                          24.8846      35.6452      90       "Solder Bridge OFF"                                                                                                          
SB22       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          19.2578      41.0210      0        "Solder Bridge ON"                                                                                                           
SB11       SB_ON                                  TopLayer    SOLDER-BRIDGE_R0603-0R                          17.0178      40.3094      90       "Solder Bridge ON"                                                                                                           
SB21       SB_OFF                                 TopLayer    SOLDER-BRIDGE_R0603-0R                          19.2578      39.4970      0        "Solder Bridge OFF"                                                                                                          
RV1        POTENTIOMETER                          TopLayer    POT_BOURNS_3386P-1-101TLF                       17.6599      5.8194       0        "Trimmer, 10K, 3386, +/-10%, 1/2W, T=4.83mm"                                                                                 
R21        Resistor                               TopLayer    R0402                                           26.2888      42.1641      90       "Resistor, 220R, 0402, +/-1%, 1/16W"                                                                                         
R69        Resistor                               BottomLayer R0402                                           18.9230      57.4040      0        "Resistor, 220R, 0402, +/-1%, 1/16W"                                                                                         
R16        Resistor                               TopLayer    R0402                                           24.0028      42.1643      90       "Resistor, 220R, 0402, +/-1%, 1/16W"                                                                                         
R70        Resistor                               BottomLayer R0402                                           29.5877      65.1434      270      "Resistor, 220R, 0402, +/-1%, 1/16W"                                                                                         
R25        Resistor                               BottomLayer R0402                                           14.9827      65.3974      90       "Resistor, 220R, 0402, +/-1%, 1/16W"                                                                                         
R72        Resistor                               TopLayer    R0402                                           28.0558      68.4422      270      "Resistor, 220R, 0402, +/-1%, 1/16W"                                                                                         
R73        Resistor                               BottomLayer R0402                                           15.7480      59.0553      0        "Resistor, 220R, 0402, +/-1%, 1/16W"                                                                                         
R64        Resistor                               TopLayer    R0402                                           69.7200      85.7174      0        "Resistor, 0R, 0402, +/-5%, 1/16W"                                                                                           
R46        Resistor                               TopLayer    R0402                                           70.4817      87.4953      90       "Resistor, 330R, 0402, +/-1%, 1/16W"                                                                                         
R63        Resistor                               TopLayer    R0402                                           52.3207      98.4173      270      "Resistor, 1K8, 0402, +/-1%, 1/16W"                                                                                          
R47        Resistor                               TopLayer    R0402                                           72.0057      87.4955      270      "Resistor, 1K, 0402, +/-0.1%, 1/16W, +/-25ppm/°C"                                                                            
R41        Resistor                               TopLayer    R0402                                           43.9400      99.0007      90       "Resistor, 0R, 0402, +/-5%, 1/16W"                                                                                           
R40        Resistor                               TopLayer    R0402                                           42.7970      99.0012      90       "Resistor, 33R, 0402, +/-1%, 1/16W"                                                                                          
R42        Resistor                               TopLayer    R0402                                           45.2100      99.0010      90       "Resistor, 0R, 0402, +/-5%, 1/16W"                                                                                           
R43        Resistor                               TopLayer    R0402                                           47.7500      99.0702      90       "Resistor, 0R, 0402, +/-5%, 1/16W"                                                                                           
R14        Resistor                               TopLayer    R0402                                           21.4628      42.1644      90       "Resistor, 220R, 0402, +/-1%, 1/16W"                                                                                         
R44        Resistor                               TopLayer    R0402                                           49.0200      99.0702      90       "Resistor, 33R, 0402, +/-1%, 1/16W"                                                                                          
R45        Resistor                               TopLayer    R0402                                           50.2900      99.0702      90       "Resistor, 33R, 0402, +/-1%, 1/16W"                                                                                          
R34        Resistor                               TopLayer    R0402                                           30.2227      91.3053      90       "Resistor, 100K, 0402, +/-1%, 1/16W"                                                                                         
R30        Resistor                               TopLayer    R0402                                           24.2537      91.0513      90       "Resistor, 100K, 0402, +/-1%, 1/16W"                                                                                         
R35        Resistor                               TopLayer    R0402                                           65.5287      96.1313      270      "Resistor, 5K1, 0402, +/-1%, 1/16W"                                                                                          
R59        Resistor                               TopLayer    R0402                                           58.2897      97.5285      270      "Resistor, 5K1, 0402, +/-1%, 1/16W"                                                                                          
R57        Resistor                               BottomLayer R0402                                           61.3380      81.2724      0        "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                                          
R58        Resistor                               TopLayer    R0402                                           57.6550      99.3064      0        "Resistor, 3K, 0402, +/-1%, 1/16W"                                                                                           
R52        Resistor                               TopLayer    R0402                                           69.6303      79.8906      0        "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                                          
R49        Resistor                               BottomLayer R0402                                           46.2247      105.1484     180      "Resistor, 100R, 0402, +/- 1%, 1/16W"                                                                                        
R51        Resistor                               TopLayer    R0402                                           69.6303      81.0336      0        "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                                          
R48        Resistor                               TopLayer    R0402                                           63.0263      90.9098      90       "Resistor, 3K, 0402, +/-1%, 1/16W"                                                                                           
R50        Resistor                               TopLayer    R0402                                           69.6305      82.1766      0        "Resistor, 5K1, 0402, +/-1%, 1/16W"                                                                                          
R53        Resistor                               TopLayer    R0402                                           69.6305      78.7476      0        "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                                          
R56        Resistor                               TopLayer    R0402                                           66.6717      96.1313      270      "Resistor, 5K1, 0402, +/-1%, 1/16W"                                                                                          
R20        Resistor                               TopLayer    R0402                                           26.4158      71.8824      270      "Resistor, 220R, 0402, +/-1%, 1/16W"                                                                                         
R67        Resistor                               BottomLayer R0402                                           29.3338      57.7774      180      "Resistor, 220R, 0402, +/-1%, 1/16W"                                                                                         
R8         Resistor                               TopLayer    R0402                                           18.1778      65.2700      270      "Resistor, 220R, 0402, +/-1%, 1/16W"                                                                                         
R61        Resistor                               BottomLayer R0402                                           36.7000      57.7774      180      "Resistor, 220R, 0402, +/-1%, 1/16W"                                                                                         
R71        Resistor                               BottomLayer R0402                                           20.8278      65.5321      270      "Resistor, 220R, 0402, +/-1%, 1/16W"                                                                                         
R65        Resistor                               BottomLayer R0402                                           32.8928      57.7853      180      "Resistor, 220R, 0402, +/-1%, 1/16W"                                                                                         
R4         Resistor                               TopLayer    R0402                                           7.7437       39.4894      180      "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                                          
R1         Resistor                               TopLayer    R0402                                           11.5537      37.4575      270      "Resistor, 100R, 0402, +/- 1%, 1/16W"                                                                                        
R15        Resistor                               TopLayer    R0402                                           23.4948      99.5683      0        "Resistor, 1K8, 0402, +/-1%, 1/16W"                                                                                          
R3         Resistor                               TopLayer    R0402                                           7.7437       42.1564      0        "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                                          
R2         Resistor                               TopLayer    R0402                                           10.4869      33.4086      90       "Resistor, 4R7, 0402, +/-5%, 1/16W, +/-200ppm/°C"                                                                            
R23        Resistor                               TopLayer    R0402                                           26.9197      8.9191       90       "Resistor, 470R, 0402, +/-1%, 1/16W"                                                                                         
R28        Resistor                               TopLayer    R0402                                           28.6977      8.9191       90       "Resistor, 270R, 0402, +/-1%, 1/16W"                                                                                         
R32        Resistor                               TopLayer    R0402                                           30.4757      8.9191       90       "Resistor, 360R, 0402, +/-1%, 1/16W"                                                                                         
R10        Resistor                               TopLayer    R0402                                           21.2057      45.0773      90       "Resistor, 220R, 0402, +/-1%, 1/16W"                                                                                         
R9         Resistor                               TopLayer    R0402                                           18.5489      13.2923      90       "Resistor, 47R, 0402, +/-1%, 1/16W"                                                                                          
R68        Resistor                               BottomLayer R0402                                           28.4447      48.8875      90       "Resistor, 220R, 0402, +/-1%, 1/16W"                                                                                         
R60        Resistor                               BottomLayer R0402                                           46.6977      59.0553      0        "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                                          
R62        Resistor                               BottomLayer R0402                                           36.0647      48.8875      90       "Resistor, 220R, 0402, +/-1%, 1/16W"                                                                                         
R31        Resistor                               TopLayer    R0402                                           30.2258      71.1201      90       "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                                          
R36        Resistor                               TopLayer    R0402                                           31.3688      64.6431      270      "Resistor, 100R, 0402, +/- 1%, 1/16W"                                                                                        
R38        Resistor                               TopLayer    R0402                                           33.7988      64.6759      270      "Resistor, 0R, 0402, +/-5%, 1/16W"                                                                                           
R66        Resistor                               BottomLayer R0402                                           32.3817      48.8875      90       "Resistor, 220R, 0402, +/-1%, 1/16W"                                                                                         
R39        Resistor                               TopLayer    R0402                                           34.9418      64.6759      270      "Resistor, 0R, 0402, +/-5%, 1/16W"                                                                                           
R33        Resistor                               TopLayer    R0402                                           30.9850      33.6474      180      "Resistor, 30K, 0402, +/-0.1%, 1/16W, +/-25ppm/°C"                                                                           
R37        Resistor                               TopLayer    R0402                                           31.4927      31.1075      90       "Resistor, 1K, 0402, +/-0.1%, 1/16W, +/-50ppm/°C"                                                                            
R29        Resistor                               TopLayer    R0402                                           28.9517      38.2152      90       "Resistor, 220R, 0402, +/-1%, 1/16W"                                                                                         
R27        Resistor                               TopLayer    R0402                                           28.9560      30.7343      180      "Resistor, 1K, 0402, +/-0.1%, 1/16W, +/-50ppm/°C"                                                                            
R26        Resistor                               TopLayer    R0402                                           26.9207      29.7104      180      "Resistor, 30K, 0402, +/-0.1%, 1/16W, +/-25ppm/°C"                                                                           
R22        Resistor                               TopLayer    R0402                                           26.9210      33.7744      180      "Resistor, 30K, 0402, +/-0.1%, 1/16W, +/-25ppm/°C"                                                                           
R24        Resistor                               TopLayer    R0402                                           27.4287      31.2345      90       "Resistor, 1K, 0402, +/-0.1%, 1/16W, +/-50ppm/°C"                                                                            
R19        Resistor                               TopLayer    R0402                                           24.8918      38.2271      90       "Resistor, 220R, 0402, +/-1%, 1/16W"                                                                                         
R18        Resistor                               TopLayer    R0402                                           24.2568      30.7343      180      "Resistor, 1K, 0402, +/-0.1%, 1/16W, +/-50ppm/°C"                                                                            
R17        Resistor                               TopLayer    R0402                                           24.2568      29.7183      0        "Resistor, 30K, 0402, +/-0.1%, 1/16W, +/-25ppm/°C"                                                                           
R12        Resistor                               TopLayer    R0402                                           19.6848      52.4511      270      "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                                          
R11        Resistor                               TopLayer    R0402                                           18.5387      42.9183      270      "Resistor, 30K, 0402, +/-0.1%, 1/16W, +/-25ppm/°C"                                                                           
R7         Resistor                               TopLayer    R0402                                           17.2687      42.9185      90       "Resistor, 1K, 0402, +/-0.1%, 1/16W, +/-50ppm/°C"                                                                            
R13        Resistor                               TopLayer    R0402                                           21.2085      38.5081      90       "Resistor, 220R, 0402, +/-1%, 1/16W"                                                                                         
R6         Resistor                               TopLayer    R0402                                           15.7447      40.5055      270      "Resistor, 1K, 0402, +/-0.1%, 1/16W, +/-50ppm/°C"                                                                            
R5         Resistor                               TopLayer    R0402                                           14.4747      40.5055      270      "Resistor, 30K, 0402, +/-0.1%, 1/16W, +/-25ppm/°C"                                                                           
LD6        LED_BICOLOR                            TopLayer    LED_BI-GR_WE-150141SV73110                      71.2440      90.9243      180      "LED Bicolor, Green/Red, 2V, 20mA,  4-PLCC"                                                                                  
LD5        LED_BICOLOR                            TopLayer    LED_BI-GR_WE-150141SV73110                      71.2440      98.2905      180      "LED Bicolor, Green/Red, 2V, 20mA,  4-PLCC"                                                                                  
LD4        LED_green                              TopLayer    LED_0603_OSRAM_LG-Q396-PS-35_GREEN_1A2K_H0P4    23.6219      97.6633      180      "LED Green, 0603 SMD, Forward Voltage Typ=2V, Max=2.5V"                                                                      
LD3        LED_yellow                             TopLayer    LED_0603_OSRAM_LY-Q396-P1Q2-36_YELLOW_1A2K_H0P4 26.9197      6.2521       90       "LED Yellow, 0603 SMD, Forward Voltage min=1.7V, Typ=2V, Max=2.3V"                                                           
LD2        LED_red                                TopLayer    LED_0603_VISHAY_VLMS1300-GS08_RED_1A2K_H0P8     28.6977      6.2521       90       "LED Red, 0603 SMD, 2V Forward Voltage"                                                                                      
LD1        LED_green                              TopLayer    LED_0603_OSRAM_LG-Q396-PS-35_GREEN_1A2K_H0P4    30.4757      6.2521       90       "LED Green, 0603 SMD, Forward Voltage Typ=2V, Max=2.5V"                                                                      
L1         BEAD                                   BottomLayer L0603                                           17.3988      54.8643      180      "Ferrite bead, 600R @1 00MHz, +/-25%, 350mA, 0R5, 0603, T=0.8mm"                                                             
JP2        "Jumper_Header 4x2 Fitted 1-2"         TopLayer    CON_SAMTEC_TSW-104-07-X-D                       16.8908      103.2513     180      "Header, 4x2, 2.54mm, VR, TH, T=5.84mm/2.54mm"                                                                               
JP1        "Jumper_Header 3x1 Fitted 1-2"         TopLayer    CON_SAMTEC_TSW-103-07-F-S                       8.5087       96.2660      0        "Header, 3x1, 2.54mm, VR, TH, T=5.84mm/2.54mm"                                                                               
HW1        STICKER_BOARD                          TopLayer    STICKER_BOARD_25X9                              -230.0004    -189.9996    90       "Sticker Board 25x9 mm"                                                                                                      
HW2        STICKER_PRODUCT                        TopLayer    STICKER_PRODUCT_25X9                            -230.0004    -189.9996    90       "Sticker product 25x9 mm"                                                                                                    
H2         "POSITION HOLE"                        BottomLayer PTH_M1261-3005-N_3P5X6_M3_H14                   74.9996      104.0001     180      "POSITION HOLE C6D3R5"                                                                                                       
H4         "POSITION HOLE"                        BottomLayer PTH_M1261-3005-N_3P5X6_M3_H14                   4.9997       104.0001     180      "POSITION HOLE C6D3R5"                                                                                                       
H1         "POSITION HOLE"                        BottomLayer PTH_M1261-3005-N_3P5X6_M3_H14                   74.9996      5.0002       180      "POSITION HOLE C6D3R5"                                                                                                       
H3         "POSITION HOLE"                        BottomLayer PTH_M1261-3005-N_3P5X6_M3_H14                   4.9997       5.0002       180      "POSITION HOLE C6D3R5"                                                                                                       
D3         SCHOTTKY_1A_2K                         TopLayer    DIO_SOD323_1A_2K                                33.7820      93.8276      0        "Signal Schottky Diode, If=1A, Ifsm=5A, Vf =0.54V@1A, Vrrm=23V, Ir = 0.65µA@5V, SOD-323"                                     
D1         SCHOTTKY_1A_2K                         TopLayer    DIO_SOD523_1A_2K                                33.7105      96.7760      0        "Small signal Schottky diodes"                                                                                               
D2         SCHOTTKY_1A_2K                         TopLayer    DIO_SOD523_1A_2K                                33.7058      95.4532      0        "Small signal Schottky diodes"                                                                                               
CN10       "Header 19x2"                          TopLayer    CON_SAMTEC_TSW-119-09-X-D                       28.0002      22.2250      180      "Header, 19x2, 2.54mm, VR, TH, T=5.84mm/10.16mm"                                                                             
CN7        "Header 19x2"                          TopLayer    CON_SAMTEC_TSW-119-09-X-D                       28.0002      83.1850      180      "Header, 19x2, 2.54mm, VR, TH, T=5.84mm/10.16mm"                                                                             
CN1        "Header 5x2"                           TopLayer    CON_SAMTEC_FTSH-105-01-L-DV-K                   30.6068      104.1401     180      "Header, 5x2, 1.27mm, VR, SMD, T=5.97mm"                                                                                     
CN4        USB_TYPE_C_Receptacle_317JD24BZTF3K3C3 TopLayer    CON_USB-TYPEC_COXOC_317JD24BZTF3K3C3            63.4677      101.9847     180      "USB_TypeC, SMD+DIP, T= 2.96mm (for 1.6mm pcb)"                                                                              
CN3        "Header 4x1"                           TopLayer    CON_SAMTEC_TSW-104-07-G-S                       52.0698      91.3130      0        "Header, 4x1, 2.54mm, VR, TH, T=5.84mm/2.54mm"                                                                               
CN5        "PCIE-Gold Finger-X16"                 TopLayer    CON_BOARD_GOLDFINGER_PCI_EXPRESS_X16            84.5773      54.5003      90       "PCI EXPRESS x16 Add-in Card Edge-Finger"                                                                                    
C23        Capacitor                              TopLayer    C0603_H0P8                                      27.4318      42.1643      90       "Capacitor, MLCC, 2.2nF, 50V, C0G/NPO, +/-5%, 0603, T=0,8mm"                                                                 
C76        Capacitor                              TopLayer    C0603_H0P8                                      18.9197      57.3964      0        "Capacitor, MLCC, 2.2nF, 50V, C0G/NPO, +/-5%, 0603, T=0,8mm"                                                                 
C20        Capacitor                              TopLayer    C0603_H0P8                                      25.1458      42.1643      90       "Capacitor, MLCC, 2.2nF, 50V, C0G/NPO, +/-5%, 0603, T=0,8mm"                                                                 
C80        Capacitor                              TopLayer    C0603_H0P8                                      29.6164      65.2780      270      "Capacitor, MLCC, 2.2nF, 50V, C0G/NPO, +/-5%, 0603, T=0,8mm"                                                                 
C24        Capacitor                              TopLayer    C0603_H0P8                                      14.9827      65.3974      90       "Capacitor, MLCC, 2.2nF, 50V, C0G/NPO, +/-5%, 0603, T=0,8mm"                                                                 
C4         Capacitor                              BottomLayer C0603_H0P8                                      28.0558      68.4423      270      "Capacitor, MLCC, 2.2nF, 50V, C0G/NPO, +/-5%, 0603, T=0,8mm"                                                                 
C5         Capacitor                              TopLayer    C0603_H0P8                                      15.7478      59.0553      0        "Capacitor, MLCC, 2.2nF, 50V, C0G/NPO, +/-5%, 0603, T=0,8mm"                                                                 
C16        Capacitor                              TopLayer    C0603_H0P8                                      22.7328      42.1643      90       "Capacitor, MLCC, 2.2nF, 50V, C0G/NPO, +/-5%, 0603, T=0,8mm"                                                                 
C9         Capacitor                              TopLayer    C0603_H0P8                                      18.9225      45.4663      0        "Capacitor, MLCC, 2.2nF, 50V, C0G/NPO, +/-5%, 0603, T=0,8mm"                                                                 
C48        Capacitor                              TopLayer    C0402                                           65.1477      76.8274      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C6         Capacitor                              TopLayer    C0402                                           15.1199      13.2923      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C27        Capacitor                              TopLayer    C0402                                           30.3497      94.0993      270      "Capacitor, MLCC, 100nF, 25V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C18        Capacitor                              TopLayer    C0603                                           24.3106      93.1911      90       "Capacitor, MLCC, 10uF, 10V, X5R, +/-10%, 0603, T=0.8mm"                                                                     
C36        Capacitor                              TopLayer    C0402                                           66.6717      90.9245      270      "Capacitor, MLCC, 10nF, 50V, X7R, +/-10%, 0402, T=0.5mm"                                                                     
C35        Capacitor                              TopLayer    C0603                                           39.1127      96.1314      270      "Capacitor, MLCC, 10uF, 10V, X5R, +/-10%, 0603, T=0.8mm"                                                                     
C58        Capacitor                              BottomLayer C0402                                           58.0441      83.6823      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C50        Capacitor                              BottomLayer C0402                                           60.3174      79.7081      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C60        Capacitor                              BottomLayer C0402                                           58.0360      84.5744      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C56        Capacitor                              BottomLayer C0402                                           58.0441      82.7933      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C49        Capacitor                              BottomLayer C0402                                           58.0360      79.7484      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C47        Capacitor                              BottomLayer C0402                                           68.0690      79.4944      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C52        Capacitor                              BottomLayer C0402                                           66.2865      79.4797      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C63        Capacitor                              BottomLayer C0402                                           62.2267      85.4633      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C62        Capacitor                              BottomLayer C0402                                           60.3217      87.3685      90       "Capacitor, MLCC, 2.2uF, 6.3V, X5R, +/-10%, 0402, T=0.5mm"                                                                   
C43        Capacitor                              TopLayer    C0402                                           69.7197      84.0664      180      "Capacitor, MLCC, 2.2uF, 6.3V, X5R, +/-10%, 0402, T=0.5mm"                                                                   
C41        Capacitor                              BottomLayer C0402                                           63.8117      86.2735      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C51        Capacitor                              BottomLayer C0402                                           62.3616      79.7457      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C55        Capacitor                              BottomLayer C0402                                           58.0441      81.7773      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C53        Capacitor                              BottomLayer C0402                                           58.0441      80.7613      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C57        Capacitor                              BottomLayer C0402                                           67.3146      83.0473      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C54        Capacitor                              BottomLayer C0402                                           64.1275      81.3846      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C61        Capacitor                              BottomLayer C0402                                           67.3146      85.0793      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C59        Capacitor                              BottomLayer C0402                                           67.3146      84.0633      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C40        Capacitor                              BottomLayer C0402                                           62.2521      87.3683      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C42        Capacitor                              TopLayer    C0402                                           60.8298      96.5124      180      "Capacitor, MLCC, 100pF, 50V, NPO, +/-5%, 0402, T=0.5mm"                                                                     
C38        Capacitor                              TopLayer    C0402                                           64.5503      90.9098      270      "Capacitor, MLCC, 2.2uF, 6.3V, X5R, +/-10%, 0402, T=0.5mm"                                                                   
C39        Capacitor                              TopLayer    C0402                                           61.3377      76.8274      180      "Capacitor, MLCC, 2.7pF, 50V, NPO, +/-0.1pF, 0402, T=0.5mm"                                                                  
C19        Capacitor                              TopLayer    C0603_H0P8                                      25.0188      68.7071      90       "Capacitor, MLCC, 2.2nF, 50V, C0G/NPO, +/-5%, 0603, T=0,8mm"                                                                 
C74        Capacitor                              BottomLayer C0603_H0P8                                      28.1938      56.2613      0        "Capacitor, MLCC, 2.2nF, 50V, C0G/NPO, +/-5%, 0603, T=0,8mm"                                                                 
C10        Capacitor                              TopLayer    C0603_H0P8                                      19.4478      65.5241      270      "Capacitor, MLCC, 2.2nF, 50V, C0G/NPO, +/-5%, 0603, T=0,8mm"                                                                 
C67        Capacitor                              BottomLayer C0603_H0P8                                      35.5598      56.3880      0        "Capacitor, MLCC, 2.2nF, 50V, C0G/NPO, +/-5%, 0603, T=0,8mm"                                                                 
C13        Capacitor                              TopLayer    C0603_H0P8                                      20.8448      65.5239      270      "Capacitor, MLCC, 2.2nF, 50V, C0G/NPO, +/-5%, 0603, T=0,8mm"                                                                 
C72        Capacitor                              BottomLayer C0603_H0P8                                      31.6799      56.2384      0        "Capacitor, MLCC, 2.2nF, 50V, C0G/NPO, +/-5%, 0603, T=0,8mm"                                                                 
C3         Capacitor                              TopLayer    C0603                                           14.0937      37.4571      90       "Capacitor, MLCC, 2.2uF, 10V, X5R, +/- 10%, 0603, T=0.8mm"                                                                   
C1         Capacitor                              TopLayer    C0402                                           10.4107      37.4575      90       "Capacitor, MLCC, 1nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                      
C15        Capacitor                              TopLayer    C0402                                           21.3360      97.6633      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C8         Capacitor                              TopLayer    C0603                                           15.6208      97.1553      90       "Capacitor, MLCC, 1uF, 16V, X5R, +/-10%, 0603, T=0.8mm"                                                                      
C14        Capacitor                              TopLayer    C0402                                           21.3360      95.6313      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C12        Capacitor                              TopLayer    C0603                                           21.2088      93.7262      180      "Capacitor, MLCC, 1uF, 16V, X5R, +/-10%, 0603, T=0.8mm"                                                                      
C2         Capacitor                              TopLayer    C0402                                           9.0899       33.4006      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C84        Capacitor                              BottomLayer C0603                                           21.0818      55.8802      270      "Capacitor, MLCC, 1uF, 16V, X5R, +/-10%, 0603, T=0.8mm"                                                                      
C81        Capacitor                              BottomLayer C0402                                           22.9868      55.8801      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C83        Capacitor                              BottomLayer C0603                                           21.0818      53.3403      90       "Capacitor, MLCC, 1uF, 16V, X5R, +/-10%, 0603, T=0.8mm"                                                                      
C82        Capacitor                              BottomLayer C0402                                           22.2248      53.2134      90       "Capacitor, MLCC, 10nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                     
C69        Capacitor                              BottomLayer C0603                                           35.3146      60.6981      0        "Capacitor, MLCC, 4.7uF, 25V, X5R, +/-10%, 0603, T=0.8mm"                                                                    
C65        Capacitor                              BottomLayer C0402                                           38.7348      58.8781      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C66        Capacitor                              BottomLayer C0402                                           36.8300      46.1013      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C73        Capacitor                              BottomLayer C0402                                           30.4798      46.1013      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C77        Capacitor                              BottomLayer C0402                                           25.6149      60.5711      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C70        Capacitor                              BottomLayer C0402                                           32.8148      60.5711      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C78        Capacitor                              BottomLayer C0402                                           24.2568      53.8484      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C79        Capacitor                              BottomLayer C0402                                           24.1298      47.1173      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C64        Capacitor                              BottomLayer C0402                                           38.7348      52.4781      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C11        Capacitor                              TopLayer    C0402                                           19.9459      13.2923      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C75        Capacitor                              BottomLayer C0603_H0P8                                      28.0668      50.4383      0        "Capacitor, MLCC, 2.2nF, 50V, C0G/NPO, +/-5%, 0603, T=0,8mm"                                                                 
C37        Capacitor                              TopLayer    C0402                                           52.7048      9.9060       0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C68        Capacitor                              BottomLayer C0603_H0P8                                      35.3708      50.5460      0        "Capacitor, MLCC, 2.2nF, 50V, C0G/NPO, +/-5%, 0603, T=0,8mm"                                                                 
C28        Capacitor                              TopLayer    C0402                                           32.0037      71.1201      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C71        Capacitor                              BottomLayer C0603_H0P8                                      31.7106      50.5277      0        "Capacitor, MLCC, 2.2nF, 50V, C0G/NPO, +/-5%, 0603, T=0,8mm"                                                                 
C29        Capacitor                              TopLayer    C0402                                           33.4447      67.2158      0        "Capacitor, MLCC, 5.6pF, 50V, NPO, +/-0.1pF, 0402, T=0.5mm"                                                                  
C31        Capacitor                              TopLayer    C0402                                           35.3497      67.2158      180      "Capacitor, MLCC, 5.6pF, 50V, NPO, +/-0.1pF, 0402, T=0.5mm"                                                                  
C25        Capacitor                              TopLayer    C0603_H0P8                                      30.3487      38.2151      90       "Capacitor, MLCC, 2.2nF, 50V, C0G/NPO, +/-5%, 0603, T=0,8mm"                                                                 
C26        Capacitor                              TopLayer    C0402                                           30.4767      31.1075      90       "Capacitor, MLCC, 1nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                      
C30        Capacitor                              TopLayer    C0402                                           35.3058      9.9060       0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C21        Capacitor                              TopLayer    C0603_H0P8                                      26.2816      38.2702      90       "Capacitor, MLCC, 2.2nF, 50V, C0G/NPO, +/-5%, 0603, T=0,8mm"                                                                 
C22        Capacitor                              TopLayer    C0402                                           26.4127      31.2345      90       "Capacitor, MLCC, 1nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                      
C17        Capacitor                              TopLayer    C0603_H0P8                                      22.6060      38.2582      90       "Capacitor, MLCC, 2.2nF, 50V, C0G/NPO, +/-5%, 0603, T=0,8mm"                                                                 
C7         Capacitor                              TopLayer    C0402                                           15.7447      42.9185      270      "Capacitor, MLCC, 1nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                      
C85        Capacitor                              BottomLayer C0402                                           18.1608      52.5781      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
B1         SW_PUSH_SMD                            TopLayer    SWI_WEALTHMETAL_TD-0341_4P_BLACK                60.0198      7.5841       90       "Push Button, NC, 0.1A, 24V, Black"                                                                                          
B2         SW_PUSH_SMD                            TopLayer    SWI_WEALTHMETAL_TD-0341_4P_BLUE                 42.5449      7.6201       90       "Push Button, NC, 0.1A, 24V, Blue"                                                                                           
C86        Capacitor                              TopLayer    C0402                                           7.7438       40.7594      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                    
C87        Capacitor                              TopLayer    C0402                                           53.5907      94.4804      90       "Capacitor, MLCC, 10nF, 50V, X7R, +/-10%, 0402, T=0.5mm"                                                                     
D5         SCHOTTKY_1A_2K                         TopLayer    DIO_SOD323_1A_2K                                33.7788      90.5434      0        "Signal Schottky Diode, If=1A, Ifsm=5A, Vf =0.54V@1A, Vrrm=23V, Ir = 0.65µA@5V, SOD-323"                                     
LNK1       link_200                               TopLayer    LINK200                                         69.6944      77.2338      270      "Track link on PCB 200um width for layout routing."                                                                          
R74        Resistor                               TopLayer    R0402                                           7.7438       44.1884      180      "Resistor, 0R, 0402, +/-5%, 1/16W"                                                                                           
R75        Resistor                               TopLayer    R0402                                           12.6968      44.1884      0        "Resistor, 0R, 0402, +/-5%, 1/16W"                                                                                           
R76        Resistor                               TopLayer    R0402                                           12.8237      37.4574      90       "Resistor, 0R, 0402, +/-5%, 1/16W"                                                                                           
R77        Resistor                               TopLayer    R0402                                           11.0458      35.9334      180      "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                                          
R78        Resistor                               TopLayer    R0402                                           14.4747      42.9184      270      "Resistor, 30K, 0402, +/-0.1%, 1/16W, +/-25ppm/°C"                                                                           
R79        Resistor                               TopLayer    R0402                                           19.6817      42.9184      270      "Resistor, 30K, 0402, +/-0.1%, 1/16W, +/-25ppm/°C"                                                                           
R80        Resistor                               TopLayer    R0402                                           23.2378      31.9964      0        "Resistor, 30K, 0402, +/-0.1%, 1/16W, +/-25ppm/°C"                                                                           
R81        Resistor                               TopLayer    R0402                                           26.9208      32.7584      180      "Resistor, 30K, 0402, +/-0.1%, 1/16W, +/-25ppm/°C"                                                                           
R82        Resistor                               TopLayer    R0402                                           28.9528      29.7104      180      "Resistor, 30K, 0402, +/-0.1%, 1/16W, +/-25ppm/°C"                                                                           
R83        Resistor                               TopLayer    R0402                                           30.9848      32.6314      180      "Resistor, 30K, 0402, +/-0.1%, 1/16W, +/-25ppm/°C"                                                                           
R84        Resistor                               TopLayer    R0402                                           53.4637      98.4174      270      "Resistor, 1K3, 0402, +/-1%, 1/16W"                                                                                          
R85        Resistor                               TopLayer    R0402                                           59.0517      90.9244      90       "Resistor, 33R, 0402, +/-1%, 1/16W"                                                                                          
R86        Resistor                               TopLayer    R0402                                           54.8607      99.3064      90       "Resistor, 3K9, 0402, +/-1%, 1/16W, +/-100ppm/°C"                                                                            
R87        Resistor                               TopLayer    R0402                                           54.6067      94.4804      90       "Resistor, 100K, 0402, +/-1%, 1/16W"                                                                                         
R88        Resistor                               TopLayer    R0402                                           72.0057      94.7344      270      "Resistor, 1K, 0402, +/-0.1%, 1/16W, +/-25ppm/°C"                                                                            
R89        Resistor                               TopLayer    R0402                                           70.4817      94.7344      270      "Resistor, 330R, 0402, +/-1%, 1/16W"                                                                                         
R90        Resistor                               TopLayer    R0402                                           60.4487      90.9244      90       "Resistor, 100R, 0402, +/- 1%, 1/16W"                                                                                        
R91        Resistor                               BottomLayer R0402                                           31.1117      48.8874      90       "Resistor, 0R, 0402, +/-5%, 1/16W"                                                                                           
R92        Resistor                               BottomLayer R0402                                           34.7947      48.8874      90       "Resistor, 0R, 0402, +/-5%, 1/16W"                                                                                           
R93        Resistor                               BottomLayer R0402                                           27.3017      48.8874      90       "Resistor, 0R, 0402, +/-5%, 1/16W"                                                                                           
R94        Resistor                               BottomLayer R0402                                           19.4277      65.5244      270      "Resistor, 0R, 0402, +/-5%, 1/16W"                                                                                           
R95        Resistor                               TopLayer    R0402                                           16.5067      65.2704      270      "Resistor, 0R, 0402, +/-5%, 1/16W"                                                                                           
R96        Resistor                               TopLayer    R0402                                           25.2697      71.8744      270      "Resistor, 0R, 0402, +/-5%, 1/16W"                                                                                           
R97        Resistor                               BottomLayer R0402                                           31.1118      57.7774      0        "Resistor, 0R, 0402, +/-5%, 1/16W"                                                                                           
R98        Resistor                               BottomLayer R0402                                           34.7948      57.7774      0        "Resistor, 0R, 0402, +/-5%, 1/16W"                                                                                           
R99        Resistor                               BottomLayer R0402                                           27.5558      57.7774      0        "Resistor, 0R, 0402, +/-5%, 1/16W"                                                                                           
TP43       "Test Point"                           TopLayer    TP_SMD_1MM                                      60.8297      92.7024      90       "Test Point 1mm"                                                                                                             
