Altium Designer Pick and Place Locations
C:\Subversion\__Boards\MB1845-MiniBoard-WBA54-QFN48-LDO-SMA\Trunk\02-Manufacturing\MB1845A_PCB\Assembly\MB1845A_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       06/03/25
Time:       10:10
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator Comment                     Layer       Footprint                        Center-X(mm) Center-Y(mm) Rotation Description                                                                   
HW1        "RF Shield (22.2x19.2x2mm)" TopLayer    SHIELD_RF_ST-CUSTOM_22P2X19P2_H2 -275.4530    -237.3752    0        "RF Shield (22.2x19.2x2mm)"                                                   
CN4        SMA-J-P-H-ST-EM1            TopLayer    CON_SMA-RF_CINCH_142-0701-851    17.8540      44.1100      0        "Jack_SMA, VR, PCB edge, 50R, T=7.92mm"                                       
L1         Inductor                    TopLayer    C0402                            17.8541      36.1064      90       "Inductor, 3.3nH, +/-0.3nH, 800 mA, 0.125Ohm, 0402, T=0.5mm"                  
L2         Inductor                    TopLayer    C0402                            17.8536      38.7858      90       "Inductor, 3.3nH, +/-0.3nH, 800 mA, 0.125Ohm, 0402, T=0.5mm"                  
SB4        SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           10.1636      17.1072      180      "Solder Bridge 0402 OFF"                                                      
SB3        SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           10.7817      24.2954      180      "Solder Bridge 0402 OFF"                                                      
SB2        SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           10.7263      33.8458      180      "Solder Bridge 0402 OFF"                                                      
CN3        "Header 7x2"                TopLayer    CON_SAMTEC_FTSH-107-01-L-DV-K-A  22.1014      4.5794       0        "Header, 7x2, 1.27mm, VR, T=5.97mm, FTSH series STDC14 without Alignment Pin" 
CN2        FTSH-125-02-L-DV            BottomLayer FTSH-125-02-L-DV                 38.6564      18.5484      180      "Header, 25x2, 12.7mm, VR, SMD, T=4.83mm"                                     
CN1        FTSH-125-02-L-DV            BottomLayer FTSH-125-02-L-DV                 4.3664       18.5484      180      "Header, 25x2, 12.7mm, VR, SMD, T=4.83mm"                                     
U1         STM32WBA52CGU6              TopLayer    ICC_UFQFPN48-EPAD_7X7_H0P55_P050 21.8948      30.6081      90       "MCU,ARM Cortex M33,1MB Flash, 128KB SRAM, Crypto, RF 2.4GHz, BLE, 802.15.4"  
SB5        SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           32.4350      2.3430       0        "Solder Bridge 0402 OFF"                                                      
SB1        SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           10.8552      22.3294      180      "Solder Bridge 0402 OFF"                                                      
C19        Capacitor                   TopLayer    C0402                            16.0036      29.5706      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
C18        Capacitor                   TopLayer    C0402                            19.5456      36.2872      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
C17        Capacitor                   TopLayer    C0402                            27.4565      33.0519      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
C16        Capacitor                   TopLayer    C0402                            24.2807      25.3697      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
C15        Capacitor                   TopLayer    C0402                            15.9963      30.3425      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
C5         Capacitor                   BottomLayer C0402                            34.6782      2.8806       90       "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                       
C3         Capacitor                   BottomLayer C0402                            8.7818       24.1515      270      "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                       
C2         Capacitor                   BottomLayer C0402                            8.6490       34.2552      270      "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                       
C1         Capacitor                   BottomLayer C0402                            9.0496       21.8036      90       "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                       
X2         XTAL_4_PINS                 TopLayer    CRY_NX1612SA_4P                  15.0255      31.8549      0        "Crystal, 32MHz, 8pF, +/-10ppm, 40R, 1612(metric), T=0.3mm"                   
X1         XTAL_2_PINS                 TopLayer    CRY_NX1610SE_2P                  26.5812      29.5724      270      "Crystal, 32.768kHz, 6pF, +/-20ppm, 70KR, 1.6x1mm"                            
SC5        Shield-clip_S0951-46R       TopLayer    CLIP_HARWIN_S0951-46R            9.1846       31.0128      90       "shield clip Harwin S0951-46R to fix RF shielded cavity"                      
SC4        Shield-clip_S0951-46R       TopLayer    CLIP_HARWIN_S0951-46R            20.5020      20.7446      180      "shield clip Harwin S0951-46R to fix RF shielded cavity"                      
SC3        Shield-clip_S0951-46R       TopLayer    CLIP_HARWIN_S0951-46R            31.1821      29.9714      90       "shield clip Harwin S0951-46R to fix RF shielded cavity"                      
SC2        Shield-clip_S0951-46R       TopLayer    CLIP_HARWIN_S0951-46R            27.2220      39.7420      180      "shield clip Harwin S0951-46R to fix RF shielded cavity"                      
SC1        Shield-clip_S0951-46R       TopLayer    CLIP_HARWIN_S0951-46R            12.8619      39.7485      180      "shield clip Harwin S0951-46R to fix RF shielded cavity"                      
SB40       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           14.9361      32.1978      180      "Solder Bridge 0402 OFF"                                                      
SB39       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           13.0057      31.0294      180      "Solder Bridge 0402 OFF"                                                      
SB38       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           28.4237      28.5688      0        "Solder Bridge 0402 OFF"                                                      
SB37       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           28.5742      30.6123      0        "Solder Bridge 0402 OFF"                                                      
SB36       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           32.4336      17.9410      0        "Solder Bridge 0402 OFF"                                                      
SB35       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           32.3298      21.7226      180      "Solder Bridge 0402 OFF"                                                      
SB34       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.3773      5.5556       0        "Solder Bridge 0402 ON"                                                       
SB33       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.3394      24.8926      180      "Solder Bridge 0402 ON"                                                       
SB32       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           27.5819      18.8454      180      "Solder Bridge 0402 OFF"                                                      
SB31       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.4196      19.1987      0        "Solder Bridge 0402 ON"                                                       
SB30       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.4301      20.2392      0        "Solder Bridge 0402 ON"                                                       
SB29       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.4030      10.6745      0        "Solder Bridge 0402 ON"                                                       
SB28       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           29.9084      18.0754      0        "Solder Bridge 0402 OFF"                                                      
SB27       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           29.8222      17.0752      180      "Solder Bridge 0402 OFF"                                                      
SB26       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.3451      22.7312      180      "Solder Bridge 0402 ON"                                                       
SB25       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           10.8644      30.0218      180      "Solder Bridge 0402 OFF"                                                      
SB24       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.3126      15.1764      180      "Solder Bridge 0402 ON"                                                       
SB23       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.4425      16.9012      0        "Solder Bridge 0402 ON"                                                       
SB22       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           29.7783      13.9880      180      "Solder Bridge 0402 OFF"                                                      
SB21       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           16.4808      6.0397       90       "Solder Bridge 0402 ON"                                                       
SB20       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           32.3458      4.5574       180      "Solder Bridge 0402 OFF"                                                      
SB19       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           10.8876      9.3366       0        "Solder Bridge 0402 OFF"                                                      
SB18       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.4110      7.2742       0        "Solder Bridge 0402 ON"                                                       
SB17       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           10.9152      8.3810       0        "Solder Bridge 0402 ON"                                                       
SB16       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.4226      8.3714       0        "Solder Bridge 0402 ON"                                                       
SB15       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           10.9227      7.4127       0        "Solder Bridge 0402 OFF"                                                      
SB14       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.4020      11.8324      0        "Solder Bridge 0402 ON"                                                       
SB13       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           10.9353      5.2264       0        "Solder Bridge 0402 OFF"                                                      
SB12       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.3843      9.6978       0        "Solder Bridge 0402 ON"                                                       
SB11       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           10.9110      12.1766      0        "Solder Bridge 0402 ON"                                                       
SB10       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.3296      28.5138      180      "Solder Bridge 0402 ON"                                                       
SB9        SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           10.9123      6.2770       0        "Solder Bridge 0402 ON"                                                       
SB8        SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           23.4212      12.0213      90       "Solder Bridge 0402 OFF"                                                      
SB7        SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.4099      26.1234      0        "Solder Bridge 0402 ON"                                                       
R9         Resistor                    BottomLayer R0402                            27.0237      3.8997       270      Resistor,47R,0402,1%,1/16W                                                    
R8         Resistor                    BottomLayer R0402                            25.9224      9.8779       90       Resistor,47R,0402,1%,1/16W                                                    
R7         Resistor                    BottomLayer R0402                            24.6584      9.8529       90       Resistor,47R,0402,1%,1/16W                                                    
R6         Resistor                    BottomLayer R0402                            24.3864      2.6308       90       Resistor,47R,0402,1%,1/16W                                                    
R5         Resistor                    BottomLayer R0402                            23.3764      9.8779       90       Resistor,47R,0402,1%,1/16W                                                    
R4         Resistor                    BottomLayer R0402                            22.0924      9.8524       90       Resistor,47R,0402,1%,1/16W                                                    
R3         Resistor                    BottomLayer R0402                            20.8874      9.8779       90       Resistor,47R,0402,1%,1/16W                                                    
R2         Resistor                    BottomLayer R0402                            19.6054      9.8779       90       Resistor,47R,0402,1%,1/16W                                                    
R1         Resistor                    TopLayer    R0402                            11.3190      28.3121      270      "Resistor, 100K, 0402, +/-1%, 1/16W"                                          
L3         Inductor                    TopLayer    IND_0603_H0P8                    21.2405      22.6973      0        "Ferrite bead, 47R @ 100MHz, +/-25%, 3.5A, 0R02, 0603, T=0.8mm"               
HW4        STICKER_PRODUCT             TopLayer    STICKER_PRODUCT_25X5             -275.4530    -237.3752    90       "Sticker product 25x5 mm"                                                     
HW3        STICKER_BOARD               TopLayer    STICKER_BOARD_25X5               -275.4530    -237.3752    90       "Sticker board 25x5 mm"                                                       
D1         SCHOTTKY_1A_2K              TopLayer    DIO_SOD523_1A_2K                 15.3840      24.8690      180      "Small signal Schottky diodes"                                                
C22        Capacitor                   BottomLayer C0603                            20.2308      2.5544       90       "Capacitor, MLCC, 1uF, 16V, X5R, 10%, 0603, T=0,8mm"                          
C21        Capacitor                   TopLayer    C0603_H0P8                       15.6494      28.5453      0        "Capacitor, MLCC, 4.7uF, 10V, X5R, +/-10%, 0603, T=0.8mm"                     
C20        Capacitor                   TopLayer    C0402                            22.1470      24.9724      180      "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                       
C10        Capacitor                   TopLayer    C0402                            14.9505      33.0452      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
C14        Capacitor                   TopLayer    C0402                            17.4036      40.1420      0        "Capacitor, MLCC, 1pF, 50V, NPO, +/-0.1pF, 0402, T=0.5mm"                     
C13        Capacitor                   TopLayer    C0402                            17.4041      37.4304      0        "Capacitor, MLCC, 1.8pF, 50V, C0G, +/-0.25pF, 0402, T=0.5mm"                  
C12        Capacitor                   TopLayer    C0402                            17.4039      34.8350      0        "Capacitor, MLCC, 1.5pF, 50V, C0G, +/-0.25pF, 0402, T=0.5mm"                  
C11        Capacitor                   TopLayer    C0603                            15.8999      34.5656      270      "Capacitor, MLCC, 470nF, 16V, X7R, +/-10%, 0603, T=0.8mm"                     
C4         Capacitor                   BottomLayer C0402                            8.5040       16.5807      270      "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                       
C9         Capacitor                   TopLayer    C0402                            28.0274      30.1185      180      "6 pF ±0,25pF 50V Condensateurs céramique C0G, NP0 0402 (1005 métrique)"      
C8         Capacitor                   TopLayer    C0402                            27.9968      29.0214      180      "6 pF ±0,25pF 50V Condensateurs céramique C0G, NP0 0402 (1005 métrique)"      
C7         Capacitor                   TopLayer    C0402                            15.5471      23.8299      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
