Altium Designer Pick and Place Locations
C:\Subversion\Boards\MB1848-LP-STM32WL-QFN48-4Layers-IPD-RefBoard\Trunk\02-Manufacturing\MB1848_LPA_PCB\Assembly\MB1848_LPA_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       01/09/22
Time:       08:26
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator   Comment           Layer       Footprint                    Center-X(mm) Center-Y(mm) Rotation Description                                                                          
Designator16 Comment           TopLayer    IMPEDANCE_TABLE              -81.1966     -58.8083     0        ""                                                                                   
C200         MCD-00198         TopLayer    0201                         46.1575      16.8263      180      "Multilayer ceramic capacitors COG +/-5%, 50V"                                       
CN1          CON20             BottomLayer CO_SAMTEC_TSW-120-07-X-S     28.7330      31.1920      180      "Connector right-angle, pitch 2.54mm, 20 contacts"                                   
C38          ""                BottomLayer 0201                         37.1034      13.8317      0        "Multilayer Ceramic Capacitors MLCC - SMD/SMT 0201 33pF 25volts C0G 5%"              
SB15         Close             TopLayer    SB_0402                      41.8034      22.9917      90       "Solder Bridge 0R [0402] (Populated with 0 Ohm)"                                     
SB14         Open              BottomLayer SB_0402                      47.6780      25.7186      270      "Solder Bridge Open [0402] (Unpopulated)"                                            
SB13         Close             TopLayer    SB_0402                      43.3034      22.9917      90       "Solder Bridge 0R [0402] (Populated with 0 Ohm)"                                     
R101         Resistor          TopLayer    R0402                        45.6034      24.2417      90       Resistor,0R,0402,5%,1/16W                                                            
R100         Resistor          TopLayer    R0402                        46.8034      24.2417      90       Resistor,0R,0402,5%,1/16W                                                            
L9           ferrite           TopLayer    IND_MURATA_LQW15A            46.3834      26.9417      0        "Inductor, 3.9nH, +-0.1nH, 750mA, 0402"                                              
C37          ""                TopLayer    0402                         41.0665      26.9419      0        "Capacitor, MLCC, 33pF, 50V, NPO, 2%, 0402, T=0,5mm"                                 
C36          ""                TopLayer    0402                         46.2382      25.8415      180      "Capacitor, MLCC, 33pF, 50V, NPO, 2%, 0402, T=0,5mm"                                 
C2           ""                TopLayer    CAPC1005X06N                 43.9094      9.7301       90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                               
C3           ""                TopLayer    0201                         43.0034      10.7317      90       "Multilayer Ceramic Capacitors MLCC - SMD/SMT 0201 25VDC 0.1uF 10% X5R 0.3mm"        
C4           ""                BottomLayer CAPC1005X06N                 37.4429      15.0477      180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                               
C5           ""                TopLayer    0201                         36.6734      18.9817      270      "Multilayer Ceramic Capacitors MLCC - SMD/SMT 0201 25VDC 0.1uF 10% X5R 0.3mm"        
C6           ""                BottomLayer CAPC1608X09N                 31.3749      16.9775      180      "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                               
C7           ""                BottomLayer CAPC1005X06N                 37.4099      16.4480      0        "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                               
C8           Capacitor         TopLayer    0402                         31.4182      22.1515      180      "Capacitor, MLCC, 6.8pF, 50V, NPO, +-0.1pF, 0402, T=0.5mm"                           
C9           Capacitor         TopLayer    0402                         31.4452      18.1715      180      "Capacitor, MLCC, 6.8pF, 50V, NPO, +-0.1pF, 0402, T=0.5mm"                           
C10          ""                BottomLayer CAPC1608X09N                 50.5990      26.8626      180      "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                               
C11          ""                BottomLayer CAPC1005X06N                 42.7234      18.8917      270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                               
C12          ""                TopLayer    0402                         49.3665      9.4919       0        "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                               
C14          ""                BottomLayer CAPC1608X09N                 38.7695      19.5220      270      "Capacitor, MLCC, 4.7 uF, 16V, X5R, 10%, 0603, T=0.8mm"                              
C15          ""                TopLayer    0402                         45.2029      20.0651      90       "Capacitor, MLCC,47nF, 16V, X7R, 10%, 0402, T=0.5mm"                                 
C26          Capacitor         TopLayer    0402                         44.4586      25.3145      270      "Capacitor, MLCC, 6.8pF, 50V, NPO, +-0.1pF, 0402, T=0.5mm"                           
C31          Capacitor         TopLayer    0402                         40.5212      25.2779      90       "Capacitor, MLCC, 6.8pF, 50V, NPO, +-0.1pF, 0402, T=0.5mm"                           
C33          ""                TopLayer    0201                         44.0564      19.5623      180      "Multilayer Ceramic Capacitors MLCC - SMD/SMT 0201 33pF 25volts C0G 5%"              
C34          ""                BottomLayer 0201                         40.8431      18.9331      90       "Multilayer Ceramic Capacitors MLCC - SMD/SMT 0201 33pF 25volts C0G 5%"              
C35          ""                BottomLayer CAPC1608X09N                 50.5271      5.5925       180      "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                               
L2           ""                BottomLayer INDC2012X13N                 34.8034      12.1117      0        "MLZ2012 Multilayer Shielded Inductor 15 uH, ±5%"                                    
L7           Ferrite           TopLayer    rlc_201_smd                  57.1620      15.9187      0        "Thick Film Resistor ±5%, 1/20W"                                                     
R1           ""                TopLayer    RESC1608X05N                 51.0159      10.7997      180      Resistor,10K,0603,1%,1/10W                                                           
U2           ""                TopLayer    DIOM0603X03N                 49.0034      8.5917       0        "ESD protection 6V1"                                                                 
U4           STM32WLxx_QFN48   TopLayer    STM32WLXX_QFN48              40.7006      15.0751      90       "STM32WL ARM MCU Multiprotocol LPWAN 32-bit Arm Cortex-M4 MCUs LoRa (G)FSK-MSK BPSK" 
X1           XTAL_2_PINS       TopLayer    OSC_NDK_NX2012SA             31.9984      20.1537      90       "Crystal 32.768kHz, 6pF, -+20PPM, R=80K, SMD"                                        
X2           ""                TopLayer    OSC_NDK_NX2016SA             42.5134      25.2947      180      "Crystal 32 MHz, 8pF, -+10 PPM, R=60O, SMD"                                          
C18          ""                TopLayer    0402                         46.3934      20.0651      270      "Capacitor, MLCC,68pF, 50V, C0G, 1%, 0402, T=0.5mm"                                  
SB11         Close             TopLayer    GC_0402                      48.9159      10.6607      180      "Solder Jumper - Close"                                                              
C1           ""                BottomLayer CAPC1608X09N                 50.5689      7.3317       180      "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                               
C110         ""                TopLayer    CAPC1005X06N                 35.6425      11.8640      270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                               
C23          MCD-00198         TopLayer    0201                         51.5515      17.1964      0        "Multilayer ceramic capacitors X7R ±10%, 50V"                                        
C39          ""                BottomLayer CAPC1005X06N                 36.8024      17.8482      0        "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                               
R2           MCD-00119         TopLayer    0201                         51.2617      12.7198      180      "Thick Film Resistors - SMD 1/20watt 100ohms 5% 200ppm"                              
C40          ""                BottomLayer CAPC1005X06N                 44.9297      20.7819      0        "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                               
L1           ""                BottomLayer INDC1608X95N                 30.7894      14.5292      90       "SMD Chip ferrite bead, 600R@100MHz +/-25%, 350mA, 500mohm DC, 0603, T=0.8mm"        
U3           BGS12SN6          TopLayer    TSNP-6-2                     51.4112      15.9187      0        "DC switch - Ultra-Low  SPDT analog switch"                                          
SB3          Close             TopLayer    0201                         50.1174      12.0339      0        "Thick Film Resistors - SMD 1/20watt ZEROohm Jumper"                                 
SB4          Open              TopLayer    0201                         50.1174      12.7182      0        "Solder Bridge Open [0402] (Unpopulated)"                                            
SB5          Open              TopLayer    0201                         51.2617      12.0355      180      "Solder Bridge Open [0402] (Unpopulated)"                                            
SB2          Open              BottomLayer SB_0402                      52.2179      28.3628      180      "Solder Bridge Open [0402] (Unpopulated)"                                            
C16          MCD-00102         TopLayer    0201                         50.9266      13.5153      0        "Multilayer ceramic capacitors X5R ±10%, 10V"                                        
C43          ""                TopLayer    CAPC1005X06N                 31.0713      13.8025      0        "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                               
C44          ""                TopLayer    0201                         33.8404      14.2225      0        "Multilayer Ceramic Capacitors MLCC - SMD/SMT 0201 25VDC 0.1uF 10% X5R 0.3mm"        
U1           "IPD STM STM32WL" TopLayer    IPD_STM                      47.7362      16.3183      180      "IPD STM STM32WL"                                                                    
L3           MCD-01330         TopLayer    IND_MURATA_LQW15A            45.0565      17.5200      270      "Inductor, 47nH, +-0.1nH, 140mA, 0402"                                               
C29          RFCapacitor_201   TopLayer    rlc_201_smd                  56.2400      15.6190      90       "RF Capacitor High-Q, 0201"                                                          
C28          RFCapacitor_201   TopLayer    rlc_201_smd                  58.0837      15.6190      90       "RF Capacitor High-Q, 0201"                                                          
J3           SMA               TopLayer    SMA_AMPHENOL_50ohms_Edge_PCB 61.3074      15.9455      90       "SMA Straight Connector"                                                             
C25          RFCapacitor_201   TopLayer    rlc_201_smd                  55.3362      15.9187      0        "Multilayer ceramic capacitors COG ±5%, 50V"                                         
C27          NC                TopLayer    0201                         48.4276      14.6210      90       "RF Capacitor High-Q, 0201"                                                          
C41          MCD-00102         TopLayer    0201                         51.5515      17.8817      180      "Multilayer ceramic capacitors X5R ±10%, 10V"                                        
R3           MCD-00119         TopLayer    0201                         51.5516      18.5659      180      "Thick Film Resistors - SMD 1/20watt 100ohms 5% 200ppm"                              
SB6          Close             TopLayer    0201                         51.0415      19.4797      270      "Thick Film Resistors - SMD 1/20watt ZEROohm Jumper"                                 
SB9          Open              TopLayer    0201                         51.8324      19.4797      270      "Solder Bridge Open [0402] (Unpopulated)"                                            
C13          MCD-00198         TopLayer    0201                         50.9266      14.1996      0        "Multilayer ceramic capacitors X7R ±10%, 50V"                                        
C42          ""                TopLayer    CAPC1608X09N                 34.2922      11.6321      270      "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                               
C17          ""                TopLayer    CAPC1005X06N                 39.8508      22.1345      180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                               
CN2          CON20             BottomLayer CO_SAMTEC_TSW-120-07-X-S     28.7330      3.1920       180      "Connector right-angle, pitch 2.54mm, 20 contacts"                                   
C19          RFCapacitor_201   TopLayer    rlc_201_smd                  49.3114      17.1583      180      "Multilayer ceramic capacitors COG ±5%, 50V"                                         
