Altium Designer Pick and Place Locations
C:\Users\tguilhot\Downloads\_SubVersion\MB1868-STM32WB1M-Tiny-Dory-Module_connectivity_expansion\02-Manufacturing\MB1868D_PCB\Assembly\MB1868D_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       17-07-23
Time:       10:17
Revision:   13
Variant:    No variations
Units used: mm

Designator  Comment              Layer       Footprint                                       Center-X(mm) Center-Y(mm) Rotation Description                                                                                                 
1           Comment              TopLayer    Sheetbox_2L2S                                   26.6436      -24.9984     0        ""                                                                                                          
Designator1 Comment              TopLayer    MIRECMS_(dia1.27-zi2.54)                        55.4500      3.8500       0        ""                                                                                                          
Designator1 Comment              BottomLayer MIRECMS_(dia1.27-zi2.54)                        55.4500      3.8500       180      ""                                                                                                          
R14         Resistor             TopLayer    R0201_H0P23                                     25.9500      2.9000       90       "Resistor, 15R, 0201, 1%, 1/20W"                                                                            
R13         Resistor             TopLayer    R0201_H0P23                                     25.7000      4.7500       0        "Resistor, 15R, 0201, 1%, 1/20W"                                                                            
R12         Resistor             TopLayer    R0201_H0P23                                     25.7000      3.9500       0        "Resistor, 15R, 0201, 1%, 1/20W"                                                                            
C18         Capacitor            TopLayer    C0201_H0P3                                      25.9500      1.6500       90       "Capacitor, MLCC, 2.7pF, 50V, NPO, +-0.05pF, 0201, T=0.3mm"."                                               
C17         Capacitor            TopLayer    C0201_H0P3                                      24.4000      4.7500       0        "Capacitor, MLCC, 2.7pF, 50V, NPO, +-0.05pF, 0201, T=0.3mm"."                                               
C16         Capacitor            TopLayer    C0201_H0P3                                      24.4000      3.9500       0        "Capacitor, MLCC, 2.7pF, 50V, NPO, +-0.05pF, 0201, T=0.3mm"."                                               
R11         Resistor             TopLayer    R0402                                           50.9749      12.8000      45       "Resistor, 0R, 0402, +/-1%, 1/16W"                                                                          
SB12        SB_ON                BottomLayer SOLDER-BRIDGE_R0402-0R                          10.7725      8.1250       180      "Solder Bridge 0402 ON"                                                                                     
C7          Capacitor            TopLayer    C0402                                           50.3750      11.3000      315      "Capacitor, MLCC, 22pF, 50V, C0G, +/-5%, 0402, T=0.5mm"                                                     
C6          Capacitor            TopLayer    C0402                                           52.4750      13.4000      315      "Capacitor, MLCC, 22pF, 50V, C0G, +/-5%, 0402, T=0.5mm"                                                     
SB18        SB_ON                BottomLayer SOLDER-BRIDGE_R0402-0R                          6.7225       28.0230      180      "Solder Bridge 0402 ON"                                                                                     
SB17        SB_ON                BottomLayer SOLDER-BRIDGE_R0402-0R                          10.5475      18.4750      180      "Solder Bridge 0402 ON"                                                                                     
SB9         SB_OFF               BottomLayer SOLDER-BRIDGE_R0402-0R                          6.7225       16.7001      180      "Solder Bridge 0402 OFF"                                                                                    
SB6         SB_OFF               BottomLayer SOLDER-BRIDGE_R0402-0R                          6.7225       19.0500      180      "Solder Bridge 0402 OFF"                                                                                    
SB7         SB_OFF               BottomLayer SOLDER-BRIDGE_R0402-0R                          6.7275       21.3617      0        "Solder Bridge 0402 OFF"                                                                                    
SB3         SB_OFF               BottomLayer SOLDER-BRIDGE_R0402-0R                          6.7225       26.3250      180      "Solder Bridge 0402 OFF"                                                                                    
SB1         SB_OFF               BottomLayer SOLDER-BRIDGE_R0402-0R                          6.7225       23.8327      180      "Solder Bridge 0402 OFF"                                                                                    
SB16        SB_OFF               BottomLayer SOLDER-BRIDGE_R0402-0R                          15.2000      14.5775      90       "Solder Bridge 0402 OFF"                                                                                    
SB14        SB_OFF               BottomLayer SOLDER-BRIDGE_R0402-0R                          19.6250      14.5726      270      "Solder Bridge 0402 OFF"                                                                                    
SB15        SB_ON                BottomLayer SOLDER-BRIDGE_R0402-0R                          16.6250      14.5726      270      "Solder Bridge 0402 ON"                                                                                     
SB13        SB_ON                BottomLayer SOLDER-BRIDGE_R0402-0R                          18.2500      14.5726      270      "Solder Bridge 0402 ON"                                                                                     
C5          Capacitor            TopLayer    C0402                                           17.1250      13.1500      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                   
SB11        SB_ON                BottomLayer SOLDER-BRIDGE_R0402-0R                          10.6850      10.1750      180      "Solder Bridge 0402 ON"                                                                                     
SB5         SB_ON                BottomLayer SOLDER-BRIDGE_R0402-0R                          6.7181       20.2500      0        "Solder Bridge 0402 ON"                                                                                     
SB21        SB_ON                BottomLayer SOLDER-BRIDGE_R0402-0R                          42.1867      21.0721      0        "Solder Bridge 0402 ON"                                                                                     
R2          Resistor             TopLayer    R0201_H0P23                                     33.5000      3.9250       270      "Resistor, 0R, 0201, 1/20W"                                                                                 
SB19        SB_ON                BottomLayer SOLDER-BRIDGE_R0402-0R                          42.1817      18.0221      180      "Solder Bridge 0402 ON"                                                                                     
CN5         ""                   TopLayer    CON_SAMTEC_TSW-102-07-G-S                       31.8592      25.4985      270      "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm - Shunt Fitted by default"                               
R9          ""                   TopLayer    R0402                                           28.3750      26.9750      90       Resistor,100R,0402,1%,1/16W                                                                                 
CN3         "Header 7x2"         TopLayer    CON_STDC14_Receiver_SMALL                       22.1400      23.3680      180      "Header, 7x2, 1.27mm, VR, SMD, T=5.97mm"                                                                    
U7          ""                   TopLayer    ESD_SOT323-5L                                   23.9500      17.0250      180      "Dual Transil array for ESD protection"                                                                     
U2          ISM330DHCX           TopLayer    ICC_LGA14_3X2P5_P050                            11.9001      16.1500      0        "iNEMO inertial module: 3D accelerometer and 3D gyroscope, with digital output for industrial applications" 
U1          STTS22H              TopLayer    ICC_UDFN6-EPAD_2X2_P065                         34.6342      18.8872      180      "temperature sensor"                                                                                        
SB10        SB_ON                BottomLayer SOLDER-BRIDGE_R0402-0R                          6.7225       15.5500      180      "Solder Bridge 0402 ON"                                                                                     
SB8         SB_ON                BottomLayer SOLDER-BRIDGE_R0402-0R                          6.7225       17.9000      180      "Solder Bridge 0402 ON"                                                                                     
SB4         SB_ON                BottomLayer SOLDER-BRIDGE_R0402-0R                          6.7225       24.9923      180      "Solder Bridge 0402 ON"                                                                                     
SB2         SB_ON                BottomLayer SOLDER-BRIDGE_R0402-0R                          6.7225       22.5000      180      "Solder Bridge 0402 ON"                                                                                     
R6          Resistor             TopLayer    R0402                                           20.6000      11.7001      180      "Resistor, 2K2, 0402, +/-1%, 1/16W"                                                                         
R5          Resistor             TopLayer    R0402                                           20.6000      10.6000      180      "Resistor, 2K2, 0402, +/-1%, 1/16W"                                                                         
CN4         ""                   TopLayer    CON_SAMTEC_TSW-102-07-G-S                       35.4842      25.4985      270      "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm - Shunt Fitted by default"                               
C1          Capacitor            TopLayer    C0402                                           9.2551       16.3450      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                   
C2          Capacitor            TopLayer    C0402                                           14.9501      16.4500      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                   
C4          Capacitor            TopLayer    C0402                                           30.7842      19.7372      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                   
B2          ""                   TopLayer    SWI_C&K_Y78B23110FP__ITT_KMR231GLFS             41.1592      26.2971      180      "Microminiature Tact Switch for SMT - KMR 2 Series - 1.9 mm height"                                         
B1          ""                   TopLayer    SWI_C&K_Y78B23110FP__ITT_KMR231GLFS             11.4250      26.1500      180      "Microminiature Tact Switch for SMT - KMR 2 Series - 1.9 mm height"                                         
C11         Capacitor            TopLayer    C0402                                           39.5592      23.4182      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                   
C10         Capacitor            TopLayer    C0402                                           9.8500       22.7000      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                   
C13         ""                   TopLayer    C0402                                           49.5093      19.7471      0        "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                                                      
C12         ""                   TopLayer    C0603                                           51.3500      20.4000      270      "Capacitor, MLCC, 1uF, 16V, X5R, 10%, 0603, T=0,8mm"                                                        
C14         ""                   TopLayer    C0603                                           46.4593      16.7971      270      "Capacitor, MLCC, 1uF, 16V, X5R, 10%, 0603, T=0,8mm"                                                        
C15         ""                   TopLayer    C0402                                           45.1843      16.5471      270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                                                      
C9          Capacitor            TopLayer    C0402                                           34.0651      10.7900      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                   
C8          ""                   TopLayer    C0603                                           34.3901      11.9150      180      "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                                                      
CN1         "Header 10x2 STMod+" TopLayer    CON_SAMTEC_TMM-110-01-L-D-RA__STMOD+            2.2700       15.0000      270      "Header 10x2, 2mm, RA, TH, Height 3.20mm/3.50mm"                                                            
CN2         ""                   TopLayer    CON_SAMTEC_SMA-J-P-X-ST-EM1                     57.5500      15.0000      90       "RF SMA connector PCB edge"                                                                                 
JP1         ""                   TopLayer    CON_SAMTEC_TSW-102-07-G-S                       49.4092      25.4571      90       "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm - Shunt Fitted by default"                               
LD2         ""                   TopLayer    LED_0603_OSRAM_LG-Q396-PS-35_GREEN_1A2K_H0P4    43.2092      19.8282      180      "LED Green, 0603 SMD, Forward Voltage Typ=2V, Max=2.5V"                                                     
LD1         ""                   TopLayer    LED_0603_OSRAM_LB-Q39G-L2OO-35-1_BLUE_1A2K_H0P4 46.4092      26.4721      90       "LED Blue, 0603 SMD, Forward Voltage Min=2,8V, Max=3,8V"                                                    
R10         ""                   TopLayer    R0402                                           44.4304      21.0721      180      Resistor,620R,0402,1%,1/16W                                                                                 
R8          ""                   TopLayer    R0402                                           13.4750      23.5500      270      Resistor,1K,0402,1%,1/16W                                                                                   
R4          ""                   TopLayer    R0402                                           31.8250      11.8750      180      Resistor,120R,0402,1%,1/16W                                                                                 
R3          Resistor             TopLayer    R0201_H0P23                                     33.8000      4.2250       180      "Resistor, 0R, 0201, +/-1%, 1/20W"                                                                          
R1          Resistor             TopLayer    R0201_H0P23                                     33.5000      3.3250       270      "Resistor, 0R, 0201, +/-1%, 1/20W"                                                                          
R7          ""                   TopLayer    R0402                                           46.4062      24.2721      90       Resistor,120R,0402,1%,1/16W                                                                                 
SB20        SB_OFF               BottomLayer SOLDER-BRIDGE_R0402-0R                          42.1867      19.5471      0        "Solder Bridge 0402 OFF"                                                                                    
U5          ""                   TopLayer    ESD_ST0201                                      9.7125       23.7000      0        "ESD protection 6V1"                                                                                        
U6          ""                   TopLayer    ESD_ST0201                                      39.4092      24.2932      0        "ESD protection 6V1"                                                                                        
U8          ""                   TopLayer    ICC_DFN6-EPAD_3X3_P095                          49.0343      17.3971      180      "Low quiescent current and low noise voltage regulators"                                                    
U4          STM32WB1M            TopLayer    ICC_LBA77_6P5X10_P0P45                          29.7500      5.1375       180      "STM32 BLE module based on STM32WB15"                                                                       
C3          Capacitor            TopLayer    C0402                                           29.8342      19.7372      90       "Capacitor, MLCC, 2.2uF, 6V3, X5R,+/-10%, 0402, T=0.5mm"                                                    
U3          M24128-DFMC6TP       TopLayer    ICC_DFN8-EPAD_2X3_P050                          16.8250      11.3500      90       "I2C Memory 3V3, 256Kbits, 2x3,0.55mm, UFDFPN8"                                                             
