Altium Designer Pick and Place Locations
C:\Subversion\Boards\MB1874-LP-STM32WL-QFN48-2Layers-IPD-RefBoard\Trunk\02-Manufacturing\MB1874_LPA_PCB\Assembly\MB1874_LPA_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       01/09/22
Time:       08:47
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator   Comment           Layer       Footprint                    Center-X(mm) Center-Y(mm) Rotation Description                                                                          
Designator16 Comment           TopLayer    IMPEDANCE_TABLE              -961.3329    -287.3863    0        ""                                                                                   
U1           "IPD STM STM32WL" TopLayer    IPD_STM                      33.7878      16.3539      180      "IPD STM STM32WL"                                                                    
C200         MCD-00198         TopLayer    0201                         32.2228      16.8566      180      "Multilayer ceramic capacitors COG +/-5%, 50V"                                       
CN2          CON20             BottomLayer CO_SAMTEC_TSW-120-07-X-S     29.1296      3.2000       180      "Connector right-angle, pitch 2.54mm, 20 contacts"                                   
CN1          CON20             BottomLayer CO_SAMTEC_TSW-120-07-X-S     29.1296      31.2000      180      "Connector right-angle, pitch 2.54mm, 20 contacts"                                   
C38          ""                BottomLayer 0201                         22.4996      13.8400      0        "Multilayer Ceramic Capacitors MLCC - SMD/SMT 0201 33pF 25volts C0G 5%"              
SB15         Close             TopLayer    SB_0402                      27.1996      23.2500      90       "Solder Bridge 0R [0402] (Populated with 0 Ohm)"                                     
SB14         Open              BottomLayer SB_0402                      34.3410      27.2094      0        "Solder Bridge Open [0402] (Unpopulated)"                                            
SB13         Close             TopLayer    SB_0402                      28.6996      23.2500      90       "Solder Bridge 0R [0402] (Populated with 0 Ohm)"                                     
R101         Resistor          TopLayer    R0402                        31.4410      24.5093      90       Resistor,0R,0402,5%,1/16W                                                            
R100         Resistor          TopLayer    R0402                        32.6410      24.5093      90       Resistor,0R,0402,5%,1/16W                                                            
L9           ferrite           TopLayer    IND_MURATA_LQW15A            31.9296      27.2500      0        "Inductor, 3.9nH, +-0.1nH, 750mA, 0402"                                              
C37          ""                TopLayer    0402                         26.4628      27.2002      0        "Capacitor, MLCC, 33pF, 50V, NPO, 2%, 0402, T=0,5mm"                                 
C36          ""                TopLayer    0402                         32.0844      26.0998      180      "Capacitor, MLCC, 33pF, 50V, NPO, 2%, 0402, T=0,5mm"                                 
C2           ""                TopLayer    CAPC1005X06N                 29.3910      9.1593       90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                               
C3           ""                TopLayer    0201                         28.3910      10.4993      90       "Multilayer Ceramic Capacitors MLCC - SMD/SMT 0201 25VDC 0.1uF 10% X5R 0.3mm"        
C4           ""                BottomLayer CAPC1005X06N                 22.6910      15.0594      180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                               
C5           ""                BottomLayer 0201                         22.7939      18.8983      180      "Multilayer Ceramic Capacitors MLCC - SMD/SMT 0201 25VDC 0.1uF 10% X5R 0.3mm"        
C6           ""                BottomLayer CAPC1608X09N                 16.7711      16.9858      180      "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                               
C7           ""                BottomLayer CAPC1005X06N                 22.5660      16.5593      0        "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                               
C8           Capacitor         TopLayer    0402                         16.8071      22.2727      180      "Capacitor, MLCC, 6.8pF, 50V, NPO, +-0.1pF, 0402, T=0.5mm"                           
C9           Capacitor         TopLayer    0402                         16.8414      18.0298      180      "Capacitor, MLCC, 6.8pF, 50V, NPO, +-0.1pF, 0402, T=0.5mm"                           
C10          ""                BottomLayer CAPC1608X09N                 50.9488      28.8548      0        "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                               
C11          ""                BottomLayer CAPC1005X06N                 28.1196      18.9000      270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                               
C12          ""                TopLayer    0402                         34.7628      9.6502       0        "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                               
C14          ""                BottomLayer CAPC1608X09N                 24.1910      19.5093      270      "Capacitor, MLCC, 0.47 uF, 16V, X5R, 10%, 0603, T=0.8mm"                             
C15          ""                TopLayer    0402                         30.4868      19.9069      90       "Capacitor, MLCC,47nF, 25V, X7R, 10%, 0402, T=0.5mm"                                 
C26          Capacitor         TopLayer    0402                         30.2048      25.5728      270      "Capacitor, MLCC, 6.8pF, 50V, NPO, +-0.1pF, 0402, T=0.5mm"                           
C27          NC                TopLayer    0402_2                       34.4642      13.7119      90       "Not connected [0402]"                                                               
C31          Capacitor         TopLayer    0402                         25.9174      25.3362      90       "Capacitor, MLCC, 6.8pF, 50V, NPO, +-0.1pF, 0402, T=0.5mm"                           
C32          ""                BottomLayer 0201                         23.0333      12.5232      180      "Multilayer Ceramic Capacitors MLCC - SMD/SMT 0201 33pF 25volts C0G 5%"              
C33          ""                TopLayer    0201                         29.0099      19.7916      270      "Multilayer Ceramic Capacitors MLCC - SMD/SMT 0201 33pF 25volts C0G 5%"              
C34          ""                BottomLayer 0201                         26.2393      18.8414      90       "Multilayer Ceramic Capacitors MLCC - SMD/SMT 0201 33pF 25volts C0G 5%"              
C35          ""                BottomLayer CAPC1608X09N                 50.9234      5.6008       180      "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                               
J4           SMA_T_9.52_NF     TopLayer    SMA_AMPHENOL_50ohms_Edge_PCB 57.1387      16.2607      90       "SMA Jack, Edge Mount, 50 Ohms"                                                      
L2           ""                BottomLayer INDC2012X13N                 20.0410      12.1094      0        "MLZ2012 Multilayer Shielded Inductor 15 uH, ±5%"                                    
L3           ""                TopLayer    0402_COIL                    31.0368      17.5730      270      "Inductor, 68nH, +-0.1nH, 140mA, 0402"                                               
L7           ""                TopLayer    0402_COIL                    50.0789      16.3093      0        "Inductor, 15nH, +-0.1nH, 640mA, 0402"                                               
R1           ""                TopLayer    RESC1608X05N                 36.7410      11.0673      180      Resistor,10K,0603,1%,1/10W                                                           
U2           ""                TopLayer    DIOM0603X03N                 34.3996      8.6000       0        "ESD protection 6V1"                                                                 
U4           STM32WLxx_QFN48   TopLayer    STM32WLXX_QFN48              26.0968      15.0834      90       "STM32WL ARM MCU Multiprotocol LPWAN 32-bit Arm Cortex-M4 MCUs LoRa (G)FSK-MSK BPSK" 
X1           XTAL_2_PINS       TopLayer    OSC_NDK_NX2012SA             17.3946      20.1620      90       "Crystal 32.768kHz, 6pF, -+20PPM, R=80K, SMD"                                        
X2           ""                TopLayer    OSC_NDK_NX2016SA             27.9096      25.5530      180      "Crystal 32 MHz, 8pF, -+10 PPM, R=60O, SMD"                                          
C18          ""                TopLayer    0402                         31.6721      19.9159      270      "Capacitor, MLCC,68pF, 50V, C0G, 1%, 0402, T=0.5mm"                                  
SB11         Close             TopLayer    GC_0402                      34.3121      10.9190      180      "Solder Jumper - Close"                                                              
C1           ""                BottomLayer CAPC1608X09N                 26.9982      10.3107      270      "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                               
C110         ""                TopLayer    CAPC1005X06N                 20.5609      11.7877      270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                               
C13          ""                TopLayer    CAPC1005X06N                 42.4690      12.3265      90       "Capacitor, MLCC, 1nF, 16V, X7R, 10%, 0402, T=0.5mm"                                 
C23          ""                TopLayer    CAPC1005X06N                 44.8927      20.2931      180      "Capacitor, MLCC, 1nF, 16V, X7R, 10%, 0402, T=0.5mm"                                 
C25          ""                TopLayer    0402_2                       46.3977      16.3093      0        "Multilayer Ceramic Capacitors MLCC - SMD/SMT 0402 68pF 50volts C0G 5%"              
C29          MCD-00102         TopLayer    0402                         48.2259      15.7112      270      "Condensateurs céramique multicouches MLCC - CMS 0402 3.3pF 50Volts C0G +/-0.05pF"   
C39          ""                BottomLayer CAPC1005X06N                 22.1910      17.7593      0        "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                               
R2           ""                TopLayer    RESC1005X04N                 44.7204      13.1375      0        Resistor,100R,0402,1%,1/16W                                                          
R3           ""                TopLayer    RESC1005X04N                 44.3979      22.0434      90       Resistor,100R,0402,1%,1/16W                                                          
C40          ""                BottomLayer CAPC1005X06N                 29.9867      20.7559      0        "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                               
C42          ""                BottomLayer CAPC1608X09N                 23.9036      22.7610      90       "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                               
L1           ""                BottomLayer INDC1608X95N                 16.1910      14.6594      90       "SMD Chip ferrite bead, 600R@100MHz +/-25%, 350mA, 500mohm DC, 0603, T=0.8mm"        
U3           BGS12SN6          TopLayer    SON40P70X40-6N               43.8843      16.3093      0        "DC switch - Ultra-Low  SPDT analog switch"                                          
SB3          Close             TopLayer    SB_0402                      44.6883      11.7373      0        "Solder Bridge 0R [0402] (Populated with 0 Ohm)"                                     
SB4          Open              TopLayer    SB_0402                      44.6883      10.3370      0        "Solder Bridge Open [0402] (Unpopulated)"                                            
SB5          Open              TopLayer    SB_0402                      44.6883      8.9232       0        "Solder Bridge Open [0402] (Unpopulated)"                                            
SB6          Close             TopLayer    SB_0402                      43.9605      23.7936      0        "Solder Bridge 0R [0402] (Populated with 0 Ohm)"                                     
SB9          Open              TopLayer    SB_0402                      43.9605      25.1939      0        "Solder Bridge Open [0402] (Unpopulated)"                                            
SB2          Open              TopLayer    SB_0402                      17.0754      11.5615      180      "Solder Bridge Open [0402] (Unpopulated)"                                            
C16          ""                TopLayer    CAPC1005X06N                 44.7419      14.5373      180      "Capacitor, MLCC, 10 pF"                                                             
C41          ""                TopLayer    CAPC1005X06N                 44.8778      18.8929      0        "Capacitor, MLCC, 10 pF"                                                             
C43          ""                TopLayer    CAPC1005X06N                 16.4675      13.8108      0        "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                               
C44          ""                TopLayer    0201                         19.2366      14.2308      0        "Multilayer Ceramic Capacitors MLCC - SMD/SMT 0201 25VDC 0.1uF 10% X5R 0.3mm"        
SB12         Close             BottomLayer GC_0402                      48.2163      28.5934      270      "Solder Jumper - Open"                                                               
C45          ""                TopLayer    CAPC1608X09N                 19.2107      11.7237      270      "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                               
C28          MCD-00102         TopLayer    0402                         51.9797      15.6963      270      "Condensateurs céramique multicouches MLCC - CMS 0402 3.3pF 50Volts C0G +/-0.05pF"   
SB10         Close             BottomLayer GC_0402                      44.1955      29.0048      0        "Solder Jumper - Open"                                                               
C19          ""                TopLayer    0402                         40.0802      16.7091      180      "Condensateurs céramique multicouches MLCC - CMS 33PF 50V 2% 0402"                   
