Altium Designer Pick and Place Locations
C:\VIRGIL\AAA__JOB\ALTIUM\STM\Projets\MB1880A\BASE\MB1880A\02-Manufacturing\MB1880A_PCB\Assembly\MB1880-A01_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       15/10/21
Time:       02:16
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator  Comment                        Layer       Footprint                            Center-X(mm) Center-Y(mm) Rotation Description                                                 
Designator3 Comment                        BottomLayer MIRE_PLACE_SMD_0P8MM                 2.5000       27.5000      180      ""                                                          
Designator2 Comment                        BottomLayer MIRE_PLACE_SMD_0P8MM                 2.5000       2.5000       180      ""                                                          
Designator4 Comment                        BottomLayer MIRE_PLACE_SMD_0P8MM                 27.5000      2.5000       180      ""                                                          
1           Comment                        TopLayer    MIRE_PLACE_SMD_0P8MM                 2.5000       27.5000      0        ""                                                          
3           Comment                        TopLayer    MIRE_PLACE_SMD_0P8MM                 2.5000       2.5000       0        ""                                                          
2           Comment                        TopLayer    MIRE_PLACE_SMD_0P8MM                 27.5000      2.5000       0        ""                                                          
U1          ESD-TRANSIL                    TopLayer    ESD_QFN2_1P6X1_P125                  12.8750      10.2750      180      "High power transient voltage suppressor, 7V breakdown"     
TP2         Test_Point_PTH_1mm_2mm         TopLayer    TP_PTH_1MM_2MM                       22.5000      3.0000       0        "Test Point trought hole 1mm/2mm"                           
TP1         Test_Point_PTH_1mm_2mm         TopLayer    TP_PTH_1MM_2MM                       7.5000       3.0000       0        "Test Point trought hole 1mm/2mm"                           
SB1         ""                             TopLayer    SOLDER-BRIDGE_R0603-0R               20.7250      12.1250      0        "Solder Bridge ON"                                          
R2          Resistor                       TopLayer    R0402                                15.9000      9.7250       270      "Resistor, 5K1, 0402, +/-1%, 1/16W"                         
R1          Resistor                       TopLayer    R0402                                14.7500      9.7250       270      "Resistor, 5K1, 0402, +/-1%, 1/16W"                         
JP2         "Jumper_Header 3x1 Fitted 1-2" TopLayer    CON_SAMTEC_TSW-103-07-F-S            16.7500      24.5000      90       "Header, 3x1, 2.54mm, VR, TH, T=5.84mm/2.54mm"              
JP1         "Jumper_Header 3x1 Fitted 1-2" TopLayer    CON_SAMTEC_TSW-103-07-F-S            13.2500      24.5000      90       "Header, 3x1, 2.54mm, VR, TH, T=5.84mm/2.54mm"              
CN3         "Socket 10X2 STMod+"           TopLayer    CON_SAMTEC_SQT-110-01-F-D-RA__STMOD+ 3.2500       15.0000      270      "Socket, 10x2, 2mm, RA, TH, T=6.35mm/2.29mm"                
CN2         "Socket 10X2 STMod+"           TopLayer    CON_SAMTEC_SQT-110-01-F-D-RA__STMOD+ 26.7500      15.0000      90       "Socket, 10x2, 2mm, RA, TH, T=6.35mm/2.29mm"                
CN1         USB_TYPE_C_Receptacle          TopLayer    CON_USB-TYPEC_MOLEX_2012670005       15.0000      4.8450       0        "USB_TypeC, 24 pins, RA, SMD, T=3.71mm (USB Certified 3.1)" 
C1          ""                             TopLayer    C0402                                13.0500      9.0250       0        "Capacitor, MLCC, 100pF, 50V, NPO, 5%, 0402, T=0,5mm"       
Designator1 Comment                        TopLayer    Sheetbox_2L2S                        14.7186      -17.8734     0        ""                                                          
