Altium Designer Pick and Place Locations
C:\VIRGIL\AAA__JOB\ALTIUM\STM\Projets\MB1897B\BASE\MB1897B\02-Manufacturing\MB1897B_PCB\Assembly\MB1897-B01_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       09/03/23
Time:       00:20
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator  Comment            Layer       Footprint                               Center-X(mm) Center-Y(mm) Rotation Description                                                                                                
CART-1      Comment            TopLayer    Sheetbox_4L2S                           34.8936      -21.5984     0        ""                                                                                                         
Designator5 Comment            BottomLayer MIRE_PLACE_SMD_0P8MM                    37.4000      25.7500      180      ""                                                                                                         
Designator6 Comment            BottomLayer MIRE_PLACE_SMD_0P8MM                    6.1250       21.6250      180      ""                                                                                                         
Designator7 Comment            BottomLayer MIRE_PLACE_SMD_0P8MM                    38.0000      2.0000       180      ""                                                                                                         
Designator1 Comment            TopLayer    MIRE_PLACE_SMD_0P8MM                    37.4000      25.7500      0        ""                                                                                                         
Designator4 Comment            TopLayer    MIRE_PLACE_SMD_0P8MM                    2.4500       3.2750       0        ""                                                                                                         
Designator2 Comment            TopLayer    MIRE_PLACE_SMD_0P8MM                    6.1250       21.6250      0        ""                                                                                                         
Designator3 Comment            TopLayer    CAM_DRAWING_AS-DB548A12M15-35           -229.6250    -189.6250    90       ""                                                                                                         
TP1         "Test Point"       BottomLayer TP_SMD_1MM                              12.8000      24.3250      90       "Test Point 1mm"                                                                                           
TP2         "Test Point"       BottomLayer TP_SMD_1MM                              18.2000      22.7500      90       "Test Point 1mm"                                                                                           
TP3         "Test Point"       BottomLayer TP_SMD_1MM                              8.3000       21.9000      90       "Test Point 1mm"                                                                                           
D1          BAT60JFILM         BottomLayer DIO_SOD323                              36.0750      6.7000       270      BAT60JFILM                                                                                                 
R4          Resistor           BottomLayer R0402                                   36.5250      9.1000       0        "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                        
C11         Capacitor          BottomLayer C0402                                   36.5250      10.0750      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                  
R1          Resistor           BottomLayer R0402                                   14.6500      22.3250      270      "Resistor, 4K7, 0402, +/-1%, 1/16W"                                                                        
CN1         FPC05024-03200_CSI BottomLayer CON_ATOM_FPC05024-03200_INV             32.3125      15.5250      90       "Socket_FFC/FPC, 24pins, 0.5mm, RA, SMD, T=2.0mm"                                                          
C2          Capacitor          BottomLayer C0402                                   13.6000      22.3250      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                  
C6          Capacitor          BottomLayer C0402                                   36.4500      20.6750      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                  
C7          Capacitor          BottomLayer C0402                                   36.4500      19.7750      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                  
C8          Capacitor          BottomLayer C0402                                   36.4500      18.8750      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                  
C12         Capacitor          BottomLayer C0402                                   5.4750       8.7750       0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                  
C4          Capacitor          BottomLayer C0402                                   14.1750      20.4250      90       "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                                                    
C5          Capacitor          BottomLayer C0402                                   17.3750      20.8000      180      "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                                                    
C3          Capacitor          BottomLayer C0402                                   11.0250      21.5500      270      "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                                                    
C1          Capacitor          BottomLayer C0402                                   11.4750      22.9000      0        "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                                                    
C10         Capacitor          BottomLayer C0402                                   36.5250      11.5500      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                  
C9          Capacitor          BottomLayer C0402                                   36.6500      14.6500      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                  
L1          BEAD               BottomLayer L0603                                   36.2000      22.8500      90       "Ferrite bead, 600R @1 00MHz, +/-25%, 350mA, 0R5, 0603, T=0.8mm"                                           
R2          Resistor           BottomLayer R0402                                   17.3750      19.6500      0        "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                        
R5          Resistor           BottomLayer R0402                                   -3.6500      9.9000       270      "Resistor, 4K7, 0402, +/-1%, 1/16W"                                                                        
R6          Resistor           BottomLayer R0402                                   -3.6000      14.5750      270      "Resistor, 4K7, 0402, +/-1%, 1/16W"                                                                        
R3          Resistor           BottomLayer R0402                                   38.3000      13.1000      270      "Resistor, 10K, 0402, +/-1%, 1/16W"                                                                        
TR2         BSN20              BottomLayer MOS_SOT23                               -0.9750      14.6000      90       "MOSFET, N-Channel , Vds: 25V, Id: 0,22A, Vgs(th): 1.06V, Vgs(max): +/-8V, Rdson:5ohm@Vgs=2.7V, Qg=0,49nC" 
TR1         BSN20              BottomLayer MOS_SOT23                               -0.9750      9.9000       90       "MOSFET, N-Channel , Vds: 25V, Id: 0,22A, Vgs(th): 1.06V, Vgs(max): +/-8V, Rdson:5ohm@Vgs=2.7V, Qg=0,49nC" 
U2          LD39020            BottomLayer REG_XDFN4-EPAD_CASE-711AJ_1X1_H0P4_P065 15.5600      20.5000      270      "LDO, output 1V8, 200 mA very low quiescent current"                                                       
U1          LD39020            BottomLayer REG_XDFN4-EPAD_CASE-711AJ_1X1_H0P4_P065 12.3250      21.5500      0        "LDO, output 2V8, 200 mA very low quiescent current"                                                       
X1          OSCILLATOR_4_PINS  BottomLayer CRY_NZ2016SH_4P                         36.4500      13.1000      180      "Oscillator, SPXO, 24MHz, +/-50ppm, 3V3, square wave, 2x1.6mm"                                             
CN2         SFW15R-1STE1LF     BottomLayer CON_FCI_SFW15R-1STE1LF                  12.9500      5.9500       180      "Socket_FFC/FPC ZIF, 15pins, 1mm ,RA, SMD, T=2.7mm"                                                        
