Altium Designer Pick and Place Locations
C:\Subversion\MB1932-Nucleo64-STLINK_Type-C\Trunk\02-Manufacturing\MB1932B_PCB\Assembly\MB1932B_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       28/04/23
Time:       17:10
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator Comment                        Layer       Footprint                                                          Center-X(mm) Center-Y(mm) Rotation Description                                                                          
JP11       "Jumper_Header 2x1 Fitted"     TopLayer    CON_SAMTEC_TSW-102-07-G-S                                          -53.1850     70.8178      0        "Header, 2x1, 2.54mm, VR, TH, T=5.84mm/2.54mm"                                       
CN1        USB_TYPE_C_Receptacle          TopLayer    CON_USB-TYPEC_AMPHENOL_12401826E412A                               -22.9000     77.1510      180      "USB_TypeC, 24 pins, RA, SMD, T=2.96mm (USB Certified 3.1)"                          
TP3        "Test Point"                   TopLayer    TP_SMD_1MM                                                         -20.3036     48.5629      180      "Test Point 1mm"                                                                     
R25        Resistor                       TopLayer    R0402                                                              -26.9051     46.5233      90       "Resistor, 47K, 0402, +/-1%, 1/16W"                                                  
R27        Resistor                       TopLayer    R0402                                                              -27.3674     45.0552      0        "Resistor, 15K, 0402, +/-1%, 1/16W"                                                  
U12        LD39100PUR                     TopLayer    ICC_DFN6-EPAD_3X3_P095                                             -24.4799     46.0381      90       "LDO, output 1.5 to 5.5V 1A adjustable"                                              
JP10       "Jumper_Header 2x1 Fitted"     TopLayer    CON_SAMTEC_TSW-102-07-G-S                                          -53.1850     60.4323      0        "Header, 2x1, 2.54mm, VR, TH, T=5.84mm/2.54mm"                                       
JP9        "Jumper_Header 2x1 Fitted"     TopLayer    CON_SAMTEC_TSW-102-07-G-S                                          -53.1850     63.0276      0        "Header, 2x1, 2.54mm, VR, TH, T=5.84mm/2.54mm"                                       
JP6        "Jumper_Header 2x1 Fitted"     TopLayer    CON_SAMTEC_TSW-102-07-G-S                                          -53.1850     73.4575      0        "Header, 2x1, 2.54mm, VR, TH, T=5.84mm/2.54mm"                                       
JP8        "Jumper_Header 2x1 Fitted"     TopLayer    CON_SAMTEC_TSW-102-07-G-S                                          -53.1850     65.6209      0        "Header, 2x1, 2.54mm, VR, TH, T=5.84mm/2.54mm"                                       
JP7        "Jumper_Header 2x1 Fitted"     TopLayer    CON_SAMTEC_TSW-102-07-G-S                                          -53.1850     68.2174      0        "Header, 2x1, 2.54mm, VR, TH, T=5.84mm/2.54mm"                                       
SB54       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                             -18.2226     3.9116       180      "Solder Bridge ON"                                                                   
SB53       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                             -15.1900     3.9116       0        "Solder Bridge OFF"                                                                  
SB50       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                             -15.1900     5.4737       0        "Solder Bridge OFF"                                                                  
SB10       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                             -54.6600     41.3925      180      "Solder Bridge OFF"                                                                  
SB49       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                             -15.2900     7.0358       180      "Solder Bridge OFF"                                                                  
SB5        SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                             -24.9375     26.4225      0        "Solder Bridge ON"                                                                   
SB13       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                             -54.5589     39.2792      0        "Solder Bridge OFF"                                                                  
SB7        SB_ON                          TopLayer    SOLDER-BRIDGE_R0603-0R                                             -37.8398     12.4179      90       "Solder Bridge ON"                                                                   
SB4        SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                             -25.0375     28.2550      180      "Solder Bridge ON"                                                                   
SB6        SB_ON                          TopLayer    SOLDER-BRIDGE_R0603-0R                                             -28.1232     12.6046      270      "Solder Bridge ON"                                                                   
R38        Resistor                       TopLayer    R0603                                                              -44.0765     14.5479      0        "Resistor, 0R, 0603, +/-5%, 1/10W"                                                   
SB2        SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                             -41.3075     31.2075      180      "Solder Bridge ON"                                                                   
SB11       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                             -15.1889     40.8540      0        "Solder Bridge OFF"                                                                  
SB30       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                             -18.2133     22.9419      0        "Solder Bridge ON"                                                                   
SB33       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                             -18.2133     21.4288      0        "Solder Bridge OFF"                                                                  
SB35       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                             -18.2118     19.0977      0        "Solder Bridge ON"                                                                   
SB38       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                             -18.2118     17.6659      0        "Solder Bridge OFF"                                                                  
SB39       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                             -18.2118     16.1528      0        "Solder Bridge ON"                                                                   
SB20       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                             -15.1889     30.8972      0        "Solder Bridge ON"                                                                   
SB21       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                             -18.3115     30.8972      180      "Solder Bridge OFF"                                                                  
SB8        SB_OFF                         TopLayer    SOLDER-BRIDGE_R0603-0R                                             -39.8997     12.2604      90       "Solder Bridge OFF"                                                                  
SB45       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                             -18.3126     10.1600      180      "Solder Bridge OFF"                                                                  
SB26       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                             -18.3087     24.7758      180      "Solder Bridge OFF"                                                                  
SB48       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                             -15.2889     8.4995       180      "Solder Bridge OFF"                                                                  
SB25       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                             -15.1861     24.7758      0        "Solder Bridge ON"                                                                   
SB44       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                             -15.2900     10.1600      180      "Solder Bridge OFF"                                                                  
SB23       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                             -15.2889     27.1558      180      "Solder Bridge OFF"                                                                  
SB40       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                             -15.2907     14.6100      180      "Solder Bridge ON"                                                                   
SB42       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                             -15.2880     13.0969      180      "Solder Bridge OFF"                                                                  
SB37       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                             -15.2892     17.6659      180      "Solder Bridge ON"                                                                   
SB34       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                             -15.2892     19.0977      180      "Solder Bridge OFF"                                                                  
SB29       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                             -15.2907     22.9419      180      "Solder Bridge ON"                                                                   
SB32       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                             -15.2907     21.4288      180      "Solder Bridge OFF"                                                                  
SB17       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                             -54.6589     34.2500      180      "Solder Bridge OFF"                                                                  
SB15       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                             -54.8075     36.7900      180      "Solder Bridge OFF"                                                                  
SB19       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                             -15.2889     32.3704      180      "Solder Bridge OFF"                                                                  
SB18       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                             -15.1889     33.7166      0        "Solder Bridge ON"                                                                   
SB16       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                             -15.2873     35.8375      180      "Solder Bridge OFF"                                                                  
R32        Resistor                       TopLayer    R0402                                                              -46.2350     30.7600      0        "Resistor, 5K1, 0402, +/-1%, 1/16W"                                                  
R33        Resistor                       TopLayer    R0402                                                              -46.2401     29.6970      0        "Resistor, 100R, 0402, +/- 1%, 1/16W"                                                
C30        Capacitor                      TopLayer    C0402                                                              -47.5909     30.1470      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                            
C33        Capacitor                      TopLayer    C0402                                                              -24.7300     26.5500      0        "Capacitor, MLCC, 2.2uF, 6.3V, X5R, +/-10%, 0402, T=0.5mm"                           
C31        Capacitor                      TopLayer    C0603                                                              -43.6400     29.8925      180      "Capacitor, MLCC, 1uF, 16V, X5R, +/-10%, 0603, T=0.8mm"                              
C41        Capacitor                      TopLayer    C0603_H0P8                                                         -30.4382     12.6930      270      "Capacitor, MLCC, 4.7uF, 10V, X5R, +/-10%, 0603, T=0.8mm"                            
CN7        "Header 19x2"                  TopLayer    CON_SAMTEC_TSW-119-09-X-D                                          -65.4801     27.9000      270      "Header, 19x2, 2.54mm, VR, TH, T=5.84mm/10.16mm"                                     
U5         FPF3380UCX                     TopLayer    ICC_WLCSP12_1P858x1P318_P040                                       -15.7527     69.3264      270      "28 V / 5 A Rated OVP with Low On-resistance and Integrated TVS"                     
R31        Resistor                       TopLayer    R0402                                                              -34.9100     31.4350      90       "Resistor, 100K, 0402, +/-1%, 1/16W"                                                 
JP2        "Jumper_Header 2x1"            TopLayer    CON_SAMTEC_TSW-102-09-X-S                                          -66.7501     77.4300      90       "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/10.16mm"                                 
JP3        "Jumper_Header 2x1"            TopLayer    CON_SAMTEC_TSW-102-09-X-S                                          -3.2501      77.4300      90       "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/10.16mm"                                 
U7         ESDALC6V1W5                    TopLayer    ESD_SOT323-5L                                                      -58.5876     62.3340      270      "Dual Transil array for ESD protection"                                              
U6         ESDALC6V1W5                    TopLayer    ESD_SOT323-5L                                                      -58.5876     66.7766      270      "Dual Transil array for ESD protection"                                              
U2         USBLC6-2SC6                    TopLayer    ESD_SOT23-6L                                                       -26.0604     69.6933      270      "Very low capacitance ESD protection"                                                
U4         ESD-TRANSIL                    TopLayer    ESD_QFN1610_2N_1K_2A                                               -19.8249     69.4081      270      "High power Transient voltage suppressor:25V/35A EOS and ESD transients protection." 
U9         ESD-TRANSIL                    TopLayer    ESD_ST0201                                                         -32.8208     51.5982      90       "ESD protection 6V1"                                                                 
TP1        "Test Point"                   TopLayer    TP_SMD_1MM                                                         -15.7526     75.0825      180      "Test Point 1mm"                                                                     
TP2        "Test Point"                   TopLayer    TP_SMD_1MM                                                         -30.0547     64.7503      90       "Test Point 1mm"                                                                     
R11        Resistor                       TopLayer    R0402                                                              -9.7106      70.5714      180      "Resistor, 100K, 0402, +/-1%, 1/16W"                                                 
R14        Resistor                       TopLayer    R0402                                                              -11.2122     69.0982      270      "Resistor, 100K, 0402, +/-1%, 1/16W"                                                 
R13        Resistor                       TopLayer    R0402                                                              -12.3268     69.0982      270      "Resistor, 1K, 0402, +/-1%,1/16W"                                                    
R15        Resistor                       TopLayer    R0402                                                              -57.8425     64.9550      180      "Resistor, 100R, 0402, +/- 1%, 1/16W"                                                
HW1        STICKER_PRODUCT                TopLayer    STICKER_PRODUCT_25X9                                               -289.1301    -184.9600    0        "Sticker product 25x9 mm"                                                            
HW2        STICKER_BOARD                  BottomLayer STICKER_BOARD_25X9                                                 -289.1301    -184.9600    180      "Sticker Board 25x9 mm"                                                              
C12        Capacitor                      TopLayer    C0402                                                              -6.2412      67.1576      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                            
C16        Capacitor                      TopLayer    C0402                                                              -26.2323     61.1334      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                            
C15        Capacitor                      TopLayer    C0603                                                              -27.4515     60.9048      90       "Capacitor, MLCC, 1uF, 16V, X5R, +/-10%, 0603, T=0.8mm"                              
C14        Capacitor                      TopLayer    C0402                                                              -21.2321     61.8623      180      "Capacitor, MLCC, 10nF, 50V, X7R, +/-10%, 0402, T=0.5mm"                             
C18        Capacitor                      TopLayer    C0603                                                              -20.3109     60.0733      270      "Capacitor, MLCC, 1uF, 16V, X5R, +/-10%, 0603, T=0.8mm"                              
C19        Capacitor                      TopLayer    C0402                                                              -21.6571     59.8193      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                            
C2         Capacitor                      TopLayer    C0402                                                              -42.2594     74.6716      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                            
R10        Resistor                       TopLayer    R0402                                                              -16.9020     71.1286      180      "Resistor, 680K, 0402, +/-1%, 1/16W"                                                 
D1         BAT60JFILM                     TopLayer    DIO_SOD323                                                         -17.4741     62.2154      180      BAT60JFILM                                                                           
U3         STMPS2141STR                   TopLayer    MOS_SOT23-5L                                                       -6.8912      69.6062      90       "Enhanced single channel power switches with active low enable pin"                  
R21        Resistor                       TopLayer    R0402                                                              -45.6682     64.2778      180      "Resistor, 10K, 0402, +/-1%, 1/16W"                                                  
R24        Resistor                       TopLayer    R0402                                                              -40.7900     61.3500      270      "Resistor, 0R, 0402, +/-5%, 1/16W"                                                   
LD2        LED_red                        TopLayer    LED_0402_KINGBRIGHT_KPHHS-1005SURCK_HYPER-RED_1A2K_H0P5            -11.7822     70.5714      0        "LED 0402 Red"                                                                       
C36        Capacitor                      TopLayer    C0402                                                              -49.0027     22.2172      90       "Capacitor, MLCC, 10pF, 50V, NPO, +/-5%, 0402, T=0.5mm"                              
C42        Capacitor                      TopLayer    C0402                                                              -29.2713     13.0102      270      "Capacitor, MLCC, 2.2uF, 6.3V, X5R, +/-10%, 0402, T=0.5mm"                           
R34        Resistor                       TopLayer    R0402                                                              -43.8984     27.5266      0        "Resistor, 0R, 0402, +/-5%, 1/16W"                                                   
R35        Resistor                       TopLayer    R0402                                                              -43.8984     26.4406      0        "Resistor, 0R, 0402, +/-5%, 1/16W"                                                   
R36        Resistor                       TopLayer    R0402                                                              -43.9303     24.0130      0        "Resistor, 0R, 0402, +/-5%, 1/16W"                                                   
T2         BSN20                          TopLayer    MOS_SOT23                                                          -26.0136     42.0021      90       "Transistor, N-channel enhancement mode field-effect transistor"                     
U11        LD1117S50TR                    TopLayer    REG_SOT223-TAB                                                     -42.0619     45.1435      270      "IC REG LDO 5V 0.8A SOT223"                                                          
X3         XTAL_2_PINS                    TopLayer    CRY_NX3225GD_2P                                                    -46.6151     23.2002      90       "Crystal, 8MHz, 8pF, +/-20ppm, 500R, 3.2x2.5mm"                                      
X1         XTAL_2_PINS                    TopLayer    CRY_NX3225GD_2P                                                    -45.4390     68.3819      90       "Crystal, 8MHz, 8pF, +/-20ppm, 500R, 3.2x2.5mm"                                      
LD1        LED_BICOLOR                    TopLayer    LED_BI-GR_WE-150141SV73110                                         -9.6001      76.1600      0        "LED Bicolor, Green/Red, 2V, 20mA,  4-PLCC"                                          
X2         XTAL_2_PINS                    TopLayer    CRY_NX2012SA_2P                                                    -45.6651     26.9475      90       "Crystal, 32.768kHz, 6pF, +/-20ppm, 80K, 2.05x1.2mm"                                 
T1         9013-SOT23                     TopLayer    NPN_SOT23                                                          -26.3843     65.4160      90       "NPN Bipolar Transistor"                                                             
U10        ESD-TRANSIL                    TopLayer    ESD_ST0201                                                         -48.8188     51.5874      90       "ESD protection 6V1"                                                                 
CN10       "Header 19x2"                  TopLayer    CON_SAMTEC_TSW-119-09-X-D                                          -4.5201      27.9000      270      "Header, 19x2, 2.54mm, VR, TH, T=5.84mm/10.16mm"                                     
CN8        "Socket 6x1"                   TopLayer    CON_SAMTEC_SSW-106-01-X-S                                          -59.1301     11.3900      270      "Socket, 6x1, 2.54mm, VR, TH, T=8.51/2.64mm"                                         
CN9        "Socket 8x1"                   TopLayer    CON_SAMTEC_SSW-108-01-X-S                                          -10.8701     13.9300      90       "Socket, 8x1, 2.54mm, VR, TH, T=8.51/2.64mm"                                         
CN6        "Socket 8x1"                   TopLayer    CON_SAMTEC_SSW-108-01-X-S                                          -59.1301     31.7100      270      "Socket, 8x1, 2.54mm, VR, TH, T=8.51/2.64mm"                                         
CN5        "Socket 10x1"                  TopLayer    CON_SAMTEC_SSW-110-01-X-S                                          -10.8701     38.3140      90       "Socket, 10x1, 2.54mm, VR, TH, T=8.51/2.64mm"                                        
B1         SW_BLUE_KSC721JLFS             TopLayer    SWI_C&K_KSC721JLFS_BLUE                                            -43.2551     53.3000      0        "Switch HW BLUE High4.3mm 2.25 Newtons, BEND type"                                   
B2         SW_BLACK_KSC321JLFS            TopLayer    SWI_C&K_KSC321JLFS_BLACK                                           -26.7451     53.3000      0        "Switch HW BLACK High3.5mm 2Newtons, BEND type"                                      
CN3        "Header 4x1"                   TopLayer    CON_SAMTEC_TSW-104-07-G-S                                          -36.1101     79.6296      0        "Header, 4x1, 2.54mm, VR, TH, T=5.84mm/2.54mm"                                       
JP5        "Jumper_Header 2x1 Fitted"     TopLayer    CON_SAMTEC_TSW-102-07-G-S                                          -33.5278     43.0083      0        "Header, 2x1, 2.54mm, VR, TH, T=5.84mm/2.54mm"                                       
D2         BAT60JFILM                     TopLayer    DIO_SOD323                                                         -17.4741     59.6500      180      BAT60JFILM                                                                           
U8         LDK120M33R                     TopLayer    REG_SOT23-5L                                                       -24.0225     60.4730      0        "200 mA low quiescent current very low noise LDO"                                    
C7         Capacitor                      TopLayer    C0402                                                              -18.6006     69.5808      270      "Capacitor, MLCC, 100pF, 50V, NPO, +/-5%, 0402, T=0.5mm"                             
C34        Capacitor                      TopLayer    C0402                                                              -47.4853     26.1732      0        "Capacitor, MLCC, 8.2pF, 50V, NPO, +/-0.25pF, 0402, T=0.5mm"                         
C40        Capacitor                      TopLayer    C0402                                                              -26.9381     13.1188      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                            
C32        Capacitor                      TopLayer    C0402                                                              -47.4845     27.6598      0        "Capacitor, MLCC, 8.2pF, 50V, NPO, +/-0.25pF, 0402, T=0.5mm"                         
C35        Capacitor                      TopLayer    C0402                                                              -49.0038     24.1800      270      "Capacitor, MLCC, 10pF, 50V, NPO, +/-5%, 0402, T=0.5mm"                              
C3         Capacitor                      TopLayer    C0402                                                              -31.1375     70.3700      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                            
C28        Capacitor                      TopLayer    C0402                                                              -37.5325     31.2400      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                            
C43        Capacitor                      TopLayer    C0402                                                              -36.7603     11.2325      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                            
C37        Capacitor                      TopLayer    C0402                                                              -43.9008     21.5169      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                            
C29        Capacitor                      TopLayer    C0402                                                              -24.7775     29.6425      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                            
C38        Capacitor                      TopLayer    C0402                                                              -43.8225     17.0371      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                            
C39        Capacitor                      TopLayer    C0603                                                              -44.0765     15.9195      180      "Capacitor, MLCC, 1uF, 16V, X5R, +/-10%, 0603, T=0.8mm"                              
C17        Capacitor                      TopLayer    C0402                                                              -35.0012     61.1175      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                            
C11        Capacitor                      TopLayer    C0402                                                              -29.1750     66.8325      180      "Capacitor, MLCC, 20pF, 50V, NPO, +/- 5%, 0402, T=0.5mm"                             
C25        Capacitor                      TopLayer    C0805                                                              -47.9476     42.8527      0        "Capacitor, MLCC, 10uF, 25V, X5R, +/-10%, 0805, T=0.85mm"                            
C22        Capacitor                      TopLayer    C0805                                                              -36.1313     46.0425      180      "Capacitor, MLCC, 10uF, 25V, X5R, +/-10%, 0805, T=0.85mm"                            
C20        Capacitor                      TopLayer    C0603                                                              -29.3352     46.2973      90       "Capacitor, MLCC, 1uF, 16V, X5R, +/-10%, 0603, T=0.8mm"                              
C21        Capacitor                      TopLayer    C0402                                                              -27.9854     46.5489      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                            
C24        Capacitor                      TopLayer    C0402                                                              -22.1483     45.5336      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                            
C23        Capacitor                      TopLayer    C0603                                                              -21.0180     45.7927      270      "Capacitor, MLCC, 1uF, 16V, X5R, +/-10%, 0603, T=0.8mm"                              
C5         Capacitor                      TopLayer    C0603                                                              -13.5750     69.3575      270      "Capacitor, MLCC, 10uF, 10V, X5R, +/-10%, 0603, T=0.8mm"                             
C6         Capacitor                      TopLayer    C0603                                                              -17.4322     69.3248      270      "Capacitor, MLCC, 100nF, 50V, X7R, +/-10%, 0603, T=0.8mm"                            
C4         Capacitor                      TopLayer    C0402                                                              -47.4727     69.7819      270      "Capacitor, MLCC, 10pF, 50V, NPO, +/-5%, 0402, T=0.5mm"                              
C10        Capacitor                      TopLayer    C0402                                                              -47.4727     66.9819      270      "Capacitor, MLCC, 10pF, 50V, NPO, +/-5%, 0402, T=0.5mm"                              
C13        Capacitor                      TopLayer    C0402                                                              -45.5456     65.5479      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                            
C1         Capacitor                      TopLayer    C0402                                                              -40.5881     74.6716      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                            
C27        Capacitor                      TopLayer    C0603_H0P8                                                         -39.5325     31.3425      0        "Capacitor, MLCC, 4.7uF, 10V, X5R, +/-10%, 0603, T=0.8mm"                            
CN4        "Header 7x2"                   TopLayer    CON_STDC14_Receiver_MEDIUM_WITH_MIPI10_3D                          -64.8959     65.4488      270      "Header, 5x2, 1.27mm, VR, SMD, T=5.97mm/3.05mm"                                      
LD4        LED_green                      TopLayer    LED_0402_EVERLIGHT_16-213SYGC/S530-E3-TR8 _YELLOW-GREEN_1A2K_H0P45 -25.4751     39.3300      180      "LED, Yellow Green, 2V, 25mA, 0402, 0.45mm"                                          
LD3        LED_green                      TopLayer    LED_0402_EVERLIGHT_16-213SYGC/S530-E3-TR8 _YELLOW-GREEN_1A2K_H0P45 -47.2561     38.0600      180      "LED, Yellow Green, 2V, 25mA, 0402, 0.45mm"                                          
R30        Resistor                       TopLayer    R0402                                                              -49.3257     38.0600      0        "Resistor, 680R, 0402, +/-1%, 1/16W"                                                 
R6         Resistor                       TopLayer    R0402                                                              -35.9907     74.6665      90       "Resistor, 5K1, 0402, +/-1%, 1/16W"                                                  
R26        Resistor                       TopLayer    R0402                                                              -47.6155     45.1387      180      "Resistor, 1K, 0402, +/-1%,1/16W"                                                    
R5         Resistor                       TopLayer    R0402                                                              -37.1856     74.6665      90       "Resistor, 10K, 0402, +/-1%, 1/16W"                                                  
R37        Resistor                       TopLayer    R0402                                                              -43.8984     22.5652      0        "Resistor, 0R, 0402, +/-5%, 1/16W"                                                   
R12        Resistor                       TopLayer    R0402                                                              -21.0866     69.3280      270      "Resistor, 5K1, 0402, +/-1%, 1/16W"                                                  
R3         Resistor                       TopLayer    R0402                                                              -24.8325     72.4675      270      "Resistor, 5K1, 0402, +/-1%, 1/16W"                                                  
R18        Resistor                       TopLayer    R0402                                                              -20.9106     64.9100      90       "Resistor, 10K, 0402, +/-1%, 1/16W"                                                  
R7         Resistor                       TopLayer    R0402                                                              -45.5456     72.2681      180      "Resistor, 10K, 0402, +/-1%, 1/16W"                                                  
R22        Resistor                       TopLayer    R0402                                                              -45.6675     63.2025      180      "Resistor, 10K, 0402, +/-1%, 1/16W"                                                  
R4         Resistor                       TopLayer    R0402                                                              -38.5064     74.6665      270      "Resistor, 100K, 0402, +/-1%, 1/16W"                                                 
R8         Resistor                       TopLayer    R0402                                                              -45.5456     71.2121      180      "Resistor, 10K, 0402, +/-1%, 1/16W"                                                  
R28        Resistor                       TopLayer    R0402                                                              -28.7415     42.0021      90       "Resistor, 680R, 0402, +/-1%, 1/16W"                                                 
R20        Resistor                       TopLayer    R0402                                                              -22.0638     64.9100      90       "Resistor, 100R, 0402, +/- 1%, 1/16W"                                                
R9         Resistor                       TopLayer    R0402                                                              -16.9020     72.1700      0        "Resistor, 180K, 0402, +/-1%, 1/16W"                                                 
R1         Resistor                       TopLayer    R0402                                                              -10.3367     80.0462      90       "Resistor, 1K, 0402, +/-1%,1/16W"                                                    
R2         Resistor                       TopLayer    R0402                                                              -8.8635      80.0462      270      "Resistor, 330R, 0402, +/-1%, 1/16W"                                                 
R16        Resistor                       TopLayer    R0402                                                              -23.5395     66.7998      270      "Resistor, 1K5, 0402, +/-1%, 1/16W"                                                  
R29        Resistor                       TopLayer    R0402                                                              -23.4431     42.0757      90       "Resistor, 1M, 0402, +/-1%, 1/16W"                                                   
R17        Resistor                       TopLayer    R0402                                                              -31.1549     66.8299      0        "Resistor, 100R, 0402, +/- 1%, 1/16W"                                                
SB24       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                             -45.2258     25.8913      180      "Solder Bridge OFF"                                                                  
SB3        SB_ON                          TopLayer    SOLDER-BRIDGE_R0603-0R                                             -49.5075     30.6425      180      "Solder Bridge ON"                                                                   
SB14       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                             -15.1873     37.1837      0        "Solder Bridge ON"                                                                   
SB27       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                             -45.1259     24.4998      0        "Solder Bridge ON"                                                                   
SB41       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                             -18.2133     14.6100      0        "Solder Bridge OFF"                                                                  
SB36       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                             -45.1258     18.0499      0        "Solder Bridge ON"                                                                   
SB1        SB_ON                          TopLayer    SOLDER-BRIDGE_R0603-0R                                             -31.6693     47.0084      180      "Solder Bridge ON"                                                                   
SB12       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                             -15.1900     39.5840      0        "Solder Bridge ON"                                                                   
SB52       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                             -53.9089     4.5616       270      "Solder Bridge ON"                                                                   
SB47       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                             -55.5995     8.1329       90       "Solder Bridge OFF"                                                                  
SB46       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                             -53.9089     8.0329       270      "Solder Bridge ON"                                                                   
SB51       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                             -55.5995     4.6616       90       "Solder Bridge OFF"                                                                  
U13        STM32_MCU_LQFP64               TopLayer    ICC_LQFP64_10X10_P050_SOCKET_YAMAICHI_IC149-064-069-B5_NM          -33.8878     22.6676      270      "MCU, ARM Cortex-M0+ 32-bit, 256K Flash, 20KB RAM, With Crypto"                      
SB28       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                             -45.2258     23.1084      180      "Solder Bridge ON"                                                                   
SB22       SB_OFF                         BottomLayer SOLDER-BRIDGE_R0603-0R                                             -45.2258     27.2828      180      "Solder Bridge OFF"                                                                  
SB43       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                             -18.3105     13.0969      180      "Solder Bridge ON"                                                                   
SB31       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                             -45.2259     21.7169      180      "Solder Bridge ON"                                                                   
U1         STLINK-V2EC                    TopLayer    ICC_LQFP48_7X7_P050                                                -37.7433     67.5799      270      "Medium-density performance line ARM-based 32-bit MCU with 128KB Flash"              
R19        Resistor                       TopLayer    R0402                                                              -23.5395     64.9100      270      "Resistor, 36K, 0402, +/-1%, 1/16W"                                                  
C9         Capacitor                      TopLayer    C0402                                                              -9.3550      69.0982      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                            
C26        Capacitor                      TopLayer    C0402                                                              -15.3913     43.1806      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                            
SB9        SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                             -15.2889     44.6640      180      "Solder Bridge ON"                                                                   
JP1        "Jumper_Header 2x1"            TopLayer    CON_SAMTEC_TSW-102-07-G-S                                          -45.2628     79.6798      180      "Header, 2x1, 2.54mm, VR, TH, T=5.84mm/2.54mm"                                       
JP4        "Jumper_Header 4x2 Fitted 1-2" TopLayer    CON_SAMTEC_TSW-104-07-X-D                                          -9.6001      60.9200      180      "Header, 4x2, 2.54mm, VR, TH, T=5.84mm/2.54mm"                                       
R23        Resistor                       TopLayer    R0402                                                              -45.6675     62.1025      180      "Resistor, 33R, 0402, +/-1%, 1/16W"                                                  
