Altium Designer Pick and Place Locations
C:\Subversion\__Boards\MB2018-MiniBoard-WBA55-WCSP41-SMPS-SMA\Trunk\02-Manufacturing\MB2018A_PCB\Assembly\MB2018A_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       10/03/25
Time:       15:55
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator Comment                     Layer       Footprint                        Center-X(mm) Center-Y(mm) Rotation Description                                                                   
L2         Inductor                    TopLayer    IND_0402_MURATA_LQG15HS_H0P5     17.8350      38.7915      90       "Inductor, 3.6nH, +/-0.1nH, 750mA, 0402, T=0.5mm"                             
CN4        SMA-J-P-H-ST-EM1            TopLayer    CON_SMA-RF_CINCH_142-0701-851    17.8540      44.7550      0        "Jack_SMA, VR, PCB edge, 50R, T=7.92mm"                                       
CN2        FTSH-125-02-L-DV            BottomLayer FTSH-125-02-L-DV                 38.6560      18.5484      180      "Header, 25x2, 12.7mm, VR, SMD, T=4.83mm"                                     
CN1        FTSH-125-02-L-DV            BottomLayer FTSH-125-02-L-DV                 4.3664       18.5484      180      "Header, 25x2, 12.7mm, VR, SMD, T=4.83mm"                                     
SB41       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           20.5724      31.0207      0        "Solder Bridge 0402 ON"                                                       
SB28       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           27.7460      29.7000      180      "Solder Bridge 0402 OFF"                                                      
SB25       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           29.5245      15.4817      180      "Solder Bridge 0402 OFF"                                                      
SB18       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           29.4903      13.9920      180      "Solder Bridge 0402 ON"                                                       
SB16       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           18.2955      23.7477      180      "Solder Bridge 0402 ON"                                                       
U1         STM32WBA55HG                TopLayer    ICC_WLCSP41_2P977X2P757_P040     17.4639      32.1788      90       "MCU, ARM Cortex-M33 32-bit, 1MB Flash, 128KB SRAM, With Crypto, SMPS"        
SH1        "RF Shield (22.2x19.2x2mm)" TopLayer    SHIELD_RF_ST-CUSTOM_22P2X19P2_H2 -275.4530    -237.3752    0        "RF Shield (22.2x19.2x2mm)"                                                   
SB43       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           32.9722      32.5254      0        "Solder Bridge 0402 OFF"                                                      
C27        Capacitor                   BottomLayer C0402                            34.3075      31.9024      90       "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                       
L7         Inductor                    TopLayer    IND_0402_MURATA_BLM15H_H0P5      22.5203      29.4348      270      "Ferrite bead, 33R @ 100MHz, +/-25%, 0.55A, 0.2R, 0402, T=0.22mm"             
L5         Inductor                    TopLayer    C0402                            17.8360      29.2028      270      "Inductor, 10nH, +/-2%, 500 mA, 0.26Ohm, 0402, T=0.5mm"                       
SB30       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           16.0247      15.3830      0        "Solder Bridge 0402 ON"                                                       
SB17       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           10.8520      8.2208       0        "Solder Bridge 0402 ON"                                                       
SB14       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           10.8712      7.2048       0        "Solder Bridge 0402 OFF"                                                      
SB10       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           27.8476      27.8171      0        "Solder Bridge 0402 ON"                                                       
SB42       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           28.5538      23.9267      0        "Solder Bridge 0402 ON"                                                       
SB6        SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           20.5004      32.0708      180      "Solder Bridge 0402 OFF"                                                      
L6         Inductor                    TopLayer    L0805_H0P9                       16.9056      27.4066      180      "Inductor, 2.2uH, +/-20%, 0.7A, 0R156, 0805, T=0.9mm"                         
L4         Inductor                    TopLayer    IND_0402_MURATA_BLM15H_H0P5      22.1948      31.2128      0        "Ferrite bead, 33R @ 100MHz, +/-25%, 0.55A, 0.2R, 0402, T=0.22mm"             
C26        Capacitor                   TopLayer    C0402                            20.1578      33.8044      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
C25        Capacitor                   TopLayer    C0402                            16.1170      29.2097      90       "Capacitor, MLCC, 2.2uF, 6V3, X5R,+/-10%, 0402, T=0.5mm"                      
C24        Capacitor                   TopLayer    C0402                            18.6658      29.2031      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
C23        Capacitor                   TopLayer    C0402                            17.0009      29.2011      270      "Capacitor, MLCC, 4.7uF, 6V3, X5R, +/-20%, 0402, T=0.5mm"                     
C6         Capacitor                   TopLayer    C0603_H0P8                       20.4769      30.1795      0        "Capacitor, MLCC, 10uF, 10V, X6S, +/-20%, 0603, T=1mm"                        
L1         Inductor                    TopLayer    C0402                            17.8399      36.0987      90       "Inductor, 3.3nH, +/-0.3nH, 800 mA, 0.125Ohm, 0402, T=0.5mm"                  
SB4        SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           10.1636      17.1072      180      "Solder Bridge 0402 OFF"                                                      
SB3        SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           32.4771      23.7477      0        "Solder Bridge 0402 OFF"                                                      
SB2        SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           32.9586      33.7884      0        "Solder Bridge 0402 OFF"                                                      
CN3        "Header 7x2"                TopLayer    CON_SAMTEC_FTSH-107-01-L-DV-K-A  22.1014      4.5794       0        "Header, 7x2, 1.27mm, VR, T=5.97mm, FTSH series STDC14 without Alignment Pin" 
SB5        SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           32.4350      2.3430       0        "Solder Bridge 0402 OFF"                                                      
SB1        SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           10.6601      23.5579      90       "Solder Bridge 0402 OFF"                                                      
C19        Capacitor                   TopLayer    C0402                            13.9367      32.7788      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
C18        Capacitor                   TopLayer    C0402                            20.1559      31.3151      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
C15        Capacitor                   TopLayer    C0402                            20.1559      32.1475      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
C5         Capacitor                   BottomLayer C0402                            34.6782      2.8806       90       "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                       
C3         Capacitor                   BottomLayer C0402                            34.2493      23.2818      90       "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                       
C2         Capacitor                   BottomLayer C0402                            34.3075      34.5854      270      "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                       
C1         Capacitor                   BottomLayer C0402                            9.0496       21.8036      90       "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                       
X2         XTAL_4_PINS                 TopLayer    CRY_NX1612SA_4P                  20.4261      28.5245      0        "Crystal, 32MHz, 8pF, +/-10ppm, 40R, 1612(metric), T=0.3mm"                   
X1         XTAL_2_PINS                 TopLayer    CRY_NX1610SE_2P                  12.9670      31.4128      90       "Crystal, 32.768kHz, 6pF, +/-20ppm, 70KR, 1.6x1mm"                            
SC5        Shield-clip_S0951-46R       TopLayer    CLIP_HARWIN_S0951-46R            9.1846       31.0128      90       "shield clip Harwin S0951-46R to fix RF shielded cavity"                      
SC4        Shield-clip_S0951-46R       TopLayer    CLIP_HARWIN_S0951-46R            20.5020      20.7551      180      "shield clip Harwin S0951-46R to fix RF shielded cavity"                      
SC3        Shield-clip_S0951-46R       TopLayer    CLIP_HARWIN_S0951-46R            31.1850      29.9714      90       "shield clip Harwin S0951-46R to fix RF shielded cavity"                      
SC2        Shield-clip_S0951-46R       TopLayer    CLIP_HARWIN_S0951-46R            27.2220      39.7551      180      "shield clip Harwin S0951-46R to fix RF shielded cavity"                      
SC1        Shield-clip_S0951-46R       TopLayer    CLIP_HARWIN_S0951-46R            12.8619      39.7485      180      "shield clip Harwin S0951-46R to fix RF shielded cavity"                      
SB40       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           20.0129      28.4711      90       "Solder Bridge 0402 OFF"                                                      
SB39       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           20.9879      28.3586      270      "Solder Bridge 0402 OFF"                                                      
SB38       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           12.0378      32.6663      90       "Solder Bridge 0402 OFF"                                                      
SB37       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           11.1249      29.9880      270      "Solder Bridge 0402 OFF"                                                      
SB35       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           32.2947      20.9984      180      "Solder Bridge 0402 OFF"                                                      
SB34       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.3773      5.5556       0        "Solder Bridge 0402 ON"                                                       
SB33       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.3565      24.7894      180      "Solder Bridge 0402 ON"                                                       
SB32       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           27.6206      18.6501      180      "Solder Bridge 0402 OFF"                                                      
SB31       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.3948      19.9317      0        "Solder Bridge 0402 ON"                                                       
SB27       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           29.8222      17.0752      180      "Solder Bridge 0402 OFF"                                                      
SB26       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.2970      22.0256      180      "Solder Bridge 0402 ON"                                                       
SB24       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           29.8660      18.2024      0        "Solder Bridge 0402 ON"                                                       
SB23       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.4921      17.2865      0        "Solder Bridge 0402 ON"                                                       
SB22       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           28.4788      22.7454      180      "Solder Bridge 0402 OFF"                                                      
SB21       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           16.4808      6.0397       90       "Solder Bridge 0402 ON"                                                       
SB20       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           26.6697      19.7576      0        "Solder Bridge 0402 OFF"                                                      
SB19       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           10.8523      9.3026       0        "Solder Bridge 0402 OFF"                                                      
SB15       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.4020      11.8324      0        "Solder Bridge 0402 ON"                                                       
SB13       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           27.8333      28.7836      0        "Solder Bridge 0402 ON"                                                       
SB11       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.4264      26.7458      0        "Solder Bridge 0402 ON"                                                       
SB9        SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           10.8813      6.1432       0        "Solder Bridge 0402 ON"                                                       
SB8        SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           23.4212      12.0213      90       "Solder Bridge 0402 OFF"                                                      
SB7        SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.4158      25.7670      0        "Solder Bridge 0402 ON"                                                       
R9         Resistor                    BottomLayer R0402                            27.0237      3.8997       270      Resistor,47R,0402,1%,1/16W                                                    
R8         Resistor                    BottomLayer R0402                            25.9224      9.8779       90       Resistor,47R,0402,1%,1/16W                                                    
R7         Resistor                    BottomLayer R0402                            24.6584      9.8529       90       Resistor,47R,0402,1%,1/16W                                                    
R6         Resistor                    BottomLayer R0402                            24.3864      2.6308       90       Resistor,47R,0402,1%,1/16W                                                    
R5         Resistor                    BottomLayer R0402                            23.3764      9.8779       90       Resistor,47R,0402,1%,1/16W                                                    
R4         Resistor                    BottomLayer R0402                            22.0924      9.8524       90       Resistor,47R,0402,1%,1/16W                                                    
R3         Resistor                    BottomLayer R0402                            20.8874      9.8779       90       Resistor,47R,0402,1%,1/16W                                                    
R2         Resistor                    BottomLayer R0402                            19.6054      9.8779       90       Resistor,47R,0402,1%,1/16W                                                    
R1         Resistor                    TopLayer    R0402                            11.7217      28.7117      0        "Resistor, 100K, 0402, +/-1%, 1/16W"                                          
L3         Inductor                    TopLayer    IND_0402_MURATA_BLM15H_H0P5      14.2123      28.5530      0        "Ferrite bead, 33R @ 100MHz, +/-25%, 0.55A, 0.2R, 0402, T=0.22mm"             
HW4        STICKER_PRODUCT             TopLayer    STICKER_PRODUCT_25X5             -275.4530    -237.3752    90       "Sticker product 25x5 mm"                                                     
HW3        STICKER_BOARD               TopLayer    STICKER_BOARD_25X5               -275.4530    -237.3752    90       "Sticker board 25x5 mm"                                                       
D1         SCHOTTKY_1A_2K              TopLayer    DIO_SOD523_1A_2K                 12.8790      25.7837      180      "Small signal Schottky diodes"                                                
C22        Capacitor                   BottomLayer C0603                            20.2308      2.5544       90       "Capacitor, MLCC, 1uF, 16V, X5R, 10%, 0603, T=0,8mm"                          
C21        Capacitor                   TopLayer    C0402                            22.1668      32.8238      180      "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                       
C20        Capacitor                   TopLayer    C0402                            14.6950      29.8124      0        "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                       
C10        Capacitor                   TopLayer    C0402                            20.1559      32.9760      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
C14        Capacitor                   TopLayer    C0402                            17.4108      40.8794      0        "Capacitor, MLCC, 1.4pF, 50V, C0G, +/-0.05pF, 0402, T=0.5mm"                  
C13        Capacitor                   TopLayer    C0402                            17.3937      37.4304      0        "Capacitor, MLCC, 1.8pF, 50V, C0G, +/-0.25pF, 0402, T=0.5mm"                  
C12        Capacitor                   TopLayer    C0402                            17.3930      34.9241      0        "Capacitor, MLCC, 1.0pF, 50V, C0G, +/-0.1pF, 0402, T=0.5mm"                   
C11        Capacitor                   TopLayer    C0603                            20.4834      34.8394      180      "Capacitor, MLCC, 470nF, 16V, X7R, +/-10%, 0603, T=0.8mm"                     
C4         Capacitor                   BottomLayer C0402                            8.5040       16.5807      270      "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                       
C9         Capacitor                   TopLayer    C0402                            11.4983      30.6904      0        "Capacitor, MLCC, 6 pF, 50V, NPO, ±0,25pF, 0402, T=0.5mm"                     
C8         Capacitor                   TopLayer    C0402                            11.9222      32.4941      270      "Capacitor, MLCC, 6 pF, 50V, NPO, ±0,25pF, 0402, T=0.5mm"                     
C7         Capacitor                   TopLayer    C0402                            13.0421      24.7447      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
