Altium Designer Pick and Place Locations
C:\Users\Jorda\Documents\Projets\STM Le Mans\MB2029B\BASE\MB2029B\02-Manufacturing\MB2029B_PCB\Assembly\MB2029B_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       31/01/24
Time:       11:22
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator     Comment               Layer       Footprint                           Center-X(mm) Center-Y(mm) Rotation Description                                                                                  
L9             Inductor              TopLayer    IND_0402_MURATA_LQG15HSXXXX02_H0P5  20.8500      20.0250      90       "Inductor, 100nH, +/-5%, 200mA, 1R25, 0402, T=0.5mm"                                         
U2             MLPF-WL-0xD3          TopLayer    ICC_CSPG5_1P5X1P9_P060              18.7491      30.4110      90       "IC, 862 To 928MHz,16dBm, 4L PCB, IPD for STM32WL3"                                          
L8             Inductor              TopLayer    IND_0402_MURATA_LQW15ANXXXX00_H0P5  16.6250      28.0000      0        "Inductor, 12nH, +/-2%, 500mA, 0R14, 0402, T=0.5mm"                                          
L4             Inductor              TopLayer    IND_0402_MURATA_LQG15HSXXXX02_H0P5  24.1000      33.7750      90       "Inductor, 6.8nH, +/-3%, 0.6A, 220mR, 0402, T=0.5mm"                                         
SC8            Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0951-46R               18.8900      11.7745      180      "shield clip Harwin S0951-46R to fix RF shielded cavity"                                     
SC13           Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0951-46R               24.0900      11.7745      0        "RFI shield clip mini TIN SMD"                                                               
SC12           Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0951-46R               31.5000      24.2780      270      "RFI shield clip mini TIN SMD"                                                               
SC11           Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0951-46R               11.5000      24.2780      90       "RFI shield clip mini TIN SMD"                                                               
CART-1         Comment               TopLayer    Sheetbox_4L2S                       30.1027      -28.4750     0        ""                                                                                           
SC10           Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0951-46R               31.5000      19.1200      90       "RFI shield clip mini TIN SMD"                                                               
SC9            Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0951-46R               11.5000      19.1200      90       "RFI shield clip mini TIN SMD"                                                               
SB2            SB_ON                 TopLayer    SOLDER-BRIDGE_R0201_0R              19.0733      27.8127      180      "Resistor, 0R, 0201, Solder Bridge ON , 1/20W,"                                              
SB1            SB_ON                 TopLayer    SOLDER-BRIDGE_R0201_0R              19.0750      28.7000      180      "Resistor, 0R, 0201, Solder Bridge ON , 1/20W,"                                              
L10            Inductor              TopLayer    IND_0805_MURATA_LQM21               22.2250      17.2085      180      "Inductor, 10uH, +/-20%, 100mA, 0R5, 0805, T=1.45mm"                                         
STICKER-PROD1  Comment               TopLayer    STICKER_PRODUCT_25X5                -265.4530    -237.3752    90       ""                                                                                           
L3             Inductor              TopLayer    IND_0402_MURATA_LQG15HSXXXX02_H0P5  24.6000      35.4250      0        "Inductor, 5.6nH, +/-0.3nH, 0.65A, 180mR, 0402, T=0.5mm"                                     
C3             Capacitor             TopLayer    C0402                               22.0000      37.7750      180      "Capacitor, MLCC, 100pF, 50V, COG, +/-1%, 0402, T=0.5mm"                                     
HW1            S02-20150300          TopLayer    SHIELD_HARWIN_S02-25200300_20X25_H3 -265.4530    -237.3752    0        "RFI shield CAN, 25x20x3mm"                                                                  
SB10           SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              33.2125      8.3125       180      "Resistor, 0R, SB0402, 5%, 0.063W"                                                           
SB11           SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              33.2125      7.1875       180      "Resistor, 0R, SB0402, 5%, 0.063W"                                                           
SB7            SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              33.2125      11.6875      180      "Resistor, 0R, SB0402, 5%, 0.063W"                                                           
SB17           SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              33.2125      3.8125       180      "Resistor, 0R, SB0402, 5%, 0.063W"                                                           
SB6            SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              33.2875      12.8125      0        "Resistor, 0R, SB0402, 5%, 0.063W"                                                           
SB9            SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              33.2875      9.4375       0        "Resistor, 0R, SB0402, 5%, 0.063W"                                                           
STICKER-BOARD1 Comment               TopLayer    STICKER_BOARD_25X5                  -265.4530    -237.3752    90       ""                                                                                           
MIRE-6         Comment               BottomLayer MIRE_PLACE_SMD_0P8MM                13.0000      2.4500       180      ""                                                                                           
MIRE-4         Comment               BottomLayer MIRE_PLACE_SMD_0P8MM                39.7500      44.2500      180      ""                                                                                           
MIRE-5         Comment               BottomLayer MIRE_PLACE_SMD_0P8MM                2.7500       44.2500      180      ""                                                                                           
MIRE-3         Comment               TopLayer    MIRE_PLACE_SMD_0P8MM                2.5000       2.4500       0        ""                                                                                           
MIRE-2         Comment               TopLayer    MIRE_PLACE_SMD_0P8MM                39.7500      44.2500      0        ""                                                                                           
MIRE-1         Comment               TopLayer    MIRE_PLACE_SMD_0P8MM                2.7500       44.2500      0        ""                                                                                           
X1             XTAL_2_PINS           TopLayer    CRY_NX2012SA_2P                     28.9000      32.4000      90       "Crystal, 32.768kHz, 7pF, +/-20ppm, 80K, 2.05x1.2mm"                                         
X2             XTAL_4_PINS           TopLayer    CRY_NX1612SA_4P                     15.3800      25.7750      0        "Crystal, 48MHz, 8pF, +/-10 ppm, 22R, 1.6x1.2mm"                                             
U1             STM32WL33             TopLayer    ICC_QFN48-EPAD-4P5X4P5_6X6_P040     23.3500      25.3500      180      "IC, Programmable Sub-1GHz wireless SoC"                                                     
SC7            Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0981-46R               29.5000      13.7745      0        "shield clip Harwin S0981-46R to fix RF shielded cavity - SMT RFI Shield Clip, Corner (T+R)" 
SC3            Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0981-46R               29.5000      34.7745      90       "shield clip Harwin S0981-46R to fix RF shielded cavity - SMT RFI Shield Clip, Corner (T+R)" 
SC2            Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0981-46R               13.5000      34.7745      180      "shield clip Harwin S0981-46R to fix RF shielded cavity - SMT RFI Shield Clip, Corner (T+R)" 
SC6            Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0981-46R               13.5000      13.7745      270      "shield clip Harwin S0981-46R to fix RF shielded cavity - SMT RFI Shield Clip, Corner (T+R)" 
SC5            Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0951-46R               31.5000      29.4330      90       "shield clip Harwin S0951-46R to fix RF shielded cavity"                                     
SC1            Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0951-46R               18.6500      36.7750      180      "shield clip Harwin S0951-46R to fix RF shielded cavity"                                     
SC4            Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0951-46R               11.5000      29.4330      90       "shield clip Harwin S0951-46R to fix RF shielded cavity"                                     
SB15           SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              33.2875      4.9375       0        "Resistor, 0R, SB0402, 5%, 0.063W"                                                           
SB14           SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              9.3125       5.2000       0        "Resistor, 0R, SB0402, 5%, 0.063W"                                                           
SB3            SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              33.5875      31.2500      0        "Resistor, 0R, SB0402, 5%, 0.063W"                                                           
SB19           SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              33.2875      1.5625       0        "Resistor, 0R, SB0402, 5%, 0.063W"                                                           
SB4            SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              33.5875      30.1500      0        "Resistor, 0R, SB0402, 5%, 0.063W"                                                           
SB18           SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              33.2125      2.6875       180      "Resistor, 0R, SB0402, 5%, 0.063W"                                                           
SB12           SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              9.2375       7.1250       180      "Resistor, 0R, SB0402, 5%, 0.063W"                                                           
SB16           SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              9.3125       3.9500       0        "Resistor, 0R, SB0402, 5%, 0.063W"                                                           
SB13           SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              33.2875      6.0625       0        "Resistor, 0R, SB0402, 5%, 0.063W"                                                           
SB8            SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              33.2125      10.5625      180      "Resistor, 0R, SB0402, 5%, 0.063W"                                                           
SB5            SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              33.7875      19.8250      0        "Resistor, 0R, SB0402, 5%, 0.063W"                                                           
R7             Resistor              TopLayer    R0402                               26.9750      3.8750       270      "Resistor, 47R, 0402, +/-1%, 1/16W"                                                          
R6             Resistor              TopLayer    R0402                               26.9750      7.0500       270      "Resistor, 47R, 0402, +/-1%, 1/16W"                                                          
R5             Resistor              TopLayer    R0402                               24.0500      9.9500       90       "Resistor, 47R, 0402, +/-1%, 1/16W"                                                          
R8             Resistor              TopLayer    R0402                               26.9750      2.0750       270      "Resistor, 100R, 0402, +/- 1%, 1/16W"                                                        
R2             Resistor              TopLayer    R0402                               33.4750      24.0500      90       "Resistor, 100K, 0402, +/-1%, 1/16W"                                                         
R4             Resistor              TopLayer    R0402                               20.2250      9.9500       90       "Resistor, 47R, 0402, +/-1%, 1/16W"                                                          
R3             Resistor              TopLayer    R0402                               18.9500      9.9500       90       "Resistor, 47R, 0402, +/-1%, 1/16W"                                                          
L1             Inductor              TopLayer    L0402                               21.5500      39.9000      90       "Resistor, 0R, 0402, +/-5%, 1/16W"                                                           
CN4            mmcx                  TopLayer    CON_SMA-RF_CINCH_142-0701-851       21.5500      44.4600      0        "Jack_SMA, VR, PCB edge, 50R, T=7.92mm"                                                      
CN3            "Header 7x2"          TopLayer    CON_SAMTEC_FTSH-107-01-L-DV-K-A     21.5000      5.4650       0        "Header, 7x2, 1.27mm, VR, T=5.97mm, FTSH series STDC14 without Alignment Pin"                
CN2            FTSH-125-02-L-DV      BottomLayer CON_SAMTEC_FTSH-125-02-L-DV_INV     38.6560      18.5480      270      "Header, 25x2, 12.7mm, VR, SMD, T=4.83mm"                                                    
CN1            FTSH-125-02-L-DV      BottomLayer CON_SAMTEC_FTSH-125-02-L-DV_INV     4.3660       18.5480      270      "Header, 25x2, 12.7mm, VR, SMD, T=4.83mm"                                                    
C13            Capacitor             TopLayer    C0402                               29.3500      30.5250      180      "Capacitor, MLCC, 6.8pF, 50V, C0G, +/-0.05pF, 0402, T=0.5mm"                                 
C9             Capacitor             TopLayer    C0402                               29.3500      34.2750      180      "Capacitor, MLCC, 6.8pF, 50V, C0G, +/-0.05pF, 0402, T=0.5mm"                                 
C5             Capacitor             TopLayer    C0402                               17.1250      29.4050      270      "Capacitor, MLCC, 100pF, 50V, COG, 1%, 0402, T=0.5mm"                                        
C1             Capacitor             TopLayer    C0402                               22.0000      41.2500      180      "Capacitor, MLCC, 1pF, 50V, NPO, +/-0.1pF, 0402, T=0.5mm"                                    
C2             Capacitor             TopLayer    C0402                               22.0000      38.5500      180      "Capacitor, MLCC, 1pF, 50V, NPO, +/-0.1pF, 0402, T=0.5mm"                                    
C21            Capacitor             TopLayer    C0402                               23.7500      20.0750      90       "Capacitor, MLCC, 220nF, 35V, X6S, +/-10%, 0402, T=0.5mm"                                    
C23            Capacitor             TopLayer    C0402                               22.3910      19.6220      180      "Capacitor, MLCC, 100nF, 25V, X7R, +/-10%, X7R, 0402, T=0.5mm"                               
C7             Capacitor             TopLayer    C0402                               20.9057      29.9022      180      "Capacitor, MLCC, 100pF, 50V, COG, +/-1%, 0402, T=0.5mm"                                     
C15            Capacitor             TopLayer    C0402                               14.5750      28.4500      270      "Capacitor, MLCC, 100nF, ±10%, X7R, 25V, 0402, T=0.5mm"                                      
C14            Capacitor             TopLayer    C0402                               13.6250      28.4500      90       "Capacitor, MLCC, 100pF, 50V, COG, 1%, 0402, T=0.5mm"                                        
C20            Capacitor             TopLayer    C0402                               16.7906      20.2520      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                    
C16            Capacitor             TopLayer    C0402                               18.1750      26.9250      0        "Capacitor, MLCC, 100nF, 25V, X7R, +/-10%, X7R, 0402, T=0.5mm"                               
C17            Capacitor             TopLayer    C0402                               27.3750      22.5000      90       "Capacitor, MLCC, 100nF, 25V, X7R, +/-10%, X7R, 0402, T=0.5mm"                               
C22            Capacitor             TopLayer    C0402                               22.3910      20.4720      0        "Capacitor, MLCC, 4.7uF, 10V, X5R, +/-20%, 0402, T=0.5mm"                                    
C19            Capacitor             TopLayer    C0402_H0P5                          19.4750      21.9250      270      "Capacitor, MLCC, 22pF, 50V, C0G, +/-5%, 0402, T=0.5mm"                                      
C18            Capacitor             TopLayer    C0402                               18.4934      20.7408      90       "Capacitor, MLCC, 4.7uF, 10V, X5R, +/-20%, 0402, T=0.5mm"                                    
