Altium Designer Pick and Place Locations
C:\Users\Jorda\Documents\Projets\STM Le Mans\MB2119A\BASE\MB2119A\02-Manufacturing\MB2119A_PCB\Assembly\MB2119A_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       17/10/23
Time:       14:48
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator  Comment                        Layer       Footprint                           Center-X(mm) Center-Y(mm) Rotation Description                                                                                  
TP1         "Test Point"                   TopLayer    TP_SMD_1MM                          22.8816      23.0435      180      "Test Point 1mm"                                                                             
U2          MLPF-WB55-01E3                 TopLayer    ICC_CSPG_6BUMPS_1X1P60_P050-P0577   19.8374      37.3634      0        "2.4 GHz low pass filter matched to BLUENRG-LP-LPS"                                          
C7          Capacitor                      TopLayer    C0201_H0P3                          19.5834      35.6870      90       "Capacitor, MLCC, 20pF, 25V, COG, +/-2%, 0201, T=0.3mm"                                      
MIRE2       Comment                        TopLayer    MIRE_PLACE_SMD_0P8MM                39.2500      1.7500       0        ""                                                                                           
MIRE1       Comment                        TopLayer    MIRE_PLACE_SMD_0P8MM                1.5000       39.7500      0        ""                                                                                           
MIRE3       Comment                        TopLayer    MIRE_PLACE_SMD_0P8MM                2.2500       1.5000       0        ""                                                                                           
MIRE5       Comment                        BottomLayer MIRE_PLACE_SMD_0P8MM                39.2500      1.7500       0        ""                                                                                           
MIRE4       Comment                        BottomLayer MIRE_PLACE_SMD_0P8MM                1.5000       39.7500      0        ""                                                                                           
MIRE6       Comment                        BottomLayer MIRE_PLACE_SMD_0P8MM                2.2500       1.5000       0        ""                                                                                           
HW2         STICKER_PRODUCT                TopLayer    STICKER_PRODUCT_25X5                -275.4530    -237.3752    90       "Sticker product 25x5 mm"                                                                    
HW3         STICKER_BOARD                  TopLayer    STICKER_BOARD_25X5                  -275.4530    -237.3752    90       "Sticker board 25x5 mm"                                                                      
HW1         S02-20150300                   TopLayer    SHIELD_HARWIN_S02-20150300_15X20_H3 -275.4530    -237.3752    0        "RFI shield can, 20x15x3mm"                                                                  
C20         Capacitor                      BottomLayer C0402                               18.6500      26.6000      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                    
C17         Capacitor                      TopLayer    C0402                               17.1500      36.5000      270      "Capacitor, MLCC, 100nF, +/-10%, X7R, 25V, 0402, T=0.5mm"                                    
Designator2 Comment                        TopLayer    PCB_SPECIFICATIONS                  -275.4530    -237.3752    0        ""                                                                                           
Designator3 Comment                        TopLayer    Sheetbox_4L2S                       40.7858      -30.4310     0        ""                                                                                           
L1          Inductor                       TopLayer    C0402                               16.4846      27.7114      0        "Inductor, MLCC, 22nH, +/-2%, 350mA, 0.58R, 0402, T=1.45mm"                                  
C18         Capacitor                      TopLayer    C0402                               18.0000      36.5000      270      "Capacitor, MLCC, 3pF, COG, 50V, +/-0.1pF, 0402, T=0.5mm"                                    
U1          STM32WB07                      TopLayer    ICC_QFN48-EPAD-4P5X4P5_6X6_P040     20.9750      31.7250      180      "IC, Bluetooth Low Energy wireless SoC, QFN48"                                               
SB21        SB_ON                          TopLayer    SOLDER-BRIDGE_R0402-0R              13.2250      28.1581      270      "Resistor, 0R, SB0402, 5%, 0.063W"                                                           
SB20        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2875      10.6500      0        "Solder Bridge 0402 ON"                                                                      
SB19        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2875      9.6250       0        "Solder Bridge 0402 ON"                                                                      
SB18        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2875      27.7000      0        "Solder Bridge 0402 ON"                                                                      
SB17        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              10.8023      29.5852      180      "Solder Bridge 0402 ON"                                                                      
SB16        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2125      16.0000      180      "Solder Bridge 0402 ON"                                                                      
SB15        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.1875      22.2500      180      "Solder Bridge 0402 ON"                                                                      
SB14        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2875      28.7250      0        "Solder Bridge 0402 ON"                                                                      
SB13        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2875      29.7500      0        "Solder Bridge 0402 ON"                                                                      
SB12        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2875      32.0250      0        "Solder Bridge 0402 ON"                                                                      
SB11        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2875      31.0000      0        "Solder Bridge 0402 ON"                                                                      
SB10        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2875      4.3000       0        "Solder Bridge 0402 ON"                                                                      
SB9         SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2875      5.3250       0        "Solder Bridge 0402 ON"                                                                      
SB8         SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2875      8.4000       0        "Solder Bridge 0402 ON"                                                                      
R10         Resistor                       TopLayer    R0402                               19.5762      45.0000      270      "Resistor, 0R, 0402, +/-5%, 1/16W"                                                           
SB1         SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              11.7250      33.1875      90       "Solder Bridge 0402 ON"                                                                      
R1          Resistor                       TopLayer    R0402                               19.5762      42.4500      90       "Resistor, 0R, 0402, +/-5%, 1/16W"                                                           
R2          Resistor                       TopLayer    r0402                               19.1262      42.0000      180      "Resistor, 0R, 0402, +/-5%, 1/16W"                                                           
SC2         Shield-clip_S0951-46R          TopLayer    CLIP_HARWIN_S0981-46R               24.0000      38.4500      90       "shield clip Harwin S0981-46R to fix RF shielded cavity - SMT RFI Shield Clip, Corner (T+R)" 
SC3         Shield-clip_S0951-46R          TopLayer    CLIP_HARWIN_S0951-46R               11.0000      33.2000      90       "shield clip Harwin S0951-46R to fix RF shielded cavity"                                     
SC1         Shield-clip_S0951-46R          TopLayer    CLIP_HARWIN_S0981-46R               13.0000      38.4500      180      "shield clip Harwin S0981-46R to fix RF shielded cavity - SMT RFI Shield Clip, Corner (T+R)" 
SC7         Shield-clip_S0951-46R          TopLayer    CLIP_HARWIN_S0981-46R               13.0000      22.4500      270      "shield clip Harwin S0981-46R to fix RF shielded cavity - SMT RFI Shield Clip, Corner (T+R)" 
SC8         Shield-clip_S0951-46R          TopLayer    CLIP_HARWIN_S0981-46R               24.0000      22.4500      0        "shield clip Harwin S0981-46R to fix RF shielded cavity - SMT RFI Shield Clip, Corner (T+R)" 
SC5         Shield-clip_S0951-46R          TopLayer    CLIP_HARWIN_S0951-46R               11.0000      27.7000      90       "shield clip Harwin S0951-46R to fix RF shielded cavity"                                     
SC4         Shield-clip_S0951-46R          TopLayer    CLIP_HARWIN_S0951-46R               26.0000      33.2000      90       "shield clip Harwin S0951-46R to fix RF shielded cavity"                                     
SC6         Shield-clip_S0951-46R          TopLayer    CLIP_HARWIN_S0951-46R               26.0000      27.7000      90       "shield clip Harwin S0951-46R to fix RF shielded cavity"                                     
SB7         SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2875      7.3750       0        "Solder Bridge 0402 ON"                                                                      
L2          Inductor                       TopLayer    IND_0805_MURATA_LQM21               14.7320      27.9400      270      "Inductor, MLCC, 10uH, +/-20%, 300mA, 845mR, 0805, T=1.45mm"                                 
JP1         "Jumper_Header 3x1 Fitted 2-3" TopLayer    CON_SAMTEC_TSW-103-07-F-S           30.7500      32.5000      270      "Header, 3x1, 2.54mm, VR, TH, T=5.84mm/2.54mm"                                               
C2          Capacitor                      TopLayer    C0402_MURATA_GRM155_H0P5            20.0262      43.6500      180      "Capacitor, MLCC, 0.9pF, 25V, +/-0.05pF, 0402, T=0.5mm"                                      
ANT1        2.4GHz_BT_ANT                  TopLayer    ANT_BT_BNRG_2P4GHZ_MB2032           19.5962      47.2500      90       "2.4 GHZ Bluetooth BNRG PCB antenna"                                                         
CN4         U.FL-R-SMT-1                   TopLayer    CON_HRS_U.FL-R-SMT-1                15.3262      42.7500      0        "Connector_RF, 0Hz to 6GHz, 50R, VR, SMD, T= 1.25mm"                                         
SB6         SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              10.0375      25.2500      0        "Solder Bridge 0402 ON"                                                                      
SB2         SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              11.2297      31.1875      270      "Solder Bridge 0402 ON"                                                                      
CN3         "Header 7x2"                   TopLayer    CON_SAMTEC_FTSH-107-01-L-DV-K-A     22.1014      4.5794       0        "Header, 7x2, 1.27mm, VR, T=5.97mm, FTSH series STDC14 without Alignment Pin"                
CN2         FTSH-125-02-L-DV               BottomLayer CON_SAMTEC_FTSH-125-02-L-DV         38.6564      18.5484      270      "Header, 25x2, 12.7mm, VR, SMD, T=4.83mm"                                                    
CN1         FTSH-125-02-L-DV               BottomLayer CON_SAMTEC_FTSH-125-02-L-DV         4.3664       18.5484      270      "Header, 25x2, 12.7mm, VR, SMD, T=4.83mm"                                                    
SB4         SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2125      6.3500       180      "Solder Bridge 0402 ON"                                                                      
SB3         SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2125      11.6750      180      "Solder Bridge 0402 ON"                                                                      
C5          Capacitor                      TopLayer    C0402                               21.7170      37.0332      180      "Capacitor, MLCC, 3pF, COG, 50V, +/-0.1pF, 0402, T=0.5mm"                                    
C6          Capacitor                      TopLayer    C0402                               21.7170      37.8714      180      "Capacitor, MLCC, 100nF, +/-10%, X7R, 25V, 0402, T=0.5mm"                                    
C16         Capacitor                      TopLayer    C0402                               16.0274      31.4198      0        "Capacitor, MLCC, 0.22uF, X5R, 6.3V, +/-10%, 0402, T=0.5mm"                                  
C13         Capacitor                      TopLayer    C0402                               16.0274      29.7942      180      "Capacitor, MLCC, 100nF, ±10%, X7R, 25V, 0402, T=0.5mm"                                      
C4          Capacitor                      TopLayer    C0402                               18.8722      26.3652      90       "Capacitor, MLCC, 100nF, +/-10%, X7R, 25V, 0402, T=0.5mm"                                    
C3          Capacitor                      TopLayer    C0402                               16.0250      33.5000      0        "Capacitor, MLCC, 100nF, +/-10%, X7R, 25V, 0402, T=0.5mm"                                    
X1          XTAL_4_PINS                    TopLayer    CRY_NX2016SA_4P                     14.3640      35.8750      90       "Crystal, 32MHz, 8pF, +/-10ppm, 60R, 2x1.6mm"                                                
X2          XTAL_2_PINS                    TopLayer    CRY_NX2012SA_2P                     13.8430      32.3850      90       "Crystal, 32.768kHz, 7pF, +/-20ppm, 80K, 2.05x1.2mm"                                         
SB5         SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              10.0375      26.5000      0        "Solder Bridge 0402 ON"                                                                      
R4          Resistor                       BottomLayer R0402                               25.9091      9.8750       90       Resistor,47R,0402,1%,1/16W                                                                   
R8          Resistor                       BottomLayer R0402                               26.7500      5.0000       270      Resistor,47R,0402,1%,1/16W                                                                   
R5          Resistor                       BottomLayer R0402                               24.6510      9.8750       90       Resistor,47R,0402,1%,1/16W                                                                   
R9          Resistor                       BottomLayer R0402                               23.0000      5.0000       270      "Resistor, 100R, 0402, +/- 1%, 1/16W"                                                        
R6          Resistor                       BottomLayer R0402                               20.8250      9.8750       90       Resistor,47R,0402,1%,1/16W                                                                   
R7          Resistor                       BottomLayer R0402                               19.5500      9.8750       90       Resistor,47R,0402,1%,1/16W                                                                   
R3          Resistor                       TopLayer    R0402                               30.7500      27.5000      90       "Resistor, 100K, 0402, +/-1%, 1/16W"                                                         
C10         Capacitor                      TopLayer    C0402                               20.1750      26.3500      90       "Capacitor, MLCC, 100nF, +/-10%, X7R, 25V, 0402, T=0.5mm"                                    
C12         Capacitor                      TopLayer    C0402                               17.2212      26.3652      90       "Capacitor, MLCC, 4.7uF, X5R, 10 V, 0402, ± 20%, T=0.5mm"                                    
C15         Capacitor                      TopLayer    C0402                               21.0000      26.3500      90       "Capacitor, MLCC, 100nF, ±10%, X7R, 25V, 0402, T=0.5mm"                                      
C11         Capacitor                      TopLayer    C0402                               18.0594      26.3652      90       "Capacitor, MLCC, 100nF, ±10%, X7R, 25V, 0402, T=0.5mm"                                      
C14         Capacitor                      TopLayer    C0402                               16.0274      30.6070      0        "Capacitor, MLCC, 4.7uF, X5R, 10 V, 0402, ± 20%, T=0.5mm"                                    
C9          Capacitor                      TopLayer    C0402                               12.5770      31.2601      90       "Capacitor, MLCC, 8.2pF, 50V, NPO, +/-4%, 0402, T=0.5mm"                                     
C8          Capacitor                      TopLayer    C0402                               12.5770      33.7250      270      "Capacitor, MLCC, 8.2pF, 50V, NPO, +/-4%, 0402, T=0.5mm"                                     
C1          Capacitor                      TopLayer    C0402                               20.0262      46.3500      180      "Capacitor, MLCC, 6.8pF, 50V, C0G, +/-0.05pF, 0402, T=0.5mm"                                 
