Altium Designer Pick and Place Locations
C:\Users\Jorda\Documents\Projets\STM Le Mans\MB2130A\BASE\MB2130A\02-Manufacturing\MB2130A_PCB\Assembly\MB2130A_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       23/02/24
Time:       09:46
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator  Comment                     Layer       Footprint                         Center-X(mm) Center-Y(mm) Rotation Description                                                                 
R15         Resistor                    BottomLayer R0402                             33.5098      5.2070       180      "Resistor, 100K, 0402, +/-1%, 1/16W"                                        
SB11        SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R            23.6341      22.7076      0        "Solder Bridge 0402 ON"                                                     
SB13        SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R            33.3260      17.2974      180      "Solder Bridge 0402 ON"                                                     
HW1         "RF Shield (22.2x19.2x2mm)" TopLayer    SHIELD_RF_ST-CUSTOM_22P2X19P2_H2  -275.4530    -237.3752    0        "RF Shield (22.2x19.2x2mm)"                                                 
C21         Capacitor                   TopLayer    C0402                             23.3426      20.7772      90       "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                     
SB19        SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R            10.0463      1.9812       180      "Solder Bridge 0402 ON"                                                     
MIRE5       Comment                     BottomLayer MIRE_PLACE_SMD_0P8MM              41.5764      1.4478       180      ""                                                                          
MIRE6       Comment                     BottomLayer MIRE_PLACE_SMD_0P8MM              1.4464       1.4406       180      ""                                                                          
MIRE4       Comment                     BottomLayer MIRE_PLACE_SMD_0P8MM              1.4464       39.8628      180      ""                                                                          
MIRE2       Comment                     TopLayer    MIRE_PLACE_SMD_0P8MM              41.5764      1.4478       0        ""                                                                          
MIRE3       Comment                     TopLayer    MIRE_PLACE_SMD_0P8MM              1.4464       1.4406       0        ""                                                                          
MIRE1       Comment                     TopLayer    MIRE_PLACE_SMD_0P8MM              1.4464       39.8628      0        ""                                                                          
U1          MLPF-WB-04D3                TopLayer    ICC_CSPG_6BUMPS_1X1P60_P050-P0577 17.5188      32.4262      180      "IC, 2.4 GHz low pass filter matched to WBA mini board"                     
CN3         SMA-J-P-H-ST-EM1            TopLayer    CON_ROSENBERGER_32K141_40ML5      37.5926      39.0144      270      "Straight Jack PCB SMA connector"                                           
ANT1        2.4GHz_BT_ANT               TopLayer    ANT_BT_BNRG_2P4GHZ_MB2032         17.7889      44.0656      90       "2.4 GHZ Bluetooth BNRG PCB antenna"                                        
C32         Capacitor                   BottomLayer C0402                             10.0080      3.3062       180      "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                     
Designator1 Comment                     TopLayer    Sheetbox_4L2S                     40.0447      -24.7904     0        ""                                                                          
SB17        SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R            22.1609      5.5880       0        "Solder Bridge 0402 ON"                                                     
R9          Resistor                    TopLayer    R0402                             27.8130      12.3698      270      "Resistor, 0R, 0402, +/-5%, 1/16W"                                          
R8          Resistor                    TopLayer    R0402                             26.5430      12.3698      270      "Resistor, 0R, 0402, +/-5%, 1/16W"                                          
R7          Resistor                    TopLayer    R0402                             25.2730      12.3698      270      "Resistor, 0R, 0402, +/-5%, 1/16W"                                          
R6          Resistor                    TopLayer    R0402                             23.9776      12.3698      270      "Resistor, 0R, 0402, +/-5%, 1/16W"                                          
R5          Resistor                    TopLayer    R0402                             22.7076      12.3698      270      "Resistor, 0R, 0402, +/-5%, 1/16W"                                          
CN4         "Header 10x2"               TopLayer    CON_SAMTEC_FTSH-110-01-L-DV       22.1010      4.5790       0        "Header, 10x2, 1.27mm, VR, SMD, T=3.05mm"                                   
CN1         FTSH-125-02-L-DV            BottomLayer CON_SAMTEC_FTSH-125-02-L-DV_INV   4.3664       18.5484      270      "Header, 25x2, 12.7mm, VR, SMD, T=4.83mm"                                   
CN2         FTSH-125-02-L-DV            BottomLayer CON_SAMTEC_FTSH-125-02-L-DV_INV   38.6564      18.5484      270      "Header, 25x2, 12.7mm, VR, SMD, T=4.83mm"                                   
"PCB SPEC1" Comment                     TopLayer    PCB_SPECIFICATIONS                -275.4530    -237.3752    0        ""                                                                          
R14         Resistor                    TopLayer    R0402                             27.8130      9.7028       90       "Resistor, 0R, 0402, +/-5%, 1/16W"                                          
C17         Capacitor                   TopLayer    C0402                             18.8722      22.8600      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                   
C15         Capacitor                   TopLayer    C0402                             14.9860      25.6032      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                   
C6          Capacitor                   TopLayer    C0402                             19.8072      33.6550      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                   
C7          Capacitor                   TopLayer    C0402                             26.4414      33.7566      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                   
C8          Capacitor                   TopLayer    C0402                             30.0482      32.1564      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                   
C14         Capacitor                   TopLayer    C0402                             30.3022      25.9080      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                   
L4          Inductor                    TopLayer    C0402                             20.7010      21.5138      270      "Inductor, 10nH, +/-2%, 0.5A, 260mR, 0402, T=0.5mm"                         
SB8         SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R            26.9119      28.3718      180      "Solder Bridge 0402 ON"                                                     
SB5         SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R            26.9266      29.4425      180      "Solder Bridge 0402 ON"                                                     
SB18        SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R            33.2994      2.3368       0        "Solder Bridge 0402 ON"                                                     
L5          Inductor                    TopLayer    L0805_H0P9                        20.7010      19.1008      270      "Inductor, 2.2uH, +/-20%, 0.7A, 0R156, 0805, T=0.9mm"                       
L3          Inductor                    TopLayer    IND_0603_H0P8                     17.6784      21.1328      270      "Ferrite bead, 47R @ 100MHz, +/-25%, 3.5A, 0R02, 0603, T=0.8mm"             
C19         Capacitor                   TopLayer    C0402                             26.3906      21.5392      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                   
C22         Capacitor                   TopLayer    C0402                             24.2570      20.7772      90       "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                     
C9          Capacitor                   TopLayer    C0402                             15.2654      31.5976      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                   
C16         Capacitor                   TopLayer    C0402                             14.9860      24.7904      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                   
C31         Capacitor                   BottomLayer C0402                             33.1349      3.3274       0        "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                     
L1          Inductor                    TopLayer    C0402                             17.7800      42.0116      90       "Inductor, 1.8nH, +/-0.3nH, 9500 mA, 0.08Ohm, 0402, T=0.5mm"                
SB14        SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R            9.8431       16.8402      180      "Solder Bridge 0402 ON"                                                     
SB10        SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R            9.8430       24.5666      180      "Solder Bridge 0402 ON"                                                     
SB3         SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R            9.8548       34.8226      180      "Solder Bridge 0402 ON"                                                     
U2          STM32WBA65RI                TopLayer    ICC_VFQFPN68-EPAD_8X8_P040        23.1141      27.5800      90       "MCU, ARM Cortex-M33, 2MB Flash, KB SRAM, Crypto, RF 2.4GHz, BLE, 802.15.4" 
SB15        SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R            10.6559      14.7320      180      "Solder Bridge 0402 ON"                                                     
SB12        SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R            10.0209      21.3360      180      "Solder Bridge 0402 ON"                                                     
C4          Capacitor                   TopLayer    C0402                             32.1404      38.5599      90       "Capacitor, MLCC, 1.8pF, 50V, C0G, +/-0.25pF, 0402, T=0.5mm"                
C3          Capacitor                   TopLayer    C0402                             29.5149      38.5671      90       "Capacitor, MLCC, 1.5pF, 50V, C0G, +/-0.25pF, 0402, T=0.5mm"                
C23         Capacitor                   TopLayer    C0402                             17.7292      19.5072      0        "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                     
C20         Capacitor                   TopLayer    C0603                             18.9738      21.2090      90       "Capacitor, MLCC, 10uF, 6V3, X5R, +/-10%, 0603, T=0.8mm"                    
C30         Capacitor                   BottomLayer C0402                             8.4582       14.2748      90       "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                     
C27         Capacitor                   BottomLayer C0402                             10.0075      23.6268      180      "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                     
C26         Capacitor                   BottomLayer C0402                             10.0193      33.8320      180      "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                     
C28         Capacitor                   BottomLayer C0402                             10.0080      22.3520      180      "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                     
X1          XTAL_2_PINS                 TopLayer    CRY_NX1610SE_2P                   29.9974      29.1592      270      "Crystal, 32.768kHz, 6pF, +/-20ppm, 70KR, 1.6x1mm"                          
X2          XTAL_4_PINS                 TopLayer    CRY_NX1612SA_4P                   15.2908      28.9814      180      "Crystal, 32MHz, 8pF, +/-10ppm, 40R, 1612(metric), T=0.3mm"                 
SC3         Shield-clip_S0951-46R       TopLayer    CLIP_HARWIN_S0951-46R             9.1948       27.0002      90       "shield clip Harwin S0951-46R to fix RF shielded cavity"                    
SC5         Shield-clip_S0951-46R       TopLayer    CLIP_HARWIN_S0951-46R             27.0002      16.5354      180      "shield clip Harwin S0951-46R to fix RF shielded cavity"                    
SC4         Shield-clip_S0951-46R       TopLayer    CLIP_HARWIN_S0951-46R             31.3944      23.7998      90       "shield clip Harwin S0951-46R to fix RF shielded cavity"                    
SC2         Shield-clip_S0951-46R       TopLayer    CLIP_HARWIN_S0951-46R             27.8384      35.7378      180      "shield clip Harwin S0951-46R to fix RF shielded cavity"                    
SC1         Shield-clip_S0951-46R       TopLayer    CLIP_HARWIN_S0951-46R             12.8524      35.7502      180      "shield clip Harwin S0951-46R to fix RF shielded cavity"                    
SB2         SB_ON                       TopLayer    SOLDER-BRIDGE_R0402-0R            13.3096      27.2663      90       "Solder Bridge 0402 ON"                                                     
SB1         SB_ON                       TopLayer    SOLDER-BRIDGE_R0402-0R            12.1666      27.1913      270      "Solder Bridge 0402 ON"                                                     
SB6         SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R            15.3537      29.4132      0        "Solder Bridge 0402 ON"                                                     
SB9         SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R            13.3725      27.8638      0        "Solder Bridge 0402 ON"                                                     
SB16        SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R            33.3514      7.1120       180      "Solder Bridge 0402 ON"                                                     
SB7         SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R            9.9435       28.9306      0        "Solder Bridge 0402 ON"                                                     
SB4         SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R            9.9298       29.9966      0        "Solder Bridge 0402 ON"                                                     
R13         Resistor                    TopLayer    R0402                             26.5430      9.7028       90       "Resistor, 0R, 0402, +/-5%, 1/16W"                                          
R12         Resistor                    TopLayer    R0402                             25.2730      9.7028       90       "Resistor, 0R, 0402, +/-5%, 1/16W"                                          
R11         Resistor                    TopLayer    R0402                             23.9776      9.7028       90       "Resistor, 0R, 0402, +/-5%, 1/16W"                                          
R10         Resistor                    TopLayer    R0402                             22.7076      9.7028       90       "Resistor, 0R, 0402, +/-5%, 1/16W"                                          
R1          Resistor                    TopLayer    R0402                             30.8103      39.0243      0        "Resistor, 0R, 0402, +/-5%, 1/16W"                                          
R3          Resistor                    TopLayer    R0402                             18.2153      36.7010      180      "Resistor, 0R, 0402, +/-5%, 1/16W"                                          
R2          Resistor                    TopLayer    R0402                             17.7653      37.1510      270      "Resistor, 0R, 0402, +/-5%, 1/16W"                                          
R4          Resistor                    TopLayer    R0402                             20.7216      33.6550      90       "Resistor, 100K, 0402, +/-1%, 1/16W"                                        
L2          Inductor                    TopLayer    IND_0603_H0P8                     12.5222      28.8544      180      "Ferrite bead, 47R @ 100MHz, +/-25%, 3.5A, 0R02, 0603, T=0.8mm"             
C24         Capacitor                   TopLayer    C0402                             18.2880      18.2626      90       "Capacitor, MLCC, 2.2uF, 6V3, X5R,+/-10%, 0402, T=0.5mm"                    
C25         Capacitor                   TopLayer    C0402                             19.1770      18.2626      270      "Capacitor, MLCC, 4.7uF, 6V3, X5R, +/-20%, 0402, T=0.5mm"                   
C18         Capacitor                   TopLayer    C0402                             28.2956      21.7678      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                   
C5          Capacitor                   TopLayer    C0603                             15.7987      33.4020      270      "Capacitor, MLCC, 470nF, 16V, X7R, +/-10%, 0603, T=0.8mm"                   
C13         Capacitor                   TopLayer    C0402                             15.6210      26.9240      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                   
C1          Capacitor                   TopLayer    C0402                             17.3482      43.2308      0        "Capacitor, MLCC, 3.9pF, 50V, C0G, +/-0.25pF, 0402, T=0.5mm"                
C2          Capacitor                   TopLayer    C0402                             17.3228      40.8178      180      "Capacitor, MLCC, 1.5pF, 50V, C0G, +/-0.25pF, 0402, T=0.5mm"                
C29         Capacitor                   BottomLayer C0402                             8.4582       16.3576      270      "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                     
C11         Capacitor                   TopLayer    C0402                             15.2654      30.4800      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                   
C12         Capacitor                   TopLayer    C0402                             30.1752      27.7876      180      "Capacitor, MLCC, 6pF, 50V, NPO, +/-0,25pF, 0402, T=0.5mm"                  
C10         Capacitor                   TopLayer    C0402                             30.3022      30.9372      270      "Capacitor, MLCC, 6pF, 50V, NPO, +/-0,25pF, 0402, T=0.5mm"                  
