Altium Designer Pick and Place Locations
C:\Subversion\MB2131-STM32WBA55-tinyBluefish-128K-M2_connectivity_expension_board\Trunk\02-Manufacturing\MB2131B_PCB\Assembly\MB2131-B02_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       26/02/25
Time:       15:49
Revision:   53
Variant:    WBA5M
Units used: mm

Designator   Comment                     Layer       Footprint                                       Center-X(mm) Center-Y(mm) Rotation Description                                                                                                                                                    
Designator11 Comment                     BottomLayer STICKER_PRODUCT_20X9                            -353.9500    -228.0000    180      ""                                                                                                                                                             
SB19         SB_ON                       TopLayer    SOLDER-BRIDGE_R0402-0R                          3.7500       22.2875      90       "Resistor, 0R, SB0402, 5%, 0.063W"                                                                                                                             
Designator9  Comment                     BottomLayer MIRE_PLACE_SMD_0P8MM                            1.6925       10.7508      180      ""                                                                                                                                                             
Designator8  Comment                     BottomLayer MIRE_PLACE_SMD_0P8MM                            20.3388      37.9264      180      ""                                                                                                                                                             
Designator7  Comment                     BottomLayer MIRE_PLACE_SMD_0P8MM                            1.7000       51.3250      180      ""                                                                                                                                                             
Designator6  Comment                     TopLayer    MIRE_PLACE_SMD_0P8MM                            20.3388      46.0907      0        ""                                                                                                                                                             
Designator5  Comment                     TopLayer    MIRE_PLACE_SMD_0P8MM                            1.5517       54.4461      0        ""                                                                                                                                                             
Designator4  Comment                     TopLayer    MIRE_PLACE_SMD_0P8MM                            4.6500       6.4500       0        ""                                                                                                                                                             
U11          ISM330DHCX                  TopLayer    ICC_LGA14_3X2P5_P050                            8.9000       23.5250      90       "MEMS, iNEMO inertial module with embedded Machine Learning Core: always-on 3D accelerometer and 3D gyroscope with digital output for industrial applications" 
CARTOUCH-1   Comment                     TopLayer    Sheetbox_2L2S                                   12.6013      -27.8750     0        ""                                                                                                                                                             
SB2          SB_ON                       TopLayer    SOLDER-BRIDGE_R0402-0R                          14.9400      31.8025      270      "Resistor, 0R, SB0402, 5%, 0.063W"                                                                                                                             
B1           SW-PUSH-CMS_KMR2_BLACK      TopLayer    SWI_C&K_Y78B23110FP__ITT_KMR231GLFS             19.2000      39.7500      270      "Switch tactile, SPST-NO, 32V, 50mA, 2.8x4.6mm"                                                                                                                
SB21         SB_ON                       TopLayer    SOLDER-BRIDGE_R0402-0R                          12.7000      24.0375      270      "Resistor, 0R, SB0402, 5%, 0.063W"                                                                                                                             
U12          M24128-DFMC6TP              TopLayer    ICC_DFN8-EPAD_2X3_P050                          18.7000      24.5150      270      "Memory, EEPROM, 1V7 to 5V5, 256Kbit, 1MHz, DFN-8"                                                                                                             
U10          SHT4X                       TopLayer    ICC_SENSOR_SHT40-AD1B-R2_DFN4-EPAD_1P5X1P5_P050 15.2250      27.4000      0        "Sensor, High-Accuracy, Ultra-Low-Power, 16-bit  Relative Humidity and Temperature"                                                                            
U9           ESD-TRANSIL                 TopLayer    ESD_QFN1610_2N_1K_2A                            12.4000      15.8250      0        "Diode, ESD TVS, 22V, 200nA, 25V8, QFN1610"                                                                                                                    
U8           LD39050PU33R                TopLayer    ICC_DFN6-EPAD_3X3_P095                          15.0000      21.1000      90       "LDO, 500mA, Low quiescent current and low noise voltage regulator"                                                                                            
U7           AP22814ASN-7                TopLayer    ICC_DFN2020-6-EPAD_2X2_P065                     2.7250       26.9500      0        "IC, Power Switch, 2V7 to 5V5, 3A"                                                                                                                             
U6           ESD-TRANSIL                 TopLayer    ESD_ST0201                                      6.8750       10.6250      0        "Diode, ESD TVS, 3V, 100nA, 8V, ST0201"                                                                                                                        
U5           ESD-TRANSIL                 TopLayer    ESD_ST0201                                      4.5411       10.6379      180      "Diode, ESD TVS, 3V, 100nA, 8V, ST0201"                                                                                                                        
U4           ESDALC6V1W5                 TopLayer    ESD_SOT323-5L                                   10.2500      18.5000      0        "Diode, ESD Transil, 3V, 1uA, 7V2, SOT323-5"                                                                                                                   
U3           ESD-TRANSIL                 TopLayer    ESD_ST0201                                      20.2125      34.5500      0        "Diode, ESD TVS, 3V, 100nA, 8V, ST0201"                                                                                                                        
U1           ESD-TRANSIL                 TopLayer    ESD_ST0201                                      20.2500      43.0000      0        "Diode, ESD TVS, 3V, 100nA, 8V, ST0201"                                                                                                                        
U2           STM32WBA5M                  TopLayer    MOD_STM_76P_8X12P5_H1P37                        9.6325       49.2625      0        "STM32 Module with RF  integer"                                                                                                                                
SB25         SB_ON                       TopLayer    SOLDER-BRIDGE_R0402-0R                          18.1000      26.6625      270      "Resistor, 0R, SB0402, 5%, 0.063W"                                                                                                                             
SB24         SB_ON                       TopLayer    SOLDER-BRIDGE_R0402-0R                          19.2500      22.1625      90       "Resistor, 0R, SB0402, 5%, 0.063W"                                                                                                                             
SB22         SB_ON                       TopLayer    SOLDER-BRIDGE_R0402-0R                          12.1875      22.3750      180      "Resistor, 0R, SB0402, 5%, 0.063W"                                                                                                                             
SB20         SB_ON                       TopLayer    SOLDER-BRIDGE_R0402-0R                          17.7125      20.1501      180      "Resistor, 0R, SB0402, 5%, 0.063W"                                                                                                                             
SB18         SB_ON                       TopLayer    SOLDER-BRIDGE_R0402-0R                          5.5500       25.4875      90       "Resistor, 0R, SB0402, 5%, 0.063W"                                                                                                                             
SB16         SB_ON                       TopLayer    SOLDER-BRIDGE_R0402-0R                          5.3000       28.9625      90       "Resistor, 0R, SB0402, 5%, 0.063W"                                                                                                                             
SB15         SB_ON                       TopLayer    SOLDER-BRIDGE_R0402-0R                          1.9250       23.6875      90       "Resistor, 0R, SB0402, 5%, 0.063W"                                                                                                                             
SB6          SB_ON                       TopLayer    SOLDER-BRIDGE_R0402-0R                          3.7000       32.8875      270      "Resistor, 0R, SB0402, 5%, 0.063W"                                                                                                                             
SB5          SB_ON                       TopLayer    SOLDER-BRIDGE_R0402-0R                          15.1250      46.0500      0        "Resistor, 0R, SB0402, 5%, 0.063W"                                                                                                                             
SB4          SB_ON                       TopLayer    SOLDER-BRIDGE_R0402-0R                          9.3250       39.0125      270      "Resistor, 0R, SB0402, 5%, 0.063W"                                                                                                                             
SB3          SB_ON                       TopLayer    SOLDER-BRIDGE_R0402-0R                          18.5375      43.0000      0        "Resistor, 0R, SB0402, 5%, 0.063W"                                                                                                                             
SB1          SB_ON                       TopLayer    SOLDER-BRIDGE_R0402-0R                          13.0375      33.8500      180      "Resistor, 0R, SB0402, 5%, 0.063W"                                                                                                                             
R17          Resistor                    TopLayer    R0402                                           12.0000      14.0000      180      "Resistor, 5K1, 0402, +/-1%, 1/16W"                                                                                                                            
R16          Resistor                    TopLayer    R0402                                           12.0000      13.0000      180      "Resistor, 5K1, 0402, +/-1%, 1/16W"                                                                                                                            
R15          Resistor                    TopLayer    R0402                                           5.6250       30.3750      180      "Resistor, 620R, 0402, +/-1%, 1/16W"                                                                                                                           
R14          Resistor                    TopLayer    R0402                                           2.5750       10.6750      180      "Resistor, 100R, 0402, +/- 1%, 1/16W"                                                                                                                          
R8           Resistor                    TopLayer    R0402                                           15.5250      47.3750      270      "Resistor, 3K3, 0402, +/-1%, 1/16W"                                                                                                                            
R7           Resistor                    TopLayer    R0402                                           9.3000       37.2250      90       "Resistor, 3K3, 0402, +/-1%, 1/16W"                                                                                                                            
R6           Resistor                    TopLayer    R0402                                           6.8038       39.8445      270      "Resistor, 150R, 0402, +/-1%, 1/16W"                                                                                                                           
R5           Resistor                    TopLayer    R0402                                           3.4750       35.3000      90       "Resistor, 3K3, 0402, +/-1%, 1/16W"                                                                                                                            
R4           Resistor                    TopLayer    R0402                                           2.5000       35.3000      90       "Resistor, 3K3, 0402, +/-1%, 1/16W"                                                                                                                            
R2           Resistor                    TopLayer    R0402                                           14.7000      51.1250      270      "Resistor, 0R, 0402, +/-5%, 1/16W"                                                                                                                             
LD2          LED_green                   TopLayer    LED_0603_OSRAM_LG-Q396-PS-35_GREEN_1A2K_H0P4    6.6900       28.5747      270      "LED, Green, 2V, 20mA, 0603"                                                                                                                                   
LD1          LED_blue                    TopLayer    LED_0603_OSRAM_LB-Q39G-L2OO-35-1_BLUE_1A2K_H0P4 6.8000       37.6000      90       "LED, Blue, 2V85, 5mA, 0603"                                                                                                                                   
CN4          USB_TYPE_C_Receptacle       TopLayer    CON_USB-TYPEC_AMPHENOL_12401826E412A            16.7700      14.0000      90       "USB_TypeC, 24 pins, RA, SMD, T=2.96mm"                                                                                                                        
CN3          "Header 7x2"                TopLayer    CON_STDC14_Receiver_SMALL                       5.4250       15.8250      270      "Header, 7x2, 1.27mm, VR, SMD, T=5.97mm"                                                                                                                       
CN2          M2_MALE-CONNECTOR_KEY-E_3V3 TopLayer    CON_BOARD_GOLDFINGER_PCI_EXPRESS_X75_M2_KEY-E   11.0625      1.2000       0        "M.2 Male connector (NGFF), 67pins, keyE"                                                                                                                      
C14          Capacitor                   TopLayer    C0402                                           17.7250      22.8500      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                                                      
C13          Capacitor                   TopLayer    C0402                                           10.8750      24.5250      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                                                      
C12          Capacitor                   TopLayer    C0402                                           10.8750      22.9000      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                                                      
C11          Capacitor                   TopLayer    C0402                                           16.7250      27.5000      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                                                      
C10          Capacitor                   TopLayer    C0402                                           12.6000      17.3500      180      "Capacitor, MLCC, 100pF, 50V, NPO, +/-5%, 0402, T=0.5mm"                                                                                                       
C7           Capacitor                   TopLayer    C0402                                           12.6000      18.9250      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                                                      
C6           Capacitor                   TopLayer    C0402                                           12.6000      18.1250      180      "Capacitor, MLCC, 1uF, 25V, X5R, +/-10%, 0402, T=0.5mm"                                                                                                        
C9           Capacitor                   TopLayer    C0402                                           14.2500      23.5000      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                                                      
C8           Capacitor                   TopLayer    C0402                                           14.2500      24.2500      180      "Capacitor, MLCC, 1uF, 25V, X5R, +/-10%, 0402, T=0.5mm"                                                                                                        
C5           Capacitor                   TopLayer    C0402                                           2.4500       25.3500      180      "Capacitor, MLCC, 1uF, 25V, X5R, +/-10%, 0402, T=0.5mm"                                                                                                        
C4           Capacitor                   TopLayer    C0402                                           4.3500       28.2000      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                                                      
C3           Capacitor                   TopLayer    C0402                                           4.6750       44.3250      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                                                                                      
C2           Capacitor                   TopLayer    C0603                                           4.4500       42.3000      90       "Capacitor, MLCC, 4.7uF, 16V, X5R, +/-10%, 0603, T=0.8mm"                                                                                                      
B2           SW-PUSH-CMS_KMR2_BLACK      TopLayer    SWI_C&K_Y78B23110FP__ITT_KMR231GLFS             19.2000      30.5750      270      "Switch tactile, SPST-NO, 32V, 50mA, 2.8x4.6mm"                                                                                                                
