Altium Designer Pick and Place Locations
C:\Reference_design\boards\02-Manufacturing\MB2161A_PCB\Assembly\MB2161A_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       05/08/24
Time:       08:43
Revision:   Not in VersionControl
Variant:    Variant A
Units used: mm

Designator   Comment               Layer    Footprint                           Center-X(mm) Center-Y(mm) Rotation Description                                                                                 
HW1          S02-20150300          TopLayer SHIELD_HARWIN_S02-20150300_15X20_H3 -63.8710     -61.9050     90       "RFI shield can, 20x15x3mm"                                                                 
Designator16 Comment               TopLayer IMPEDANCE_TABLE                     -63.8710     -61.9050     0        ""                                                                                          
C11          Capacitor             TopLayer C0402                               19.7000      15.9500      270      "Capacitor, MLCC, 100nF, +/-10%, X7R, 25V, 0402, T=0.5mm"                                   
L2           Inductor              TopLayer C0402                               19.5000      17.5500      0        "Inductor, MLCC, 22nH, +/-2%, 350mA, 0.58R, 0402, T=1.45mm"                                 
C4           Capacitor             TopLayer C0201_H0P3                          20.7510      18.3044      0        "Capacitor, MLCC,100nF, 10V, X5R, +/-10%, 0201, T=0.3mm"                                    
C3           Capacitor             TopLayer C0402                               20.5550      19.1045      0        "Capacitor, MLCC, 4.7uF, X5R, 10V, +/-20%, 0402, T=0.5mm"                                   
SC7          Shield-clip_S0951-46R TopLayer CLIP_HARWIN_S0951-46R               13.6754      15.9324      270      "RFI shield clip mini TIN SMD"                                                              
L1           Inductor              TopLayer IND_0805_MURATA_LQM21               17.6077      16.6020      90       "Inductor, MLCC, 10uH, +/-20%, 300mA, 845mR, 0805, T=1.45mm"                                
C6           Capacitor             TopLayer 20p_capacitor_SMD_0201              32.2904      15.5024      90       "Capacitor, MLCC, 20pF, 25V, COG, +/-2%, 0201, T=0.3mm"                                     
C13          Capacitor             TopLayer 0_5p_capacitor_SMD_0201             28.3447      15.8734      90       "0201 0.3 pF 25 V ±0.05 pF Tolerance C0G SMT Multilayer Ceramic Capacitor"                  
C12          Capacitor             TopLayer 0_8p_capacitor_SMD_0201             27.3488      15.7683      0        "Multilayer Ceramic Capacitor, 0.8 pF, 25 V, ± 0.05pF, C0G (NP0), 0201 [0603 Metric]"       
C14          Capacitor             TopLayer 1_5p_capacitor_SMD_0201             29.3524      15.8033      0        "Multilayer Ceramic Capacitor, 1.5 pF, 25 V, ± 0.1pF, C0G (NP0), 0201 [0603 Metric]"        
C15          Capacitor             TopLayer 0_8p_capacitor_SMD_0201             31.3263      15.2317      180      "Multilayer Ceramic Capacitor, 0.8 pF, 25 V, ± 0.05pF, C0G (NP0), 0201 [0603 Metric]"       
L3           Inductor              TopLayer 2n4_inductor_SMD_0201               28.3457      15.1484      90       "Inductor RF Chip Thin Film 2.4nH 0.1nH 500MHz 14Q-Factor 500mA 200mOhm DCR 0201 Paper T/R" 
L4           Inductor              TopLayer 3n3_inductor_SMD_0201               30.3443      15.5024      90       "Inductor RF Chip Thin Film 3.3nH 0.1nH 500MHz 14Q-Factor 450mA 250mOhm DCR 0201 Paper T/R" 
C5           Capacitor             TopLayer C0402                               28.5000      17.5000      135      "Capacitor, MLCC, 1uF, X7R, 6.3V,+/- 10%, 0402, T=0.5mm"                                    
J1           SMA_connector         TopLayer SMA_AMPHENOL_132415                 38.5909      15.5000      180      "Rf Connector, Sma End Launch Recept Jack For .032" Pcb / Individual Bag"                   
SC8          Shield-clip_S0951-46R TopLayer CLIP_HARWIN_S0951-46R               26.4254      8.3582       180      "RFI shield clip mini TIN SMD"                                                              
SC9          Shield-clip_S0951-46R TopLayer CLIP_HARWIN_S0951-46R               20.9254      8.3582       180      "RFI shield clip mini TIN SMD"                                                              
SC6          Shield-clip_S0951-46R TopLayer CLIP_HARWIN_S0951-46R               26.4254      23.3582      180      "RFI shield clip mini TIN SMD"                                                              
SC5          Shield-clip_S0951-46R TopLayer CLIP_HARWIN_S0951-46R               20.9254      23.3582      180      "RFI shield clip mini TIN SMD"                                                              
SC4          Shield-clip_S0951-46R TopLayer CLIP_HARWIN_S0981-46R               15.6754      10.3582      270      "Shield clip Harwin S0981-46R to fix RF shielded cavity"                                    
SC3          Shield-clip_S0951-46R TopLayer CLIP_HARWIN_S0981-46R               31.6754      10.3582      0        "Shield clip Harwin S0981-46R to fix RF shielded cavity"                                    
SC2          Shield-clip_S0951-46R TopLayer CLIP_HARWIN_S0981-46R               15.6754      21.3582      180      "Shield clip Harwin S0981-46R to fix RF shielded cavity"                                    
SC1          Shield-clip_S0951-46R TopLayer CLIP_HARWIN_S0981-46R               31.6754      21.3582      90       "Shield clip Harwin S0981-46R to fix RF shielded cavity"                                    
X2           XTAL_4_PINS           TopLayer CRY_NX2016SA_4P                     27.4000      20.0000      270      "Crystal, 32MHz, 8pF, +/-10ppm, 60R, 2x1.6mm"                                               
X1           XTAL_2_PINS           TopLayer CRY_NX2012SA_2P                     23.7000      20.4000      0        "Crystal, 32.768kHz, 7pF, +/-20ppm, 80K, 2.05x1.2mm"                                        
U1           STM32WB09             TopLayer ICC_QFN32-EPAD_5X5_P050             23.7160      14.7500      0        "Bluetooth® Low Energy wireless SoC"                                                        
C10          Capacitor             TopLayer C0402                               19.3067      14.7000      0        "Capacitor, MLCC, 0.22uF, X5R, 6.3V, +/-10%, 0402, T=0.5mm"                                 
C9           Capacitor             TopLayer C0402                               28.6500      13.7500      225      "Capacitor, MLCC, 1uF, X7R, 6.3V,+/- 10%, 0402, T=0.5mm"                                    
C8           Capacitor             TopLayer C0402                               20.0500      12.2000      90       "Capacitor, MLCC, 1uF, X7R, 6.3V,+/- 10%, 0402, T=0.5mm"                                    
C7           Capacitor             TopLayer C0402                               18.9500      15.9500      270      "Capacitor, MLCC, 4.7uF, X5R, 10V, +/-20%, 0402, T=0.5mm"                                   
C2           Capacitor             TopLayer C0402                               24.6500      22.2500      180      "Capacitor, MLCC, 10pF, 50V, NPO, +/-5%, 0402, T=0.5mm"                                     
C1           Capacitor             TopLayer C0402                               22.4372      22.2500      180      "Capacitor, MLCC, 10pF, 50V, NPO, +/-5%, 0402, T=0.5mm"                                     
