Altium Designer Pick and Place Locations
C:\Users\galvagng\OneDrive - STMicroelectronics\Documents\Validation Reference Design\Zip folder to stwebsite publication\MB2218\MB2218A\Project Outputs\02-Manufacturing\MB2218A_PCB\Assembly\MB2218A_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       09/01/25
Time:       12:28
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator     Comment               Layer       Footprint                           Center-X(mm) Center-Y(mm) Rotation Description                                                                                  
C7             Capacitor             BottomLayer GRM155--GJM155-0_05-MFG             8.4200       13.8820      90       "Capacitor, MLCC, 100pF, 50V, COG, 1%, 0402, T=0.5mm"                                        
SB2            SB_ON                 TopLayer    SOLDER-BRIDGE_R0201_0R              19.0750      25.9000      180      "Resistor, 0R, 0201, Solder Bridge ON , 1/20W,"                                              
SB1            SB_ON                 TopLayer    SOLDER-BRIDGE_R0201_0R              19.0750      26.8205      180      "Resistor, 0R, 0201, Solder Bridge ON , 1/20W,"                                              
L9             Inductor              TopLayer    LQG15HH_02-IPC_C                    20.7253      17.7730      270      "Inductor, MLCC, 100nH, ±5%, 200mA, 1.25R, 0402, T=0.5mm"                                    
SC2            Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0981-46R               13.5000      34.7745      180      "shield clip Harwin S0981-46R to fix RF shielded cavity - SMT RFI Shield Clip, Corner (T+R)" 
SC13           Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0951-46R               24.0900      11.7750      180      "RFI shield clip mini TIN SMD"                                                               
SC12           Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0951-46R               31.5000      19.1200      90       "RFI shield clip mini TIN SMD"                                                               
SC11           Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0951-46R               11.5000      24.2780      270      "RFI shield clip mini TIN SMD"                                                               
SC10           Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0951-46R               31.5000      24.2780      90       "RFI shield clip mini TIN SMD"                                                               
SC9            Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0951-46R               11.5000      19.1200      270      "RFI shield clip mini TIN SMD"                                                               
SB10           SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              33.2125      8.3125       180      "Solder Bridge 0402 ON"                                                                      
SB11           SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              33.2125      7.1875       180      "Solder Bridge 0402 ON"                                                                      
SB7            SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              33.2125      11.6875      180      "Solder Bridge 0402 ON"                                                                      
SB17           SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              33.2125      3.8125       180      "Solder Bridge 0402 ON"                                                                      
SB6            SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              33.2875      12.8125      0        "Solder Bridge 0402 ON"                                                                      
SB9            SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              33.2875      9.4375       0        "Solder Bridge 0402 ON"                                                                      
STICKER-BOARD1 Comment               TopLayer    STICKER_BOARD_25X5                  -265.4530    -237.3752    90       ""                                                                                           
STICKER-PROD1  Comment               TopLayer    STICKER_PRODUCT_25X5                -265.4530    -237.3752    90       ""                                                                                           
MIRE-6         Comment               BottomLayer MIRE_PLACE_SMD_0P8MM                13.0000      2.4500       180      ""                                                                                           
MIRE-4         Comment               BottomLayer MIRE_PLACE_SMD_0P8MM                39.7500      44.2500      180      ""                                                                                           
MIRE-5         Comment               BottomLayer MIRE_PLACE_SMD_0P8MM                2.7500       44.2500      180      ""                                                                                           
MIRE-3         Comment               TopLayer    MIRE_PLACE_SMD_0P8MM                2.5000       2.4500       0        ""                                                                                           
MIRE-2         Comment               TopLayer    MIRE_PLACE_SMD_0P8MM                39.7500      44.2500      0        ""                                                                                           
MIRE-1         Comment               TopLayer    MIRE_PLACE_SMD_0P8MM                2.7500       44.2500      0        ""                                                                                           
HW1            S02-20150300          TopLayer    SHIELD_HARWIN_S02-25200300_20X25_H3 -265.4530    -237.3752    0        "RFI shield CAN, 25x20x3mm"                                                                  
X1             XTAL_2_PINS           TopLayer    CRY_NX2012SA_2P                     28.9000      30.5000      90       "Crystal, 32.768kHz, 7pF, +/-20ppm, 80K, 2.05x1.2mm"                                         
X2             XTAL_4_PINS           TopLayer    CRY_NX1612SA_4P                     15.3800      23.8750      0        "Crystal, 48MHz, 8pF, +/-10 ppm, 22R, 1.6x1.2mm"                                             
U1             STM32WL33             TopLayer    ICC_QFN48-EPAD-4P5X4P5_6X6_P040     23.3500      23.4500      180      "IC, Programmable Sub-1GHz wireless SoC"                                                     
SC7            Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0981-46R               29.5000      13.7745      0        "shield clip Harwin S0981-46R to fix RF shielded cavity - SMT RFI Shield Clip, Corner (T+R)" 
SC3            Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0981-46R               29.5000      34.7745      90       "shield clip Harwin S0981-46R to fix RF shielded cavity - SMT RFI Shield Clip, Corner (T+R)" 
SC6            Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0981-46R               13.5000      13.7745      270      "shield clip Harwin S0981-46R to fix RF shielded cavity - SMT RFI Shield Clip, Corner (T+R)" 
SC8            Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0951-46R               18.8900      11.7745      180      "shield clip Harwin S0951-46R to fix RF shielded cavity"                                     
SC5            Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0951-46R               31.5000      29.4330      90       "shield clip Harwin S0951-46R to fix RF shielded cavity"                                     
SC1            Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0951-46R               18.7500      36.7750      180      "shield clip Harwin S0951-46R to fix RF shielded cavity"                                     
SC4            Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0951-46R               11.5000      29.4330      90       "shield clip Harwin S0951-46R to fix RF shielded cavity"                                     
SB15           SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              33.2875      4.9375       0        "Solder Bridge 0402 ON"                                                                      
SB14           SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              9.3125       5.2000       0        "Solder Bridge 0402 ON"                                                                      
SB3            SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              33.5875      31.2500      0        "Solder Bridge 0402 ON"                                                                      
SB19           SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              33.2875      1.5625       0        "Solder Bridge 0402 ON"                                                                      
SB4            SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              33.5875      30.1500      0        "Solder Bridge 0402 ON"                                                                      
SB18           SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              33.2125      2.6875       180      "Solder Bridge 0402 ON"                                                                      
SB12           SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              9.2375       7.1250       180      "Solder Bridge 0402 ON"                                                                      
SB16           SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              9.3125       3.9500       0        "Solder Bridge 0402 ON"                                                                      
SB13           SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              33.2875      6.0625       0        "Solder Bridge 0402 ON"                                                                      
SB8            SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              33.2125      10.5625      180      "Solder Bridge 0402 ON"                                                                      
SB5            SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R              33.7875      19.8250      0        "Solder Bridge 0402 ON"                                                                      
R7             Resistor              TopLayer    R0402                               26.9750      3.8750       270      Resistor,47R,0402,1%,1/16W                                                                   
R6             Resistor              TopLayer    R0402                               26.9750      7.0500       270      Resistor,47R,0402,1%,1/16W                                                                   
R5             Resistor              TopLayer    R0402                               24.0500      9.9500       90       Resistor,47R,0402,1%,1/16W                                                                   
R8             Resistor              TopLayer    R0402                               26.9750      2.0750       270      Resistor,47R,0402,1%,1/16W                                                                   
R2             Resistor              TopLayer    R0402                               33.4750      24.0500      90       "Resistor, 100K, 0402, +/-1%, 1/16W"                                                         
R4             Resistor              TopLayer    R0402                               20.2250      9.9500       90       Resistor,47R,0402,1%,1/16W                                                                   
R3             Resistor              TopLayer    R0402                               18.9500      9.9500       90       Resistor,47R,0402,1%,1/16W                                                                   
L1             Inductor              TopLayer    L0402                               21.5500      39.9000      90       "Resistor, 0R, 0402, +/-5%, 1/16W"                                                           
L3             Inductor              TopLayer    L0402                               24.5500      34.4250      0        "Inductor, MLCC, 5.6nH, ±0.3nH, 650mA, 180mR, 0402, T=0.5mm"                                 
L4             Inductor              TopLayer    L0402                               24.1000      32.9000      90       "Inductor, 6.8nH, +/-3%, 0.6A, 220mR, 0402, T=0.5mm"                                         
L6             Inductor              TopLayer    LQW15AN_00-W0_6-0_1-MFG             21.5500      30.1500      90       "Inductor, 15nH, +/-2%, Itemp=460mA max, 0R16, 0402, T= 0.6mm, Qmin=30"                      
L2             Inductor              TopLayer    LQW15AN_00-W0_6-0_1-MFG             17.9750      34.0000      90       "Inductor, Wire-wound, 5.6nH, ±0.1nH, 1770mA, 40mR, 0402, T=0.5mm"                           
L5             Inductor              TopLayer    LQW15AN_00-W0_6-0_1-MFG             17.2750      30.9000      90       "Inductor, Wire-wound, 6.2nH, ±0.1nH, 1600mA, 56mR, 0402, T=0.5mm"                           
L7             Inductor              TopLayer    LQW15AN_00-W0_6-0_1-MFG             17.2750      27.8500      90       "Inductor, Wire-wound, 3.6nH, ±0.1nH, 1950mA, 30mR, 0402, T=0.5mm"                           
L8             Inductor              TopLayer    LQW15AN_00-W0_6-0_1-MFG             16.8100      26.1000      0        "Inductor, Wire-wound, 12nHH, ±2%, 500mA, 1405mR, 0402, T=0.5mm"                             
L10            Inductor              TopLayer    LQM21FN_70-IPC_C                    21.6629      16.0080      180      "Inductor, 10uH, +/-20%, 100mA, 1R36, 0805, T=0.8mm"                                         
CN4            mmcx                  TopLayer    CON_SMA-RF_CINCH_142-0701-851       21.5500      44.4600      0        "Jack_SMA, VR, PCB edge, 50R, T=7.92mm"                                                      
CN3            "Header 7x2"          TopLayer    CON_SAMTEC_FTSH-107-01-L-DV-K-A     21.5000      5.4650       0        "Header, 7x2, 1.27mm, VR, T=5.97mm, FTSH series STDC14 without Alignment Pin"                
CN2            FTSH-125-02-L-DV      BottomLayer CON_SAMTEC_FTSH-125-02-L-DV_INV     38.6560      18.5480      270      "Header, 25x2, 12.7mm, VR, SMD, T=4.83mm"                                                    
CN1            FTSH-125-02-L-DV      BottomLayer CON_SAMTEC_FTSH-125-02-L-DV_INV     4.3660       18.5480      270      "Header, 25x2, 12.7mm, VR, SMD, T=4.83mm"                                                    
C13            Capacitor             TopLayer    GRM155--GJM155-0_05-MFG             29.3500      28.6250      180      "Capacitor, MLCC, 6.8pF, ±0.05pF, C0G, 50V, 0402, T=0.5mm"                                   
C9             Capacitor             TopLayer    GRM155--GJM155-0_05-MFG             29.3500      32.3750      180      "Capacitor, MLCC, 6.8pF, ±0.05pF, C0G, 50V, 0402, T=0.5mm"                                   
C5             Capacitor             TopLayer    GRM155--GJM155-0_05-MFG             20.2000      34.4250      180      "Capacitor, MLCC, 100pF, 50V, COG, 1%, 0402, T=0.5mm"                                        
C1             Capacitor             TopLayer    GRM155--GJM155-0_05-MFG             21.9500      41.2500      180      "Capacitor, MLCC, 1pF, 50V, NPO, +/-0.1pF, 0402, T=0.5mm"                                    
C2             Capacitor             TopLayer    GRM155--GJM155-0_05-MFG             21.9500      38.5500      180      "Capacitor, MLCC, 1pF, 50V, NPO, +/-0.1pF, 0402, T=0.5mm"                                    
C21            Capacitor             TopLayer    GRM155--GJM155-0_05-MFG             23.7500      18.1750      90       "Capacitor, MLCC, 220nF, 35V, X6S, +/-10%, 0402, T=0.5mm"                                    
C3             Capacitor             TopLayer    GRM155--GJM155-0_05-MFG             21.9500      37.7751      180      "Capacitor, MLCC, 100pF, 50V, COG, +/-1%, 0402, T=0.5mm"                                     
C23            Capacitor             TopLayer    GRM155--GJM155-0_05-MFG             22.5500      18.3210      180      "Capacitor, MLCC, 100nF, ±10%, X7R, 25V, 0402, T=0.5mm"                                      
C15            Capacitor             TopLayer    GRM155--GJM155-0_05-MFG             14.5750      26.5000      270      "Capacitor, MLCC, 100nF, ±10%, X7R, 25V, 0402, T=0.5mm"                                      
C14            Capacitor             TopLayer    GRM155--GJM155-0_05-MFG             13.6250      26.5000      90       "Capacitor, MLCC, 100pF, 50V, COG, 1%, 0402, T=0.5mm"                                        
C26            Capacitor             TopLayer    C0603                               15.8750      3.0250       270      "Capacitor, MLCC, 1uF, 16V, X5R, 10%, 0603, T=0,8mm"                                         
C20            Capacitor             TopLayer    GRM155--GJM155-0_05-MFG             17.1720      18.3520      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                    
C10            Capacitor             TopLayer    GRM155--GJM155-0_05-MFG             21.1500      31.6750      0        "Capacitor, MLCC, 1.5pF, 50V, C0G, +/-0.25pF, 0402, T=0.5mm"                                 
C12            Capacitor             TopLayer    GRM155--GJM155-0_05-MFG             21.1500      28.6250      0        "Capacitor, MLCC, 0.5pF, 50V, C0G, +/-0.1pF, 0402, T=0.5mm"                                  
C16            Capacitor             TopLayer    GRM155--GJM155-0_05-MFG             18.7755      24.9846      0        "Capacitor, MLCC, 100nF, +/-10%, X7R, 25V, 0402, T=0.5mm"                                    
C17            Capacitor             TopLayer    GRM155--GJM155-0_05-MFG             27.1629      21.6500      90       "Capacitor, MLCC, 100nF, +/-10%, X7R, 25V, 0402, T=0.5mm"                                    
C4             Capacitor             TopLayer    GRM155--GJM155-0_05-MFG             16.8250      35.4750      0        "Capacitor, MLCC, 2.7pF, 50V, C0G, +/-0.05pF, C0G, 0402, T=0.5mm"                            
C8             Capacitor             TopLayer    GRM155--GJM155-0_05-MFG             16.8600      32.4250      0        "Capacitor, MLCC, 5.6pF, 50V, NPO, +/-0.1pF, 0402, T=0.5mm"                                  
C11            Capacitor             TopLayer    GRM155--GJM155-0_05-MFG             16.8600      29.3750      0        "Capacitor, MLCC, 5.3pF, 50V, C0G, +/-0.1pF, 0402, T=0.5mm"                                  
C6             Capacitor             TopLayer    GRM155--GJM155-0_05-MFG             16.8000      34.0250      90       "Capacitor, Monolithic CC, 1.2pF, 50V, +/-0.05pf, 0402, T=0.5mm"                             
C22            Capacitor             TopLayer    GRM155--GJM155-0_05-MFG             22.5500      17.5250      0        "Capacitor, MLCC, 4.7uF, X5R, 10 V, 0402, ± 20%, T=0.5mm"                                    
C19            Capacitor             TopLayer    GRM155--GJM155-0_05-MFG             19.8570      20.2250      90       "Capacitor, MLCC, 100nF, ±10%, X7R, 25V, 0402, T=0.5mm"                                      
C18            Capacitor             TopLayer    GRM155--GJM155-0_05-MFG             18.8517      18.9900      90       "Capacitor, MLCC, 4.7uF, X5R, 10 V, 0402, ± 20%, T=0.5mm"                                    
CART-1         Comment               TopLayer    Sheetbox_4L2S                       21.8436      -21.1484     0        ""                                                                                           
