Altium Designer Pick and Place Locations
C:\Subversion\01_Boards\MB2296_Miniboard_STM32WBA64CIU6_QFN48_SMA_LDO_USB\Trunk\02-Manufacturing\MB2296A_PCB\Assembly\MB2296A_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       09/09/24
Time:       10:34
Revision:   5
Variant:    No variations
Units used: mm

Designator Comment                     Layer       Footprint                        Center-X(mm) Center-Y(mm) Rotation Description                                                                   
C29        Capacitor                   TopLayer    C0603_H0P8                       15.4592      27.5865      180      "Capacitor, MLCC, 4.7uF, 10V, X5R, +/-10%, 0603, T=0.8mm"                     
U1         STM32WBA64CIU6              TopLayer    STM32WB64CGU6                    21.8948      30.6081      0        "STM32WBA64CIU6 QFN48_USB_LDO"                                                
SB8        SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           23.4442      12.3141      90       "Solder Bridge 0402 ON"                                                       
SB37       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           28.5742      30.6123      0        "Solder Bridge 0402 OFF"                                                      
C28        Capacitor                   TopLayer    C0402                            27.1233      26.1240      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
CN4        mmcx                        TopLayer    CON_SMA-RF_CINCH_142-0701-851    17.8186      44.1198      0        "Jack_SMA, VR, PCB edge, 50R, T=7.92mm"                                       
SH1        "RF Shield (22.2x19.2x2mm)" TopLayer    SHIELD_RF_ST-CUSTOM_22P2X19P2_H2 -275.4530    -237.3752    0        "RF Shield (22.2x19.2x2mm)"                                                   
SB43       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           9.8531       13.8804      180      "Solder Bridge 0402 OFF"                                                      
C27        Capacitor                   BottomLayer C0402                            10.0289      14.7823      180      "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                       
SB30       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           14.7912      17.6278      0        "Solder Bridge 0402 ON"                                                       
SB17       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           10.8579      8.2804       0        "Solder Bridge 0402 ON"                                                       
SB14       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           10.8712      7.2048       0        "Solder Bridge 0402 OFF"                                                      
SB10       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           31.6001      28.8225      0        "Solder Bridge 0402 ON"                                                       
SB42       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           29.5523      27.1272      0        "Solder Bridge 0402 ON"                                                       
SB6        SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           13.0840      28.4005      0        "Solder Bridge 0402 ON"                                                       
L1         Inductor                    TopLayer    C0402                            17.8308      36.1950      90       "Inductor, 1.8nH, +/-0.3nH, 0.95A, 80mR, 0402, T=0.5mm"                       
L2         Inductor                    TopLayer    C0402                            17.7964      38.7757      90       "Inductor, 3.3nH, +/-0.3nH, 0.8A,125mR, 0402, T=0.5mm"                        
SB4        SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           10.1636      17.1072      180      "Solder Bridge 0402 OFF"                                                      
SB3        SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           10.7817      24.2954      180      "Solder Bridge 0402 OFF"                                                      
SB2        SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           10.7263      33.8458      180      "Solder Bridge 0402 OFF"                                                      
CN3        "Header 7x2"                TopLayer    CON_SAMTEC_FTSH-107-01-L-DV-K-A  22.1014      4.5794       0        "Header, 7x2, 1.27mm, VR, T=5.97mm, FTSH series STDC14 without Alignment Pin" 
CN2        FTSH-125-02-L-DV            BottomLayer FTSH-125-02-L-DV                 38.6564      18.5484      180      "Header, 25x2, 12.7mm, VR, SMD, T=4.83mm"                                     
CN1        FTSH-125-02-L-DV            BottomLayer FTSH-125-02-L-DV                 4.3664       18.5484      180      "Header, 25x2, 12.7mm, VR, SMD, T=4.83mm"                                     
SB5        SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           32.4350      2.3430       0        "Solder Bridge 0402 OFF"                                                      
SB1        SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           10.8552      22.3294      180      "Solder Bridge 0402 OFF"                                                      
C19        Capacitor                   TopLayer    C0402                            15.6578      28.5752      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
C18        Capacitor                   TopLayer    C0402                            19.5456      36.2872      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
C17        Capacitor                   TopLayer    C0402                            27.4565      33.0519      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
C16        Capacitor                   TopLayer    C0402                            25.4739      25.8314      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
C15        Capacitor                   TopLayer    C0402                            15.6680      29.4139      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
C5         Capacitor                   BottomLayer C0402                            34.3248      2.8408       90       "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                       
C3         Capacitor                   BottomLayer C0402                            8.7818       24.1515      270      "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                       
C2         Capacitor                   BottomLayer C0402                            8.6490       34.2552      270      "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                       
C1         Capacitor                   BottomLayer C0402                            9.0496       21.8036      90       "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                       
X2         XTAL_4_PINS                 TopLayer    CRY_NX1612SA_4P                  15.0089      31.1725      0        "Crystal, 32MHz, 8pF, +/-10ppm, 40R, 1612(metric), T=0.3mm"                   
X1         XTAL_2_PINS                 TopLayer    CRY_NX1610SE_2P                  26.7462      29.8450      270      "Crystal, 32.768kHz, 6pF, +/-20ppm, 70KR, 1.6x1mm"                            
SC5        Shield-clip_S0951-46R       TopLayer    CLIP_HARWIN_S0951-46R            9.1846       31.0128      90       "shield clip Harwin S0951-46R to fix RF shielded cavity"                      
SC4        Shield-clip_S0951-46R       TopLayer    CLIP_HARWIN_S0951-46R            20.5020      20.7446      180      "shield clip Harwin S0951-46R to fix RF shielded cavity"                      
SC3        Shield-clip_S0951-46R       TopLayer    CLIP_HARWIN_S0951-46R            31.1821      29.9714      90       "shield clip Harwin S0951-46R to fix RF shielded cavity"                      
SC2        Shield-clip_S0951-46R       TopLayer    CLIP_HARWIN_S0951-46R            27.0002      39.7256      180      "shield clip Harwin S0951-46R to fix RF shielded cavity"                      
SC1        Shield-clip_S0951-46R       TopLayer    CLIP_HARWIN_S0951-46R            12.8619      39.7485      180      "shield clip Harwin S0951-46R to fix RF shielded cavity"                      
SB40       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           14.7474      32.2376      180      "Solder Bridge 0402 OFF"                                                      
SB39       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           12.8242      31.1166      180      "Solder Bridge 0402 OFF"                                                      
SB38       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           28.4237      28.5688      0        "Solder Bridge 0402 OFF"                                                      
SB36       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           32.4336      17.9410      0        "Solder Bridge 0402 OFF"                                                      
SB35       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           32.3298      21.7226      180      "Solder Bridge 0402 OFF"                                                      
SB34       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.3971      5.3594       0        "Solder Bridge 0402 ON"                                                       
SB33       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.3565      24.7894      180      "Solder Bridge 0402 ON"                                                       
SB32       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           27.6206      18.6501      180      "Solder Bridge 0402 OFF"                                                      
SB31       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.3971      19.7104      0        "Solder Bridge 0402 ON"                                                       
SB29       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.3895      10.6680      180      "Solder Bridge 0402 ON"                                                       
SB28       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           29.7946      17.9998      180      "Solder Bridge 0402 OFF"                                                      
SB27       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           29.8222      17.0752      180      "Solder Bridge 0402 OFF"                                                      
SB26       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.3451      22.7312      180      "Solder Bridge 0402 ON"                                                       
SB24       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.3126      15.1764      180      "Solder Bridge 0402 ON"                                                       
SB22       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           29.7783      13.9880      180      "Solder Bridge 0402 OFF"                                                      
SB21       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           16.4808      6.0397       90       "Solder Bridge 0402 ON"                                                       
SB20       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           27.6207      19.5311      180      "Solder Bridge 0402 OFF"                                                      
SB19       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           10.8876      9.3366       0        "Solder Bridge 0402 OFF"                                                      
SB18       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.4110      7.2742       0        "Solder Bridge 0402 ON"                                                       
SB16       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           32.4226      8.3714       0        "Solder Bridge 0402 OFF"                                                      
SB15       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.4020      11.8324      0        "Solder Bridge 0402 ON"                                                       
SB13       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           31.5858      29.7890      0        "Solder Bridge 0402 ON"                                                       
SB12       SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           32.4875      9.6978       180      "Solder Bridge 0402 OFF"                                                      
SB11       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.4264      26.7458      0        "Solder Bridge 0402 ON"                                                       
SB9        SB_OFF                      BottomLayer SOLDER-BRIDGE_R0402-0R           10.8718      6.2770       0        "Solder Bridge 0402 OFF"                                                      
SB7        SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R           32.4158      25.7670      0        "Solder Bridge 0402 ON"                                                       
R9         Resistor                    BottomLayer R0402                            27.0237      3.8997       270      Resistor,47R,0402,1%,1/16W                                                    
R8         Resistor                    BottomLayer R0402                            25.9224      9.8779       90       Resistor,47R,0402,1%,1/16W                                                    
R7         Resistor                    BottomLayer R0402                            24.6584      9.8529       90       Resistor,47R,0402,1%,1/16W                                                    
R6         Resistor                    BottomLayer R0402                            24.3864      2.6308       90       Resistor,47R,0402,1%,1/16W                                                    
R5         Resistor                    BottomLayer R0402                            23.3764      9.8779       90       Resistor,47R,0402,1%,1/16W                                                    
R4         Resistor                    BottomLayer R0402                            22.0924      9.8524       90       Resistor,47R,0402,1%,1/16W                                                    
R3         Resistor                    BottomLayer R0402                            20.8874      9.8779       90       Resistor,47R,0402,1%,1/16W                                                    
R2         Resistor                    BottomLayer R0402                            19.6054      9.8779       90       Resistor,47R,0402,1%,1/16W                                                    
R1         Resistor                    TopLayer    R0402                            11.1249      28.3196      270      "Resistor, 100K, 0402, +/-1%, 1/16W"                                          
L3         Inductor                    TopLayer    IND_0603_H0P8                    21.9950      24.1586      90       "Ferrite bead, 47R @ 100MHz, +/-25%, 3.5A, 0R02, 0603, T=0.8mm"               
HW4        STICKER_PRODUCT             TopLayer    STICKER_PRODUCT_25X5             -275.4530    -237.3752    90       "Sticker product 25x5 mm"                                                     
HW3        STICKER_BOARD               TopLayer    STICKER_BOARD_25X5               -275.4530    -237.3752    90       "Sticker board 25x5 mm"                                                       
D1         SCHOTTKY_1A_2K              TopLayer    DIO_SOD523_1A_2K                 12.8790      25.7837      180      "Small signal Schottky diodes"                                                
C22        Capacitor                   BottomLayer C0603                            20.2308      2.5544       90       "Capacitor, MLCC, 1uF, 16V, X5R, 10%, 0603, T=0,8mm"                          
C20        Capacitor                   TopLayer    C0402                            23.0632      24.0284      90       "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                       
C10        Capacitor                   TopLayer    C0402                            15.0279      32.3337      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
C14        Capacitor                   TopLayer    C0402_MURATA_GRM155_H0P5         17.3664      40.1574      0        "Capacitor, MLCC, 1pF, 50V, C0G, +/-0.1pF, 0402, T=0.5mm"                     
C13        Capacitor                   TopLayer    C0402                            17.3482      37.6174      0        "Capacitor, MLCC, 1.8pF, 50V, C0G, +/-0.25pF, 0402, T=0.5mm"                  
C12        Capacitor                   TopLayer    C0402                            17.2974      34.7726      0        "Capacitor, MLCC, 1.5pF, 50V, C0G, +/-0.25pF, 0402, T=0.5mm"                  
C11        Capacitor                   TopLayer    C0603                            15.5448      34.6202      270      "Capacitor, MLCC, 470nF, 16V, X7R, +/-10%, 0603, T=0.8mm"                     
C4         Capacitor                   BottomLayer C0402                            8.5040       16.5807      270      "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                       
C9         Capacitor                   TopLayer    C0402                            28.0416      30.4038      180      "Capacitor, MLCC, 6 pF, 50V, NPO, ±0,25pF, 0402, T=0.5mm"                     
C8         Capacitor                   TopLayer    C0402                            28.0416      29.3624      180      "Capacitor, MLCC, 6 pF, 50V, NPO, ±0,25pF, 0402, T=0.5mm"                     
C7         Capacitor                   TopLayer    C0402                            13.0421      24.7447      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
