Altium Designer Pick and Place Locations
C:\Subversion\Boards\MB2350_MCU_RF_Miniboard_STM32WBA2_QFN32_LDO\Trunk\02-Manufacturing\MB2350A_PCB\Assembly\MB2350A_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       29/09/25
Time:       16:20
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator Comment               Layer       Footprint                       Center-X(mm) Center-Y(mm) Rotation Description                                                                   
HW1        "Shield Cover"        TopLayer    SHIELD_WURTH_36003200_21P8X21P8 -275.4530    -237.3752    0        "RF Shield cover, 21.5x21.5x3.3mm"                                            
SB29       SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          13.4625      5.2926       180      "Solder Bridge 0402 ON"                                                       
C16        Capacitor             BottomLayer C0402                           9.0004       15.1892      270      "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                       
SB27       SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          28.1509      6.6477       0        "Solder Bridge 0402 ON"                                                       
SB26       SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          29.9625      28.0899      180      "Solder Bridge 0402 ON"                                                       
SB19       SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          29.9625      25.9516      180      "Solder Bridge 0402 ON"                                                       
SB10       SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          32.0750      25.4392      0        "Solder Bridge 0402 ON"                                                       
SB30       SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          9.1952       7.1184       0        "Solder Bridge 0402 ON"                                                       
SB28       SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          32.9625      31.9482      180      "Solder Bridge 0402 ON"                                                       
SB25       SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          31.9625      9.0119       180      "Solder Bridge 0402 ON"                                                       
SB24       SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          31.9631      10.9156      180      "Solder Bridge 0402 ON"                                                       
SB23       SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          10.9929      10.8597      0        "Solder Bridge 0402 ON"                                                       
SB22       SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          31.9625      13.2641      180      "Solder Bridge 0402 ON"                                                       
SB20       SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          9.2613       3.9687       0        "Solder Bridge 0402 ON"                                                       
SB18       SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          31.9625      22.7209      180      "Solder Bridge 0402 ON"                                                       
SB16       SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          30.0375      27.1405      0        "Solder Bridge 0402 ON"                                                       
SB14       SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          12.0287      17.8816      0        "Solder Bridge 0402 ON"                                                       
SB13       SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          31.9625      7.1184       180      "Solder Bridge 0402 ON"                                                       
SB12       SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          31.9625      5.8484       180      "Solder Bridge 0402 ON"                                                       
SB9        SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          13.9988      18.8826      180      "Solder Bridge 0402 ON"                                                       
SB8        SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          13.9572      17.8816      180      "Solder Bridge 0402 ON"                                                       
SB6        SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          10.9625      14.7734      180      "Solder Bridge 0402 ON"                                                       
SB42       SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          32.9625      33.1526      180      "Solder Bridge 0402 ON"                                                       
U1         IC_STM32WBA23KEU7     TopLayer    ICC_UFQFPN32-EPAD_5X5_P050      21.0138      31.5753      0        "MCU, ARM Cortex-M33 32-bit, 512KB Flash, 96KB RAM, Crypto"                   
CN4        SMA-J-P-H-ST-EM1      TopLayer    CON_SMA-RF_CINCH_142-0701-851   17.8540      50.4050      0        "Jack_SMA, VR, PCB edge, 50R, T=7.92mm"                                       
L1         Inductor              TopLayer    C0402                           17.8541      36.1064      90       "Inductor, 3.3nH, +/-0.3nH, 800 mA, 0.125Ohm, 0402, T=0.5mm"                  
L2         Inductor              TopLayer    C0402                           17.8536      38.7858      90       "Inductor, 3.3nH, +/-0.3nH, 800 mA, 0.125Ohm, 0402, T=0.5mm"                  
SB4        SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          10.9625      16.5599      180      "Solder Bridge 0402 ON"                                                       
SB3        SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          10.9625      24.1065      180      "Solder Bridge 0402 ON"                                                       
SB2        SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          10.9625      33.8458      180      "Solder Bridge 0402 ON"                                                       
CN3        "Header 7x2"          TopLayer    CON_SAMTEC_FTSH-107-01-L-DV-K-A 22.1014      4.5794       0        "Header, 7x2, 1.27mm, VR, T=5.97mm, FTSH series STDC14 without Alignment Pin" 
CN2        "Header 25x2"         BottomLayer FTSH-125-02-L-DV                38.6564      18.5484      180      "Header, 25x2, 1.27mm, VR, SMD, T=4.83mm"                                     
CN1        "Header 25x2"         BottomLayer FTSH-125-02-L-DV                4.3664       18.5484      180      "Header, 25x2, 1.27mm, VR, SMD, T=4.83mm"                                     
SB5        SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          32.0375      3.3084       0        "Solder Bridge 0402 ON"                                                       
SB1        SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          10.9625      22.3294      180      "Solder Bridge 0402 ON"                                                       
C19        Capacitor             TopLayer    C0402                           15.8259      29.4640      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
C18        Capacitor             TopLayer    C0402                           19.5627      36.5693      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
C17        Capacitor             TopLayer    C0402                           26.3259      33.5440      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
C15        Capacitor             TopLayer    C0402                           15.8259      30.3253      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
C5         Capacitor             BottomLayer C0402                           34.3188      2.9370       90       "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                       
C3         Capacitor             BottomLayer C0402                           9.0000       24.1515      270      "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                       
C2         Capacitor             BottomLayer C0402                           9.0000       34.2552      270      "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                       
C1         Capacitor             BottomLayer C0402                           9.0000       21.8036      90       "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                       
X2         XTAL_4_PINS           TopLayer    CRY_NX1612SA_4P                 14.7611      31.8253      0        "Crystal, 32MHz, 8pF, +/-10ppm, 40R, 1612(metric), T=0.3mm"                   
X1         XTAL_2_PINS           TopLayer    CRY_NX1610SE_2P                 25.4205      31.5228      270      "Crystal, 32.768kHz, 6pF, +/-20ppm, 70KR, 1.6x1mm"                            
SC5        Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0951-46R           9.1500       34.0130      90       "shield clip Harwin S0951-46R to fix RF shielded cavity"                      
SC4        Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0951-46R           19.2827      22.2670      180      "shield clip Harwin S0951-46R to fix RF shielded cavity"                      
SC3        Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0951-46R           30.6500      37.9030      90       "shield clip Harwin S0951-46R to fix RF shielded cavity"                      
SC2        Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0951-46R           27.2220      43.7420      180      "shield clip Harwin S0951-46R to fix RF shielded cavity"                      
SC1        Shield-clip_S0951-46R TopLayer    CLIP_HARWIN_S0951-46R           12.8619      43.7485      180      "shield clip Harwin S0951-46R to fix RF shielded cavity"                      
SB40       SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          14.9361      32.1978      180      "Solder Bridge 0402 ON"                                                       
SB39       SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          13.3840      30.6109      180      "Solder Bridge 0402 ON"                                                       
SB38       SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          27.1215      31.0695      0        "Solder Bridge 0402 ON"                                                       
SB37       SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          27.1211      32.0228      0        "Solder Bridge 0402 ON"                                                       
SB35       SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          31.9439      21.1055      180      "Solder Bridge 0402 ON"                                                       
SB33       SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          32.4352      30.1830      180      "Solder Bridge 0402 ON"                                                       
SB32       SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          28.7815      19.6004      180      "Solder Bridge 0402 ON"                                                       
SB31       SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          32.0255      19.5168      0        "Solder Bridge 0402 ON"                                                       
SB21       SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          32.0255      16.0084      0        "Solder Bridge 0402 ON"                                                       
SB17       SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          31.9625      17.1024      180      "Solder Bridge 0402 ON"                                                       
SB15       SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          10.9492      12.1501      0        "Solder Bridge 0402 ON"                                                       
SB11       SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          12.0287      18.8826      0        "Solder Bridge 0402 ON"                                                       
SB7        SB_ON                 BottomLayer SOLDER-BRIDGE_R0402-0R          30.1450      29.8866      0        "Solder Bridge 0402 ON"                                                       
R9         Resistor              BottomLayer R0402                           27.0237      4.3497       270      Resistor,47R,0402,1%,1/16W                                                    
R8         Resistor              BottomLayer R0402                           25.9224      9.8779       90       Resistor,47R,0402,1%,1/16W                                                    
R7         Resistor              BottomLayer R0402                           24.6584      9.8529       90       Resistor,47R,0402,1%,1/16W                                                    
R6         Resistor              BottomLayer R0402                           25.1334      2.5870       90       Resistor,47R,0402,1%,1/16W                                                    
R5         Resistor              BottomLayer R0402                           23.3764      9.8779       90       Resistor,47R,0402,1%,1/16W                                                    
R4         Resistor              BottomLayer R0402                           22.0924      9.8524       90       Resistor,47R,0402,1%,1/16W                                                    
R3         Resistor              BottomLayer R0402                           20.8874      9.8779       90       Resistor,47R,0402,1%,1/16W                                                    
R2         Resistor              BottomLayer R0402                           19.6054      9.8779       90       Resistor,47R,0402,1%,1/16W                                                    
R1         Resistor              TopLayer    R0402                           10.8824      30.1334      270      "Resistor, 100K, 0402, +/-1%, 1/16W"                                          
HW4        STICKER_ES            TopLayer    STICKER_ES_6X6                  -275.4530    -237.3752    0        "Sticker ES, 6x6mm"                                                           
HW3        STICKER_PRODUCT       TopLayer    STICKER_PRODUCT_25X9            -275.4530    -237.3752    90       "Sticker product, 25x9mm"                                                     
D1         SCHOTTKY_1A_2K        TopLayer    DIO_SOD523_1A_2K                15.0000      26.6120      180      "Small signal Schottky diodes"                                                
C22        Capacitor             BottomLayer C0603                           20.2308      2.5544       90       "Capacitor, MLCC, 1uF, 16V, X5R, 10%, 0603, T=0,8mm"                          
C21        Capacitor             TopLayer    C0603_H0P8                      16.0668      28.3927      0        "Capacitor, MLCC, 4.7uF, 10V, X5R, +/-10%, 0603, T=0.8mm"                     
C20        Capacitor             TopLayer    C0402                           22.1014      26.6120      180      "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                       
C10        Capacitor             TopLayer    C0402                           14.8571      33.0265      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
C14        Capacitor             TopLayer    C0402                           18.2970      40.1251      180      "Capacitor, MLCC, 1.0pF, 50V, C0G, +/-0.25pF, 0402, T=0.5mm"                  
C13        Capacitor             TopLayer    C0402                           17.4041      37.4304      0        "Capacitor, MLCC, 1.8pF, 50V, C0G, +/-0.25pF, 0402, T=0.5mm"                  
C12        Capacitor             TopLayer    C0402                           17.4039      34.8350      0        "Capacitor, MLCC, 1.5pF, 50V, C0G, +/-0.25pF, 0402, T=0.5mm"                  
C11        Capacitor             TopLayer    C0603                           15.8999      34.5656      270      "Capacitor, MLCC, 470nF, 16V, X7R, +/-10%, 0603, T=0.8mm"                     
C4         Capacitor             BottomLayer C0402                           9.0000       17.0099      270      "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                       
C9         Capacitor             TopLayer    C0402                           26.8412      32.0689      180      "Capacitor, MLCC, 6pF, 50V, C0G/NP0, +/-0,25pF, 0402, T=0.5mm"                
C8         Capacitor             TopLayer    C0402                           26.8383      30.9320      180      "Capacitor, MLCC, 6pF, 50V, C0G/NP0, +/-0,25pF, 0402, T=0.5mm"                
C7         Capacitor             TopLayer    C0402                           15.0035      25.5882      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                     
