Altium Designer Pick and Place Locations
D:\CAP'1G\Projets\ST Microelectronics\Le Mans\MB989C\BASE\MB989C\03-Manufacturing\MB989C_PCB\Assembly\MB989-C01_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       05/11/18
Time:       16:16
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator Comment                            Layer       Footprint                     Center-X(mm) Center-Y(mm) Rotation Description                                                                                            
MIRE4      Comment                            TopLayer    MIRE_PLACE_SMD_0P8MM          11.4000      47.7000      180      ""                                                                                                     
MIRE3      Comment                            TopLayer    MIRE_PLACE_SMD_0P8MM          72.3000      7.1000       180      ""                                                                                                     
MIRE2      Comment                            BottomLayer MIRE_PLACE_SMD_0P8MM          73.2000      6.4000       360      ""                                                                                                     
MIRE1      Comment                            BottomLayer MIRE_PLACE_SMD_0P8MM          10.9000      47.8000      360      ""                                                                                                     
HW1        LCD_MODULE                         TopLayer    LCD_DRAWING_PROJET-MB989      -863.8859    -915.5805    180      "Display 2.8inch SPI or 16-bit parallel"                                                               
CN4        "Header 2x2_LCD_BACKLIGHT_MB989_S" BottomLayer CON_SAMTEC_TSW-102-07-X-D     85.0650      29.8522      270      "Header, 2x2, 2,54mm, VR, TH, Height 5.84mm/2.54mm, for TFT LCD MB989_P: Backlight"                    
TP2        Test_Point_PTH_1mm_2mm             BottomLayer TP_PTH_1MM_2MM                50.7746      23.3244      180      "Test Point trought hole 1mm/2mm"                                                                      
R45        Resistor                           BottomLayer R0402                         41.8000      41.9000      180      Resistor,10K,0402,1%,1/16W                                                                             
R44        Resistor                           BottomLayer R0402                         68.3006      39.3264      90       Resistor,10K,0402,1%,1/16W                                                                             
R43        Resistor                           BottomLayer R0402                         41.8000      40.9000      180      Resistor,10K,0402,1%,1/16W                                                                             
R42        Resistor                           BottomLayer R0402                         67.2592      39.3446      90       Resistor,10K,0402,1%,1/16W                                                                             
R41        Resistor                           BottomLayer R0402                         41.8000      39.9000      180      Resistor,10K,0402,1%,1/16W                                                                             
R40        Resistor                           BottomLayer R0402                         66.2432      39.3264      90       Resistor,10K,0402,1%,1/16W                                                                             
R39        Resistor                           BottomLayer R0402                         41.8846      43.8730      180      Resistor,10K,0402,1%,1/16W                                                                             
R38        Resistor                           BottomLayer R0402                         41.8000      38.9000      180      Resistor,10K,0402,1%,1/16W                                                                             
R37        Resistor                           BottomLayer R0402                         65.2526      39.3336      90       Resistor,10K,0402,1%,1/16W                                                                             
R36        Resistor                           BottomLayer R0402                         41.8846      44.8890      180      Resistor,10K,0402,1%,1/16W                                                                             
R35        Resistor                           BottomLayer R0402                         41.8846      45.9050      180      Resistor,10K,0402,1%,1/16W                                                                             
R34        Resistor                           BottomLayer R0402                         41.8846      46.9210      180      Resistor,10K,0402,1%,1/16W                                                                             
R33        Resistor                           BottomLayer R0402                         67.8496      34.5313      270      Resistor,10K,0402,1%,1/16W                                                                             
R32        Resistor                           BottomLayer R0402                         46.3000      40.2000      180      Resistor,10K,0402,1%,1/16W                                                                             
R31        Resistor                           BottomLayer R0402                         66.8782      34.5258      270      Resistor,10K,0402,1%,1/16W                                                                             
R30        Resistor                           BottomLayer R0402                         46.3000      39.2000      180      Resistor,10K,0402,1%,1/16W                                                                             
R29        Resistor                           BottomLayer R0402                         65.8368      34.5584      270      Resistor,10K,0402,1%,1/16W                                                                             
R28        Resistor                           BottomLayer R0402                         46.3000      38.2000      180      Resistor,10K,0402,1%,1/16W                                                                             
R27        Resistor                           BottomLayer R0402                         64.7416      34.5368      270      Resistor,10K,0402,1%,1/16W                                                                             
R26        Resistor                           BottomLayer R0402                         46.3000      37.2000      180      Resistor,10K,0402,1%,1/16W                                                                             
R25        Resistor                           BottomLayer R0603                         50.7173      27.3000      270      Resistor,0R,0603,5%,1/10W                                                                              
Q1         PNP_SOT23                          BottomLayer ICC_SOT23-3L_H1P12            38.7350      21.1400      180      "Transistor Bipolar PNP, 45V, 500mA, 100MHz, 300mW, SOT23-3"                                           
CN5        "Header 4x2_LCD_PWR_MB989_S"       BottomLayer CON_SAMTEC_TSW-104-07-X-D_INV 85.0650      17.1522      270      "Header, 4x2, 2,54mm, VR, TH, Height 5.84mm/2.54mm for TFT LCD MODULE MB989_S: pinning inverted"       
C2         Capacitor                          BottomLayer C0402                         36.8000      34.7859      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                 
C1         Capacitor                          BottomLayer C0603                         38.5000      34.4000      180      "Capacitor, MLCC, 4.7µF, 10V, X5R, 20%, 0603, T=0,8mm"                                                 
CN1        "Header 4x2_LCD_IO_MB989_S"        BottomLayer CON_SAMTEC_TSW-104-07-X-D_INV 85.0650      42.5522      270      "Header, 4x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm, for TFT LCD MODULE MB989_S: pinning inverted"      
CN2        "Header 17x2_LCD_TFT_MB989_P"      BottomLayer CON_SAMTEC_TSW-117-07-X-D_INV 79.9850      26.0422      270      "Header, 17x2, 2,54mm, VR, TH, Height 5.84mm/2.54mm for TFT_LCD MB989_P"                               
T2         FDC606P                            BottomLayer MOS_SOT23-6L                  34.9250      20.9622      360      "MOSFET, P-Channel , Vgs(th): -1.5V, Id: -6A, Vds(max): -12V, Vgs(max): +/-8V, Rdson:26mohm@Vgs=-4.5V" 
R24        Resistor                           BottomLayer R0603                         41.9100      20.9622      270      Resistor,4K7,0603,1%,1/10W                                                                             
R23        Resistor                           BottomLayer R0603                         33.6550      48.9022      90       Resistor,4K7,0603,1%,1/10W                                                                             
R22        Resistor                           BottomLayer R0603                         41.2496      48.9022      90       Resistor,4K7,0603,1%,1/10W                                                                             
R21        Resistor                           BottomLayer R0603                         41.9068      32.3922      360      Resistor,4K7,0603,1%,1/10W                                                                             
R20        Resistor                           BottomLayer R0603                         41.8846      27.3122      360      Resistor,4K7,0603,1%,1/10W                                                                             
R19        Resistor                           BottomLayer R0603                         41.8846      29.8522      360      Resistor,4K7,0603,1%,1/10W                                                                             
R18        Resistor                           BottomLayer R0603                         41.9068      24.7722      360      Resistor,4K7,0603,1%,1/10W                                                                             
R17        Resistor                           BottomLayer R0603                         31.7500      20.9622      90       Resistor,75R,0603,1%,1/10W                                                                             
R16        Resistor                           BottomLayer R0603                         26.0350      20.9622      90       Resistor,75R,0603,1%,1/10W                                                                             
TP3        Test_Point_PTH_1mm_2mm             BottomLayer TP_PTH_1MM_2MM                50.8000      31.1222      180      "Test Point trought hole 1mm/2mm"                                                                      
TP1        Test_Point_PTH_1mm_2mm             BottomLayer TP_PTH_1MM_2MM                50.8000      40.1000      180      "Test Point trought hole 1mm/2mm"                                                                      
R15        Resistor                           BottomLayer R0603                         29.8450      20.9622      90       Resistor,75R,0603,1%,1/10W                                                                             
R14        Resistor                           BottomLayer R0603                         27.9400      20.9622      90       Resistor,75R,0603,1%,1/10W                                                                             
R13        Resistor                           BottomLayer R0603                         45.7200      32.3922      360      Resistor,4K7,0603,1%,1/10W                                                                             
R12        Resistor                           BottomLayer R0603                         45.6946      27.3122      360      Resistor,4K7,0603,1%,1/10W                                                                             
R11        Resistor                           BottomLayer R0603                         45.6946      29.8522      360      Resistor,4K7,0603,1%,1/10W                                                                             
C3         Capacitor                          BottomLayer C0603                         38.5000      36.8000      180      "Capacitor, MLCC, 4.7µF, 10V, X5R, 20%, 0603, T=0,8mm"                                                 
R9         Resistor                           BottomLayer R0603                         46.3550      45.7272      360      Resistor,4K7,0603,1%,1/10W                                                                             
R10        Resistor                           BottomLayer R0603                         46.3550      43.8222      360      Resistor,4K7,0603,1%,1/10W                                                                             
R1         Resistor                           BottomLayer R0603                         36.1696      48.9022      90       Resistor,0R,0603,5%,1/10W                                                                              
R2         Resistor                           BottomLayer R0603                         38.7096      48.9022      90       Resistor,0R,0603,5%,1/10W                                                                              
R3         Resistor                           BottomLayer R0603                         43.8150      20.9622      270      Resistor,1K,0603,1%,1/10W                                                                              
R4         Resistor                           BottomLayer R0603                         45.7200      24.7722      360      Resistor,4K7,0603,1%,1/10W                                                                             
R5         Resistor                           BottomLayer R0603                         28.5496      48.9022      90       Resistor,4K7,0603,1%,1/10W                                                                             
R6         Resistor                           BottomLayer R0603                         46.3550      41.9172      360      Resistor,4K7,0603,1%,1/10W                                                                             
R7         Resistor                           BottomLayer R0603                         41.9000      34.2000      360      Resistor,4K7,0603,1%,1/10W                                                                             
R8         Resistor                           BottomLayer R0603                         31.1150      48.9022      90       Resistor,4K7,0603,1%,1/10W                                                                             
C6         Capacitor                          BottomLayer C0402                         36.8000      36.6000      270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                 
CN3        SOCKET_MRE028_xxxxx-51P-TP-A       BottomLayer CON_OMRON_XF2B-5145-31A_INV   31.8018      37.3152      90       "FCP connector for MRE028_xxxxx-51P-TP-A TFT LCD 2.8inch 320x240"                                      
