Altium Designer Pick and Place Locations
D:\Virgil\Altium\STM\Projets\MB1311C\BASE\MB1311C\.\Generate Files\Pick Place for MB1311C.txt

========================================================================================================================
File Design Information:

Date:       26/07/17
Time:       00:46
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator  Comment     Layer       Footprint                               Center-X(mm) Center-Y(mm) Rotation Description                                                                         
R120        R120        BottomLayer R0603                                   20.4000      53.3750      180      "Resistor, 0 ,0603,1%,YAGEO"                                                        
R119        R119        BottomLayer R0603                                   32.4000      53.3750      180      "Resistor, 0 ,0603,1%,YAGEO"                                                        
R118        R118        BottomLayer R0603                                   25.4500      53.3750      180      "Resistor, 0 ,0603,1%,YAGEO"                                                        
R117        R117        BottomLayer R0603                                   17.7750      54.8250      360      Resistor,6.8K,0603,1%,YAGEO                                                         
R116        R116        BottomLayer R0603                                   23.4750      53.8500      270      Resistor,56K,0603,1%,YAGEO                                                          
C101        C101        BottomLayer C0603                                   32.4000      52.0250      180      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C100        C100        BottomLayer C0603                                   25.4500      52.0250      180      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C99         C99         BottomLayer C0603                                   20.4000      52.0250      180      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
U32         .designator BottomLayer ESD_SOT323-5L                           72.2130      3.3630       180      "Quad Transil array for ESD protection"                                             
SB28        .designator BottomLayer SOLDER-BRIDGE_R0603-0R                  84.7880      51.3130      90       "Solder Bridge OFF"                                                                 
R12         R12         TopLayer    R0603                                   54.4130      44.5130      0        Resistor,10K,0603,1%,YAGEO                                                          
B1          .designator TopLayer    SWI_WEALTHMETAL_TD-0341_4P              5.0130       49.3130      0        "SE Push Button TD-0341 [RESET/Black]"                                              
SW1         SW1         BottomLayer SWI_GRAYHILL-INC_EDG-501S_DI            84.9230      6.0830       0        "Gold Plated Contacts,4PST,1x4 Switch"                                              
U9          .designator TopLayer    ICC_DSBGA8_0P88X1P57_P040               6.1729       21.2629      180      "High Efficiency Buck Converter"                                                    
U14         .designator TopLayer    ICC_DSBGA8_0P88X1P57_P040               6.1531       16.1829      180      "High Efficiency Buck Converter"                                                    
CN11        .designator BottomLayer CON_SAMTEC_SSW-108-22-X-S-VS            31.5317      58.1605      180      "Header, 8-Pin, Single row,female"                                                  
R56         .designator BottomLayer R0603                                   77.4530      46.2030      180      Resistor                                                                            
R54         .designator BottomLayer R0603                                   77.4530      47.5530      180      Resistor                                                                            
U20         .designator BottomLayer MIC_STM_MP23DB01MMTR                    15.2630      64.0085      180      "MEMS micro"                                                                        
U19         .designator BottomLayer MIC_STM_MP23DB01MMTR                    36.2630      64.0085      180      "MEMS micro"                                                                        
L4          .designator TopLayer    IND_MURATA_DFE201610C                   8.3728       21.7630      90       Inductor                                                                            
L5          .designator TopLayer    IND_MURATA_DFE201610C                   8.3630       16.6730      90       Inductor                                                                            
H4          .designator TopLayer    PTH_350_700                             95.5130      4.5130       0        ""                                                                                  
H3          .designator TopLayer    PTH_350_700                             4.5130       4.5130       0        ""                                                                                  
H2          .designator TopLayer    PTH_350_700                             95.5130      62.5130      0        ""                                                                                  
H1          .designator TopLayer    PTH_350_700                             4.5130       62.5130      0        ""                                                                                  
CN8         .designator TopLayer    CON_TAG-C_TC2050-IDC-NL                 72.2030      3.7380       180      "Footprint for TC2050-IDC-430 plug of nails (TM) cable for MP430"                   
U27         .designator BottomLayer ICC_MINISO8_3X3_P065                    30.4930      37.0183      270      "Very high accuracy (5 ?) zero drift 5 V dual OpAmp"                                
U25         .designator BottomLayer ICC_MINISO8_3X3_P065                    30.4930      41.9713      270      "Very high accuracy (5 ?) zero drift 5 V dual OpAmp"                                
U12         .designator TopLayer    ESD_SOT323-5L                           94.5130      19.1030      360      "Quad Transil array for ESD protection"                                             
U3          .designator TopLayer    ESD_SOT323-5L                           24.9730      62.7430      180      "Quad Transil array for ESD protection"                                             
JP2         .designator TopLayer    CON_988-JIUBABA_PHFS25-11-02-G0B115-T-1 57.0010      48.2030      0        ""                                                                                  
JP8         .designator BottomLayer CON_988-JIUBABA_PHFS25-11-02-G0B115-T-1 78.0830      13.3530      180      ""                                                                                  
JP6         .designator BottomLayer CON_988-JIUBABA_PHFS25-11-02-G0B115-T-1 2.3130       40.4030      270      "2 PIN Jumper"                                                                      
JP9         .designator BottomLayer CON_988-JIUBABA_PHFS25-11-02-G0B115-T-1 2.3130       11.7130      90       ""                                                                                  
JP7         .designator BottomLayer CON_988-JIUBABA_PHFS25-11-03-G0B115-T-1 2.3130       19.8030      270      ""                                                                                  
JP1         .designator TopLayer    CON_988-JIUBABA_PHFS25-11-03-G0B115-T-1 74.5970      51.0270      0        "Jumper 3 pins"                                                                     
JP10        .designator BottomLayer CON_988-JIUBABA_PHFS25-11-03-G0B115-T-1 95.1873      9.6130       180      ""                                                                                  
JP5         .designator TopLayer    CON_988-JIUBABA_PHFS25-11-03-G0B115-T-1 62.0630      15.4030      360      ""                                                                                  
JP3         .designator TopLayer    CON_988-JIUBABA_PHFS25-11-03-G0B115-T-1 71.0630      24.0130      180      ""                                                                                  
CN5         .designator TopLayer    CON_988-JIUBABA_PHFS25-11-06-G0B115-T-1 97.4130      18.5130      90       "Header, 6-Pin"                                                                     
JP4         .designator TopLayer    CON_988-JIUBABA_PHFS25-12-10-G0B115-T-1 56.9630      21.7830      360      "Pin Header male,2.54mm,2*5,L=11.6,180,1U,DIP"                                      
CN3         .designator TopLayer    CON_SAMTEC_SSW-106-02-F-D-RA__PMOD      88.5960      47.9630      90       "Header, 6-Pin, Dual row"                                                           
CN1         .designator TopLayer    CON_SAMTEC_SQT-110-01-F-D-RA__STMOD+    80.4630      58.4070      180      "Header, 10-Pin, Dual row"                                                          
CN2         .designator TopLayer    CON_TOWNES_FPU330ZH-BT1D3-CA_P050       58.8822      62.2605      180      "TOWNES -  Connector FFC/FPC ZIF 0.5mm 30 pins, Lower Contacts"                     
U6          .designator TopLayer    ICC_VFBGA54_6X8_P075                    54.1937      39.0080      0        "32Mb Burst PSRAM , 104 MHz, 3V, organized as 2M words by 16 bits"                  
U7          .designator TopLayer    ICC_UFBGA169_7X7_P050                   73.1167      36.2080      270      ""                                                                                  
X3          .designator BottomLayer CRY_NX3225GD_2P                         77.0430      18.9730      270      "Crystal 8Mhz, 8pF, -+50PPM, SMD"                                                   
U17         .designator TopLayer    ESD_SOT323-5L                           41.8530      10.2430      135      "Quad Transil array for ESD protection"                                             
U5          .designator TopLayer    ICC_MINI-BGA48_6X8_P075                 54.1940      39.3830      0        "16M bit static RAMs organized as 1024K words by 16 bits"                           
U8          .designator TopLayer    ICC_VSSOP8_DCU_R-PDSO-G8_2X2P30_P050    89.4830      34.5030      180      ""                                                                                  
U10         .designator TopLayer    ICC_VSSOP8_DCU_R-PDSO-G8_2X2P30_P050    86.2930      19.2630      180      ""                                                                                  
R62         .designator BottomLayer R0805                                   39.2427      40.6520      0        Resistor,10K,0805,1%,YAGEO                                                          
R85         .designator BottomLayer R0805                                   38.5230      30.6730      270      Resistor,620,0805,1%,YAGEO                                                          
R81         .designator BottomLayer R0805                                   39.5230      33.8930      0        Resistor,24,0805,1%,YAGEO                                                           
R55         .designator BottomLayer R0805                                   38.8970      46.6130      360      Resistor,1,0805,1%,YAGEO                                                            
CN15        .designator BottomLayer CON_988-JIUBABA_PHFS25-11-04-G0B115-T-1 88.2730      26.7630      180      "Header, 4-Pin"                                                                     
CN14        .designator BottomLayer CON_988-JIUBABA_PHFS25-11-04-G0B115-T-1 2.3130       30.7930      270      "Header, 4-Pin"                                                                     
CN4         .designator TopLayer    CON_SAMTEC_QSH-030-01-F-D-A             32.5630      46.9430      360      "HIGH SPEED SOCKET STRIP, .5mm PITCH, 60 PINS"                                      
CN9         .designator TopLayer    CON_USBMICROAB_MOLEX_47590-0001_H3      58.7630      2.6179       0        ""                                                                                  
CN17        .designator BottomLayer CON_SAMTEC_SSW-106-22-X-S-VS            28.9917      9.9005       0        "Header, 6-Pin, Single row,female"                                                  
CN10        .designator BottomLayer CON_SAMTEC_SSW-110-22-X-S-VS            55.9157      58.1610      180      "Header, 10-Pin, Single row,female"                                                 
D4          .designator BottomLayer DIO_SOD323                              71.8030      13.4030      90       BAT60JFILM                                                                          
D5          .designator BottomLayer DIO_SOD323                              69.8330      13.4030      90       BAT60JFILM                                                                          
D6          .designator BottomLayer DIO_SOD323                              67.8730      13.4030      90       BAT60JFILM                                                                          
D3          .designator BottomLayer DIO_SOD323                              16.4330      28.4630      180      BAT60JFILM                                                                          
D7          .designator BottomLayer DIO_SOD323                              91.4430      13.2830      180      BAT60JFILM                                                                          
X1          .designator TopLayer    CRY_NX3215SA_2P                         73.4230      45.8430      180      "32.768kHz Crystal"                                                                 
C39         .designator TopLayer    CPOL_TAJ-B_1210_H210                    48.5030      14.2830      270      "Tan Capacitor,10uF,10%,25V,Tan-B,TAJB106K025RNJ"                                   
C50         .designator BottomLayer C0603                                   79.2630      48.0330      90       Capacitor,6.8pF,0.25P,50V,NPO,0603                                                  
L3          .designator TopLayer    L0603                                   64.5680      48.5480      0        "100uH Bead"                                                                        
L6          .designator BottomLayer L0603                                   22.0460      35.3970      270      Bead,600R,350mA,0603,FCM1608KF-601T03,Tai-tech                                      
L1          .designator TopLayer    L0603                                   32.3730      57.0930      270      "100uH Bead"                                                                        
L2          .designator TopLayer    L0603                                   34.6630      57.0930      270      "100uH Bead"                                                                        
LD4         .designator TopLayer    LED_BI-GR_HSMF-A201-A00J1               89.5530      30.2130      270      "Bicolor Led"                                                                       
U1          .designator TopLayer    MIC_HCLGA_3X4X1_4LD                     12.0130      64.0130      90       "MEMS audio sensor"                                                                 
U2          .designator TopLayer    MIC_HCLGA_3X4X1_4LD                     33.0130      64.0130      90       "MEMS audio sensor"                                                                 
CN12        .designator BottomLayer CON_PHONE-JACK-3P5_HY_PJ3028B           9.2630       53.4790      0        ""                                                                                  
U28         .designator BottomLayer ESD_SOT23-6L                            92.9530      31.3530      270      ""                                                                                  
T3          .designator BottomLayer MOS_SOT23-6L                            36.0130      49.4230      0        "STripFET VII DeepGATE Power MOSFET, P-CHANNEL 20 V, 0.0146, 7 A - SOT23-6L"        
T11         .designator BottomLayer MOS_SOT23-6L                            35.2630      25.2261      0        "STripFET VII DeepGATE Power MOSFET, P-CHANNEL 20 V, 0.0146, 7 A - SOT23-6L"        
T4          .designator BottomLayer MOS_SOT23-6L                            31.0130      49.4230      0        "STripFET VII DeepGATE Power MOSFET, P-CHANNEL 20 V, 0.0146, 7 A - SOT23-6L"        
T5          .designator BottomLayer MOS_SOT23-6L                            26.0130      49.4230      0        "STripFET VII DeepGATE Power MOSFET, P-CHANNEL 20 V, 0.0146, 7 A - SOT23-6L"        
T10         .designator BottomLayer MOS_SOT23-6L                            41.3730      25.2261      0        "STripFET VII DeepGATE Power MOSFET, P-CHANNEL 20 V, 0.0146, 7 A - SOT23-6L"        
T8          .designator BottomLayer MOS_SOT23-6L                            41.3730      30.9861      0        "STripFET VII DeepGATE Power MOSFET, P-CHANNEL 20 V, 0.0146, 7 A - SOT23-6L"        
T9          .designator BottomLayer MOS_SOT23-6L                            35.2630      30.9861      360      "STripFET VII DeepGATE Power MOSFET, P-CHANNEL 20 V, 0.0146, 7 A - SOT23-6L"        
T7          .designator BottomLayer MOS_SOT23-6L                            41.3630      37.3961      0        "STripFET VII DeepGATE Power MOSFET, P-CHANNEL 20 V, 0.0146, 7 A - SOT23-6L"        
T2          .designator BottomLayer MOS_SOT23-6L                            41.3630      49.4230      0        "STripFET VII DeepGATE Power MOSFET, P-CHANNEL 20 V, 0.0146, 7 A - SOT23-6L"        
CN13        .designator BottomLayer CON_USBMICROB_MOLEX_105017-0001_H2P90   97.2130      31.0130      270      ""                                                                                  
U26         .designator BottomLayer ICC_QFN32-EPAD_5X5_P050                 11.1179      37.8629      90       "Low-Power, Stereo Codec with Headphone Amp"                                        
U30         .designator BottomLayer ICC_LQFP48_7X7_P050                     86.2330      19.4430      90       IC,STM32F103CBT6,LQFP-48                                                            
U29         .designator BottomLayer ICC_LQFP48_7X7_P050                     25.5210      28.0330      90       "Multifunction expander"                                                            
U11         .designator TopLayer    ICC_SO8_5X4_P127_DI-DFN8                77.9430      17.9330      90       ""                                                                                  
C46         .designator BottomLayer CPOL_TAJ-A_1206_H180                    58.0037      63.3860      0        "TAN Capacitor,10uF,10%,16V,A Type,AVX"                                             
C87         .designator BottomLayer CPOL_TAJ-A_1206_H180                    76.1830      26.9930      0        "Tan Capacitor,1uF,10%,16V,Tan-A,TAJA105K016R"                                      
C13         .designator TopLayer    CPOL_TAJ-A_1206_H180                    64.6560      42.1770      180      "Tan Capacitor,1uF,10%,16V,Tan-A,TAJA105K016R"                                      
C8          .designator TopLayer    CPOL_TAJ-A_1206_H180                    64.6560      44.4630      180      "Tan Capacitor,1uF,10%,16V,Tan-A,TAJA105K016R"                                      
C75         .designator BottomLayer CPOL_TAJ-A_1206_H180                    20.0140      35.5240      90       "Tan Capacitor,1uF,10%,16V,Tan-A,TAJA105K016R"                                      
C4          .designator TopLayer    CPOL_TAJ-A_1206_H180                    33.5230      54.4130      180      "TAN Capacitor,10uF,10%,16V,A Type,AVX"                                             
C6          .designator TopLayer    CPOL_TAJ-A_1206_H180                    64.6560      50.4320      180      "TAN Capacitor,4.7uF,10%,16V,A Type,AVX"                                            
C36         .designator TopLayer    CPOL_TAJ-A_1206_H180                    52.8430      17.6230      180      "TAN Capacitor,10uF,10%,16V,A Type,AVX"                                             
U31         .designator BottomLayer MOS_SOT23-5L                            69.0830      18.8030      90       "Ultra low drop-low noise BiCMOS voltage, regulators low ESR capacitors compatible" 
U16         .designator TopLayer    MOS_SOT23-5L                            68.9000      10.7260      270      "Enhanced single channel power switches"                                            
T13         .designator BottomLayer NPN_SOT23                               52.2630      3.1380       360      "NPN Bipolar Transistor"                                                            
T1          .designator TopLayer    MOS_SOT23                               41.0130      58.6630      0        ""                                                                                  
T12         .designator BottomLayer NPN_SOT23                               93.8830      15.8230      360      "NPN Bipolar Transistor"                                                            
SB17        .designator BottomLayer SOLDER-BRIDGE_R0603-0R                  67.0930      63.7830      90       "Solder Bridge OFF"                                                                 
SB19        .designator BottomLayer SOLDER-BRIDGE_R0603-0R                  61.9630      63.7830      90       "Solder Bridge OFF"                                                                 
SB5         SB5         TopLayer    SOLDER-BRIDGE_R0603-0R                  48.9500      40.9250      90       "Solder Bridge ON"                                                                  
SB11        SB11        TopLayer    SOLDER-BRIDGE_R0603-0R                  38.3058      40.6730      270      "Solder Bridge ON"                                                                  
SB10        SB10        TopLayer    SOLDER-BRIDGE_R0603-0R                  36.6887      40.6730      270      "Solder Bridge ON"                                                                  
SB20        .designator BottomLayer SOLDER-BRIDGE_R0603-0R                  50.0330      63.7830      90       "Solder Bridge OFF"                                                                 
SB1         .designator TopLayer    SOLDER-BRIDGE_R0603-0R                  22.4930      61.4830      90       "Solder Bridge ON"                                                                  
SB2         .designator TopLayer    SOLDER-BRIDGE_R0603-0R                  38.4530      56.7330      90       "Solder Bridge ON"                                                                  
SB30        .designator BottomLayer SOLDER-BRIDGE_R0603-0R                  14.0340      32.5790      90       "Solder Bridge ON"                                                                  
SB29        .designator BottomLayer SOLDER-BRIDGE_R0603-0R                  10.2240      43.2740      270      "Solder Bridge ON"                                                                  
SB12        SB12        TopLayer    SOLDER-BRIDGE_R0603-0R                  39.9230      40.6730      270      "Solder Bridge ON"                                                                  
SB9         SB9         TopLayer    SOLDER-BRIDGE_R0603-0R                  35.0716      40.6730      270      "Solder Bridge ON"                                                                  
SB16        .designator BottomLayer SOLDER-BRIDGE_R0603-0R                  68.7330      63.7830      90       "Solder Bridge OFF"                                                                 
SB18        .designator BottomLayer SOLDER-BRIDGE_R0603-0R                  63.5930      63.7830      90       "Solder Bridge OFF"                                                                 
SB27        .designator BottomLayer SOLDER-BRIDGE_R0603-0R                  60.0530      54.3230      180      "Solder Bridge OFF"                                                                 
SB14        .designator TopLayer    SOLDER-BRIDGE_R0603-0R                  86.2230      22.3030      180      "Solder Bridge ON"                                                                  
SB15        .designator TopLayer    SOLDER-BRIDGE_R0603-0R                  72.1830      11.7430      180      "Solder Bridge ON"                                                                  
SB36        .designator BottomLayer SOLDER-BRIDGE_R0603-0R                  84.8630      12.9130      90       "Solder Bridge OFF"                                                                 
SB21        .designator BottomLayer SOLDER-BRIDGE_R0603-0R                  48.4030      63.7830      90       "Solder Bridge OFF"                                                                 
SB31        .designator BottomLayer SOLDER-BRIDGE_R0603-0R                  27.7730      21.5930      180      "Solder Bridge ON"                                                                  
SB34        .designator BottomLayer SOLDER-BRIDGE_R0603-0R                  22.2470      14.3130      270      "Solder Bridge OFF"                                                                 
SB23        .designator BottomLayer SOLDER-BRIDGE_R0603-0R                  97.3830      57.1830      180      "Solder Bridge ON"                                                                  
SB33        .designator BottomLayer SOLDER-BRIDGE_R0603-0R                  24.4130      14.3130      270      "Solder Bridge ON"                                                                  
SB35        .designator BottomLayer SOLDER-BRIDGE_R0603-0R                  20.7230      14.3130      270      "Solder Bridge ON"                                                                  
SB32        .designator BottomLayer SOLDER-BRIDGE_R0603-0R                  25.9330      14.3130      270      "Solder Bridge OFF"                                                                 
C33         .designator TopLayer    C0402                                   5.5130       19.3130      180      Capacitor,0402,4.7uF                                                                
C42         .designator TopLayer    C0402                                   5.9080       14.3228      360      Capacitor,0402,4.7uF                                                                
C30         .designator TopLayer    C0402                                   4.7830       21.2030      270      Capacitor,10uF,0402,GRM155R60J106ME11                                               
C38         .designator TopLayer    C0402                                   4.7830       16.1530      270      Capacitor,10uF,0402,GRM155R60J106ME11                                               
C79         .designator BottomLayer C0603                                   88.2330      33.3730      180      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C66         .designator BottomLayer C0603                                   92.8730      39.8930      180      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C25         .designator TopLayer    C0603                                   70.7490      30.3660      90       Capacitor,2.2uF,16V,X5R,10%,0603,YAGEO                                              
C53         .designator BottomLayer C0603                                   29.9130      44.6830      360      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C41         .designator TopLayer    C0603                                   82.0630      14.6130      90       Capacitor,1uF,0603,16V,10%,X5R,YAGEO                                                
C85         .designator BottomLayer C0603                                   76.1330      29.4130      0        Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C72         .designator BottomLayer C0603                                   79.7230      37.9230      360      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C88         .designator BottomLayer C0603                                   31.4900      25.6200      90       Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C78         .designator BottomLayer C0603                                   35.0930      34.3130      0        Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C64         .designator BottomLayer C0603                                   25.5400      40.0663      360      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C69         .designator BottomLayer C0603                                   33.2130      39.4930      360      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C45         .designator BottomLayer C0603                                   12.4030      64.9130      180      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C71         .designator BottomLayer C0603                                   5.8051       38.3873      180      Capacitor,1uF,0603,16V,10%,X5R,YAGEO                                                
C81         .designator BottomLayer C0603                                   11.4940      32.5290      270      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C65         .designator BottomLayer C0603                                   97.9130      39.5330      270      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C34         .designator TopLayer    C0603                                   88.3930      18.0630      90       Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C48         .designator BottomLayer C0603                                   57.5430      54.3230      180      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C5          .designator TopLayer    C0603                                   33.5430      52.3330      180      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C44         .designator BottomLayer C0603                                   33.3830      64.9130      180      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C96         .designator BottomLayer C0603                                   72.9430      18.5430      90       Capacitor,1uF,0603,16V,10%,X5R,YAGEO                                                
C94         .designator BottomLayer C0603                                   66.3530      18.5530      90       Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C14         .designator TopLayer    C0603                                   59.3490      39.7660      90       Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C60         .designator BottomLayer C0603                                   23.9730      42.2730      180      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C2          .designator TopLayer    C0603                                   15.4530      65.1330      360      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C55         .designator BottomLayer C0603                                   14.5420      43.3240      270      Capacitor,1uF,0603,16V,10%,X5R,YAGEO                                                
C74         .designator BottomLayer C0603                                   5.8051       37.0566      180      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C77         .designator BottomLayer C0603                                   16.3200      35.5770      360      Capacitor,150pF,0603,50V,5%,NPO                                                     
C67         .designator BottomLayer C0603                                   36.0930      39.3330      90       Capacitor,1uF,0603,16V,10%,X5R,YAGEO                                                
C22         .designator TopLayer    C0603                                   91.6530      33.3830      270      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C93         .designator BottomLayer C0603                                   79.7030      19.7630      360      Capacitor,10pF,5%,50V,NPO,0603,YAGEO                                                
C3          .designator TopLayer    C0603                                   50.9530      58.9030      270      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C40         .designator TopLayer    C0603                                   83.8930      15.3230      360      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C31         .designator TopLayer    C0603                                   82.1230      20.4430      270      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C91         .designator BottomLayer C0603                                   69.1630      21.2030      180      Capacitor,10nF,0603,50V,10%,X7R,YAGEO;                                              
C16         .designator TopLayer    C0603                                   49.9000      38.1500      270      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C98         .designator BottomLayer C0603                                   79.7030      18.1730      360      Capacitor,10pF,5%,50V,NPO,0603,YAGEO                                                
C92         .designator BottomLayer C0603                                   79.7030      21.1130      180      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C21         .designator TopLayer    C0603                                   79.6420      35.8270      0        Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C27         .designator TopLayer    C0603                                   73.7057      30.3660      270      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C90         .designator BottomLayer C0603                                   22.7709      21.6391      270      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C73         .designator BottomLayer C0603                                   34.1470      37.0200      270      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C80         .designator BottomLayer C0603                                   12.7640      32.5290      90       Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C84         .designator BottomLayer C0603                                   18.9730      30.4030      180      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C47         .designator BottomLayer C0603                                   44.4730      62.2330      360      Capacitor,1uF,16V,X5R,10%,0603,YAGEO                                                
C24         .designator TopLayer    C0603                                   69.4440      30.3660      270      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C86         .designator BottomLayer C0603                                   19.0440      28.5410      90       Capacitor,10nF,0603,50V,10%,X7R,YAGEO;                                              
C63         .designator BottomLayer C0603                                   5.8051       41.0364      360      Capacitor,1uF,0603,16V,10%,X5R,YAGEO                                                
C43         .designator TopLayer    C0603                                   66.3030      11.0030      270      "Capacitor,4.7uF,16V, X5R,10%,0603"                                                 
C76         .designator BottomLayer C0603                                   16.3200      36.8470      360      Capacitor,150pF,0603,50V,5%,NPO                                                     
C51         .designator BottomLayer C0603                                   79.2630      45.7330      270      Capacitor,6.8pF,0.25P,50V,NPO,0603                                                  
C56         .designator BottomLayer C0603                                   13.2720      43.3240      270      Capacitor,1uF,0603,16V,10%,X5R,YAGEO                                                
C54         .designator BottomLayer C0603                                   15.8120      43.3240      270      Capacitor,10uF,10%,10V,X5R,0603,C1608X5R1A106KT000E                                 
C62         .designator BottomLayer C0603                                   16.3200      41.1650      180      Capacitor,1uF,0603,16V,10%,X5R,YAGEO                                                
C59         .designator BottomLayer C0603                                   6.7950       42.8240      90       Capacitor,22nF,10%,25V,X7R,0603                                                     
C97         .designator BottomLayer C0603                                   71.6330      18.5430      90       Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C57         .designator BottomLayer C0603                                   12.0020      43.3240      90       Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C32         .designator TopLayer    C0603                                   88.3930      20.3930      90       Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C19         .designator TopLayer    C0603                                   91.6530      35.7330      270      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C1          .designator TopLayer    C0603                                   36.4930      65.1430      360      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C70         .designator BottomLayer C0603                                   16.3200      38.6250      180      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C10         .designator TopLayer    C0603                                   71.1330      42.6850      90       Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C9          .designator TopLayer    C0603                                   74.3613      42.7358      270      Capacitor,5.6pF,0.25P,50V,NPO,0603                                                  
C11         .designator TopLayer    C0603                                   72.4817      42.6850      270      Capacitor,5.6pF,0.25P,50V,NPO,0603                                                  
C28         .designator TopLayer    C0603                                   76.1647      30.2390      270      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C17         .designator TopLayer    C0603                                   79.6420      38.4940      0        Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C58         .designator BottomLayer C0603                                   8.5730       42.8240      90       Capacitor,22nF,10%,25V,X7R,0603                                                     
C35         .designator TopLayer    C0603                                   73.8030      18.0330      270      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C68         .designator BottomLayer C0603                                   5.8051       39.7223      360      Capacitor,1uF,0603,16V,10%,X5R,YAGEO                                                
C82         .designator BottomLayer C0603                                   9.7160       32.5290      270      Capacitor,1uF,0603,16V,10%,X5R,YAGEO                                                
C26         .designator TopLayer    C0603                                   72.0547      30.3660      270      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C83         .designator BottomLayer C0603                                   31.4417      31.7160      270      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C89         .designator BottomLayer C0603                                   18.9720      24.9610      180      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C52         .designator BottomLayer C0603                                   32.2130      44.6830      180      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C49         .designator BottomLayer C0603                                   93.4930      51.7030      90       Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C12         .designator TopLayer    C0603                                   76.0377      42.6850      90       Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C23         .designator TopLayer    C0603                                   67.5320      31.6130      270      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C18         .designator TopLayer    C0603                                   66.8937      38.2400      180      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C61         .designator BottomLayer C0603                                   73.2930      41.6930      180      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C15         .designator TopLayer    C0603                                   64.4020      40.0180      180      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C95         .designator BottomLayer C0603                                   65.0730      18.5530      90       Capacitor,1uF,0603,16V,10%,X5R,YAGEO                                                
C37         .designator TopLayer    C0603                                   90.4530      16.8830      90       Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C20         .designator TopLayer    C0603                                   66.8937      36.2080      180      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C7          .designator TopLayer    C0603                                   64.4020      46.6220      180      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
C29         .designator TopLayer    C0603                                   88.6430      23.8130      180      Capacitor,100nF,10%,16V,X7R,0603,YAGEO                                              
LD6         .designator TopLayer    LED_0603_GREEN_H0P8                     53.0630      3.5130       270      LED,Green,0603                                                                      
LD1         .designator TopLayer    LED_0603_ORANGE_H0P4                    44.8030      61.4530      270      LED,Orange,0603                                                                     
LD2         .designator TopLayer    LED_0603_GREEN_H0P8                     46.9130      61.4530      270      LED,Green,0603                                                                      
LD7         .designator TopLayer    LED_0603_RED_H0P4                       64.1470      7.1070       270      "LED, Red ,0603"                                                                    
LD3         .designator TopLayer    LED_0603_GREEN_H0P8                     42.6930      61.4530      270      LED,Green,0603                                                                      
LD8         .designator TopLayer    LED_0603_GREEN_H0P8                     7.8130       11.7030      90       LED,Green,0603                                                                      
LD5         .designator TopLayer    LED_0603_RED_H0P4                       73.7930      15.2730      90       "LED, Red ,0603"                                                                    
R2          .designator TopLayer    R0603                                   42.6930      64.4630      270      "Resistor, 510R , 0603,1%,YAGEO"                                                    
R13         .designator TopLayer    R0603                                   48.4630      43.7630      180      "Resistor, 0 ,0603,1%,YAGEO"                                                        
R11         .designator TopLayer    R0603                                   48.4630      45.1730      180      "Resistor, 0 ,0603,1%,YAGEO"                                                        
R6          .designator TopLayer    R0603                                   41.0030      56.0230      360      "Resistor, 1M , 0603"                                                               
R112        .designator BottomLayer R0603                                   13.0430      6.9430       90       Resistor                                                                            
R32         .designator TopLayer    R0603                                   92.8730      15.9230      180      "Resistor, 100 ,0603,1%,YAGEO"                                                      
R28         .designator TopLayer    R0603                                   92.3930      20.1430      90       "Resistor, 100 ,0603,1%,YAGEO"                                                      
R94         .designator BottomLayer R0603                                   92.1930      23.0230      90       "Resistor, 100 ,0603,1%,YAGEO"                                                      
R61         .designator BottomLayer R0603                                   75.8330      41.7030      180      "Resistor, 0 ,0603,1%,YAGEO"                                                        
R100        .designator BottomLayer R0603                                   11.6130      16.0630      270      Resistor,1.5K,0603,1%,YAGEO                                                         
R99         .designator BottomLayer R0603                                   14.1430      16.0630      270      Resistor,1.5K,0603,1%,YAGEO                                                         
R47         .designator BottomLayer R0603                                   94.7930      57.1830      360      Resistor,10K,0603,1%,YAGEO                                                          
R79         .designator BottomLayer R0603                                   25.5400      35.9057      360      "Resistor, 0 ,0603,1%,YAGEO"                                                        
R25         .designator TopLayer    R0603                                   86.2130      24.1930      360      Resistor,100K,0603,1%,YAGEO                                                         
R84         .designator BottomLayer R0603                                   43.8030      31.0230      90       Resistor,100K,0603,1%,YAGEO                                                         
R49         .designator BottomLayer R0603                                   42.2930      52.6100      270      Resistor,100K,0603,1%,YAGEO                                                         
R74         .designator BottomLayer R0603                                   43.8030      37.3530      270      Resistor,100K,0603,1%,YAGEO                                                         
R95         .designator BottomLayer R0603                                   25.4380      21.6391      270      Resistor,510R,0603,1%,YAGEO                                                         
R7          .designator TopLayer    R0603                                   25.8130      54.7130      270      Resistor,10K,0603,1%,YAGEO                                                          
R108        .designator BottomLayer R0603                                   10.5130      12.3230      270      Resistor                                                                            
R43         .designator TopLayer    R0603                                   53.9380      5.9380       360      "Resistor, 330R , 0603,1%,YAGEO"                                                    
R114        .designator BottomLayer R0603                                   49.8130      3.9130       90       "Resistor, 10K,0603,1%,YAGEO"                                                       
R113        .designator BottomLayer R0603                                   50.6880      5.7880       180      "Resistor, 47K,0603,1%,YAGEO"                                                       
R38         .designator TopLayer    R0603                                   63.6630      9.7530       270      "Resistor, 620R , 0603,1%,YAGEO"                                                    
R39         .designator TopLayer    R0603                                   65.0030      9.7530       270      "Resistor, 47K,0603,1%,YAGEO"                                                       
R40         .designator TopLayer    R0603                                   75.0730      9.8030       180      "Resistor, 47K,0603,1%,YAGEO"                                                       
R65         .designator BottomLayer R0603                                   30.8740      39.5080      0        Resistor,6.04K,0603,1%,YAGEO                                                        
R89         .designator BottomLayer R0603                                   43.8030      25.2230      90       Resistor,100K,0603,1%,YAGEO                                                         
R30         .designator TopLayer    R0603                                   92.3930      17.7930      270      "Resistor, 100 ,0603,1%,YAGEO"                                                      
R15         .designator TopLayer    R0603                                   77.6100      42.6850      270      Resistor,100K,0603,1%,YAGEO                                                         
R17         .designator TopLayer    R0603                                   59.7220      42.6530      360      "Resistor, 0 ,0603,1%,YAGEO"                                                        
R97         .designator BottomLayer R0603                                   21.1130      21.6391      90       "Resistor, 0 ,0603,1%,YAGEO"                                                        
R33         .designator TopLayer    R0603                                   72.0630      14.5230      180      Resistor                                                                            
R106        .designator BottomLayer R0603                                   83.4230      13.0730      270      Resistor,100K,0603,1%,YAGEO                                                         
R91         .designator BottomLayer R0603                                   80.1630      23.0330      270      Resistor,100K,0603,1%,YAGEO                                                         
R3          .designator TopLayer    R0603                                   35.5730      60.1730      360      Resistor,680R,0603,1%,YAGEO                                                         
R27         .designator TopLayer    R0603                                   78.0980      21.4520      360      Resistor,2.2K,0603,1%,YAGEO                                                         
R92         .designator BottomLayer R0603                                   78.8130      23.0330      90       Resistor,4.7K,0603,1%,YAGEO                                                         
R9          R9          TopLayer    R0603                                   50.8830      45.5530      0        Resistor,10K,0603,1%,YAGEO                                                          
R77         .designator BottomLayer R0603                                   25.5400      37.2723      360      Resistor,357K,0603,1%,YAGEO                                                         
R70         .designator BottomLayer R0603                                   25.5400      38.6693      180      Resistor,11K,0603,1%,YAGEO                                                          
R34         .designator TopLayer    R0603                                   87.5530      13.4030      270      Resistor,10K,0603,1%,YAGEO                                                          
R22         .designator TopLayer    R0603                                   85.9630      29.4630      360      "Resistor, 0 ,0603,1%,YAGEO"                                                        
R98         .designator BottomLayer R0603                                   93.8530      18.4430      180      Resistor,1.5K,0603,1%,YAGEO                                                         
R31         .designator TopLayer    R0603                                   86.3830      15.9430      90       "Resistor, 0 ,0603,1%,YAGEO"                                                        
R88         .designator BottomLayer R0603                                   80.1630      25.3330      90       "Resistor, 0 ,0603,1%,YAGEO"                                                        
R103        .designator BottomLayer R0603                                   88.9930      13.0730      90       Resistor,0,0603,5%,YAGEO                                                            
R8          R8          TopLayer    R0603                                   54.4130      45.9130      180      Resistor,10K,0603,1%,YAGEO                                                          
R20         .designator TopLayer    R0603                                   87.4030      34.5430      270      "Resistor, 0 ,0603,1%,YAGEO"                                                        
R60         .designator BottomLayer R0603                                   34.3230      41.6130      90       Resistor,6.04K,0603,1%,YAGEO                                                        
R75         .designator BottomLayer R0603                                   36.8030      37.0200      270      "Resistor, 100 ,0603,1%,YAGEO"                                                      
R111        .designator BottomLayer R0603                                   73.3030      8.2230       360      "Resistor, 100 ,0603,1%,YAGEO"                                                      
R115        .designator BottomLayer R0603                                   65.0330      3.6530       270      "Resistor, 100 ,0603,1%,YAGEO"                                                      
R110        .designator BottomLayer R0603                                   75.7730      8.2230       360      "Resistor, 100 ,0603,1%,YAGEO"                                                      
R83         .designator BottomLayer R0603                                   15.4230      32.5290      90       Resistor,10K,0603,1%,YAGEO                                                          
R101        .designator BottomLayer R0603                                   80.0830      16.1730      360      Resistor,10K,0603,1%,YAGEO                                                          
R16         .designator TopLayer    R0603                                   79.1340      42.6850      270      Resistor,100K,0603,1%,YAGEO                                                         
R96         .designator BottomLayer R0603                                   24.0961      21.6391      270      Resistor,10K,0603,1%,YAGEO                                                          
R109        .designator BottomLayer R0603                                   60.9630      9.8930       270      Resistor,1K,0603,1%                                                                 
R29         .designator TopLayer    R0603                                   82.6230      18.3530      180      Resistor,10K,0603,1%,YAGEO                                                          
R87         .designator BottomLayer R0603                                   18.9730      26.3230      360      Resistor,100K,0603,1%,YAGEO                                                         
R24         .designator TopLayer    R0603                                   82.6230      24.1930      360      "Resistor, 0 ,0603,1%,YAGEO"                                                        
R19         .designator TopLayer    R0603                                   90.1707      37.8760      90       Resistor,100K,0603,1%,YAGEO                                                         
R35         .designator TopLayer    R0603                                   88.9730      13.4030      90       "Resistor, 100 ,0603,1%,YAGEO"                                                      
R57         .designator BottomLayer R0603                                   8.5730       45.2450      90       Resistor,50R,0603,1%,YAGEO                                                          
R42         .designator TopLayer    R0603                                   53.1830      7.2830       180      "Resistor, 100 ,0603,1%,YAGEO"                                                      
R58         .designator BottomLayer R0603                                   6.7950       45.2450      90       Resistor,50R,0603,1%,YAGEO                                                          
R107        .designator BottomLayer R0603                                   13.0730      12.3230      270      Resistor                                                                            
R102        .designator BottomLayer R0603                                   77.7830      16.1730      360      Resistor,100K,0603,1%,YAGEO                                                         
R104        .designator BottomLayer R0603                                   87.6430      13.0730      270      Resistor,2.7K,0603,1%,YAGEO                                                         
R36         .designator TopLayer    R0603                                   90.3730      13.4030      90       Resistor,36K,0603,1%,YAGEO                                                          
R41         .designator TopLayer    R0603                                   72.0230      9.7870       360      "Resistor, 0 ,0603,1%,YAGEO"                                                        
R76         .designator BottomLayer R0603                                   35.4630      37.0200      270      Resistor,300K,0603,1%,YAGEO                                                         
R26         .designator TopLayer    R0603                                   82.6230      22.8530      180      "Resistor, 100 ,0603,1%,YAGEO"                                                      
R21         .designator TopLayer    R0603                                   93.1630      30.9430      180      "Resistor, 100 ,0603,1%,YAGEO"                                                      
R5          .designator TopLayer    R0603                                   46.9130      58.8530      90       Resistor,510R,0603,1%,YAGEO                                                         
R82         .designator BottomLayer R0603                                   17.4230      32.5290      90       "Resistor, 0 ,0603,1%,YAGEO"                                                        
R80         .designator BottomLayer R0603                                   5.8051       35.2287      360      Resistor,10K,0603,1%,YAGEO                                                          
R105        .designator BottomLayer R0603                                   86.2730      13.0730      90       Resistor,4.7K,0603,1%,YAGEO                                                         
R93         .designator BottomLayer R0603                                   77.4630      23.0330      90       Resistor,4.7K,0603,1%,YAGEO                                                         
R1          .designator TopLayer    R0603                                   24.9430      65.0430      360      Resistor,10K,0603,1%,YAGEO                                                          
R86         .designator BottomLayer R0603                                   93.7380      28.9630      360      Resistor,100K,0603,1%,YAGEO                                                         
R10         R10         TopLayer    R0603                                   57.3870      45.5510      0        Resistor,10K,0603,1%,YAGEO                                                          
R64         .designator BottomLayer R0603                                   16.3200      39.8950      180      Resistor,2.2K,0603,1%,YAGEO                                                         
R48         .designator BottomLayer R0603                                   97.8630      54.2330      90       Resistor,10K,0603,1%,YAGEO                                                          
R59         .designator BottomLayer R0603                                   17.0820      43.3240      90       Resistor,100K,0603,1%,YAGEO                                                         
R14         .designator TopLayer    R0603                                   68.3740      42.6850      90       "Resistor, 0 ,0603,1%,YAGEO"                                                        
R4          .designator TopLayer    R0603                                   56.1230      58.9930      270      "Resistor, 22 ,0603,1%,YAGEO"                                                       
R66         .designator BottomLayer R0603                                   28.4830      39.5080      180      Resistor,300K,0603,1%,YAGEO                                                         
R18         .designator TopLayer    R0603                                   88.7737      37.8760      90       Resistor,100K,0603,1%,YAGEO                                                         
R37         .designator TopLayer    R0603                                   5.3330       10.4630      180      Resistor                                                                            
R23         .designator TopLayer    R0603                                   93.1630      29.4430      180      "Resistor, 100 ,0603,1%,YAGEO"                                                      
R44         .designator BottomLayer R0603                                   17.9930      64.3330      360      Resistor,10K,0603,1%,YAGEO                                                          
R50         .designator BottomLayer R0603                                   30.5500      53.8500      270      Resistor,100K,0603,1%,YAGEO                                                         
CN7         .designator TopLayer    CON_SAMTEC_SSM-104-L-DH                 14.1130      7.9830       180      "Header, 5-Pin, Dual row"                                                           
D1          .designator TopLayer    ESD_QFN2_1P6X1_P125                     49.0630      22.4430      270      "High power transient voltage suppressor, 7V breakdown"                             
R51         .designator BottomLayer R0603                                   97.8880      51.7030      270      "Resistor, 33 ,0603,1%,YAGEO"                                                       
R52         .designator BottomLayer R0603                                   96.5330      51.7030      270      "Resistor, 33 ,0603,1%,YAGEO"                                                       
R73         .designator BottomLayer R0603                                   91.2530      37.6930      90       "Resistor, 33 ,0603,1%,YAGEO"                                                       
R68         .designator BottomLayer R0603                                   87.6740      39.2970      360      "Resistor, 33 ,0603,1%,YAGEO"                                                       
R71         .designator BottomLayer R0603                                   93.9430      37.6930      90       "Resistor, 33 ,0603,1%,YAGEO"                                                       
R53         .designator BottomLayer R0603                                   95.1730      51.7030      270      "Resistor, 33 ,0603,1%,YAGEO"                                                       
R78         .designator BottomLayer R0603                                   89.4140      36.9170      360      "Resistor, 33 ,0603,1%,YAGEO"                                                       
R67         .designator BottomLayer R0603                                   89.5940      38.8270      90       "Resistor, 33 ,0603,1%,YAGEO"                                                       
R72         .designator BottomLayer R0603                                   92.6030      37.6930      90       "Resistor, 33 ,0603,1%,YAGEO"                                                       
R69         .designator BottomLayer R0603                                   95.2830      38.7930      90       "Resistor, 33 ,0603,1%,YAGEO"                                                       
R63         .designator BottomLayer R0603                                   96.6130      39.5330      90       "Resistor, 33 ,0603,1%,YAGEO"                                                       
R46         .designator BottomLayer R0402                                   42.8030      62.2930      270      Resistor,10K,0402,1%,YAGEO                                                          
R45         .designator BottomLayer R0402                                   39.1380      63.3070      90       Resistor,10K,0402,1%,YAGEO                                                          
SB13        .designator TopLayer    SOLDER-BRIDGE_R0603-0R                  28.4130      40.6530      270      "Solder Bridge OFF"                                                                 
SB7         .designator TopLayer    SOLDER-BRIDGE_R0603-0R                  31.9030      40.6730      270      "Solder Bridge OFF"                                                                 
SB22        .designator BottomLayer SOLDER-BRIDGE_R0603-0R                  40.3230      63.7830      90       "Solder Bridge ON"                                                                  
SB25        .designator BottomLayer SOLDER-BRIDGE_R0603-0R                  94.4530      54.6830      90       "Solder Bridge OFF"                                                                 
SB4         .designator TopLayer    SOLDER-BRIDGE_R0603-0R                  50.1850      47.8650      90       "Solder Bridge OFF"                                                                 
SB6         .designator TopLayer    SOLDER-BRIDGE_R0603-0R                  29.9601      40.6730      270      "Solder Bridge ON"                                                                  
SB8         .designator TopLayer    SOLDER-BRIDGE_R0603-0R                  33.4544      40.6730      270      "Solder Bridge ON"                                                                  
SB37        .designator BottomLayer SOLDER-BRIDGE_R0603-0R                  18.1130      7.1830       90       "Solder Bridge ON"                                                                  
SB26        .designator BottomLayer SOLDER-BRIDGE_R0603-0R                  92.8730      54.6830      90       "Solder Bridge ON"                                                                  
SB24        .designator BottomLayer SOLDER-BRIDGE_R0603-0R                  96.0330      54.5830      270      "Solder Bridge ON"                                                                  
T6          .designator BottomLayer MOS_SOT23-6L                            21.0130      49.4230      0        "STripFET VII DeepGATE Power MOSFET, P-CHANNEL 20 V, 0.0146, 7 A - SOT23-6L"        
U21         .designator BottomLayer ICC_UFQFN16-EPAD_2P6X1P8_P040           43.4130      64.3130      180      "Low voltage high bandwidth quad SPDT switch"                                       
U24         .designator BottomLayer ICC_BGA24_5X5-BALL-ARRAY_6X8_P1         95.2830      45.5830      180      "512Mb, 3V, CMOS, MXSMIO Octal I/O FLASH MEMORY, 133 MHz, DTR"                      
U23         .designator BottomLayer ICC_BGA24_5X5-BALL-ARRAY_6X8_P1         95.2830      45.5830      180      "512Mb, 3V, Octal I/O XTRM Flash Memory, 133 MHz, DDR"                              
U4          .designator TopLayer    ESD_SOT23                               10.2830      57.0430      360      "Dual Transil array ESD protection"                                                 
U13         .designator TopLayer    ESD_UQFN16L-EPAD_3P5X1P2_P040           27.3130      17.7470      180      "6-line IPAD, EMI filter and ESD for SDcard2.0"                                     
U22         .designator BottomLayer ESD_SOT23-6L                            11.3230      48.4630      90       "Quad Bidir supressor ESD protection"                                               
U18         .designator TopLayer    ESD_SOT23-6L                            59.0770      7.0056       270      "USB ESD protection"                                                                
X2          .designator BottomLayer CRY_NX3225HA_4P                         81.9630      46.9330      180      ""                                                                                  
U15         .designator TopLayer    REG_SOT223-TAB                          53.9830      12.2530      180      "Adjustable and fixed low drop positive voltage regulator"                          
CN16        .designator BottomLayer CON_SAMTEC_SSW-108-22-X-S-VS            49.3117      9.9005       0        "Header, 8-Pin, Single row,female"                                                  
B2          .designator TopLayer    SWI_XIEJIA_MT-008A_6P                   46.7130      5.9130       45       Joystick                                                                            
R90         .designator BottomLayer R0603                                   37.6930      25.2230      270      Resistor,100K,0603,1%,YAGEO                                                         
SB3         .designator TopLayer    SOLDER-BRIDGE_R0603-0R                  50.1860      50.5440      270      "Solder Bridge ON"                                                                  
D2          .designator TopLayer    ESD_QFN2_1P6X1_P125                     62.2230      7.0570       360      "High power transient voltage suppressor, 7V breakdown"                             
CN6         .designator TopLayer    CON_MICROSD_ATOM_MR01A-01211            28.8930      9.2630       0        "micro-SD card connector top mount push-push"                                       
Designator2 Designator2 TopLayer    CARTOUCHE_STM_BOTTOM                    -51.1870     -55.0370     0        ""                                                                                  
Designator3 Designator3 TopLayer    CARTOUCHE_STM_TOP                       -51.1870     -55.0370     0        ""                                                                                  
SB38        SB38        TopLayer    SOLDER-BRIDGE_R0603-0R                  48.4250      37.1000      90       "Solder Bridge ON"                                                                  
SB39        SB39        TopLayer    SOLDER-BRIDGE_R0603-0R                  36.3750      36.3750      180      "Solder Bridge OFF"                                                                 
U33         U33         TopLayer    ICC_DFN8-EPAD_3X3_P065_DI-SO8           77.9430      17.9330      90       ""                                                                                  
