Field=#~Integer~#~50|Field=Comment~String~Comment~100|Field=Description~String~Description~100|Field=Designator~String~Designator~100|Field=Footprint~String~Footprint~100|Field=LibRef~String~LibRef~100|Field=Quantity~Integer~Quantity~100|ReportField=Currency~<none>|ReportField=ProductionQuantity~1|ReportField=ProjectFileName~VIPer31 flyback iso PSR-SSR-Ada.PrjPcb|ReportField=ProjectFullPath~C:\Users\Public\Documents\Altium\Projects\PCB_Project\VIPer31 flyback iso PSR_SSR project\PCB_Project\VIPer31 flyback iso PSR-SSR-Ada.PrjPcb|ReportField=Title~Bill of Materials For Project [VIPer31 flyback iso PSR-SSR-Ada.PrjPcb] (No PCB Document Selected)|ReportField=TotalQuantity~55|ReportField=ReportTime~3:26:17 PM|ReportField=ReportDate~5/3/2019|ReportField=ReportDateTime~5/3/2019 3:26:17 PM|ReportField=OutputName~Bill of Materials|ReportField=OutputType~BOM_PartType|ReportField=GeneratorName~BOM|ReportField=GeneratorDescription~Bill of Materials|ReportField=VariantName~None|ReportField=Address1~|ReportField=Address2~|ReportField=Address3~|ReportField=Address4~|ReportField=Application_BuildNumber~|ReportField=ApprovedBy~|ReportField=Author~|ReportField=CheckedBy~|ReportField=CompanyName~|ReportField=CurrentDate~5/3/2019|ReportField=CurrentTime~3:26:14 PM|ReportField=Date~|ReportField=DocumentFullPathAndName~C:\Users\Public\Documents\Altium\Projects\PCB_Project\VIPer31 flyback iso PSR_SSR project\VIPer31 flyback iso PSR-SSR.SchDoc|ReportField=DocumentName~VIPer31 flyback iso PSR-SSR.SchDoc|ReportField=DocumentNumber~|ReportField=DrawnBy~|ReportField=Engineer~|ReportField=ImagePath~|ReportField=ModifiedDate~4/29/2019|ReportField=Organization~|ReportField=PageSetup~Record=PageOptions:CenterHorizontal=True:CenterVertical=True:PrintScale=0.73:XCorrection=1.00:YCorrection=1.00:PrintKind=1:BorderSize=5000000:LeftOffset=0:BottomOffset=0:Orientation=2:PaperLength=1000:PaperWidth=1000:Scale=100:PaperSource=7:PrintQuality=-3:MediaType=1:DitherType=10:PrintScaleMode=1:PaperKind=A4:PaperIndex=9|ReportField=ProjectName~VIPer31 flyback iso PSR-SSR-Ada.PrjPcb|ReportField=Revision~|ReportField=Rule~|ReportField=SheetNumber~|ReportField=SheetTotal~|ReportField=Time~|ReportField=Title~|ReportField=DataSourceFileName~VIPer31 flyback iso PSR-SSR-Ada.PrjPcb|ReportField=DataSourceFullPath~C:\Users\Public\Documents\Altium\Projects\PCB_Project\VIPer31 flyback iso PSR_SSR project\PCB_Project\VIPer31 flyback iso PSR-SSR-Ada.PrjPcb|ReportField=PCBConfigurationName~Default Configuration|ReportField=Item~|ReportField=ItemRevision~|ReportField=ItemAndRevision~|ReportField=ItemRevisionBase~|ReportField=ItemRevisionLevel1~|ReportField=ItemRevisionLevel2~|ReportField=ItemRevisionLevel1AndBase~|ReportField=ItemRevisionLevel2AndLevel1~
1|MB6S-E3|Diode Bridge|BR|BRIDGE|BRIDGE1|1
2|100nF|100 pF 250 Vdc multi layer capacitor|C1, C2|CAP-13X6|CAP|2
3|22 uF 400 Vcc|Polarized Capacitor (Radial)|C3, C4|CAPOL-7.5X16|Cap Pol1|2
4|4.7uF|Vcc cap 4.7uF 50 Vcc, Kemet|C5|R-1206-B2|Cap Pol1|1
5|1 nF 200 Vdc|1 nF 200 Vdc multi layer capacitor|C7|R-0603-B2|CAP|1
6|NC|NC, NC, NC, Not connected, Not connected, Not connected|C8, C14, C16, R5, R8, R14|R-0603-B2|CAP, CAP, CAP, Res1, Res1, Res1|6
7|1nF +/-5% 630V|1 nF 630 V multi layer capacitor|C9|R-1206-B2|CAP|1
8|47nF|22 nF +/-10%, 100 Vcc, MLCC|C10|R-0603-B2|CAP|1
9|680 uF, 25 Vcc|470 uF +/-20%, 35 Vcc, +105°C|C11|CAPOL-5X10|Cap Pol1|1
10|100 uF, 35 Vcc|100 uF +/-20%, 35 Vcc, +105°C|C12|CAPOL-2.5X6.3|Cap Pol1|1
11|2.2nF 250Vac X1 Y2|2.2 nF 2000 V single layer capacitor|C13|MYLAR-10X6|CAP|1
12|100 nF|100nF ±10%, 25 Vcc, MLCC|C15|R-0603-B2|CAP|1
13|1N4148|small signal diode|D1|SOD-123|Diode|1
14|STPS3150U|Schottky diode, 10A, 200 V|D2|SMB-2|Diode|1
15|MRA4007T3G|Silicon Diode, 1 A, 1000 V|D3|SMA-2|Diode|1
16|18V|Zener Diode|Dz|SOD-123|D Zener|1
17|2A|Fuse 2A,  250 Vca|F|Fuse_3821200041_Wick|Fuse 1|1
18|HOLE||H1, H2, H3, H4|FORO|HOLE|4
19|VIPER31_SO16|Integrato|IC1|SO-16N_2|VIPER31_SO16|1
20|TS3431BILT|1.24 V VREF SHUNT|IC2|SOT23-3-MIRR|TS432|1
21|input connector|Morsetti|IN|SM.2VITE|M.2VITE|1
22|1mH|FIXED IND 3.3UH 3.23A 33 MOHM|L1|CAPOL-5X10|Inductor|1
23|3.3 uH|FIXED IND 3.3UH 3.23A 33 MOHM|L2|WE_74404043033A_4x4|Inductor|1
24|10 Ohm|10 Ohm|NTC|B57237S100M-NTC|Res2|1
25|SFH610A-2|Opto ingresso 60 Vdc|Opto|DIP4|OPTO_1|1
26|output connector|Morsetti|OUT|SM.2VITE|M.2VITE|1
27|BC807|PNP Transitstor 0.5A, 45 V, hfe 30|Q1|BC817_NEW|PNP_BC807|1
28|3 MOhm|3 MOhm +/-1%  0.125W, 0805 Vishay|R1, R2|R-0805-B2|Res1|2
29|6.8 kOhm|6.8 kOhm +/-1% 0.125W, 0805 Panasonic|R3|R-0805-B2|Res1|1
30|60.4 kOhm|60.4 kOhm +/-1% 0.125W, 0805 Panasonic|R4|R-0805-B2|Res1|1
31|0R|0Ω, 0.25W, pkg 0603, serie CRCW|R6|R-0603-B2|Res1|1
32|0R|0Ω, 0.25W, pkg 0603, serie CRCW|R7|RES-1/4W-3|Res1|1
33|220 kOhm|220 KOhm +/-5%, 0.33W, 1206, serie ERJT08|R9|R-1206-B2|Res1|1
34|82k|470kΩ ±1%, 0.1W|R10|R-0603-B2|Res1|1
35|15k|22KΩ ±1%, 0.1W|R11|R-0603-B2|Res1|1
36|100 kOhm|Not connected|R12|R-0603-B2|Res1|1
37|9 kOhm|15 kΩ ±1%, 0.1W, 0603|R13|R-0603-B2|Res1|1
38|10R|10Ω, 0.1W, pkg 0603, serie CRG0603|R15|R-0805-B|Res1|1
39|2.2k|470Ω ±1%, 0.1W|R16|R-0603-B2|Res1|1
40|RESISTENZA|Resistor|R17, R18|R-0603-B2|RESISTENZA|2
41|47R|47Ω ±1%, 0.125W|Rz|R-0603-B2|Res1|1
42|2 X 10 mH|Common Mode Choke, Lo=10 mH, Rdc=350 mOhm, Idc=0.7A, Un=230 Vac|T1|WE_744821110_Choke|CM CHOKE|1
43|TRANSFORMER_WURTH_750317580-VIPer31|Center-tapped transformer|T2|WURTH-750317580-VIPer31|TRANSFORMER_WURTH_750317580-VIPer31|1
