; 
; USB-IF Vendor Info File Editor 3.1.0.2
; 
$VIF_Producer: "USB-IF Vendor Info File Editor 3.1.0.2"
$VIF_Specification: "Version 3.12"

$Vendor_Name:                                           "STMicroelectronics"
$Model_Part_Number:                                     "STEVAL-USBPD27S"
$Product_Revision:                                      "V1.0"
$TID:                                                   "Full"
VIF_Product_Type:                                       0             ; Port Product


;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
;   Product
;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
Certification_Type:                                     1             ; Reference Platform
Product_VID:                                            0x0483        ; 0483

;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
;   Component
;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
$Port_Label:                                            "0"
Connector_Type:                                         2             ; Type-C®
USB4_Supported:                                         NO
USB_PD_Support:                                         YES
PD_Port_Type:                                           3             ; Provider Only
Type_C_State_Machine:                                   0             ; SRC
Port_Battery_Powered:                                   NO
BC_1_2_Support:                                         0             ; None
Captive_Cable:                                          NO

;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
;   General PD
;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
PD_Spec_Revision_Major:                                 3
PD_Spec_Revision_Minor:                                 0
PD_Spec_Version_Major:                                  2
PD_Spec_Version_Minor:                                  0
PD_Specification_Revision:                              2             ; Revision 3
SOP_Capable:                                            YES
SOP_P_Capable:                                          YES
SOP_PP_Capable:                                         YES
SOP_P_Debug_Capable:                                    NO
SOP_PP_Debug_Capable:                                   NO
Manufacturer_Info_Supported_Port:                       YES
Manufacturer_Info_VID_Port:                             0x0483        ; 0483
Manufacturer_Info_PID_Port:                             0x0002        ; 0002
Chunking_Implemented_SOP:                               YES
Unchunked_Extended_Messages_Supported:                  YES
Security_Msgs_Supported_SOP:                            NO
Unconstrained_Power:                                    YES
Num_Fixed_Batteries:                                    0
Num_Swappable_Battery_Slots:                            0
ID_Header_Connector_Type_SOP:                           3             ; USB Type-C® Plug

;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
;   PD Capabilities
;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
USB_Comms_Capable:                                      NO
DR_Swap_To_DFP_Supported:                               NO
DR_Swap_To_UFP_Supported:                               NO
VCONN_Swap_To_On_Supported:                             YES
VCONN_Swap_To_Off_Supported:                            YES
Responds_To_Discov_SOP_UFP:                             NO
Responds_To_Discov_SOP_DFP:                             NO
Attempts_Discov_SOP:                                    NO

;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
;   USB Type-C®
;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
Type_C_Can_Act_As_Host:                                 NO
Type_C_Can_Act_As_Device:                               NO
Type_C_Supports_Audio_Accessory:                        NO
Type_C_Is_Debug_Target_SRC:                             NO
RP_Value:                                               2             ; 3A
Type_C_Port_On_Hub:                                     NO
Type_C_Power_Source:                                    0             ; Externally Powered
Type_C_Sources_VCONN:                                   YES
Type_C_Is_Alt_Mode_Controller:                          NO

;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
;   Product Power
;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
Product_Total_Source_Power_mW:                          27000         ; 27000 mW
Port_Source_Power_Type:                                 0             ; Assured

;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
;   PD Source
;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;;
PD_Power_As_Source:                                     27000         ; 27000 mW
USB_Suspend_May_Be_Cleared:                             YES
Sends_Pings:                                            NO
FR_Swap_Type_C_Current_Capability_As_Initial_Sink:      0             ; FR_Swap not supported
Master_Port:                                            NO
Num_Src_PDOs:                                           4
PD_OC_Protection:                                       YES
PD_OCP_Method:                                          0             ; Over-Current Response

    Src_PDO_Supply_Type1:                                   0             ; Fixed
    Src_PDO_Peak_Current1:                                  0             ; 100% IOC
    Src_PDO_Voltage1:                                       100           ; 5000 mV
    Src_PDO_Max_Current1:                                   500           ; 5000 mA
    Src_PD_OCP_OC_Debounce1:                                1000          ; 1000 msec
    Src_PD_OCP_OC_Threshold1:                               510           ; 5100 mA

    Src_PDO_Supply_Type2:                                   0             ; Fixed
    Src_PDO_Peak_Current2:                                  0             ; 100% IOC
    Src_PDO_Voltage2:                                       180           ; 9000 mV
    Src_PDO_Max_Current2:                                   300           ; 3000 mA
    Src_PD_OCP_OC_Debounce2:                                1000          ; 1000 msec
    Src_PD_OCP_OC_Threshold2:                               310           ; 3100 mA

    Src_PDO_Supply_Type3:                                   3             ; PPS
    Src_PDO_Max_Current3:                                   100           ; 5000 mA
    Src_PDO_Min_Voltage3:                                   33            ; 3300 mV
    Src_PDO_Max_Voltage3:                                   59            ; 5900 mV

    Src_PDO_Supply_Type4:                                   3             ; PPS
    Src_PDO_Max_Current4:                                   60            ; 3000 mA
    Src_PDO_Min_Voltage4:                                   33            ; 3300 mV
    Src_PDO_Max_Voltage4:                                   110           ; 11000 mV


