Altium Designer Pick and Place Locations
C:\SubVersion\MB1397-STM32G4-RockFish512K-469_EVAL\Trunk\03-Manufacturing\MB1397B_PCB\Assembly\MB1397-B01_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       06/09/18
Time:       15:48
Revision:   76
Variant:    G474E
Units used: mm

Designator   Comment                                                                                                                                        Layer       Footprint                                               Center-X(mm) Center-Y(mm) Rotation Description                                                                                                                                                                                       
SB123        SB_ON                                                                                                                                          BottomLayer SOLDER-BRIDGE_R0603-0R                                  55.9300      129.4874     0        "Solder Bridge ON"                                                                                                                                                                                
CN32         "Jumper_Header 2x1"                                                                                                                            TopLayer    CON_SAMTEC_TSW-102-07-G-S                               88.0618      118.6129     360      "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm"                                                                                                                                               
U11          IS61WV51216BLL-10MLI                                                                                                                           TopLayer    ICC_MINI-BGA48_9X11_P075                                66.1243      101.2099     180      "SRAM,?8Mb,?10ns, 512Kx16bits, Async,?3.3v"                                                                                                                                                       
LD5          LED_white                                                                                                                                      TopLayer    LED_EVERLUCK_CWC12100_WHITE_1A2K                        44.7761      84.1613      360      "White SMD LED lamp, Forward Voltage Typ=2.8V, Max=3.6V"                                                                                                                                          
U42          ST8024CTR                                                                                                                                      TopLayer    ICC_SO28_18P10X7P60_P127                                56.2983      24.1747      360      "Smartcard interfaces"                                                                                                                                                                            
R290         Resistor                                                                                                                                       TopLayer    R0603                                                   58.9001      16.2992      270      Resistor,100K,0603,1%,1/10W                                                                                                                                                                       
R291         Resistor                                                                                                                                       TopLayer    R0402                                                   46.1029      16.4023      270      Resistor,4K7,0402,1%,1/16W                                                                                                                                                                        
R274         Resistor                                                                                                                                       TopLayer    R0603                                                   49.3133      31.3121      90       Resistor,10K,0603,1%,1/10W                                                                                                                                                                        
R273         Resistor                                                                                                                                       TopLayer    R0603                                                   47.9739      31.3121      90       Resistor,10K,0603,1%,1/10W                                                                                                                                                                        
D10          EMIF03-SIM02M8                                                                                                                                 TopLayer    ESD_UQFN8-EPAD_1P7X1P5_P040                             64.0938      31.4826      360      "3 line IPAD, EMI filter for SIM card applications"                                                                                                                                               
C126         Capacitor                                                                                                                                      TopLayer    C0603                                                   62.0133      31.2883      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0603, T=0,8mm"                                                                                                                                            
C127         Capacitor                                                                                                                                      TopLayer    C0603                                                   56.2766      31.0883      360      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0603, T=0,8mm"                                                                                                                                            
C121         Cap_POL_TANA                                                                                                                                   TopLayer    CPOL_TAJ-C_2312_H2P6                                    54.6361      34.3130      180      "Capacitor, Tantalum, 47uF, 16V, 10%, TypeC"                                                                                                                                                      
C155         Capacitor                                                                                                                                      TopLayer    C0603                                                   57.6301      16.3043      270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0603, T=0,8mm"                                                                                                                                            
C153         Capacitor                                                                                                                                      TopLayer    C0603                                                   54.9885      16.3297      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0603, T=0,8mm"                                                                                                                                            
C152         Cap_POL_TANA                                                                                                                                   TopLayer    CPOL_TAJ-C_2312_H2P6                                    50.3955      16.2499      180      "Capacitor, Tantalum, 47uF, 16V, 10%, TypeC"                                                                                                                                                      
C154         Capacitor                                                                                                                                      TopLayer    C0603                                                   56.3601      16.3043      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0603, T=0,8mm"                                                                                                                                            
U44          ESD-TRANSIL                                                                                                                                    TopLayer    ESD_ST0201                                              43.3555      23.8001      360      "ESD protection 6V1"                                                                                                                                                                              
U12          MT25QL512ABB8ESF-0SIT                                                                                                                          TopLayer    ICC_SOP2-SF_16P_10P3X7P5_P127                           82.9036      101.0143     90       "Micron Serial NOR Flash Memory"                                                                                                                                                                  
SB120        SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  90.0850      101.3493     180      "Solder Bridge OFF"                                                                                                                                                                               
U8           TS432AILT                                                                                                                                      TopLayer    ICC_SOT23-3L_H1P12                                      111.8589     119.3012     90       "1.24V adjustable shunt voltage reference, Precision 0.5%"                                                                                                                                        
C32          Capacitor                                                                                                                                      TopLayer    C0603                                                   25.1456      118.6844     360      Capacitor,120pF,50V,NPO,5%,0603                                                                                                                                                                   
C14          Capacitor                                                                                                                                      TopLayer    C0603                                                   25.1130      152.4483     180      Capacitor,120pF,50V,NPO,5%,0603                                                                                                                                                                   
C15          Capacitor                                                                                                                                      TopLayer    C0603                                                   25.1206      148.5113     180      Capacitor,120pF,50V,NPO,5%,0603                                                                                                                                                                   
C18          Capacitor                                                                                                                                      TopLayer    C0603                                                   25.1456      141.7320     180      Capacitor,120pF,50V,NPO,5%,0603                                                                                                                                                                   
C21          Capacitor                                                                                                                                      TopLayer    C0603                                                   25.1130      135.5090     360      Capacitor,120pF,50V,NPO,5%,0603                                                                                                                                                                   
C25          Capacitor                                                                                                                                      TopLayer    C0603                                                   25.1206      125.1204     360      Capacitor,120pF,50V,NPO,5%,0603                                                                                                                                                                   
U36          ESD-TRANSIL                                                                                                                                    TopLayer    ESD_QFN1610_2N_1K_2A                                    9.9060       46.4820      360      "High power transient voltage suppressor"                                                                                                                                                         
U55          USBLC6-2SC6                                                                                                                                    BottomLayer ESD_SOT23-6L                                            11.6561      53.2613      360      "Very low capacitance ESD protection"                                                                                                                                                             
U43          ESD-TRANSIL                                                                                                                                    TopLayer    DIO_SMC_DO214-AB_1K_2A                                  15.3975      22.6490      90       "3000 W Transil"                                                                                                                                                                                  
F1           0ZCG0260FF2C                                                                                                                                   TopLayer    PTC_BEL-FUSE_1812_0ZCG0260FF2C                          15.3972      15.5538      360      "SMD, PTC resettable fuse, IH:2.6A, IT:5A, Vdc_max:8V, Rmax:47mohm, BELFUSE"                                                                                                                      
U30          ESDAxxL                                                                                                                                        TopLayer    ESD_SOT23                                               11.7831      53.3400      0        "Dual Transil array ESD protection"                                                                                                                                                               
U1           USBLC6-2SC6                                                                                                                                    TopLayer    ESD_SOT23-6L                                            31.0970      167.6266     90       "Very low capacitance ESD protection"                                                                                                                                                             
SB22         SB_OFF                                                                                                                                         TopLayer    SOLDER-BRIDGE_R0603-0R                                  114.7700     119.3070     270      "Solder Bridge OFF"                                                                                                                                                                               
SB102        SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  113.0328     119.4283     360      "Solder Bridge OFF"                                                                                                                                                                               
SB30         SB_OFF                                                                                                                                         TopLayer    SOLDER-BRIDGE_R0603-0R                                  113.3653     113.4290     90       "Solder Bridge OFF"                                                                                                                                                                               
SB31         SB_ON                                                                                                                                          TopLayer    SOLDER-BRIDGE_R0603-0R                                  114.9071     113.4102     90       "Solder Bridge ON"                                                                                                                                                                                
Q4           9013-SOT23                                                                                                                                     BottomLayer NPN_SOT23                                               113.4110     116.7384     180      "NPN Bipolar Transistor"                                                                                                                                                                          
C181         Capacitor                                                                                                                                      BottomLayer C0402                                                   114.9071     119.0473     270      "Capacitor, MLCC, 100pF, 50V, NPO, 5%, 0402, T=0,5mm"                                                                                                                                             
C59          Capacitor                                                                                                                                      TopLayer    C0402                                                   68.2269      85.1480      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C30          Capacitor                                                                                                                                      TopLayer    C0603                                                   114.7572     121.8082     180      "Capacitor, MLCC, 10¦ÌF, 10V, X5R, 10%, 0603, T=0.8mm"                                                                                                                                             
C180         Capacitor                                                                                                                                      BottomLayer C0603                                                   109.6010     118.8198     90       "Capacitor, MLCC, 10¦ÌF, 10V, X5R, 10%, 0603, T=0.8mm"                                                                                                                                             
SB16         SB_ON                                                                                                                                          TopLayer    SOLDER-BRIDGE_R0603-0R                                  113.8911     135.1266     270      "Solder Bridge ON"                                                                                                                                                                                
SB75         SB_ON                                                                                                                                          BottomLayer SOLDER-BRIDGE_R0603-0R                                  113.8911     135.7266     90       "Solder Bridge ON"                                                                                                                                                                                
L2           Inductor                                                                                                                                       TopLayer    IND_POWER_CYNTEC_PSI054T                                40.6420      100.5053     180      "SMD power inductor. 82uH, 1.0A, 400mohm, 4.9x4.9x4.0mm"                                                                                                                                          
U9           ESD-TRANSIL                                                                                                                                    TopLayer    ESD_ST0201                                              89.6341      112.0419     360      "ESD protection 6V1"                                                                                                                                                                              
U5           ESD-TRANSIL-BIDIR                                                                                                                              TopLayer    ESD_ST0201                                              114.1950     145.2880     360      "Single-line low capacitance Transil for bidirectional ESD protection 6V1"                                                                                                                        
U3           STTS751-0DP3F                                                                                                                                  TopLayer    ICC_UDFN6_2X2_P065                                      28.7824      155.3210     270      "IC, 2.25 V low-voltage local digital temperature sensor, UDFN-6L"                                                                                                                                
R177         Resistor                                                                                                                                       TopLayer    R1206_H0P55                                             48.5688      96.1644      180      "Resistor, 1R, 1206, 1%, 1/4W"                                                                                                                                                                    
CN19         "Header 10x2"                                                                                                                                  TopLayer    CON_SAMTEC_FTSH-110-01-L-DV-A                           8.0010       61.5950      360      "Header 10x2, 1.27mm, VR, CMS, Height 3.05mm with alignment pin"                                                                                                                                  
CN24         "Socket 4x2_LCD_PWR_MODULE_MB895C"                                                                                                             TopLayer    CON_SOCKET-LCD_LYCN_216208S141                          100.3300     31.7500      270      "socket, 4x2, 2.54mm, VR, TH, Height 6.8mm, Double row"                                                                                                                                           
CN20         "Socket 4x2_LCD_IO_MODULE_MB895C"                                                                                                              TopLayer    CON_SOCKET-LCD_LYCN_216208S141                          100.3300     57.1500      270      "Socket, 4x2, 2.54mm, VR, TH, Height 6.8mm, Double row"                                                                                                                                           
B1           "Joystick MT-008A_M"                                                                                                                           TopLayer    SWI_XIEJIA_MT-008A_6P                                   64.8893      6.3700       45       "Joystick, 4 dir, 1 OK"                                                                                                                                                                           
B2           SW_BLUE_KSC721GLFS                                                                                                                             TopLayer    SWI_C&K_KSC721GLFS_BLUE                                 50.4140      6.3180       360      "Switch HW BLUE High4.3mm 2.25 Newtons"                                                                                                                                                           
B3           SW-PUSH-CMS                                                                                                                                    TopLayer    SWI_WEALTHMETAL_TD-0341_4P_BLACK                        80.1400      5.8750       90       "Non-Open Push-Button 0.1A 24V BLACK"                                                                                                                                                             
C53          Capacitor                                                                                                                                      TopLayer    C0402                                                   37.4505      95.1244      270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C52          Capacitor                                                                                                                                      TopLayer    C0402                                                   29.3033      97.4804      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C44          Capacitor                                                                                                                                      TopLayer    C0402                                                   37.4505      104.3062     270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C40          Capacitor                                                                                                                                      TopLayer    C0402                                                   29.2501      106.3642     90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C185         Capacitor                                                                                                                                      BottomLayer C0603                                                   12.9134      49.0830      360      "Capacitor, MLCC, 10pF, 50V, NPO, 5%, 0603, T=0,8mm"                                                                                                                                              
C186         Capacitor                                                                                                                                      BottomLayer C0402                                                   96.3655      15.4153      360      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C69          Capacitor                                                                                                                                      TopLayer    C0603                                                   84.0713      58.6191      180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0603, T=0,8mm"                                                                                                                                            
C70          Capacitor                                                                                                                                      TopLayer    C0603                                                   91.0309      58.5936      180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0603, T=0,8mm"                                                                                                                                            
C64          Capacitor                                                                                                                                      TopLayer    C0603                                                   84.0205      61.4639      180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0603, T=0,8mm"                                                                                                                                            
C65          Capacitor                                                                                                                                      TopLayer    C0603                                                   91.0309      61.3368      180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0603, T=0,8mm"                                                                                                                                            
C129         Capacitor                                                                                                                                      TopLayer    C0805                                                   94.9452      29.2354      270      "Capacitor, MLCC, 10uF, 25V, X5R, 10%, 0805, T=0,85mm"                                                                                                                                            
C132         Capacitor                                                                                                                                      TopLayer    C0402                                                   96.3422      29.2862      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C48          Capacitor                                                                                                                                      TopLayer    C0402                                                   59.8759      101.0879     180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C47          Capacitor                                                                                                                                      TopLayer    C0402                                                   72.5327      101.5731     360      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C157         Capacitor                                                                                                                                      TopLayer    C0402                                                   50.8000      10.6680      270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C89          Capacitor                                                                                                                                      TopLayer    C0603                                                   111.0269     49.3022      360      "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                                                                                                                                            
C43          Capacitor                                                                                                                                      TopLayer    C0603                                                   42.4400      104.8352     270      "Capacitor, MLCC, 1uF, 16V, X5R, 10%, 0603, T=0,8mm"                                                                                                                                              
C45          Capacitor                                                                                                                                      TopLayer    C0603                                                   40.4420      104.1508     360      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0603, T=0,8mm"                                                                                                                                            
C41          Cap_POL_TANA                                                                                                                                   TopLayer    CPOL_TAJ-C_2312_H2P6                                    49.4538      103.3424     270      "Capacitor, Tantalum, 47uF, 16V, 10%, TypeC"                                                                                                                                                      
C49          Capacitor                                                                                                                                      TopLayer    C0402                                                   50.1498      98.4504      180      "Capacitor, MLCC, 1nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                              
C13          Capacitor                                                                                                                                      TopLayer    C0603                                                   25.6515      154.8968     180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0603, T=0,8mm"                                                                                                                                            
C109         Cap_POL_TANA                                                                                                                                   TopLayer    CPOL_TAJ-C_2312_H2P6                                    32.4587      38.8620      180      "Capacitor, Tantalum, 220uF, 10V, 10%, TypeC"                                                                                                                                                     
C147         Capacitor                                                                                                                                      TopLayer    C0402                                                   19.3040      20.2632      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C149         Capacitor                                                                                                                                      TopLayer    C0603                                                   38.2146      17.6938      270      "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                                                                                                                                            
C156         Capacitor                                                                                                                                      TopLayer    C0603                                                   42.4419      15.2044      90       "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                                                                                                                                            
C146         Capacitor                                                                                                                                      TopLayer    C0402                                                   41.3235      20.7418      180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C150         Capacitor                                                                                                                                      TopLayer    C0603                                                   34.6626      17.6558      90       "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                                                                                                                                            
C151         Capacitor                                                                                                                                      TopLayer    C0603                                                   29.5504      17.5402      270      "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                                                                                                                                            
C79          Capacitor                                                                                                                                      TopLayer    C0603                                                   83.9543      53.9113      360      "Capacitor, MLCC, 1uF, 16V, X5R, 10%, 0603, T=0,8mm"                                                                                                                                              
C73          Capacitor                                                                                                                                      TopLayer    C0603                                                   90.4122      54.8573      90       "Capacitor, MLCC, 1uF, 16V, X5R, 10%, 0603, T=0,8mm"                                                                                                                                              
C74          Capacitor                                                                                                                                      TopLayer    C0402                                                   83.9542      55.5271      360      "Capacitor, MLCC, 10nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                             
C58          Capacitor                                                                                                                                      TopLayer    C0402                                                   26.9240      85.5980      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C57          Capacitor                                                                                                                                      TopLayer    C0402                                                   28.4201      87.6554      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C56          Capacitor                                                                                                                                      TopLayer    C0402                                                   26.9240      87.7130      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C55          Capacitor                                                                                                                                      TopLayer    C0402                                                   16.2560      88.6204      270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C54          Capacitor                                                                                                                                      TopLayer    C0402                                                   15.2400      88.6454      270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C61          Capacitor                                                                                                                                      TopLayer    C0603                                                   24.0387      66.4870      270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0603, T=0,8mm"                                                                                                                                            
C62          Capacitor                                                                                                                                      TopLayer    C0603                                                   25.5627      66.4824      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0603, T=0,8mm"                                                                                                                                            
C60          Capacitor                                                                                                                                      TopLayer    C0603                                                   15.7480      77.6893      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0603, T=0,8mm"                                                                                                                                            
C148         Capacitor                                                                                                                                      TopLayer    C0402                                                   75.7297      20.3103      360      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C141         Capacitor                                                                                                                                      TopLayer    C0402                                                   79.5903      23.4486      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C114         Capacitor                                                                                                                                      TopLayer    C0603                                                   81.0115      37.4720      270      "Capacitor, MLCC, 2.2uF, 10V, X5R, 10%, 0603, T=0,8mm"                                                                                                                                            
C122         Capacitor                                                                                                                                      TopLayer    C1206_H1P15                                             86.4020      33.6752      270      "Capacitor, MLCC, 2.2uF, 16V, X7R, 10%, 1206, T=1,15mm"                                                                                                                                           
C115         Capacitor                                                                                                                                      TopLayer    C1206_H1P15                                             74.4327      37.4720      360      "Capacitor, MLCC, 2.2uF, 16V, X7R, 10%, 1206, T=1,15mm"                                                                                                                                           
C118         Capacitor                                                                                                                                      TopLayer    C0402                                                   82.3067      37.4186      270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C117         Capacitor                                                                                                                                      TopLayer    C0402                                                   78.4967      37.4186      270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C142         Capacitor                                                                                                                                      TopLayer    C0402                                                   83.5767      23.4486      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C130         Capacitor                                                                                                                                      TopLayer    C0402                                                   86.3317      29.9181      180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C131         Capacitor                                                                                                                                      TopLayer    C0402                                                   72.4007      29.7986      360      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C140         Capacitor                                                                                                                                      TopLayer    C0402                                                   77.6467      23.4486      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C137         Capacitor                                                                                                                                      TopLayer    C0402                                                   80.5396      23.4486      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C138         Capacitor                                                                                                                                      TopLayer    C0402                                                   75.7027      23.4486      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C81          Capacitor                                                                                                                                      TopLayer    C0603                                                   111.0269     50.5722      180      Capacitor,100pF,50V,X7R,10%,0603                                                                                                                                                                  
C133         Capacitor                                                                                                                                      TopLayer    C0402                                                   72.3927      28.9116      360      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C134         Capacitor                                                                                                                                      TopLayer    C0402                                                   72.4007      25.7976      360      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C145         Capacitor                                                                                                                                      TopLayer    C0402                                                   82.6068      23.4485      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C128         Capacitor                                                                                                                                      TopLayer    C0402                                                   86.3707      30.9260      180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C116         Capacitor                                                                                                                                      TopLayer    C0402                                                   77.3467      37.4186      270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C144         Capacitor                                                                                                                                      TopLayer    C0402                                                   85.4707      23.4486      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C143         Capacitor                                                                                                                                      TopLayer    C0402                                                   84.5407      23.4486      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C139         Capacitor                                                                                                                                      TopLayer    C0402                                                   76.7579      23.4486      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C113         Capacitor                                                                                                                                      TopLayer    C0603                                                   83.7823      37.4861      270      "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                                                                                                                                            
C135         Capacitor                                                                                                                                      TopLayer    C0603                                                   72.2327      23.7026      90       "Capacitor, MLCC, 1uF, 16V, X5R, 10%, 0603, T=0,8mm"                                                                                                                                              
C136         Capacitor                                                                                                                                      TopLayer    C0402                                                   73.4167      23.5180      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C67          Capacitor                                                                                                                                      TopLayer    C0603                                                   54.8386      58.2159      270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0603, T=0,8mm"                                                                                                                                            
C68          Capacitor                                                                                                                                      TopLayer    C0603                                                   56.5434      58.2159      270      "Capacitor, MLCC, 1uF, 16V, X5R, 10%, 0603, T=0,8mm"                                                                                                                                              
C66          Capacitor                                                                                                                                      TopLayer    C0603                                                   51.7509      61.1556      360      "Capacitor, MLCC, 1uF, 16V, X5R, 10%, 0603, T=0,8mm"                                                                                                                                              
C63          Capacitor                                                                                                                                      TopLayer    C0402                                                   51.7573      62.5373      180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C71          Capacitor                                                                                                                                      TopLayer    C0402                                                   49.8170      58.0659      270      "Capacitor, MLCC, 10nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                             
C72          Capacitor                                                                                                                                      TopLayer    C0402                                                   60.7060      57.2973      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C183         Capacitor                                                                                                                                      BottomLayer C0402                                                   62.4586      119.1260     360      "Capacitor, MLCC, 5.6pF, 50V, NPO, 5%, 0402, T=0,5mm"                                                                                                                                             
C182         Capacitor                                                                                                                                      BottomLayer C0402                                                   64.3484      119.1514     180      "Capacitor, MLCC, 5.6pF, 50V, NPO, 5%, 0402, T=0,5mm"                                                                                                                                             
C178         Capacitor                                                                                                                                      BottomLayer C0402                                                   71.0028      118.9990     270      "Capacitor, MLCC, 3.9pF, 50V, NPO, +-0.25pF, 0402, T=0,5mm"                                                                                                                                       
C177         Capacitor                                                                                                                                      BottomLayer C0402                                                   69.8028      120.8659     180      "Capacitor, MLCC, 3.9pF, 50V, NPO, +-0.25pF, 0402, T=0,5mm"                                                                                                                                       
C163         Capacitor                                                                                                                                      BottomLayer C0603                                                   59.8170      129.6924     90       "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                                                                                                                                            
C161         Capacitor                                                                                                                                      BottomLayer C0402                                                   67.6028      136.5659     180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C160         Capacitor                                                                                                                                      BottomLayer C0402                                                   60.9027      136.5859     180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C173         Capacitor                                                                                                                                      BottomLayer C0402                                                   59.0827      123.1659     270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C162         Capacitor                                                                                                                                      BottomLayer C0402                                                   74.3227      134.7159     90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C176         Capacitor                                                                                                                                      BottomLayer C0402                                                   72.3392      121.6378     360      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C165         Capacitor                                                                                                                                      BottomLayer C0402                                                   72.1027      128.3033     90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C175         Capacitor                                                                                                                                      BottomLayer C0402                                                   65.1002      121.3358     270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C164         Capacitor                                                                                                                                      BottomLayer C0402                                                   58.6028      129.6659     270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C174         Capacitor                                                                                                                                      BottomLayer C0402                                                   69.8246      122.0216     180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C167         Capacitor                                                                                                                                      BottomLayer C0603                                                   76.4171      125.8986     270      "Capacitor, MLCC, 1uF, 16V, X5R, 10%, 0603, T=0,8mm"                                                                                                                                              
C166         Capacitor                                                                                                                                      BottomLayer C0805                                                   71.7042      126.0259     90       "Capacitor, MLCC, 10uF, 25V, X5R, 10%, 0805, T=0,85mm"                                                                                                                                            
C168         Capacitor                                                                                                                                      BottomLayer C0402                                                   73.6600      126.1593     90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C170         Capacitor                                                                                                                                      BottomLayer C0402                                                   75.3969      126.1110     90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C159         Capacitor                                                                                                                                      BottomLayer C0603                                                   110.9312     147.4411     270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0603, T=0,8mm"                                                                                                                                            
C158         Capacitor                                                                                                                                      BottomLayer C0603                                                   113.4030     150.6070     0        "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0603, T=0,8mm"                                                                                                                                            
C171         Capacitor                                                                                                                                      BottomLayer C0603                                                   75.7174      123.7488     180      Capacitor,100pF,50V,X7R,10%,0603                                                                                                                                                                  
C35          Capacitor                                                                                                                                      TopLayer    C0603                                                   79.7814      111.4329     270      Capacitor,100pF,50V,X7R,10%,0603                                                                                                                                                                  
C50          Capacitor                                                                                                                                      TopLayer    C0402                                                   106.9340     97.9483      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C28          Capacitor                                                                                                                                      TopLayer    C0603                                                   111.8580     123.1749     360      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0603, T=0,8mm"                                                                                                                                            
C179         Capacitor                                                                                                                                      BottomLayer C0603                                                   110.8456     118.8198     90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0603, T=0,8mm"                                                                                                                                            
C96          Capacitor                                                                                                                                      TopLayer    C0402                                                   92.4216      45.4660      360      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C84          Capacitor                                                                                                                                      TopLayer    C0603                                                   85.5287      49.6257      270      "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                                                                                                                                            
C94          Capacitor                                                                                                                                      TopLayer    C0402                                                   83.5967      46.0766      180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C92          Capacitor                                                                                                                                      TopLayer    C0603                                                   83.5967      47.1187      360      "Capacitor, MLCC, 1uF, 16V, X5R, 10%, 0603, T=0,8mm"                                                                                                                                              
C100         Capacitor                                                                                                                                      TopLayer    C0402                                                   92.3028      43.0784      360      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C97          Capacitor                                                                                                                                      TopLayer    C0603                                                   83.5469      44.8564      360      "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                                                                                                                                            
C93          Capacitor                                                                                                                                      TopLayer    C0402                                                   92.4216      46.2839      360      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C91          Capacitor                                                                                                                                      TopLayer    C0603                                                   92.4867      47.3728      180      "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                                                                                                                                            
C101         Capacitor                                                                                                                                      TopLayer    C0603                                                   83.5967      42.8218      360      "Capacitor, MLCC, 1uF, 16V, X5R, 10%, 0603, T=0,8mm"                                                                                                                                              
C85          Capacitor                                                                                                                                      TopLayer    C0603                                                   86.7627      49.6257      90       "Capacitor, MLCC, 1uF, 16V, X5R, 10%, 0603, T=0,8mm"                                                                                                                                              
C90          Capacitor                                                                                                                                      TopLayer    C0603                                                   92.4867      48.7007      180      "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                                                                                                                                            
C86          Capacitor                                                                                                                                      TopLayer    C0603                                                   89.3387      49.6257      270      "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                                                                                                                                            
C88          Capacitor                                                                                                                                      TopLayer    C0603                                                   88.0397      49.6007      270      "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                                                                                                                                            
C106         Capacitor                                                                                                                                      TopLayer    C0402                                                   89.0473      40.5654      270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C107         Capacitor                                                                                                                                      TopLayer    C0402                                                   86.7613      40.5384      270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C99          Capacitor                                                                                                                                      TopLayer    C0603                                                   92.4331      44.1173      360      "Capacitor, MLCC, 1uF, 16V, X5R, 10%, 0603, T=0,8mm"                                                                                                                                              
C87          Capacitor                                                                                                                                      TopLayer    C0603                                                   90.5517      49.6257      90       "Capacitor, MLCC, 1uF, 16V, X5R, 10%, 0603, T=0,8mm"                                                                                                                                              
C103         Capacitor                                                                                                                                      TopLayer    C0603                                                   92.7100      40.6654      90       "Capacitor, MLCC, 2.2uF, 10V, X5R, 10%, 0603, T=0,8mm"                                                                                                                                            
C105         Capacitor                                                                                                                                      TopLayer    C0603                                                   91.4484      40.6559      90       "Capacitor, MLCC, 2.2uF, 10V, X5R, 10%, 0603, T=0,8mm"                                                                                                                                            
C104         Capacitor                                                                                                                                      TopLayer    C0603                                                   94.1070      40.6654      90       "Capacitor, MLCC, 2.2uF, 10V, X5R, 10%, 0603, T=0,8mm"                                                                                                                                            
C1           Capacitor                                                                                                                                      TopLayer    C0402                                                   90.1700      158.1150     90       "Capacitor, MLCC, 1nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                              
C4           Capacitor                                                                                                                                      TopLayer    C0402                                                   77.9380      157.8872     90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C7           Capacitor                                                                                                                                      TopLayer    C0402                                                   64.8011      157.8372     270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C5           Capacitor                                                                                                                                      TopLayer    C0402                                                   62.2704      157.8452     270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C12          Capacitor                                                                                                                                      TopLayer    C0402                                                   53.5269      157.0872     360      "Capacitor, MLCC, 10nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                             
C16          Capacitor                                                                                                                                      TopLayer    C0402                                                   10.6680      148.7090     180      "Capacitor, MLCC, 1nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                              
C22          Capacitor                                                                                                                                      TopLayer    C0402                                                   10.6680      134.9410     180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C38          Capacitor                                                                                                                                      TopLayer    C0402                                                   11.2940      109.7732     270      "Capacitor, MLCC, 10nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                             
C98          Capacitor                                                                                                                                      TopLayer    C0402                                                   62.8578      44.4551      360      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C80          Capacitor                                                                                                                                      TopLayer    C0402                                                   78.1291      53.2381      180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C82          Capacitor                                                                                                                                      TopLayer    C0402                                                   79.9084      50.2210      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C83          Capacitor                                                                                                                                      TopLayer    C0402                                                   80.7720      50.2133      270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C75          Capacitor                                                                                                                                      TopLayer    C0603                                                   76.3131      54.3953      270      "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                                                                                                                                            
C77          Capacitor                                                                                                                                      TopLayer    C0402                                                   69.1451      54.3950      270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C78          Capacitor                                                                                                                                      TopLayer    C0402                                                   69.9452      54.3527      270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C108         Capacitor                                                                                                                                      TopLayer    C0603                                                   46.9552      40.6070      180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0603, T=0,8mm"                                                                                                                                            
C120         Capacitor                                                                                                                                      TopLayer    C0603                                                   38.2188      36.7231      360      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0603, T=0,8mm"                                                                                                                                            
C119         Capacitor                                                                                                                                      TopLayer    C0603                                                   52.5394      37.4720      360      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0603, T=0,8mm"                                                                                                                                            
C110         Capacitor                                                                                                                                      TopLayer    C0603                                                   38.2188      39.4250      360      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0603, T=0,8mm"                                                                                                                                            
C112         Capacitor                                                                                                                                      TopLayer    C0603                                                   50.1894      38.7352      270      "Capacitor, MLCC, 1uF, 16V, X5R, 10%, 0603, T=0,8mm"                                                                                                                                              
C111         Capacitor                                                                                                                                      TopLayer    C0603                                                   46.4052      38.7441      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0603, T=0,8mm"                                                                                                                                            
C51          Capacitor                                                                                                                                      TopLayer    C0402                                                   89.7616      97.9663      180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C184         Capacitor                                                                                                                                      BottomLayer C0402                                                   89.6447      103.7600     90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C76          Capacitor                                                                                                                                      TopLayer    C0603                                                   67.8612      54.3530      270      "Capacitor, MLCC, 1uF, 16V, X5R, 10%, 0603, T=0,8mm"                                                                                                                                              
CN12         "Header 2x1"                                                                                                                                   TopLayer    CON_988-JIUBABA_PHFS25-11-02-G0B115-T-1                 19.1863      95.0373      90       "Header, 2x1, 2.54mm, VR, TH, Height 6mm/3mm"                                                                                                                                                     
CN17         "Header 10x2"                                                                                                                                  TopLayer    CON_SAMTEC_FTSH-110-01-L-DV-A                           96.3930      73.4580      270      "Header 10x2, 1.27mm, VR, CMS, Height 3.05mm with alignment pin"                                                                                                                                  
CN14         "Header 10x2"                                                                                                                                  TopLayer    CON_CVILUX_CH87-20-2-V-1-00                             112.3950     74.9300      270      "Header, 2.54mm, 10x2, VR, TH, Height 9.1mm/3,1mm"                                                                                                                                                
CN28         microSD-PJS008-2003                                                                                                                            TopLayer    CON_MICROSD_YAMAICHI_PJS008-2003-1                      94.7980      9.0500       270      "MicroSD Card Conn, Reversed-Type, Mnt Push-Push, Positionning holes"                                                                                                                             
CN1          "Socket 4x2"                                                                                                                                   TopLayer    CON_SAMTEC_SSM-104-L-DH                                 22.1354      165.1588     90       "Socket, 4x2, 2.54mm, RA, SMT, Height 5.72mm"                                                                                                                                                     
CN25         Power_Jack_DC10B                                                                                                                               TopLayer    CON_DC-POWER-SOCKET_CLIFF_FC68149_DC10B                 6.9750       17.4767      180      "DC-Power-Jack, 2.5mm, 5A, RA, TH"                                                                                                                                                                
CN11         DB9_Header_male_3-1634580-2                                                                                                                    TopLayer    CON_DB9-MALE_TYCO_3-1634580-2                           9.1440       84.8332      270      "Header, DB9, RA, TH, Height 13.57mm"                                                                                                                                                             
CN21         USB_uB_105017.0001                                                                                                                             TopLayer    CON_USBMICROB_MOLEX_105017-0001_H2P90                   115.2881     52.7210      90       "USB-MICRO-B, 0.65mm, RA, SMT, Bottom Mount,"                                                                                                                                                     
CN16         "Header 7x2"                                                                                                                                   TopLayer    CON_STDC14_Receiver_MEDIUM_WITH_MIPI10_3D               86.2264      73.5774      90       "Header 5x2, 1.27mm, Dual row, Straight, Surface mount, vertical male connector. 3.05mm lead. Mates with FFSD connector. Footprint compatible with FTSH-107-01-L-DV,-K,-A,-P,-ES (STDC14 MEDIUM)" 
CN13         "BATTERY HOLDER"                                                                                                                               TopLayer    BAT_HARWIN_S8411-45R_SMD_2P                             59.9923      82.8040      90       "Battery Coin Cell holder, CR1220_12mm, Height 4.25mm"                                                                                                                                            
CN5          "Header 30x2"                                                                                                                                  TopLayer    CON_SAMTEC_FTR-130-53-L-D-LC                            33.8349      131.3956     270      "Header 30x2, 1.27mm, VR, CMS, Height 7.24mm"                                                                                                                                                     
CN6          "Header 30x2"                                                                                                                                  TopLayer    CON_SAMTEC_FTR-130-53-L-D-LC                            102.4149     131.3956     270      "Header 30x2, 1.27mm, VR, CMS, Height 7.24mm"                                                                                                                                                     
CN3          SMB-ZJWE-3                                                                                                                                     TopLayer    CON_JACK-RIGHT-ANGLE_YJ-ELECTRONIC_SMB-ZJWE-3           113.8842     156.4640     360      "SMB type right angle jack for PCB"                                                                                                                                                               
CN9          "Jumper_Header 2x1"                                                                                                                            TopLayer    CON_SAMTEC_TSW-102-07-G-S                               88.1471      115.2787     360      "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm"                                                                                                                                               
CN26         Jack_PJ3028B-3_3P                                                                                                                              TopLayer    CON_PHONE-JACK-3P5_HY_PJ3028B                           108.8406     20.5740      180      "Connector Jack socket Stereo 3.5mm, 3 pins, RA, SMT, Green (Line output)"                                                                                                                        
CN23         Jack_PJ3028B-3_3P                                                                                                                              TopLayer    CON_PHONE-JACK-3P5_HY_PJ3028B                           108.8600     41.7830      180      "Connector Jack socket Stereo 3.5mm, 3 pins, RA, SMT, Blue (Line input)"                                                                                                                          
CN2          "Header 17x2 IDC34 MotorControl"                                                                                                               TopLayer    CON_SAMTEC_TST-117-01-T-D                               71.1200      164.4650     180      "Header, 17x2, 2.54mm, VR, TH, Height 8.89mm/2.92mm, shrouded"                                                                                                                                    
CN4          "Header 17x2 IDC34 MotorControl"                                                                                                               TopLayer    CON_SAMTEC_TST-117-01-T-D                               4.4450       128.9050     270      "Header, 17x2, 2.54mm, VR, TH, Height 8.89mm/2.92mm, shrouded"                                                                                                                                    
CN10         "Header 2x1"                                                                                                                                   TopLayer    CON_988-JIUBABA_PHFS25-11-02-G0B115-T-1                 19.1863      104.0596     90       "Header, 2x1, 2.54mm, VR, TH, Height 6mm/3mm"                                                                                                                                                     
CN22         "USB Type-C"                                                                                                                                   TopLayer    CON_USB-TYPEC_LITKCONN-TECHNOLOGY_CNG008S130R           4.3512       48.1590      270      "USB Type C certified Connector SMT Mid-mount"                                                                                                                                                    
D1           SCHOTTKY                                                                                                                                       TopLayer    DIO_SMA_1A_2K                                           45.3390      103.7082     270      "Low Drop power Schottky rectifier(1A, 40V, 0.37 V)"                                                                                                                                              
D6           BAT60JFILM                                                                                                                                     TopLayer    DIO_SOD323                                              47.5943      61.7403      270      BAT60JFILM                                                                                                                                                                                        
D5           BAT60JFILM                                                                                                                                     TopLayer    DIO_SOD323                                              42.2185      61.8085      270      BAT60JFILM                                                                                                                                                                                        
D8           STPS2L40UF                                                                                                                                     TopLayer    DIO_SMB-FLAT_1A_2K                                      16.3231      52.0805      270      "Low drop power Schottky rectifier(2A, 40V, 0.34V)"                                                                                                                                               
D4           BAT60JFILM                                                                                                                                     TopLayer    DIO_SOD323                                              44.0411      61.8153      270      BAT60JFILM                                                                                                                                                                                        
D3           BAT60JFILM                                                                                                                                     TopLayer    DIO_SOD323                                              45.8002      61.8241      270      BAT60JFILM                                                                                                                                                                                        
D9           STPS2L40UF                                                                                                                                     TopLayer    DIO_SMB-FLAT_1A_2K                                      21.0527      52.0230      270      "Low drop power Schottky rectifier(2A, 40V, 0.34V)"                                                                                                                                               
D11          BAT60JFILM                                                                                                                                     TopLayer    DIO_SOD323                                              78.2828      10.3632      180      BAT60JFILM                                                                                                                                                                                        
D2           BAT60JFILM                                                                                                                                     TopLayer    DIO_SOD323                                              84.4005      82.2194      90       BAT60JFILM                                                                                                                                                                                        
D7           BAT60JFILM                                                                                                                                     TopLayer    DIO_SOD323                                              72.2066      55.0673      90       BAT60JFILM                                                                                                                                                                                        
JP4          "Jumper_Header 2x1"                                                                                                                            TopLayer    CON_SAMTEC_TSW-102-07-G-S                               26.7825      95.1244      90       "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm"                                                                                                                                               
JP2          "Jumper_Header 2x1"                                                                                                                            TopLayer    CON_SAMTEC_TSW-102-07-G-S                               26.7825      104.3136     90       "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm"                                                                                                                                               
JP9          "Jumper_Header 3x1"                                                                                                                            TopLayer    CON_SAMTEC_TSW-103-07-F-S                               33.9949      81.0505      90       "Header, 3x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm"                                                                                                                                               
JP11         "Jumper_Header 3x1"                                                                                                                            TopLayer    CON_SAMTEC_TSW-103-07-F-S                               73.8302      72.1625      270      "Header, 3x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm"                                                                                                                                               
JP6          "Jumper_Header 3x1"                                                                                                                            TopLayer    CON_SAMTEC_TSW-103-07-F-S                               80.7720      88.3770      270      "Header, 3x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm"                                                                                                                                               
JP7          "Jumper_Header 3x1"                                                                                                                            TopLayer    CON_SAMTEC_TSW-103-07-F-S                               70.9243      88.1870      270      "Header, 3x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm"                                                                                                                                               
JP18         "Jumper_Header 2x1"                                                                                                                            TopLayer    CON_SAMTEC_TSW-102-07-G-S                               62.0776      68.8848      90       "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm"                                                                                                                                               
JP8          "Jumper_Header 2x1"                                                                                                                            TopLayer    CON_SAMTEC_TSW-102-07-G-S                               87.5383      84.5401      90       "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm"                                                                                                                                               
JP5          "Jumper_Header 3x1"                                                                                                                            TopLayer    CON_SAMTEC_TSW-103-07-F-S                               103.7008     97.6269      270      "Header, 3x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm"                                                                                                                                               
JP16         "Jumper_Header 2x1"                                                                                                                            TopLayer    CON_SAMTEC_TSW-102-07-G-S                               111.3539     34.4170      360      "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm"                                                                                                                                               
JP17         "Jumper_Header 2x1"                                                                                                                            TopLayer    CON_SAMTEC_TSW-102-07-G-S                               111.5060     29.3136      360      "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm"                                                                                                                                               
JP13         "Jumper_Header 3x1"                                                                                                                            TopLayer    CON_SAMTEC_TSW-103-07-F-S                               55.3045      69.2865      270      "Header, 3x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm"                                                                                                                                               
JP15         "Jumper_Header 3x1"                                                                                                                            TopLayer    CON_SAMTEC_TSW-103-07-F-S                               34.1172      69.0880      270      "Header, 3x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm"                                                                                                                                               
JP14         "Jumper_Header 3x1"                                                                                                                            TopLayer    CON_SAMTEC_TSW-103-07-F-S                               29.3370      69.0880      270      "Header, 3x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm"                                                                                                                                               
JP1          "Jumper_Header 2x1"                                                                                                                            TopLayer    CON_SAMTEC_TSW-102-07-G-S                               46.4058      116.0983     180      "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm"                                                                                                                                               
JP10         "Jumper_Header 2x1"                                                                                                                            TopLayer    CON_SAMTEC_TSW-102-07-G-S                               29.3370      82.1690      90       "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm"                                                                                                                                               
L6           BEAD                                                                                                                                           TopLayer    L0603                                                   92.6338      30.0228      360      "SMD Chip ferrite bead, 600R@100MHz +/-25%, 350mA, 500mohm DC, 0603, T=0.8mm"                                                                                                                     
L7           BEAD                                                                                                                                           TopLayer    L0603                                                   92.6338      28.3854      0        "SMD Chip ferrite bead, 600R@100MHz +/-25%, 350mA, 500mohm DC, 0603, T=0.8mm"                                                                                                                     
L4           BNX002-01                                                                                                                                      TopLayer    FIL_MURATA_BNX002-01                                    6.7764       33.5763      180      "Through HOLE DC power EMI line filter, 40dB min (1MHz - 1GHz) insertion loss"                                                                                                                    
L9           BEAD                                                                                                                                           BottomLayer L0603                                                   79.0516      125.7046     90       "SMD Chip ferrite bead, 600R@100MHz +/-25%, 350mA, 500mohm DC, 0603, T=0.8mm"                                                                                                                     
L3           BEAD                                                                                                                                           TopLayer    L0603                                                   62.8371      45.6915      180      "SMD Chip ferrite bead, 600R@100MHz +/-25%, 350mA, 500mohm DC, 0603, T=0.8mm"                                                                                                                     
LD1          LED_green                                                                                                                                      TopLayer    LED_0603_OSRAM_LG-Q396-PS-35_GREEN_1A2K_H0P4            26.9241      4.7661       90       "LED Green, 0603 SMD, Forward Voltage Typ=2V, Max=2.5V"                                                                                                                                           
LD2          LED_orange                                                                                                                                     TopLayer    LED_0603_OSRAM_LO-Q976-PS-25_ORANGE_1A2K_H0P8           29.1433      4.7661       90       "LED Orange, 0603 SMD, Forward Voltage Min=1.6V, Max=2.4V"                                                                                                                                        
LD3          LED_red                                                                                                                                        TopLayer    LED_0603_VISHAY_VLMS1300-GS08_RED_1A2K_H0P8             31.5665      4.7519       90       "LED Red, 0603 SMD, 2V Forward Voltage"                                                                                                                                                           
LD4          LED_blue                                                                                                                                       TopLayer    LED_0603_OSRAM_LB-Q39G-L2OO-35-1_BLUE_1A2K_H0P4         33.8099      4.7519       90       "LED Blue, 0603 SMD, Forward Voltage Min=2,8V, Max=3,8V"                                                                                                                                          
LD6          LED_green                                                                                                                                      TopLayer    LED_0603_OSRAM_LG-Q396-PS-35_GREEN_1A2K_H0P4            43.5337      75.4418      360      "LED Green, 0603 SMD, Forward Voltage Typ=2V, Max=2.5V"                                                                                                                                           
LD8          LD_BICOLOR_CMS                                                                                                                                 TopLayer    LED_BI-GR_HSMF-A201-A00J1                               38.0056      6.0500       0        "LED Bicolor"                                                                                                                                                                                     
LD7          LED_red                                                                                                                                        TopLayer    LED_0603_VISHAY_VLMS1300-GS08_RED_1A2K_H0P8             62.6374      57.0284      90       "LED Red, 0603 SMD, 2V Forward Voltage"                                                                                                                                                           
Q1           BSN20                                                                                                                                          TopLayer    MOS_SOT23                                               95.1230      55.8800      270      "N-channel enhancement mode field-effect transistor"                                                                                                                                              
Q3           STL9P3LLH6                                                                                                                                     TopLayer    MOS_POWERFLAT_3P3X3P3_P065                              21.3084      46.5287      360      "Power Mosfet, P-channel,VDS -30V,RDS 12mohm typ,ID -9A"                                                                                                                                          
Q2           STL9P3LLH6                                                                                                                                     TopLayer    MOS_POWERFLAT_3P3X3P3_P065                              16.6017      46.5303      360      "Power Mosfet, P-channel,VDS -30V,RDS 12mohm typ,ID -9A"                                                                                                                                          
R180         Resistor                                                                                                                                       TopLayer    R0402                                                   29.3033      92.7876      270      Resistor,10K,0402,1%,1/16W                                                                                                                                                                        
R181         Resistor                                                                                                                                       TopLayer    R0603                                                   22.8201      92.7876      0        Resistor,120R,0603,1%,1/10W                                                                                                                                                                       
R163         Resistor                                                                                                                                       TopLayer    R0402                                                   29.2501      102.7822     90       Resistor,10K,0402,1%,1/16W                                                                                                                                                                        
R165         Resistor                                                                                                                                       TopLayer    R0603                                                   22.8213      102.0268     360      Resistor,120R,0603,1%,1/10W                                                                                                                                                                       
R188         Resistor                                                                                                                                       TopLayer    R0402                                                   106.5531     79.3391      180      Resistor,22R,0402,1%,1/16W                                                                                                                                                                        
R193         Resistor                                                                                                                                       TopLayer    R0402                                                   106.5530     78.0390      180      Resistor,22R,0402,1%,1/16W                                                                                                                                                                        
R209         Resistor                                                                                                                                       TopLayer    R0402                                                   106.5406     70.4851      180      Resistor,22R,0402,1%,1/16W                                                                                                                                                                        
R185         Resistor                                                                                                                                       TopLayer    R0402                                                   106.5531     81.5341      180      Resistor,22R,0402,1%,1/16W                                                                                                                                                                        
R205         Resistor                                                                                                                                       TopLayer    R0402                                                   106.5531     72.6901      360      Resistor,22R,0402,1%,1/16W                                                                                                                                                                        
R211         Resistor                                                                                                                                       TopLayer    R0402                                                   106.5406     68.0721      180      Resistor,22R,0402,1%,1/16W                                                                                                                                                                        
R203         Resistor                                                                                                                                       TopLayer    R0402                                                   106.5531     73.6601      360      Resistor,10K,0402,1%,1/16W                                                                                                                                                                        
R214         Resistor                                                                                                                                       TopLayer    R0402                                                   106.5531     63.5001      360      Resistor,10K,0402,1%,1/16W                                                                                                                                                                        
R212         Resistor                                                                                                                                       TopLayer    R0402                                                   106.5406     66.2941      360      Resistor,10K,0402,1%,1/16W                                                                                                                                                                        
R287         Resistor                                                                                                                                       TopLayer    R0603                                                   93.3230      18.4764      90       Resistor,100K,0603,1%,1/10W                                                                                                                                                                       
R222         Resistor                                                                                                                                       TopLayer    R0603                                                   91.0309      57.2221      360      Resistor,100K,0603,1%,1/10W                                                                                                                                                                       
R218         Resistor                                                                                                                                       TopLayer    R0603                                                   84.0205      60.1938      180      Resistor,100K,0603,1%,1/10W                                                                                                                                                                       
R233         Resistor                                                                                                                                       TopLayer    R0603                                                   95.0976      51.1302      360      Resistor,100K,0603,1%,1/10W                                                                                                                                                                       
R219         Resistor                                                                                                                                       TopLayer    R0603                                                   95.0106      59.6392      180      Resistor,10K,0603,1%,1/10W                                                                                                                                                                        
R220         Resistor                                                                                                                                       TopLayer    R0603                                                   95.0106      58.3184      360      Resistor,270R,0603,1%,1/10W                                                                                                                                                                       
R216         Resistor                                                                                                                                       TopLayer    R0603                                                   95.0106      60.9600      360      Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R226         Resistor                                                                                                                                       TopLayer    R0402                                                   95.1230      53.6194      360      Resistor,4K7,0402,1%,1/16W                                                                                                                                                                        
R231         Resistor                                                                                                                                       TopLayer    R0603                                                   95.0976      52.4256      360      Resistor,270R,0603,1%,1/10W                                                                                                                                                                       
R171         Resistor                                                                                                                                       TopLayer    R0402                                                   59.9166      98.9823      180      Resistor,10K,0402,1%,1/16W                                                                                                                                                                        
R318         Resistor                                                                                                                                       BottomLayer R0603                                                   116.3406     118.9482     270      Resistor,180R,0603,1%,1/10W                                                                                                                                                                       
R162         Resistor                                                                                                                                       TopLayer    R0402                                                   59.8658      103.8846     360      Resistor,220K,0402,1%,1/16W                                                                                                                                                                       
R156         Resistor                                                                                                                                       TopLayer    R0402                                                   67.4096      107.8723     270      Resistor,220K,0402,1%,1/16W                                                                                                                                                                       
R124         Resistor                                                                                                                                       TopLayer    R0603                                                   111.9328     116.6979     360      Resistor,47K,0603,1%,1/10W                                                                                                                                                                        
R311         Resistor                                                                                                                                       BottomLayer R0603                                                   112.3671     121.6076     270      Resistor,47K,0603,1%,1/10W                                                                                                                                                                        
R215         Resistor                                                                                                                                       TopLayer    R0603                                                   59.1668      60.6781      270      Resistor,100K,0603,1%,1/10W                                                                                                                                                                       
R297         Resistor                                                                                                                                       TopLayer    R0603                                                   26.9241      7.8429       90       Resistor,270R,0603,1%,1/10W                                                                                                                                                                       
R298         Resistor                                                                                                                                       TopLayer    R0603                                                   29.1365      7.8429       90       Resistor,360R,0603,1%,1/10W                                                                                                                                                                       
R175         Resistor                                                                                                                                       TopLayer    R0805                                                   41.5997      96.1973      90       Resistor,10R,0805,1%,Stackpole,1/4W                                                                                                                                                               
R299         Resistor                                                                                                                                       TopLayer    R0603                                                   31.5665      7.7999       90       Resistor,470R,0603,1%,1/10W                                                                                                                                                                       
R300         Resistor                                                                                                                                       TopLayer    R0603                                                   33.7821      7.7999       90       Resistor,270R,0603,1%,1/10W                                                                                                                                                                       
R172         Resistor                                                                                                                                       TopLayer    R0603                                                   48.0314      98.4250      360      Resistor,33R,0603,1%,1/10W                                                                                                                                                                        
R176         Resistor                                                                                                                                       TopLayer    R0603                                                   43.3248      96.3944      90       Resistor,10K,0603,1%,1/10W                                                                                                                                                                        
R16          Resistor                                                                                                                                       TopLayer    R0402                                                   32.6390      155.5095     90       Resistor,4K7,0402,1%,1/16W                                                                                                                                                                        
R14          Resistor                                                                                                                                       TopLayer    R0603                                                   31.4452      155.4226     90       Resistor,7K5,0603,1%,1/10W                                                                                                                                                                        
R1           Resistor                                                                                                                                       TopLayer    R0402                                                   14.1922      166.8266     90       Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R13          Resistor                                                                                                                                       TopLayer    R0603                                                   29.4386      157.7086     270      Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R15          Resistor                                                                                                                                       TopLayer    R0603                                                   25.6794      156.5074     360      Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R17          Resistor                                                                                                                                       TopLayer    R0603                                                   27.9908      157.7086     270      Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R198         Resistor                                                                                                                                       TopLayer    R0603                                                   40.3619      75.4418      360      Resistor,620R,0603,1%,1/10W                                                                                                                                                                       
R289         Resistor                                                                                                                                       TopLayer    R0402                                                   43.4725      18.0522      270      Resistor,10K,0402,1%,1/16W                                                                                                                                                                        
R292         Resistor                                                                                                                                       TopLayer    R0603                                                   31.8164      15.5002      180      Resistor,20K,0603,1%,1/10W                                                                                                                                                                        
R293         Resistor                                                                                                                                       TopLayer    R0603                                                   33.8681      14.7502      90       Resistor,10K2,0603,1%,1/10W                                                                                                                                                                       
R191         Resistor                                                                                                                                       TopLayer    R0603                                                   19.8472      77.7090      270      Resistor,22K,0603,1%,1/10W                                                                                                                                                                        
R190         Resistor                                                                                                                                       TopLayer    R0603                                                   18.5006      77.7090      90       Resistor,22K,0603,1%,1/10W                                                                                                                                                                        
R201         Resistor                                                                                                                                       TopLayer    R0603                                                   23.8968      73.4653      90       Resistor,100K,0603,1%,1/10W                                                                                                                                                                       
R202         Resistor                                                                                                                                       TopLayer    R0603                                                   25.2008      73.4653      90       Resistor,100K,0603,1%,1/10W                                                                                                                                                                       
R192         Resistor                                                                                                                                       TopLayer    R0603                                                   17.0440      77.6872      270      Resistor,120R,0603,1%,1/10W                                                                                                                                                                       
R213         Resistor                                                                                                                                       TopLayer    R0603                                                   19.3472      65.5320      180      Resistor,10K,0603,1%,1/10W                                                                                                                                                                        
R285         Resistor                                                                                                                                       TopLayer    R0402                                                   81.6365      23.4486      90       Resistor,100R,0402,1%,1/16W                                                                                                                                                                       
R284         Resistor                                                                                                                                       TopLayer    R0402                                                   78.6636      23.4486      90       Resistor,100R,0402,1%,1/16W                                                                                                                                                                       
R288         Resistor                                                                                                                                       TopLayer    R0402                                                   75.7415      18.9607      360      Resistor,10K,0402,1%,1/16W                                                                                                                                                                        
R282         Resistor                                                                                                                                       TopLayer    R0402                                                   86.3707      25.6556      360      Resistor,4K7,0402,1%,1/16W                                                                                                                                                                        
R280         Resistor                                                                                                                                       TopLayer    R0402                                                   72.4007      26.7506      360      Resistor,10K,0402,1%,1/16W                                                                                                                                                                        
R281         Resistor                                                                                                                                       TopLayer    R0402                                                   86.3707      26.6895      360      Resistor,4K7,0402,1%,1/16W                                                                                                                                                                        
R277         Resistor                                                                                                                                       TopLayer    R0402                                                   86.3707      28.8512      360      Resistor,2K7,0402,1%,1/16W                                                                                                                                                                        
R278         Resistor                                                                                                                                       TopLayer    R0402                                                   72.4007      27.8877      360      Resistor,10K,0402,1%,1/16W                                                                                                                                                                        
R279         Resistor                                                                                                                                       TopLayer    R0402                                                   86.3707      27.7776      180      Resistor,4K7,0402,1%,1/16W                                                                                                                                                                        
R269         Resistor                                                                                                                                       TopLayer    R0402                                                   79.7965      37.4720      270      Resistor,3K,0402,1%,1/16W                                                                                                                                                                         
R283         Resistor                                                                                                                                       TopLayer    R0402                                                   74.4327      23.5180      90       Resistor,10K,0402,1%,1/16W                                                                                                                                                                        
R296         Resistor                                                                                                                                       TopLayer    R0603                                                   37.2436      10.0608      90       Resistor,330R,0603,1%,1/10W                                                                                                                                                                       
R295         Resistor                                                                                                                                       TopLayer    R0603                                                   38.6848      10.0768      90       Resistor,330R,0603,1%,1/10W                                                                                                                                                                       
R208         Resistor                                                                                                                                       TopLayer    R0402                                                   81.2800      71.0362      180      Resistor,47R,0402,1%,1/16W                                                                                                                                                                        
R206         Resistor                                                                                                                                       TopLayer    R0402                                                   81.2500      72.2865      180      Resistor,47R,0402,1%,1/16W                                                                                                                                                                        
R204         Resistor                                                                                                                                       TopLayer    R0402                                                   81.2735      73.5774      180      Resistor,47R,0402,1%,1/16W                                                                                                                                                                        
R187         Resistor                                                                                                                                       TopLayer    R0402                                                   81.2470      79.7077      180      Resistor,100R,0402,1%,1/16W                                                                                                                                                                       
R196         Resistor                                                                                                                                       TopLayer    R0402                                                   81.2735      76.0774      180      Resistor,47R,0402,1%,1/16W                                                                                                                                                                        
R189         Resistor                                                                                                                                       TopLayer    R0402                                                   81.2470      78.5275      360      Resistor,22R,0402,1%,1/16W                                                                                                                                                                        
R194         Resistor                                                                                                                                       TopLayer    R0402                                                   81.2500      77.2613      180      Resistor,47R,0402,1%,1/16W                                                                                                                                                                        
R217         Resistor                                                                                                                                       TopLayer    R0402                                                   63.9801      60.5431      90       Resistor,10K,0402,1%,1/16W                                                                                                                                                                        
R221         Resistor                                                                                                                                       TopLayer    R0402                                                   64.0277      57.1500      270      Resistor,820R,0402,1%,1/16W                                                                                                                                                                       
R317         Resistor                                                                                                                                       BottomLayer R0402                                                   66.4027      120.8659     360      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R313         Resistor                                                                                                                                       BottomLayer R0402                                                   68.1028      121.3459     90       Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R182         Resistor                                                                                                                                       TopLayer    R0402                                                   84.4101      85.7501      180      Resistor,10K,0402,1%,1/16W                                                                                                                                                                        
R309         Resistor                                                                                                                                       BottomLayer R0402                                                   36.1954      132.0800     360      Resistor,820R,0402,1%,1/16W                                                                                                                                                                       
R304         Resistor                                                                                                                                       BottomLayer R0603                                                   113.4110     149.3572     0        Resistor,1K,0603,1%,1/10W                                                                                                                                                                         
R302         Resistor                                                                                                                                       BottomLayer R0603                                                   115.5421     150.0378     270      Resistor,1K,0603,1%,1/10W                                                                                                                                                                         
R310         Resistor                                                                                                                                       BottomLayer R0603                                                   75.7469      122.1960     180      Resistor,33R,0603,1%,1/10W                                                                                                                                                                        
R19          Resistor                                                                                                                                       TopLayer    R0603                                                   113.4110     152.0952     360      Resistor,51R,0603,1%,1/10W                                                                                                                                                                        
R307         Resistor                                                                                                                                       BottomLayer R0603                                                   112.9030     147.4034     270      Resistor,1K,0603,1%,1/10W                                                                                                                                                                         
R308         Resistor                                                                                                                                       BottomLayer R0603                                                   114.3110     147.3729     90       Resistor,1K,0603,1%,1/10W                                                                                                                                                                         
R303         Resistor                                                                                                                                       BottomLayer R0603                                                   108.6841     150.0322     90       Resistor,1K,0603,1%,1/10W                                                                                                                                                                         
R306         Resistor                                                                                                                                       BottomLayer R0603                                                   108.6866     147.6223     90       Resistor,1K,0603,1%,1/10W                                                                                                                                                                         
R152         Resistor                                                                                                                                       TopLayer    R0603                                                   78.4606      111.4298     90       Resistor,33R,0603,1%,1/10W                                                                                                                                                                        
R305         Resistor                                                                                                                                       BottomLayer R0603                                                   111.0616     149.3370     180      Resistor,1K,0603,1%,1/10W                                                                                                                                                                         
R301         Resistor                                                                                                                                       BottomLayer R0603                                                   111.0616     150.6070     360      Resistor,1K,0603,1%,1/10W                                                                                                                                                                         
R179         Resistor                                                                                                                                       TopLayer    R0603                                                   106.9340     95.2015      90       Resistor,8K2,0603,1%,1/10W                                                                                                                                                                        
R111         Resistor                                                                                                                                       TopLayer    R0603                                                   111.8514     121.8560     180      Resistor,270R,0603,1%,1/10W                                                                                                                                                                       
R153         Resistor                                                                                                                                       TopLayer    R0603                                                   86.0338      111.3419     90       Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R154         Resistor                                                                                                                                       TopLayer    R0603                                                   87.6471      111.3419     90       Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R164         Resistor                                                                                                                                       TopLayer    R0603                                                   106.9340     101.9003     90       Resistor,1K,0603,1%,1/10W                                                                                                                                                                         
R157         Resistor                                                                                                                                       TopLayer    R0603                                                   107.4420     107.4787     180      Resistor,1K,0603,1%,1/10W                                                                                                                                                                         
R257         Resistor                                                                                                                                       TopLayer    R0603                                                   84.4550      40.6324      270      Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R237         Resistor                                                                                                                                       TopLayer    R0402                                                   83.5967      48.2246      360      Resistor,4K7,0402,1%,1/16W                                                                                                                                                                        
R258         Resistor                                                                                                                                       TopLayer    R0603                                                   83.1467      40.6146      270      Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R255         Resistor                                                                                                                                       TopLayer    R0603                                                   90.1516      40.6559      270      Resistor,20R,0603,1%,1/10W                                                                                                                                                                        
R256         Resistor                                                                                                                                       TopLayer    R0603                                                   87.8397      40.6557      270      Resistor,20R,0603,1%,1/10W                                                                                                                                                                        
R9           Resistor                                                                                                                                       TopLayer    R0402                                                   91.9452      158.1150     270      Resistor,3K3,0402,1%,1/16W                                                                                                                                                                        
R3           Resistor                                                                                                                                       TopLayer    R0603                                                   76.6945      157.9372     270      Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R2           Resistor                                                                                                                                       TopLayer    R0603                                                   75.3279      157.9372     90       Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R4           Resistor                                                                                                                                       TopLayer    R0603                                                   72.7265      157.9242     90       Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R6           Resistor                                                                                                                                       TopLayer    R0603                                                   70.2029      157.8609     90       Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R5           Resistor                                                                                                                                       TopLayer    R0603                                                   63.6340      157.8872     270      Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R7           Resistor                                                                                                                                       TopLayer    R0603                                                   61.0704      157.8452     270      Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R8           Resistor                                                                                                                                       TopLayer    R0603                                                   59.6033      157.8182     90       Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R11          Resistor                                                                                                                                       TopLayer    R0603                                                   57.9299      157.7371     90       Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R10          Resistor                                                                                                                                       TopLayer    R0603                                                   56.3880      157.7524     270      Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R12          Resistor                                                                                                                                       TopLayer    R0603                                                   51.9604      157.6872     270      Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R23          Resistor                                                                                                                                       TopLayer    R0402                                                   10.6680      149.6060     360      Resistor,3K3,0402,1%,1/16W                                                                                                                                                                        
R21          Resistor                                                                                                                                       TopLayer    R0603                                                   10.6598      150.8760     180      Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R18          Resistor                                                                                                                                       TopLayer    R0603                                                   10.6401      152.4254     360      Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R77          Resistor                                                                                                                                       TopLayer    R0603                                                   10.6598      133.8660     360      Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R86          Resistor                                                                                                                                       TopLayer    R0603                                                   10.6598      130.3020     180      Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R92          Resistor                                                                                                                                       TopLayer    R0603                                                   10.6598      127.8890     180      Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R100         Resistor                                                                                                                                       TopLayer    R0603                                                   10.6598      125.1030     180      Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R120         Resistor                                                                                                                                       TopLayer    R0603                                                   10.6598      118.6030     360      Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R66          Resistor                                                                                                                                       TopLayer    R0603                                                   25.1130      136.9247     360      Resistor,9K1,0603,1%,1/10W                                                                                                                                                                        
R76          Resistor                                                                                                                                       TopLayer    R0603                                                   25.0952      134.1628     180      Resistor,1K3,0603,1%,1/10W                                                                                                                                                                        
R72          Resistor                                                                                                                                       TopLayer    R0603                                                   22.0421      134.7470     360      Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R61          Resistor                                                                                                                                       TopLayer    R0603                                                   25.1130      138.6744     360      Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R64          Resistor                                                                                                                                       TopLayer    R0603                                                   22.0510      137.0167     360      Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R51          Resistor                                                                                                                                       TopLayer    R0603                                                   25.1456      143.1839     180      Resistor,9K1,0603,1%,1/10W                                                                                                                                                                        
R55          Resistor                                                                                                                                       TopLayer    R0603                                                   22.0510      141.8752     360      Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R59          Resistor                                                                                                                                       TopLayer    R0603                                                   25.1456      140.2285     360      Resistor,1K3,0603,1%,1/10W                                                                                                                                                                        
R58          Resistor                                                                                                                                       TopLayer    R0603                                                   22.0510      140.2285     360      Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R52          Resistor                                                                                                                                       TopLayer    R0603                                                   22.0510      143.1787     360      Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R31          Resistor                                                                                                                                       TopLayer    R0603                                                   25.1206      144.5417     180      Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R25          Resistor                                                                                                                                       TopLayer    R0603                                                   25.1460      145.9484     180      Resistor,9K1,0603,1%,1/10W                                                                                                                                                                        
R24          Resistor                                                                                                                                       TopLayer    R0603                                                   25.1460      147.2413     360      Resistor,1K3,0603,1%,1/10W                                                                                                                                                                        
R20          Resistor                                                                                                                                       TopLayer    R0603                                                   25.1206      151.1808     180      Resistor,9K1,0603,1%,1/10W                                                                                                                                                                        
R22          Resistor                                                                                                                                       TopLayer    R0603                                                   25.1206      149.9108     360      Resistor,1K3,0603,1%,1/10W                                                                                                                                                                        
R119         Resistor                                                                                                                                       TopLayer    R0603                                                   22.0510      118.7073     360      Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R91          Resistor                                                                                                                                       TopLayer    R0603                                                   25.1206      128.0795     360      Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R95          Resistor                                                                                                                                       TopLayer    R0603                                                   25.1206      126.6698     360      Resistor,9K1,0603,1%,1/10W                                                                                                                                                                        
R99          Resistor                                                                                                                                       TopLayer    R0603                                                   22.0510      125.1658     360      Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R104         Resistor                                                                                                                                       TopLayer    R0603                                                   25.1206      123.8794     180      Resistor,1K3,0603,1%,1/10W                                                                                                                                                                        
R110         Resistor                                                                                                                                       TopLayer    R0603                                                   22.0510      122.0819     360      Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R103         Resistor                                                                                                                                       TopLayer    R0603                                                   22.0510      123.8794     360      Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R122         Resistor                                                                                                                                       TopLayer    R0603                                                   25.1460      117.3734     360      Resistor,9K1,0603,1%,1/10W                                                                                                                                                                        
R125         Resistor                                                                                                                                       TopLayer    R0603                                                   25.1460      116.0272     360      Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R115         Resistor                                                                                                                                       TopLayer    R0603                                                   25.1714      120.5408     180      Resistor,1K3,0603,1%,1/10W                                                                                                                                                                        
R114         Resistor                                                                                                                                       TopLayer    R0603                                                   22.0510      120.5453     360      Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R245         Resistor                                                                                                                                       TopLayer    R0603                                                   64.9961      45.1318      270      Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R236         Resistor                                                                                                                                       TopLayer    R0402                                                   78.1291      48.7381      360      Resistor,510R,0402,1%,1/16W                                                                                                                                                                       
R232         Resistor                                                                                                                                       TopLayer    R0603                                                   78.1291      52.0631      180      Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R223         Resistor                                                                                                                                       TopLayer    R0603                                                   74.9294      54.4094      90       Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R243         Resistor                                                                                                                                       TopLayer    R0402                                                   78.1540      46.7381      180      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R239         Resistor                                                                                                                                       TopLayer    R0402                                                   78.1291      47.7381      180      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R234         Resistor                                                                                                                                       TopLayer    R0402                                                   78.1291      50.7414      360      Resistor,10K,0402,1%,1/16W                                                                                                                                                                        
R241         Resistor                                                                                                                                       TopLayer    R0603                                                   60.4557      46.7371      90       Resistor,100K,0603,1%,1/10W                                                                                                                                                                       
R267         Resistor                                                                                                                                       TopLayer    R0603                                                   52.5394      38.8505      360      Resistor,0R,0603,5%,1/10W                                                                                                                                                                         
R228         Resistor                                                                                                                                       TopLayer    R0603                                                   55.5122      52.6418      90       Resistor,100K,0603,1%,1/10W                                                                                                                                                                       
R268         Resistor                                                                                                                                       TopLayer    R0603                                                   38.2188      38.0513      180      Resistor,357K,0603,1%,1/10W                                                                                                                                                                       
R271         Resistor                                                                                                                                       TopLayer    R0603                                                   40.8686      36.7218      180      Resistor,11K,0603,1%,1/10W                                                                                                                                                                        
R270         Resistor                                                                                                                                       TopLayer    R0603                                                   56.9774      37.2082      180      Resistor,6K04,0603,1%,1/10W                                                                                                                                                                       
R260         Resistor                                                                                                                                       TopLayer    R0603                                                   38.2187      40.7405      360      Resistor,300K,0603,1%,1/10W                                                                                                                                                                       
R266         Resistor                                                                                                                                       TopLayer    R0402                                                   49.0536      38.7641      270      Resistor,100R,0402,1%,1/16W                                                                                                                                                                       
R230         Resistor                                                                                                                                       TopLayer    R0603                                                   44.5770      52.4333      270      Resistor,100K,0603,1%,1/10W                                                                                                                                                                       
R229         Resistor                                                                                                                                       TopLayer    R0603                                                   50.0693      52.6396      270      Resistor,100K,0603,1%,1/10W                                                                                                                                                                       
R242         Resistor                                                                                                                                       TopLayer    R0603                                                   55.3901      46.7360      270      Resistor,100K,0603,1%,1/10W                                                                                                                                                                       
R265         Resistor                                                                                                                                       TopLayer    R0603                                                   47.8020      38.7124      90       Resistor,300K,0603,1%,1/10W                                                                                                                                                                       
R227         Resistor                                                                                                                                       TopLayer    R0805                                                   39.3421      52.4510      270      "Resistor, 1R, 0805, 1%, 1/8W"                                                                                                                                                                    
R238         Resistor                                                                                                                                       TopLayer    R0805                                                   45.9715      46.9329      90       Resistor,24R,0805,1%,1/8W                                                                                                                                                                         
R252         Resistor                                                                                                                                       TopLayer    R0805                                                   52.8041      42.7507      90       Resistor,620R,0805,1%,1/8W                                                                                                                                                                        
R253         Resistor                                                                                                                                       TopLayer    R0805                                                   54.8208      42.7257      90       Resistor,10K,0805,1%,1/8W                                                                                                                                                                         
R262         Resistor                                                                                                                                       TopLayer    R0603                                                   52.5394      40.1786      180      Resistor,6K04,0603,1%,1/10W                                                                                                                                                                       
R178         Resistor                                                                                                                                       TopLayer    R0402                                                   89.7616      96.5693      180      Resistor,33R,0402,1%,1/16W                                                                                                                                                                        
R173         Resistor                                                                                                                                       TopLayer    R0402                                                   75.5142      97.9932      180      Resistor,33R,0402,1%,1/16W                                                                                                                                                                        
R159         Resistor                                                                                                                                       TopLayer    R0402                                                   89.8302      105.8606     180      Resistor,33R,0402,1%,1/16W                                                                                                                                                                        
R160         Resistor                                                                                                                                       TopLayer    R0402                                                   75.4969      105.4085     180      Resistor,33R,0402,1%,1/16W                                                                                                                                                                        
R161         Resistor                                                                                                                                       TopLayer    R0402                                                   90.8385      103.7829     90       Resistor,10K,0402,1%,1/16W                                                                                                                                                                        
R166         Resistor                                                                                                                                       TopLayer    R0402                                                   91.2597      101.7285     90       Resistor,10K,0402,1%,1/16W                                                                                                                                                                        
R319         Resistor                                                                                                                                       BottomLayer R0402                                                   89.7971      105.4847     180      Resistor,33R,0402,1%,1/16W                                                                                                                                                                        
R320         Resistor                                                                                                                                       BottomLayer R0402                                                   75.5376      103.6813     180      Resistor,33R,0402,1%,1/16W                                                                                                                                                                        
R321         Resistor                                                                                                                                       BottomLayer R0402                                                   89.7616      96.5693      180      Resistor,33R,0402,1%,1/16W                                                                                                                                                                        
R322         Resistor                                                                                                                                       BottomLayer R0402                                                   75.9287      96.4677      180      Resistor,33R,0402,1%,1/16W                                                                                                                                                                        
R108         Resistor                                                                                                                                       TopLayer    R0402                                                   82.3214      123.0176     360      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R102         Resistor                                                                                                                                       TopLayer    R0402                                                   82.2939      124.0790     360      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R150         Resistor                                                                                                                                       TopLayer    R0402                                                   82.3722      113.6000     180      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R129         Resistor                                                                                                                                       TopLayer    R0402                                                   82.3572      114.6230     180      Resistor,33R,0402,1%,1/16W                                                                                                                                                                        
R107         Resistor                                                                                                                                       TopLayer    R0402                                                   52.0446      123.3932     180      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R112         Resistor                                                                                                                                       TopLayer    R0402                                                   52.0777      121.4120     180      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R146         Resistor                                                                                                                                       TopLayer    R0402                                                   56.6166      114.1047     90       Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R121         Resistor                                                                                                                                       TopLayer    R0402                                                   82.2836      118.6844     180      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R143         Resistor                                                                                                                                       TopLayer    R0402                                                   58.6486      114.1377     90       Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R118         Resistor                                                                                                                                       TopLayer    R0402                                                   82.2960      119.6674     180      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R30          Resistor                                                                                                                                       TopLayer    R0402                                                   63.1904      145.2629     270      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R127         Resistor                                                                                                                                       TopLayer    R0402                                                   52.0967      116.0983     180      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R46          Resistor                                                                                                                                       TopLayer    R0402                                                   59.1809      143.0991     270      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R45          Resistor                                                                                                                                       TopLayer    R0402                                                   58.1660      143.0991     270      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R44          Resistor                                                                                                                                       TopLayer    R0402                                                   56.9460      143.1265     270      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R47          Resistor                                                                                                                                       TopLayer    R0402                                                   54.4297      143.1011     270      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R35          Resistor                                                                                                                                       TopLayer    R0402                                                   79.4766      143.3251     90       Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R54          Resistor                                                                                                                                       TopLayer    R0402                                                   51.6103      142.0851     360      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R36          Resistor                                                                                                                                       TopLayer    R0402                                                   78.1939      143.3331     90       Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R83          Resistor                                                                                                                                       TopLayer    R0402                                                   51.9717      131.6954     180      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R130         Resistor                                                                                                                                       TopLayer    R0402                                                   72.6028      114.3000     90       Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R85          Resistor                                                                                                                                       TopLayer    R0402                                                   51.9938      130.7084     180      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R133         Resistor                                                                                                                                       TopLayer    R0402                                                   73.8886      114.2884     90       Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R131         Resistor                                                                                                                                       TopLayer    R0402                                                   74.8881      114.3000     90       Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R90          Resistor                                                                                                                                       TopLayer    R0402                                                   52.0188      128.3659     180      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R116         Resistor                                                                                                                                       TopLayer    R0402                                                   82.3214      120.7008     180      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R94          Resistor                                                                                                                                       TopLayer    R0402                                                   52.0216      127.3409     180      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R97          Resistor                                                                                                                                       TopLayer    R0402                                                   52.0192      126.3650     180      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R98          Resistor                                                                                                                                       TopLayer    R0402                                                   52.0192      125.3755     180      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R101         Resistor                                                                                                                                       TopLayer    R0402                                                   52.0192      124.3838     180      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R26          Resistor                                                                                                                                       TopLayer    R0402                                                   64.5011      145.2880     270      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R34          Resistor                                                                                                                                       TopLayer    R0402                                                   77.1881      143.3123     90       Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R49          Resistor                                                                                                                                       TopLayer    R0402                                                   63.1904      143.0532     270      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R37          Resistor                                                                                                                                       TopLayer    R0402                                                   76.2000      143.2829     90       Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R38          Resistor                                                                                                                                       TopLayer    R0402                                                   75.2094      143.2754     90       Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R39          Resistor                                                                                                                                       TopLayer    R0402                                                   74.1957      143.2653     90       Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R42          Resistor                                                                                                                                       TopLayer    R0402                                                   73.1516      143.2361     90       Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R141         Resistor                                                                                                                                       TopLayer    R0402                                                   63.0428      114.1668     90       Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R41          Resistor                                                                                                                                       TopLayer    R0402                                                   72.1032      143.2361     90       Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R29          Resistor                                                                                                                                       TopLayer    R0402                                                   70.9027      145.2880     90       Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R40          Resistor                                                                                                                                       TopLayer    R0402                                                   70.8520      143.2361     90       Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R148         Resistor                                                                                                                                       TopLayer    R0402                                                   53.4670      114.0384     90       Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R149         Resistor                                                                                                                                       TopLayer    R0402                                                   54.5341      114.0206     90       Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R132         Resistor                                                                                                                                       TopLayer    R0402                                                   75.8881      114.3000     270      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R139         Resistor                                                                                                                                       TopLayer    R0402                                                   64.0277      114.1730     270      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R140         Resistor                                                                                                                                       TopLayer    R0402                                                   65.0164      114.1730     270      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R137         Resistor                                                                                                                                       TopLayer    R0402                                                   66.0146      114.1984     270      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R43          Resistor                                                                                                                                       TopLayer    R0402                                                   55.7022      143.1214     90       Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R84          Resistor                                                                                                                                       TopLayer    R0402                                                   82.2866      131.4893     180      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R138         Resistor                                                                                                                                       TopLayer    R0402                                                   67.0386      114.1984     270      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R82          Resistor                                                                                                                                       TopLayer    R0402                                                   82.2502      132.4799     180      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R135         Resistor                                                                                                                                       TopLayer    R0402                                                   68.0164      114.2149     270      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R79          Resistor                                                                                                                                       TopLayer    R0402                                                   82.2113      133.4734     180      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R134         Resistor                                                                                                                                       TopLayer    R0402                                                   69.0118      114.2238     270      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R75          Resistor                                                                                                                                       TopLayer    R0402                                                   82.2082      134.5358     180      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R136         Resistor                                                                                                                                       TopLayer    R0402                                                   70.0288      114.2149     270      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R71          Resistor                                                                                                                                       TopLayer    R0402                                                   82.1944      135.5598     180      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R96          Resistor                                                                                                                                       TopLayer    R0402                                                   82.2620      126.4509     360      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R69          Resistor                                                                                                                                       TopLayer    R0402                                                   82.1690      136.5504     180      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R93          Resistor                                                                                                                                       TopLayer    R0402                                                   82.2620      127.4550     360      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R63          Resistor                                                                                                                                       TopLayer    R0402                                                   82.1494      137.5410     180      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R89          Resistor                                                                                                                                       TopLayer    R0402                                                   82.2924      128.4413     360      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R62          Resistor                                                                                                                                       TopLayer    R0402                                                   82.1182      138.5824     180      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R88          Resistor                                                                                                                                       TopLayer    R0402                                                   82.2866      129.4573     360      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R60          Resistor                                                                                                                                       TopLayer    R0402                                                   82.0994      139.5730     180      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R87          Resistor                                                                                                                                       TopLayer    R0402                                                   82.3048      130.4678     360      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R48          Resistor                                                                                                                                       TopLayer    R0402                                                   67.0028      143.0742     90       Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R28          Resistor                                                                                                                                       TopLayer    R0402                                                   67.0028      145.2880     90       Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R50          Resistor                                                                                                                                       TopLayer    R0402                                                   65.7860      143.0532     90       Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R27          Resistor                                                                                                                                       TopLayer    R0402                                                   65.7027      145.2880     90       Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R53          Resistor                                                                                                                                       TopLayer    R0402                                                   64.5011      143.0242     90       Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R68          Resistor                                                                                                                                       TopLayer    R0402                                                   51.9176      136.6266     180      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R70          Resistor                                                                                                                                       TopLayer    R0402                                                   51.9188      135.6360     180      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R74          Resistor                                                                                                                                       TopLayer    R0402                                                   51.9438      134.6454     180      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R78          Resistor                                                                                                                                       TopLayer    R0402                                                   51.9604      133.6659     180      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R81          Resistor                                                                                                                                       TopLayer    R0402                                                   51.9717      132.6896     180      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R109         Resistor                                                                                                                                       TopLayer    R0402                                                   52.0777      122.4110     0        Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R147         Resistor                                                                                                                                       TopLayer    R0402                                                   55.6006      114.0714     90       Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R145         Resistor                                                                                                                                       TopLayer    R0402                                                   57.6072      114.1222     90       Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R144         Resistor                                                                                                                                       TopLayer    R0402                                                   59.6646      114.1309     90       Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R80          Resistor                                                                                                                                       TopLayer    R0603                                                   48.3362      133.0452     180      Resistor,1K5,0603,1%,1/10W                                                                                                                                                                        
R73          Resistor                                                                                                                                       TopLayer    R0603                                                   48.3616      134.6454     180      Resistor,1K5,0603,1%,1/10W                                                                                                                                                                        
R142         Resistor                                                                                                                                       TopLayer    R0402                                                   62.0522      114.1552     90       Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R246         Resistor                                                                                                                                       TopLayer    R0603                                                   12.9541      44.9041      180      Resistor,1K,0603,1%,1/10W                                                                                                                                                                         
R250         Resistor                                                                                                                                       TopLayer    R0603                                                   12.9541      43.6341      180      Resistor,1K,0603,1%,1/10W                                                                                                                                                                         
R254         Resistor                                                                                                                                       TopLayer    R0603                                                   12.9541      42.3055      180      Resistor,1K,0603,1%,1/10W                                                                                                                                                                         
R259         Resistor                                                                                                                                       TopLayer    R0603                                                   12.9541      40.9055      180      Resistor,1K,0603,1%,1/10W                                                                                                                                                                         
R248         Resistor                                                                                                                                       TopLayer    R0603                                                   16.7361      43.7363      180      Resistor,21K,0603,1%,1/10W                                                                                                                                                                        
R249         Resistor                                                                                                                                       TopLayer    R0603                                                   21.3360      43.6448      360      Resistor,100R,0603,1%,1/10W                                                                                                                                                                       
R244         Resistor                                                                                                                                       TopLayer    R0603                                                   12.9540      46.4033      180      Resistor,330K,0603,1%,1/10W                                                                                                                                                                       
R263         Resistor                                                                                                                                       TopLayer    R0603                                                   16.8427      39.8581      180      Resistor,49K9,0603,1%                                                                                                                                                                             
R123         Resistor                                                                                                                                       TopLayer    R0402                                                   52.1243      117.2986     360      Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R323         Resistor                                                                                                                                       BottomLayer R0603                                                   12.9261      47.7774      360      Resistor,49K9,0603,1%                                                                                                                                                                             
R315         Resistor                                                                                                                                       BottomLayer R0402                                                   62.9027      121.3459     90       Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R314         Resistor                                                                                                                                       BottomLayer R0402                                                   63.9064      121.3459     90       Resistor,0R,0402,5%,1/16W                                                                                                                                                                         
R264         Resistor                                                                                                                                       TopLayer    R0603                                                   21.4097      39.6723      180      Resistor,10K,0603,1%,1/10W                                                                                                                                                                        
R316         Resistor                                                                                                                                       BottomLayer R0603                                                   110.2212     121.1360     180      Resistor,10K,0603,1%,1/10W                                                                                                                                                                        
R117         Resistor                                                                                                                                       TopLayer    R0603                                                   116.1760     119.4067     90       Resistor,10K,0603,1%,1/10W                                                                                                                                                                        
RV3          POTENTIOMETER                                                                                                                                  TopLayer    POT_BOURNS_3386P                                        17.7977      6.4635       360      "TRIMMER 50K OHM 0.5W PC PIN"                                                                                                                                                                     
RV2          POTENTIOMETER                                                                                                                                  TopLayer    POT_BOURNS_3386P                                        113.9190     99.9803      90       "TRIMMER 10K OHM 0.5W PC PIN"                                                                                                                                                                     
SB45         SB_OFF                                                                                                                                         TopLayer    SOLDER-BRIDGE_R0603-0R                                  89.5850      30.0228      360      "Solder Bridge OFF"                                                                                                                                                                               
SB46         SB_ON                                                                                                                                          TopLayer    SOLDER-BRIDGE_R0603-0R                                  89.5850      28.4734      360      "Solder Bridge ON"                                                                                                                                                                                
SB34         SB_ON                                                                                                                                          TopLayer    SOLDER-BRIDGE_R0603-0R                                  40.3000      105.5183     180      "Solder Bridge ON"                                                                                                                                                                                
SB33         SB_ON                                                                                                                                          TopLayer    SOLDER-BRIDGE_R0603-0R                                  40.2920      106.9772     180      "Solder Bridge ON"                                                                                                                                                                                
SB47         SB_ON                                                                                                                                          TopLayer    SOLDER-BRIDGE_R0603-0R                                  39.9121      15.0670      270      "Solder Bridge ON"                                                                                                                                                                                
SB48         SB_ON                                                                                                                                          TopLayer    SOLDER-BRIDGE_R0603-0R                                  31.7369      14.0502      360      "Solder Bridge ON"                                                                                                                                                                                
SB42         SB_ON                                                                                                                                          TopLayer    SOLDER-BRIDGE_R0603-0R                                  84.0327      52.4333      180      "Solder Bridge ON"                                                                                                                                                                                
SB38         SB_OFF                                                                                                                                         TopLayer    SOLDER-BRIDGE_R0603-0R                                  17.0440      74.9118      270      "Solder Bridge OFF"                                                                                                                                                                               
SB37         SB_OFF                                                                                                                                         TopLayer    SOLDER-BRIDGE_R0603-0R                                  19.8804      75.0270      90       "Solder Bridge OFF"                                                                                                                                                                               
SB39         SB_OFF                                                                                                                                         TopLayer    SOLDER-BRIDGE_R0603-0R                                  18.5010      75.0072      90       "Solder Bridge OFF"                                                                                                                                                                               
SB1          SB_ON                                                                                                                                          TopLayer    SOLDER-BRIDGE_R0603-0R                                  14.1922      161.9216     90       "Solder Bridge ON"                                                                                                                                                                                
SB40         SB_ON                                                                                                                                          TopLayer    SOLDER-BRIDGE_R0603-0R                                  26.5787      73.4616      270      "Solder Bridge ON"                                                                                                                                                                                
SB41         SB_ON                                                                                                                                          TopLayer    SOLDER-BRIDGE_R0603-0R                                  59.3065      57.0658      270      "Solder Bridge ON"                                                                                                                                                                                
SB84         SB_ON                                                                                                                                          BottomLayer SOLDER-BRIDGE_R0603-0R                                  79.0956      129.2166     90       "Solder Bridge ON"                                                                                                                                                                                
SB85         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  77.6732      129.2166     90       "Solder Bridge OFF"                                                                                                                                                                               
SB82         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  66.0566      125.1458     180      "Solder Bridge OFF"                                                                                                                                                                               
SB87         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  63.9293      124.3874     270      "Solder Bridge OFF"                                                                                                                                                                               
SB88         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  62.2554      124.4180     90       "Solder Bridge OFF"                                                                                                                                                                               
SB81         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  68.3514      124.3606     270      "Solder Bridge OFF"                                                                                                                                                                               
SB2          SB_OFF                                                                                                                                         TopLayer    SOLDER-BRIDGE_R0603-0R                                  55.0269      157.6476     270      "Solder Bridge OFF"                                                                                                                                                                               
SB32         SB_OFF                                                                                                                                         TopLayer    SOLDER-BRIDGE_R0603-0R                                  10.9348      108.3120     360      "Solder Bridge OFF"                                                                                                                                                                               
SB14         SB_OFF                                                                                                                                         TopLayer    SOLDER-BRIDGE_R0603-0R                                  22.3260      138.8118     360      "Solder Bridge OFF"                                                                                                                                                                               
SB19         SB_OFF                                                                                                                                         TopLayer    SOLDER-BRIDGE_R0603-0R                                  25.3738      122.1960     360      "Solder Bridge OFF"                                                                                                                                                                               
SB36         SB_OFF                                                                                                                                         TopLayer    SOLDER-BRIDGE_R0603-0R                                  75.3513      96.5718      360      "Solder Bridge OFF"                                                                                                                                                                               
SB35         SB_OFF                                                                                                                                         TopLayer    SOLDER-BRIDGE_R0603-0R                                  89.4182      103.8618     270      "Solder Bridge ON"                                                                                                                                                                                
SB119        SB_ON                                                                                                                                          BottomLayer SOLDER-BRIDGE_R0603-0R                                  75.4469      105.4085     180      "Solder Bridge ON"                                                                                                                                                                                
SB26         SB_ON                                                                                                                                          TopLayer    SOLDER-BRIDGE_R0603-0R                                  77.0636      114.3088     90       "Solder Bridge ON"                                                                                                                                                                                
SB69         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  82.5279      140.7880     180      "Solder Bridge OFF"                                                                                                                                                                               
SB27         SB_ON                                                                                                                                          TopLayer    SOLDER-BRIDGE_R0603-0R                                  78.4352      114.3037     90       "Solder Bridge ON"                                                                                                                                                                                
SB78         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  82.4166      132.7659     180      "Solder Bridge OFF"                                                                                                                                                                               
SB18         SB_ON                                                                                                                                          TopLayer    SOLDER-BRIDGE_R0603-0R                                  82.5746      125.3236     360      "Solder Bridge ON"                                                                                                                                                                                
SB79         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  82.4166      131.4704     180      "Solder Bridge OFF"                                                                                                                                                                               
SB76         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  82.4003      135.3566     180      "Solder Bridge OFF"                                                                                                                                                                               
SB25         SB_ON                                                                                                                                          TopLayer    SOLDER-BRIDGE_R0603-0R                                  82.5004      115.9510     180      "Solder Bridge ON"                                                                                                                                                                                
SB96         SB_ON                                                                                                                                          BottomLayer SOLDER-BRIDGE_R0603-0R                                  51.9217      122.6566     180      "Solder Bridge ON"                                                                                                                                                                                
SB77         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  82.3994      134.0612     180      "Solder Bridge OFF"                                                                                                                                                                               
SB24         SB_ON                                                                                                                                          TopLayer    SOLDER-BRIDGE_R0603-0R                                  82.4396      117.5512     180      "Solder Bridge ON"                                                                                                                                                                                
SB73         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  82.3994      138.0160     180      "Solder Bridge OFF"                                                                                                                                                                               
SB21         SB_ON                                                                                                                                          TopLayer    SOLDER-BRIDGE_R0603-0R                                  51.9286      120.2639     180      "Solder Bridge ON"                                                                                                                                                                                
SB74         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  82.3948      136.6786     180      "Solder Bridge OFF"                                                                                                                                                                               
SB23         SB_ON                                                                                                                                          TopLayer    SOLDER-BRIDGE_R0603-0R                                  52.0306      118.7542     360      "Solder Bridge ON"                                                                                                                                                                                
SB98         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  99.8714      121.9708     180      "Solder Bridge OFF"                                                                                                                                                                               
SB89         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  52.0467      127.8382     360      "Solder Bridge OFF"                                                                                                                                                                               
SB4          SB_ON                                                                                                                                          TopLayer    SOLDER-BRIDGE_R0603-0R                                  61.7210      143.7011     270      "Solder Bridge ON"                                                                                                                                                                                
SB92         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  52.0438      124.6124     360      "Solder Bridge OFF"                                                                                                                                                                               
SB3          SB_ON                                                                                                                                          TopLayer    SOLDER-BRIDGE_R0603-0R                                  60.3759      143.7136     270      "Solder Bridge ON"                                                                                                                                                                                
SB11         SB_ON                                                                                                                                          TopLayer    SOLDER-BRIDGE_R0603-0R                                  82.5279      140.7880     360      "Solder Bridge ON"                                                                                                                                                                                
SB62         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  36.4986      143.6370     360      "Solder Bridge OFF"                                                                                                                                                                               
SB8          SB_ON                                                                                                                                          TopLayer    SOLDER-BRIDGE_R0603-0R                                  84.0461      143.7347     90       "Solder Bridge ON"                                                                                                                                                                                
SB103        SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  36.3462      119.3038     360      "Solder Bridge OFF"                                                                                                                                                                               
SB7          SB_ON                                                                                                                                          TopLayer    SOLDER-BRIDGE_R0603-0R                                  82.6491      143.7347     90       "Solder Bridge ON"                                                                                                                                                                                
SB118        SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  55.8030      113.4110     360      "Solder Bridge OFF"                                                                                                                                                                               
SB5          SB_ON                                                                                                                                          TopLayer    SOLDER-BRIDGE_R0603-0R                                  81.2503      143.7607     90       "Solder Bridge ON"                                                                                                                                                                                
SB109        SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  62.1857      114.2649     90       "Solder Bridge OFF"                                                                                                                                                                               
SB97         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  31.4249      122.1246     360      "Solder Bridge OFF"                                                                                                                                                                               
SB100        SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  82.4724      121.8413     180      "Solder Bridge OFF"                                                                                                                                                                               
SB29         SB_ON                                                                                                                                          TopLayer    SOLDER-BRIDGE_R0603-0R                                  71.1790      114.2019     90       "Solder Bridge ON"                                                                                                                                                                                
SB115        SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  71.1962      114.1860     90       "Solder Bridge OFF"                                                                                                                                                                               
SB55         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  77.2195      144.4242     180      "Solder Bridge OFF"                                                                                                                                                                               
SB17         SB_OFF                                                                                                                                         TopLayer    SOLDER-BRIDGE_R0603-0R                                  52.0432      129.5146     360      "Solder Bridge OFF"                                                                                                                                                                               
SB56         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  75.1832      143.6726     270      "Solder Bridge OFF"                                                                                                                                                                               
SB20         SB_ON                                                                                                                                          TopLayer    SOLDER-BRIDGE_R0603-0R                                  82.4746      121.8438     180      "Solder Bridge ON"                                                                                                                                                                                
SB49         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  104.3686     150.4853     270      "Solder Bridge OFF"                                                                                                                                                                               
SB9          SB_ON                                                                                                                                          TopLayer    SOLDER-BRIDGE_R0603-0R                                  69.5158      143.6290     270      "Solder Bridge ON"                                                                                                                                                                                
SB64         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  31.4210      142.2400     0        "Solder Bridge OFF"                                                                                                                                                                               
SB6          SB_ON                                                                                                                                          TopLayer    SOLDER-BRIDGE_R0603-0R                                  68.1848      143.6420     270      "Solder Bridge ON"                                                                                                                                                                                
SB50         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  99.7446      150.0353     180      "Solder Bridge OFF"                                                                                                                                                                               
SB68         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  31.3930      140.8913     0        "Solder Bridge OFF"                                                                                                                                                                               
SB51         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  31.3349      149.8106     0        "Solder Bridge OFF"                                                                                                                                                                               
SB12         SB_ON                                                                                                                                          TopLayer    SOLDER-BRIDGE_R0603-0R                                  51.9647      140.7643     360      "Solder Bridge ON"                                                                                                                                                                                
SB66         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  36.4984      142.1130     0        "Solder Bridge OFF"                                                                                                                                                                               
SB13         SB_ON                                                                                                                                          TopLayer    SOLDER-BRIDGE_R0603-0R                                  52.0243      139.1194     360      "Solder Bridge ON"                                                                                                                                                                                
SB52         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  31.3352      145.9992     0        "Solder Bridge OFF"                                                                                                                                                                               
SB15         SB_ON                                                                                                                                          TopLayer    SOLDER-BRIDGE_R0603-0R                                  52.0358      137.7633     360      "Solder Bridge ON"                                                                                                                                                                                
SB108        SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  66.8778      114.2649     90       "Solder Bridge OFF"                                                                                                                                                                               
SB106        SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  104.9149     115.5206     180      "Solder Bridge OFF"                                                                                                                                                                               
SB58         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  72.4790      143.6659     270      "Solder Bridge OFF"                                                                                                                                                                               
SB61         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  68.3277      143.6136     270      "Solder Bridge OFF"                                                                                                                                                                               
SB112        SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  69.6038      114.2072     90       "Solder Bridge OFF"                                                                                                                                                                               
SB83         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  82.4290      130.0457     180      "Solder Bridge OFF"                                                                                                                                                                               
SB111        SB_ON                                                                                                                                          BottomLayer SOLDER-BRIDGE_R0603-0R                                  59.4462      114.2529     90       "Solder Bridge ON"                                                                                                                                                                                
SB72         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  82.4494      139.3698     180      "Solder Bridge OFF"                                                                                                                                                                               
SB110        SB_ON                                                                                                                                          BottomLayer SOLDER-BRIDGE_R0603-0R                                  58.0898      114.2631     90       "Solder Bridge ON"                                                                                                                                                                                
SB107        SB_ON                                                                                                                                          BottomLayer SOLDER-BRIDGE_R0603-0R                                  60.8584      114.2738     90       "Solder Bridge ON"                                                                                                                                                                                
SB93         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  99.9049      124.5362     180      "Solder Bridge OFF"                                                                                                                                                                               
SB28         SB_ON                                                                                                                                          TopLayer    SOLDER-BRIDGE_R0603-0R                                  60.8584      114.2738     90       "Solder Bridge ON"                                                                                                                                                                                
SB113        SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  72.6028      114.2000     90       "Solder Bridge OFF"                                                                                                                                                                               
SB114        SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  73.8886      114.1884     90       "Solder Bridge OFF"                                                                                                                                                                               
SB99         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  36.4478      121.8946     360      "Solder Bridge OFF"                                                                                                                                                                               
SB60         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  69.6468      143.6136     270      "Solder Bridge OFF"                                                                                                                                                                               
SB59         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  71.0960      143.6659     270      "Solder Bridge OFF"                                                                                                                                                                               
SB57         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  73.8311      143.6659     270      "Solder Bridge OFF"                                                                                                                                                                               
SB95         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  104.8246     123.1113     180      "Solder Bridge OFF"                                                                                                                                                                               
SB105        SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  82.4238      115.7886     180      "Solder Bridge OFF"                                                                                                                                                                               
SB117        SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  82.4394      114.3874     180      "Solder Bridge OFF"                                                                                                                                                                               
SB101        SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  82.4724      120.1903     180      "Solder Bridge OFF"                                                                                                                                                                               
SB70         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  68.9908      139.8016     360      "Solder Bridge OFF"                                                                                                                                                                               
SB104        SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  82.4724      118.7933     180      "Solder Bridge OFF"                                                                                                                                                                               
SB67         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  99.7421      141.1453     180      "Solder Bridge OFF"                                                                                                                                                                               
SB63         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  82.4642      143.3068     180      "Solder Bridge OFF"                                                                                                                                                                               
SB71         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  99.9152      139.6492     360      "Solder Bridge OFF"                                                                                                                                                                               
SB65         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  104.2746     141.4712     270      "Solder Bridge OFF"                                                                                                                                                                               
SB94         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  82.4572      124.0282     180      "Solder Bridge OFF"                                                                                                                                                                               
SB80         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  104.9516     130.8583     180      "Solder Bridge OFF"                                                                                                                                                                               
SB91         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  82.4483      125.3236     180      "Solder Bridge OFF"                                                                                                                                                                               
SB10         SB_OFF                                                                                                                                         TopLayer    SOLDER-BRIDGE_R0603-0R                                  85.4431      143.7220     90       "Solder Bridge OFF"                                                                                                                                                                               
SB54         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  61.7210      143.7011     270      "Solder Bridge OFF"                                                                                                                                                                               
SB53         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  60.3758      143.7295     270      "Solder Bridge OFF"                                                                                                                                                                               
SB116        SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  75.2831      114.1462     90       "Solder Bridge OFF"                                                                                                                                                                               
SB122        SB_ON                                                                                                                                          BottomLayer SOLDER-BRIDGE_R0603-0R                                  7.6200       59.9305      90       "Solder Bridge ON"                                                                                                                                                                                
SB121        SB_ON                                                                                                                                          BottomLayer SOLDER-BRIDGE_R0603-0R                                  7.3381       63.5977      90       "Solder Bridge ON"                                                                                                                                                                                
SB43         SB_ON                                                                                                                                          TopLayer    SOLDER-BRIDGE_R0603-0R                                  78.1899      45.5022      360      "Solder Bridge ON"                                                                                                                                                                                
SB44         SB_ON                                                                                                                                          TopLayer    SOLDER-BRIDGE_R0603-0R                                  16.9977      38.4389      180      "Solder Bridge ON"                                                                                                                                                                                
SW7          SW_MECA_1K2                                                                                                                                    TopLayer    SWI_EAO_09-03290-01_EXTENDED_STRAIGHT_BLACK             88.6663      91.1070      90       "Mechanical Slide Switches 1K2 BLK ACT GOLD STRT MNT"                                                                                                                                             
T1           STL6N2VH5                                                                                                                                      TopLayer    MOS_POWERFLAT_2X2_P065                                  45.0748      99.1138      270      "N-channel 20 V, 0.025 O typ., 6 A STripFET? V Power MOSFET in a PowerFLAT? 2x2 package"                                                                                                          
T5           STT7P2UH7                                                                                                                                      TopLayer    MOS_SOT23-6L                                            42.1843      46.7803      360      "[Obsolete] Power MOSFET - P-channel 20 V, 0.0195 OHM typ., 7 A STripFET H7 -  SOT23-6L"                                                                                                          
T8           STT7P2UH7                                                                                                                                      TopLayer    MOS_SOT23-6L                                            58.0009      46.5588      360      "[Obsolete] Power MOSFET - P-channel 20 V, 0.0195 OHM typ., 7 A STripFET H7 -  SOT23-6L"                                                                                                          
T2           STT7P2UH7                                                                                                                                      TopLayer    MOS_SOT23-6L                                            53.0009      52.7342      360      "[Obsolete] Power MOSFET - P-channel 20 V, 0.0195 OHM typ., 7 A STripFET H7 -  SOT23-6L"                                                                                                          
T4           STT7P2UH7                                                                                                                                      TopLayer    MOS_SOT23-6L                                            42.1259      52.5393      360      "[Obsolete] Power MOSFET - P-channel 20 V, 0.0195 OHM typ., 7 A STripFET H7 -  SOT23-6L"                                                                                                          
T3           STT7P2UH7                                                                                                                                      TopLayer    MOS_SOT23-6L                                            47.6250      52.7050      360      "[Obsolete] Power MOSFET - P-channel 20 V, 0.0195 OHM typ., 7 A STripFET H7 -  SOT23-6L"                                                                                                          
T6           STT7P2UH7                                                                                                                                      TopLayer    MOS_SOT23-6L                                            53.0073      46.7767      360      "[Obsolete] Power MOSFET - P-channel 20 V, 0.0195 OHM typ., 7 A STripFET H7 -  SOT23-6L"                                                                                                          
T7           STT7P2UH7                                                                                                                                      TopLayer    MOS_SOT23-6L                                            49.1998      46.7353      360      "[Obsolete] Power MOSFET - P-channel 20 V, 0.0195 OHM typ., 7 A STripFET H7 -  SOT23-6L"                                                                                                          
T9           STL6N2VH5                                                                                                                                      TopLayer    MOS_POWERFLAT_2X2_P065                                  16.7894      41.7576      270      "N-channel 20 V, 0.025 O typ., 6 A STripFET? V Power MOSFET in a PowerFLAT? 2x2 package"                                                                                                          
T10          STL6N2VH5                                                                                                                                      TopLayer    MOS_POWERFLAT_2X2_P065                                  21.4079      41.6126      270      "N-channel 20 V, 0.025 O typ., 6 A STripFET? V Power MOSFET in a PowerFLAT? 2x2 package"                                                                                                          
U15          MCP2562FD                                                                                                                                      TopLayer    ICC_SO8_5X4_P127                                        33.3865      95.1244      90       "High-Speed CAN Flexible Data Rate Transceiver"                                                                                                                                                   
U16          ESD-TRANSIL-DUAL-BIDIR                                                                                                                         TopLayer    DIO_SOT323                                              23.0233      95.1244      270      "Automotive dual-line Transil, transient voltage suppressor (TVS) for CAN bus. Compliant with interfaces in automotive: CAN-FD, LIN, FlexRay, MOST, SENT, USB"                                    
U10          MCP2562FD                                                                                                                                      TopLayer    ICC_SO8_5X4_P127                                        33.3865      104.2658     90       "High-Speed CAN Flexible Data Rate Transceiver"                                                                                                                                                   
U13          ESD-TRANSIL-DUAL-BIDIR                                                                                                                         TopLayer    DIO_SOT323                                              23.0239      104.1852     270      "Automotive dual-line Transil, transient voltage suppressor (TVS) for CAN bus. Compliant with interfaces in automotive: CAN-FD, LIN, FlexRay, MOST, SENT, USB"                                    
U24          ESDALC6V1W5                                                                                                                                    TopLayer    ESD_SOT323-5L                                           102.1080     69.7191      90       "Dual Transil array for ESD protection"                                                                                                                                                           
U20          ESDALC6V1W5                                                                                                                                    TopLayer    ESD_SOT323-5L                                           102.1406     73.3580      90       "Dual Transil array for ESD protection"                                                                                                                                                           
U46          HSP051-4M10                                                                                                                                    TopLayer    ESD_UQFN-10L_2P5X1_P050                                 96.0422      18.6990      90       "4-line ESD protection for high speed lines"                                                                                                                                                      
U28          SN74LVC2T45DCUT                                                                                                                                TopLayer    ICC_VSSOP8_DCU_R-PDSO-G8_2X2P30_P050                    87.6019      57.8659      270      "Dual bit dual supply bus transceiver"                                                                                                                                                            
U26          SN74LVC2T45DCUT                                                                                                                                TopLayer    ICC_VSSOP8_DCU_R-PDSO-G8_2X2P30_P050                    87.6013      60.9853      270      "Dual bit dual supply bus transceiver"                                                                                                                                                            
U50          ESD-TRANSIL                                                                                                                                    TopLayer    ESD_ST0201                                              51.9140      10.6680      90       "ESD protection 6V1"                                                                                                                                                                              
U49          ESDA6V1-5SC6                                                                                                                                   TopLayer    ESD_SOT23-6L                                            59.8990      12.1920      90       "5 unidirectional Transil diodes ESD protection"                                                                                                                                                  
U47          ST1L05CPU33R                                                                                                                                   TopLayer    ICC_DFN6-EPAD_3X3_P095                                  40.8919      18.2772      180      "LDO, 3.3V, 1.3A, Very low quiescent current BiCMOS voltage regulator"                                                                                                                            
U48          ST1L05BPUR                                                                                                                                     TopLayer    ICC_DFN6-EPAD_3X3_P095                                  32.1664      18.2236      180      "LDO Linear Voltage Regulator IC Positive Adjustable 1 Output Adjustable 1.3A 6-DFN (3x3)"                                                                                                        
U29          LD3985M18R                                                                                                                                     TopLayer    REG_SOT23-5L                                            87.3642      54.5093      90       "Ultra low drop-low noise BiCMOS voltage, regulators low ESR capacitors compatible"                                                                                                               
U17          ST3241EBPR                                                                                                                                     TopLayer    ICC_SSOP28_10P2X5P3_P065                                21.5900      84.7880      270      "RS-232 transceiver with auto-power-down"                                                                                                                                                         
U23          SN74LVC2T45DCUT                                                                                                                                TopLayer    ICC_VSSOP8_DCU_R-PDSO-G8_2X2P30_P050                    24.8007      69.9223      180      "Dual bit dual supply bus transceiver"                                                                                                                                                            
U34          ESD-TRANSIL                                                                                                                                    TopLayer    ESD_QFN2_1P6X1_P125                                     111.0269     47.7782      180      "High power transient voltage suppressor, 7V breakdown"                                                                                                                                           
U31          ECMF02-2AMX6                                                                                                                                   TopLayer    ESD_QFN-6L_1P7X1P5_P050                                 111.0040     52.3162      270      "Common mode filter with ESD protection for USB 2.0 interface"                                                                                                                                    
U25          STMPS2151STR                                                                                                                                   TopLayer    MOS_SOT23-5L                                            61.7027      60.6056      360      "500mA, Enhanced single channel power switches with active high enable pin"                                                                                                                       
U27          LD3985M33R                                                                                                                                     TopLayer    REG_SOT23-5L                                            52.1541      58.2524      180      "Ultra low drop-low noise BiCMOS voltage, regulators low ESR capacitors compatible"                                                                                                               
U21          ESDALC6V1W5                                                                                                                                    TopLayer    ESD_SOT323-5L                                           78.6130      72.5960      180      "Dual Transil array for ESD protection"                                                                                                                                                           
U19          ESDALC6V1W5                                                                                                                                    TopLayer    ESD_SOT323-5L                                           78.6062      76.9274      360      "Dual Transil array for ESD protection"                                                                                                                                                           
U51          ESD-TRANSIL                                                                                                                                    TopLayer    ESD_ST0201                                              80.7669      10.2696      90       "ESD protection 6V1"                                                                                                                                                                              
U35          WM8994ECS/R                                                                                                                                    TopLayer    ICC_W-CSP-BGA72_4P511X4P023_P050                        88.0767      45.2158      360      "Multi-Channel Audio Hub CODEC for Smartphones"                                                                                                                                                   
U41          ESDA6V1BC6                                                                                                                                     TopLayer    ESD_SOT23-6L                                            105.8901     31.9253      270      "Quad Bidir ESD protection"                                                                                                                                                                       
U32          STM32L152CCT6                                                                                                                                  TopLayer    ICC_LQFP48_7X7_P050                                     71.0566      48.0420      180      "Ultra-low-power 32-bit MCU ARM"                                                                                                                                                                  
U39          TSZ122IST                                                                                                                                      TopLayer    ICC_MINISO8_3X3_P065                                    42.6550      39.1155      90       "Very high accuracy (5 ¦ÌV) zero drift micropower 5 V operational amplifiers"                                                                                                                      
U38          TSZ122IST                                                                                                                                      TopLayer    ICC_MINISO8_3X3_P065                                    56.9732      39.5655      270      "Very high accuracy (5 ¦ÌV) zero drift micropower 5 V operational amplifiers"                                                                                                                      
U54          MT25QL512ABB8ESF-0SIT                                                                                                                          BottomLayer ICC_SOP2-SF_16P_10P3X7P5_P127                           82.9036      101.0143     270      "Micron Serial NOR Flash Memory"                                                                                                                                                                  
U18          ESDALC6V1W5                                                                                                                                    TopLayer    ESD_SOT323-5L                                           102.1373     77.6761      270      "Dual Transil array for ESD protection"                                                                                                                                                           
U45          ESDALC6V1W5                                                                                                                                    TopLayer    ESD_SOT323-5L                                           81.3365      19.3857      0        "Dual Transil array for ESD protection"                                                                                                                                                           
X1           OSCILLATOR_4_PINS                                                                                                                              TopLayer    OSC_NDK_NZ2520SB_4P                                     78.1634      19.6062      360      "Oscillator 25.00Mhz, -+50PPM, 3.3V, Temp -55 to +125¡ãC"                                                                                                                                          
X3           XTAL_2_PINS                                                                                                                                    BottomLayer CRY_NX3215SA_2P                                         63.4027      117.3762     180      "Crystal 32.768kHz, 6pF, -+20PPM, R=50K, SMD"                                                                                                                                                     
X2           XTAL_4_PINS                                                                                                                                    BottomLayer CRY_NX2016SA_4P                                         68.8086      118.9736     180      "24MHz crystal oscillator - Cl:6pf -"                                                                                                                                                             
U52          ESD-TRANSIL                                                                                                                                    TopLayer    ESD_ST0201                                              103.8860     5.2070       90       "ESD protection 6V1"                                                                                                                                                                              
U22          ST3485EBDR                                                                                                                                     TopLayer    ICC_SO8_5X4_P127                                        19.2722      69.7660      360      "RS-485/RS-422 transceiver Up to 12Mbps"                                                                                                                                                          
U4           TSH82IDT                                                                                                                                       TopLayer    ICC_SO8_5X4_P127                                        113.3604     148.7020     90       "Wide-band Rail-to-Rail operational amplifiers with standby function"                                                                                                                             
U53          TL1431ACL5T                                                                                                                                    BottomLayer ICC_SOT23-5L_H1P45                                      115.2406     121.7930     270      "Programmable voltage reference"                                                                                                                                                                  
U2           ESD-TRANSIL-BIDIR                                                                                                                              TopLayer    ESD_ST0201                                              114.1730     160.6550     360      "Single-line low capacitance Transil for bidirectional ESD protection 6V1"                                                                                                                        
U7           ESD-TRANSIL-BIDIR                                                                                                                              TopLayer    ESD_ST0201                                              113.5030     125.3490     180      "Single-line low capacitance Transil for bidirectional ESD protection 6V1"                                                                                                                        
U14          ESD-TRANSIL                                                                                                                                    TopLayer    ESD_ST0201                                              106.9340     99.7724      90       "ESD protection 6V1"                                                                                                                                                                              
C169         Capacitor                                                                                                                                      BottomLayer C0402                                                   74.5236      126.1440     90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
L8           BEAD                                                                                                                                           BottomLayer L0603                                                   74.7776      128.4402     180      "SMD Chip ferrite bead, 600R@100MHz +/-25%, 350mA, 500mohm DC, 0603, T=0.8mm"                                                                                                                     
JP12         "Jumper_Header 5x2 Fitted 1-2"                                                                                                                 TopLayer    CON_SAMTEC_TSW-105-07-X-D                               44.7968      70.8026      360      "Header, 5x2, 2,54mm, VR, TH, Height 5.84mm/2.54mm - Shunt Fitted 1-2"                                                                                                                            
R174         PT100                                                                                                                                          TopLayer    PHO_SENBAN_GL55XX                                       98.7619      95.0767      90       "GL55 series? photoconductive cell: Light resistance 10Lux range 10-20KOhm, Dark 1MOhm"                                                                                                           
RV1          POTENTIOMETER                                                                                                                                  TopLayer    POT_BOURNS_3314J-1                                      112.6490     108.1287     270      "4mm Square Trimming Potentiometer 10K OHM 0.25W PC PIN"                                                                                                                                          
SW5          SWITCH_SS42D02                                                                                                                                 TopLayer    SWI_DHS-ELECTRONICS_SS42D02_4P2T                        17.2004      138.6497     90       "Vertical slide switch 4x (A to 2B)"                                                                                                                                                              
SW3          SWITCH_SS42D02                                                                                                                                 TopLayer    SWI_DHS-ELECTRONICS_SS42D02_4P2T                        81.1465      151.4719     360      "Vertical slide switch 4x (A to 2B)"                                                                                                                                                              
SW4          SWITCH_MS-22D16                                                                                                                                TopLayer    SWI_DHS-ELECTRONICS_MS-22D16_2P2T                       48.8888      151.4919     360      "vertical slider switch 2x(A to 2B)"                                                                                                                                                              
SW1          SWITCH_MS-22D16                                                                                                                                TopLayer    SWI_DHS-ELECTRONICS_MS-22D16_2P2T                       17.3667      152.9074     270      "vertical slider switch 2x(A to 2B)"                                                                                                                                                              
SW2          SWITCH_SS42D02                                                                                                                                 TopLayer    SWI_DHS-ELECTRONICS_SS42D02_4P2T                        63.4460      151.5119     360      "Vertical slide switch 4x (A to 2B)"                                                                                                                                                              
SW6          SWITCH_SS42D02                                                                                                                                 TopLayer    SWI_DHS-ELECTRONICS_SS42D02_4P2T                        17.2007      121.2023     90       "Vertical slide switch 4x (A to 2B)"                                                                                                                                                              
C95          Capacitor                                                                                                                                      TopLayer    C0402                                                   25.0635      46.0384      180      "Capacitor, MLCC, 22pF, 50V, C0G, 5%, 0402, T=0,5mm"                                                                                                                                              
C124         Capacitor                                                                                                                                      TopLayer    C1210                                                   18.0594      33.0962      90       "Capacitor, X7R, 10¦ÌF, 50V, 20%, 1210, T=2.5mm"                                                                                                                                                   
C123         Capacitor                                                                                                                                      TopLayer    C1210                                                   21.4884      33.1064      90       "Capacitor, X7R, 10¦ÌF, 50V, 20%, 1210, T=2.5mm"                                                                                                                                                   
C125         Capacitor                                                                                                                                      TopLayer    C0402                                                   23.6405      32.9296      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                                                                                                            
C102         Capacitor                                                                                                                                      TopLayer    C0805                                                   32.3317      41.7043      360      "Capacitor, MLCC, 22uF, 6V3, X5R, 20%, 0805, T=1,25mm"                                                                                                                                            
R247         Resistor                                                                                                                                       TopLayer    R0402                                                   25.0635      44.8155      180      Resistor,82K,0402,1%,1/16W                                                                                                                                                                        
R272         Resistor                                                                                                                                       TopLayer    R0402                                                   24.6750      32.9413      90       Resistor,10K,0402,1%,1/16W                                                                                                                                                                        
R251         Resistor                                                                                                                                       TopLayer    R0402                                                   25.0635      43.7280      360      Resistor,15K,0402,5%,1/16W                                                                                                                                                                        
U33          ESD-TRANSIL                                                                                                                                    TopLayer    DIO_SMC_DO214-AB_1K_2A                                  33.4010      46.1618      180      "3000 W Transil"                                                                                                                                                                                  
LPB1         LPB-S01110101S                                                                                                                                 TopLayer    LIGHT_10MM-SQUARE-LIGHT-BAR_LUMEX_LPB-S01110101S-110945 44.4155      84.1488      0        "10mm Square Light Bar."                                                                                                                                                                          
U6           "?Please validate the IC position on the socket (pin1) not mention on the datasheet.
Eric: please add pin1 outside of socket to show MCU Pin1" TopLayer    ICC_LQFP128_14X14_P040_SOCKET_IRONWOOD_SG-QFE-7011MF    66.7027      128.9659     90       "ARM? Cortex?-M4 32-bit MCU, 512 KB Flash, 96 KB RAM, 5x USART, timers, ADC, DAC, comm. I/F, 1.65-3.6V, with footprint for socket IRONWOOD SG-QFE-7011MF"                                         
CN31         "Please to check it carefuly. Pin 8 and 9 not clearly define on datasheet. Need to validate with schematics symbol"                            BottomLayer CON_CARD-SOCKET_GUANG-LIAN-WEI_2480-208-503-100-RC      52.5460      20.6652      270      "IC Card Socket 8 pin, SMT Open for Smartcard"                                                                                                                                                    
L5           INDUCTOR_POWER                                                                                                                                 TopLayer    IND_TDK_VLS6045EX-4R7M                                  35.3314      32.5374      360      "FIXED IND 4.7UH 4.2A 35 MOHM SMD"                                                                                                                                                                
U37          ST1S41                                                                                                                                         TopLayer    ICC_HSOP8-EPAD_3P90X4P90_P127                           26.2890      39.3612      270      "4A step-down switching regulator"                                                                                                                                                                
SB90         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  77.6791      125.8054     90       "Solder Bridge OFF"                                                                                                                                                                               
SB86         SB_OFF                                                                                                                                         BottomLayer SOLDER-BRIDGE_R0603-0R                                  74.7118      129.8092     180      "Solder Bridge OFF"                                                                                                                                                                               
U40          ST-LINKV3E_SWD                                                                                                                                 TopLayer    ICC_UFBGA201_176+25_10X10_P065                          79.4547      30.2026      90       "STM32F723IEK ?(STM32F7) BGA176"                                                                                                                                                                  
HW7          Comment                                                                                                                                        BottomLayer STICKER_25X9                                            -225.0714    -180.0366    180      ""                                                                                                                                                                                                
Designator42 Comment                                                                                                                                        BottomLayer STICKER_25X9                                            -225.0714    -180.0366    180      ""                                                                                                                                                                                                
