Altium Designer Pick and Place Locations
D:\CAD_Activity\Altium_Projects\STM_LEMANS\MB1404C\03-Manufacturing\MB1404C_PCB\Assembly\MB1404-C01_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       14/09/22
Time:       20:55
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator Comment                        Layer       Footprint                                                  Center-X(mm) Center-Y(mm) Rotation Description                                                                                 
SB84       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     2.5000       116.4625     270      "Solder Bridge 0402 ON"                                                                     
U5         ESD-TRANSIL                    TopLayer    ESD_ST0201                                                 10.0000      117.0000     0        "ESD protection 6V1"                                                                        
R100       Resistor                       TopLayer    R0402                                                      10.0000      111.0000     0        Resistor,0R,0402,5%,1/16W                                                                   
R99        Resistor                       TopLayer    R0402                                                      10.0000      112.2500     0        Resistor,0R,0402,5%,1/16W                                                                   
R98        Resistor                       TopLayer    R0402                                                      10.0000      113.5000     0        Resistor,0R,0402,5%,1/16W                                                                   
R97        Resistor                       TopLayer    R0402                                                      10.0000      114.7500     0        Resistor,0R,0402,5%,1/16W                                                                   
R89        Resistor                       TopLayer    R0402                                                      10.0000      116.0000     0        Resistor,0R,0402,5%,1/16W                                                                   
CN13       USB_TYPE_C_Receptacle          TopLayer    CON_USB-TYPEC_WE_632723300011                              20.9000      7.0200       0        "Connector_USB_TypeC, 24pins, RA, TH, T=1.9mm (USB certified)"                              
U4         ESDALC6V1W5                    BottomLayer ESD_SOT323-5L                                              6.1500       112.9000     90       "Dual Transil array for ESD protection"                                                     
SB83       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     27.2000      61.6375      90       "Solder Bridge 0402 ON"                                                                     
SB82       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     25.2000      61.6375      90       "Solder Bridge 0402 ON"                                                                     
SB81       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     26.2000      61.6375      90       "Solder Bridge 0402 ON"                                                                     
SB80       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     24.2000      59.3375      90       "Solder Bridge 0402 ON"                                                                     
SB79       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     23.2000      60.4375      90       "Solder Bridge 0402 ON"                                                                     
SB78       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     23.2000      57.5375      90       "Solder Bridge 0402 ON"                                                                     
SB9        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     25.2000      59.3375      90       "Solder Bridge 0402 ON"                                                                     
SB8        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     26.2000      59.3375      90       "Solder Bridge 0402 ON"                                                                     
CN3        "Jumper_Header 2x1"            BottomLayer CON_SAMTEC_TSW-102-09-X-S                                  3.1750       128.2800     90       "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/10.16mm"                                        
CN4        "Jumper_Header 2x1"            BottomLayer CON_SAMTEC_TSW-102-09-X-S                                  66.6500      128.2550     90       "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/10.16mm"                                        
U24        ESDALC6V1W5                    BottomLayer ESD_SOT323-5L                                              7.7500       121.7500     270      "Dual Transil array for ESD protection"                                                     
R96        Resistor                       TopLayer    R0402                                                      10.3250      93.8750      180      "Resistor, 1K, 0402, +/-1%,1/16W"                                                           
R95        Resistor                       TopLayer    R0402                                                      17.0000      125.7500     180      Resistor,100K,0402,1%,1/16W                                                                 
R93        Resistor                       TopLayer    R0402                                                      50.2500      107.7500     180      "Resistor, 100K, 0402, +/-1%, 1/16W"                                                        
R92        Resistor                       TopLayer    R0402                                                      13.5000      120.2500     270      Resistor,47R,0402,1%,1/16W                                                                  
R91        Resistor                       TopLayer    R0402                                                      38.4250      116.5000     0        "Resistor, 0R, 0402, +/-5%, 1/16W"                                                          
R90        Resistor                       TopLayer    R0402                                                      15.5000      120.2500     270      Resistor,100K,0402,1%,1/16W                                                                 
R88        Resistor                       TopLayer    R0402                                                      45.0000      107.5000     180      "Resistor, 3K9, 0402, +/-1%, 1/16W, +/-100ppm/°C"                                           
R87        Resistor                       TopLayer    R0402                                                      45.0000      105.5000     180      "Resistor, 1K3, 0402, +/-1%, 1/16W"                                                         
R86        Resistor                       TopLayer    R0402                                                      45.0000      106.5000     180      "Resistor, 1K8, 0402, +/-1%, 1/16W"                                                         
R85        Resistor                       TopLayer    R0402                                                      45.0000      109.5000     180      "Resistor, 5K1, 0402, +/-1%, 1/16W"                                                         
R84        Resistor                       TopLayer    R0402                                                      14.5000      120.2500     270      Resistor,47R,0402,1%,1/16W                                                                  
R83        Resistor                       TopLayer    R0402                                                      16.5000      120.2500     270      Resistor,47R,0402,1%,1/16W                                                                  
R82        Resistor                       TopLayer    R0402                                                      17.5000      120.2500     270      Resistor,47R,0402,1%,1/16W                                                                  
R81        Resistor                       TopLayer    R0402                                                      13.5000      126.2500     90       Resistor,100K,0402,1%,1/16W                                                                 
R80        Resistor                       TopLayer    R0402                                                      14.5000      126.2500     90       Resistor,100K,0402,1%,1/16W                                                                 
R79        Resistor                       TopLayer    R0402                                                      15.5000      126.2500     270      Resistor,100K,0402,1%,1/16W                                                                 
R78        Resistor                       TopLayer    R0402                                                      16.7500      113.2500     180      Resistor,100K,0402,1%,1/16W                                                                 
R77        Resistor                       TopLayer    R0402                                                      15.7500      107.5000     270      "Resistor, 100R, 0402, +/- 1%, 1/16W"                                                       
R76        Resistor                       TopLayer    R0402                                                      43.0000      123.2500     270      "Resistor, 5K1, 0402, +/-1%, 1/16W"                                                         
LD6        LED_BICOLOR                    TopLayer    LED_BI-GR_WE-150141SV73110                                 57.8750      129.4790     180      "LED Bicolor, Green/Red, 2V, 20mA,  4-PLCC"                                                 
C92        Capacitor                      TopLayer    C0402                                                      49.2500      106.2500     180      "Capacitor, MLCC, 10nF, 50V, X7R, +/-10%, 0402, T=0.5mm"                                    
TP13       "Test Point"                   TopLayer    TP_SMD_1MM                                                 20.8500      126.3750     180      "Test Point 1mm"                                                                            
R94        Resistor                       TopLayer    R0402                                                      13.0000      99.5000      270      "Resistor, 100K, 0402, +/-1%, 1/16W"                                                        
C89        Capacitor                      TopLayer    C0805                                                      24.6250      14.0000      0        "Capacitor, MLCC, 2.2uF, 25V, X7R, +/-10%, 0805, T=1,25mm"                                  
C90        Capacitor                      TopLayer    C0402                                                      11.3250      9.8250       0        "Capacitor, MLCC, 10nF, 50V ,X7R, +/-10%, 0402, T=0.5mm"                                    
R56        Resistor                       TopLayer    R0402                                                      14.9500      15.1000      270      "Resistor, 2K4, 0402, +/-1%, 1/16W"                                                         
R55        Resistor                       TopLayer    R0402                                                      13.8750      15.1000      270      Resistor,10K,0402,1%,1/16W                                                                  
Q1         STL11N3LLH6                    TopLayer    MOS_POWERFLAT_3P3X3P3_P065                                 12.3750      12.2000      270      "N-channel 30 V, 6 mO typ, 11 A STripFET™ H6, Power MOSFET in a PowerFLAT™ 3.3x3.3 package" 
D1         SCHOTTKY_1A_2K                 TopLayer    DIO_SOD523_1A_2K                                           16.8500      19.5000      180      "Small signal Schottky diodes"                                                              
C46        Capacitor                      TopLayer    C0402                                                      35.9250      85.4000      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                   
C88        Capacitor                      TopLayer    C0402                                                      17.6250      16.0250      270      "Capacitor, MLCC, 330pF, 50V, NPO, +/-5%, 0402, T=0,5mm"                                    
C86        Capacitor                      TopLayer    C0402                                                      16.0000      21.3500      90       "Capacitor, MLCC, 330pF, 50V, NPO, +/-5%, 0402, T=0,5mm"                                    
C87        Capacitor                      TopLayer    C0603                                                      16.8750      18.1000      0        Capacitor,100nF,50V,X7R,10%,0603                                                            
SB63       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     51.1625      55.2750      0        "Solder Bridge 0402 ON"                                                                     
SB65       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     51.0875      54.1750      180      "Solder Bridge 0402 ON"                                                                     
SB13       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     51.4625      92.3750      180      "Solder Bridge 0402 ON"                                                                     
SB75       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     11.4125      14.1250      180      "Solder Bridge 0402 ON"                                                                     
SB2        SB_ON                          TopLayer    SOLDER-BRIDGE_R0603-0R                                     26.6000      91.8500      0        "Solder Bridge ON"                                                                          
SB60       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     18.3625      57.6250      180      "Solder Bridge 0402 ON"                                                                     
R67        Resistor                       BottomLayer R0603                                                      33.4660      103.3789     0        Resistor,100K,0603,1%,1/10W                                                                 
R66        Resistor                       BottomLayer R0603                                                      36.8660      103.3789     0        Resistor,100K,0603,1%,1/10W                                                                 
R26        Resistor                       TopLayer    R0402                                                      36.6160      103.8789     270      Resistor,470R,0402,1%,1/16W                                                                 
R69        Resistor                       BottomLayer R0603                                                      33.4660      101.9789     0        Resistor,47K,0603,1%,1/10W                                                                  
R68        Resistor                       BottomLayer R0603                                                      36.8660      101.9789     0        Resistor,47K,0603,1%,1/10W                                                                  
R25        Resistor                       TopLayer    R0402                                                      33.2160      103.8789     270      Resistor,270R,0402,1%,1/16W                                                                 
Q4         9013-SOT23                     BottomLayer NPN_SOT23                                                  33.2080      106.1469     180      "NPN Bipolar Transistor"                                                                    
Q3         9013-SOT23                     BottomLayer NPN_SOT23                                                  36.6160      106.1469     180      "NPN Bipolar Transistor"                                                                    
LD3        LED_red                        TopLayer    LED_0603_OSRAM_LS-Q976-NR-1_RED_1A2K_H0P8                  33.2080      106.4969     90       "LED Red, 0603 SMD, Forward Voltage Typ=2V, Max=2.5V"                                       
LD2        LED_yellow                     TopLayer    LED_0603_OSRAM_LY-Q396-P1Q2-36_YELLOW_1A2K_H0P4            36.6160      106.4969     90       "LED Yellow, 0603 SMD, Forward Voltage min=1.7V, Typ=2V, Max=2.3V"                          
SB7        SB_ON                          TopLayer    SOLDER-BRIDGE_R0402-0R                                     11.3375      14.8500      0        "Solder Bridge 0402 ON"                                                                     
SB69       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                     45.1060      45.1560      180      "Solder Bridge ON"                                                                          
SB21       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     29.0000      84.9125      270      "Solder Bridge 0402 ON"                                                                     
SB6        SB_ON                          TopLayer    SOLDER-BRIDGE_R0402-0R                                     16.6500      15.9375      90       "Solder Bridge 0402 ON"                                                                     
SB26       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     26.4750      84.9375      270      "Solder Bridge 0402 ON"                                                                     
SB31       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     33.0000      78.0375      90       "Solder Bridge 0402 ON"                                                                     
SB29       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                     45.7750      82.1500      0        "Solder Bridge ON"                                                                          
SB70       SB_ON                          TopLayer    SOLDER-BRIDGE_R0402-0R                                     24.2018      57.7875      270      "Solder Bridge 0402 ON"                                                                     
JP6        "Jumper_Header 2x1 Fitted"     TopLayer    CON_SAMTEC_TSW-102-07-G-S                                  45.1560      92.0739      180      "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm - Shunt Fitted by default"               
U3         ECMF02-2AMX6                   TopLayer    ESD_QFN-6L_1P7X1P5_P050                                    48.2500      120.1250     180      "Common mode filter with ESD protection for USB 2.0 interface"                              
U14        STM32H563ZIT6                  TopLayer    ICC_LQFP144_20X20_P050_SOCKET_YAMAICHI_IC149-144-145-B5_NM 35.1160      71.3039      90       "STM32H563ZIT6, LQFP144 package, 20x20"                                                     
CN12       "Header 35x2"                  TopLayer    CON_SAMTEC_TSW-135-07-X-D                                  65.4760      58.3939      270      "Header, 35x2, 2,54mm, VR, TH, Height 5.84mm/2.54mm"                                        
CN11       "Header 35x2"                  TopLayer    CON_SAMTEC_TSW-135-07-X-D                                  4.5160       58.4189      270      "Header, 35x2, 2,54mm, VR, TH, Height 5.84mm/2.54mm"                                        
CN5        "Header 10x2"                  TopLayer    CON_SAMTEC_FTSH-110-01-L-DV                                5.5110       116.6850     270      "Header, 10x2, 1.27mm, VR, SMD, T=3.05mm"                                                   
CN1        USB_TYPE_C_Receptacle          TopLayer    CON_USB-TYPEC_WE_632723300011                              48.9750      126.2800     180      "Connector_USB_TypeC, 24pins, RA, TH, T=1.9mm (USB certified)"                              
B1         SW_PUSH_SMD                    TopLayer    SWI_KNITTER_TSS644S                                        7.7750       6.1000       0        "Push Button, NO, 0.05A, 12V, 2.6N, SMD, 9.0x6.2mm, T=7.3mm, changeable caps KTSC-6xx"      
B2         SW_PUSH_SMD                    TopLayer    SWI_KNITTER_TSS644S                                        62.4026      6.1000       0        "Push Button, NO, 0.05A, 12V, 2.6N, SMD, 9.0x6.2mm, T=7.3mm, changeable caps KTSC-6xx"      
JP2        "Jumper_Header 5x2 Fitted 1-2" TopLayer    CON_SAMTEC_TSW-105-07-X-D                                  60.3710      114.3139     270      "Header, 5x2, 2,54mm, VR, TH, Height 5.84mm/2.54mm - Shunt Fitted 1-2"                      
C59        Capacitor                      TopLayer    C0603                                                      39.9750      57.5000      90       "Capacitor, MLCC, 100nF, 6V3, X5R, 10%, 0603, T=0,8mm"                                      
JP4        "Jumper_Header 3x1 Fitted 1-2" TopLayer    CON_SAMTEC_TSW-103-07-F-S                                  34.9960      97.1540      180      "Header, 3x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm - Shunt Fitted 1-2 by default"           
U12        LD1117S50TR                    TopLayer    REG_SOT223-TAB                                             23.0910      104.0539     270      "IC REG LDO 5V 0.8A SOT223"                                                                 
CN8        "Socket 8x2_N144_ARD"          TopLayer    CON_SAMTEC_SSQ-108-23-F-D                                  12.1360      82.5489      270      "Socket, 8x2, 2.54mm, VR, TH, T=8.51mm/10mm"                                                
CN9        "Socket 15x2_N144_ARD"         TopLayer    CON_SAMTEC_SSQ-115-23-F-D                                  12.1360      50.7989      270      "Socket, 15x2, 2.54mm, VR, TH, T=8.51mm/10mm"                                               
CN7        "Socket 10x2_N144_ARD"         TopLayer    CON_SAMTEC_SSQ-110-23-F-D                                  57.8560      89.1529      270      "Socket, 10x2, 2.54mm, VR, TH, T=8.51mm/10mm"                                               
CN10       "Socket 17x2_N144_ARD"         TopLayer    CON_SAMTEC_SSQ-117-23-F-D                                  57.8560      53.3389      270      "Socket, 17x2, 2.54mm, VR, TH, T=8.51mm/10mm"                                               
C66        Capacitor                      TopLayer    C0603                                                      44.1500      56.3000      90       "Capacitor, MLCC, 100nF, 6V3, X5R, 10%, 0603, T=0,8mm"                                      
C79        Capacitor                      TopLayer    C0603                                                      41.5410      36.0789      180      "Capacitor, MLCC, 100nF, 6V3, X5R, 10%, 0603, T=0,8mm"                                      
C81        Capacitor                      TopLayer    C0603                                                      32.9410      33.1789      90       "Capacitor, MLCC, 100nF, 6V3, X5R, 10%, 0603, T=0,8mm"                                      
C82        Capacitor                      TopLayer    C0603                                                      34.2910      33.1789      90       "Capacitor, MLCC, 10µF, 10V, X5R, 10%, 0603, T=0.8mm"                                       
C80        Capacitor                      TopLayer    C0603                                                      33.7660      35.4789      180      "Capacitor, MLCC, 100nF, 6V3, X5R, 10%, 0603, T=0,8mm"                                      
C77        Capacitor                      TopLayer    C0402                                                      41.2910      40.6039      180      "Capacitor, MLCC, 470pF, 50V, NPO, 5%, 0402, T=0,5mm"                                       
C75        Capacitor                      TopLayer    C0402                                                      41.2910      41.5289      180      "Capacitor, MLCC, 1uF, 6V3, X5R, 10%, 0402, T=0,5mm"                                        
C74        Capacitor                      TopLayer    C0603                                                      37.0910      43.1789      270      "Capacitor, MLCC, 100nF, 6V3, X5R, 10%, 0603, T=0,8mm"                                      
C84        Capacitor                      TopLayer    C0603                                                      33.9750      28.1000      90       "Capacitor, MLCC, 100nF, 6V3, X5R, 10%, 0603, T=0,8mm"                                      
C83        Capacitor                      TopLayer    C0603                                                      47.4290      29.0090      180      "Capacitor, MLCC, 100nF, 6V3, X5R, 10%, 0603, T=0,8mm"                                      
C91        Capacitor                      TopLayer    C1206_H1P6                                                 34.2500      6.5250       90       "Capacitor, MLCC, 1nF, 2KV, X7R, 10%, 1206, T=1,25mm"                                       
C78        Capacitor                      TopLayer    C0402                                                      45.2660      39.1539      270      "Capacitor, MLCC, 5.6pF, 50V, NPO, 5%, 0402, T=0,5mm"                                       
C76        Capacitor                      TopLayer    C0402                                                      43.5910      41.1789      180      "Capacitor, MLCC, 5.6pF, 50V, NPO, 5%, 0402, T=0,5mm"                                       
C42        Capacitor                      TopLayer    C0805                                                      17.3410      101.7741     0        "Capacitor, MLCC, 10uF, 25V, X5R, 10%, 0805, T=0,85mm"                                      
C41        Capacitor                      TopLayer    C0805                                                      17.3410      104.0741     0        "Capacitor, MLCC, 10uF, 25V, X5R, 10%, 0805, T=0,85mm"                                      
C39        Capacitor                      TopLayer    C0603                                                      43.2500      97.2500      270      "Capacitor, MLCC, 4.7µF, 10V, X5R, 20%, 0603, T=0,8mm"                                      
C40        Capacitor                      TopLayer    C0603                                                      48.2160      97.0289      270      "Capacitor, MLCC, 4.7uF, 16V, X5R, 20%, 0603, T=0,8mm"                                      
C38        Capacitor                      TopLayer    C0402                                                      48.6660      98.6539      180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                      
C43        Capacitor                      TopLayer    C0603                                                      21.2500      97.5000      0        "Capacitor, MLCC, 4.7uF, 16V, X5R, 20%, 0603, T=0,8mm"                                      
C44        Capacitor                      TopLayer    C0402                                                      18.0750      95.4250      270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                      
C45        Capacitor                      TopLayer    C0603                                                      22.3750      92.3250      0        "Capacitor, MLCC, 4.7µF, 10V, X5R, 20%, 0603, T=0,8mm"                                      
C37        Capacitor                      TopLayer    C0402                                                      49.5000      109.2500     270      "Capacitor, MLCC, 100nF, 25V, X7R, +/-10%, 0402, T=0.5mm"                                   
C28        Capacitor                      TopLayer    C0402                                                      27.2500      130.7500     90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                      
C5         Capacitor                      TopLayer    C0402                                                      51.7250      120.1000     90       "Capacitor, MLCC, 10nF, 50V, X7R, +/-10%, 0402, T=0.5mm"                                    
C7         Capacitor                      TopLayer    C0402                                                      30.4160      126.4289     270      "Capacitor, MLCC, 2.2uF, 6.3V, X5R, +/-10%, 0402, T=0.5mm"                                  
C14        Capacitor                      TopLayer    C0402                                                      35.5750      123.3500     180      "Capacitor, MLCC, 2.2uF, 6.3V, X5R, +/-10%, 0402, T=0.5mm"                                  
C12        Capacitor                      TopLayer    C0402                                                      22.4500      124.0500     0        "Capacitor, MLCC, 2.2uF, 6.3V, X5R, +/-10%, 0402, T=0.5mm"                                  
C34        Capacitor                      TopLayer    C0402                                                      34.4750      113.4000     270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                      
C8         Capacitor                      TopLayer    C0402                                                      24.4910      126.4289     90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                      
C33        Capacitor                      TopLayer    C0402                                                      33.2250      113.4000     270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                      
C22        Capacitor                      TopLayer    C0402                                                      35.6000      119.6289     0        "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                      
C17        Capacitor                      TopLayer    C0402                                                      35.5750      120.8789     0        "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                      
C15        Capacitor                      TopLayer    C0402                                                      35.5750      122.1289     0        "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                      
C9         Capacitor                      TopLayer    C0402                                                      26.9160      126.4289     90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                      
C10        Capacitor                      TopLayer    C0402                                                      28.4910      126.4289     90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                      
C21        Capacitor                      TopLayer    C0402                                                      22.5410      118.6289     180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                      
C25        Capacitor                      TopLayer    C0402                                                      22.5410      116.6789     180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                      
C13        Capacitor                      TopLayer    C0402                                                      22.5410      121.4539     180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                      
C30        Capacitor                      TopLayer    C0402                                                      26.4910      113.4039     270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                      
C29        Capacitor                      TopLayer    C0402                                                      25.2410      113.4039     270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                      
C31        Capacitor                      TopLayer    C0402                                                      30.6160      113.4039     270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                      
C32        Capacitor                      TopLayer    C0402                                                      31.8660      113.4039     270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                      
C11        Capacitor                      TopLayer    C0402                                                      31.6910      126.4289     90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                      
C35        Capacitor                      TopLayer    C0402                                                      16.7500      107.5000     90       "Capacitor, MLCC, 20pF, 50V, NPO, 5%, 0402, T=0,5mm"                                        
C36        Capacitor                      TopLayer    C0603                                                      47.7500      110.0000     180      "Capacitor, MLCC, 10uF, 10V, X5R, +/-10%, 0603, T=0.8mm"                                    
C16        Capacitor                      TopLayer    C0402                                                      22.5410      120.2039     180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                      
C6         Capacitor                      TopLayer    C0402                                                      54.1750      120.7750     270      "Capacitor, MLCC, 100pF, 50V, NPO, +/-5%, 0402, T=0.5mm"                                    
C26        Capacitor                      TopLayer    C0402                                                      17.5000      111.5000     270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                      
C27        Capacitor                      TopLayer    C0402                                                      17.5000      109.7500     270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                      
C3         Capacitor                      TopLayer    C0402                                                      42.4000      128.6750     270      "Capacitor, MLCC, 100nF, 25V, X7R, +/-10%, 0402, T=0.5mm"                                   
C1         Capacitor                      TopLayer    C0603                                                      40.4000      131.6250     0        "Capacitor, MLCC, 10uF, 10V, X5R, +/-10%, 0603, T=0.8mm"                                    
C24        Capacitor                      TopLayer    C0402                                                      30.1500      110.8500     90       "Capacitor, MLCC, 2.7pF, 50V, NPO, +/-0.1pF, 0402, T=0.5mm"                                 
C23        Capacitor                      TopLayer    C0603                                                      44.6289      117.5965     0        "Capacitor, MLCC, 10uF, 10V, X5R, +/-10%, 0603, T=0.8mm"                                    
C18        Capacitor                      TopLayer    C0805                                                      41.5000      114.2500     90       "Capacitor, MLCC, 2.2uF, 25V, X7R, +/-10%, 0805, T=1,25mm"                                  
C20        Capacitor                      TopLayer    C0402                                                      26.8250      110.7000     270      "Capacitor, MLCC, 2.7pF, 50V, NPO, +/-0.1pF, 0402, T=0.5mm"                                 
C19        Capacitor                      TopLayer    C0402                                                      42.5000      121.7500     0        "Capacitor, MLCC, 10nF, 50V, X7R, +/-10%, 0402, T=0.5mm"                                    
C69        Capacitor                      TopLayer    C0603                                                      41.3250      54.7250      90       "Capacitor, MLCC, 100nF, 6V3, X5R, 10%, 0603, T=0,8mm"                                      
C71        Capacitor                      TopLayer    C0402                                                      35.5500      54.3500      90       "Capacitor, MLCC, 5.6pF, 50V, NPO, 5%, 0402, T=0,5mm"                                       
C70        Capacitor                      TopLayer    C0402                                                      39.1500      54.5000      270      "Capacitor, MLCC, 5.6pF, 50V, NPO, 5%, 0402, T=0,5mm"                                       
C72        Capacitor                      TopLayer    C0402                                                      28.8250      53.3500      180      "Capacitor, MLCC, 3.3pF, 50V, NPO, +/-0.1pF, 0402, T=0.5mm"                                 
C73        Capacitor                      TopLayer    C0402                                                      31.0250      53.3500      0        "Capacitor, MLCC, 3.3pF, 50V, NPO, +/-0.1pF, 0402, T=0.5mm"                                 
C64        Capacitor                      TopLayer    C0402                                                      48.4250      56.6250      270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                      
C63        Capacitor                      TopLayer    C0402                                                      47.5250      56.6250      270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                      
C47        Capacitor                      TopLayer    C0402                                                      38.3500      84.7750      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                   
C67        Capacitor                      TopLayer    C0603                                                      46.4000      56.3000      270      "Capacitor, MLCC, 1uF, 6V3, X5R, 10%, 0603, T=0,8mm"                                        
C68        Capacitor                      TopLayer    C0402                                                      45.2750      56.0500      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                   
C65        Capacitor                      TopLayer    C0603                                                      42.8000      56.3000      270      "Capacitor, MLCC, 1uF, 6V3, X5R, 10%, 0603, T=0,8mm"                                        
C61        Capacitor                      TopLayer    C0402                                                      42.8500      58.2250      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                   
C60        Capacitor                      TopLayer    C0603                                                      41.3250      57.5000      90       "Capacitor, MLCC, 4.7µF, 10V, X5R, 20%, 0603, T=0,8mm"                                      
C57        Capacitor                      TopLayer    C0402                                                      21.8000      62.4750      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                   
C49        Capacitor                      TopLayer    C0402                                                      48.6000      81.0000      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                   
C53        Capacitor                      TopLayer    C0402                                                      48.6000      69.6500      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                   
C51        Capacitor                      TopLayer    C0402                                                      48.6000      74.9250      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                   
C58        Capacitor                      TopLayer    C0402                                                      33.4250      58.2250      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                   
C48        Capacitor                      TopLayer    C0402                                                      24.8000      84.6750      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                   
C52        Capacitor                      TopLayer    C0402                                                      21.6250      69.9750      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                   
C54        Capacitor                      TopLayer    C0402                                                      21.6250      69.0500      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                   
C56        Capacitor                      TopLayer    C0402                                                      48.2000      62.5750      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                   
C85        Capacitor                      TopLayer    C0603                                                      17.5500      26.7250      270      "Capacitor, MLCC, 10pF, 50V, NPO, 5%, 0603, T=0,8mm"                                        
CN16       "Jumper_Header 2x1"            BottomLayer CON_SAMTEC_TSW-102-09-X-S                                  4.5160       12.6989      0        "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/10.16mm"                                        
CN15       "Jumper_Header 2x1"            BottomLayer CON_SAMTEC_TSW-102-09-X-S                                  65.4760      12.6739      0        "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/10.16mm"                                        
CN14       RJ45_KRJ-CB4.2GYZNL            TopLayer    CON_RJ45_DGKYD_KRJ-CB4.2GYZNL                              44.3686      7.9499       0        "RJ45 jack, single port, with LEDS, Metal shielded dip low profile"                         
CN2        "Header 4x1"                   TopLayer    CON_SAMTEC_TSW-104-07-G-S                                  19.2250      130.7250     0        "Header, 4x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm"                                         
JP3        "Jumper_Header 2x1"            TopLayer    CON_SAMTEC_TSW-102-07-G-S                                  31.2000      130.7750     0        "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm"                                         
JP1        "Jumper_Header 2x1"            TopLayer    CON_SAMTEC_TSW-102-07-G-S                                  10.8660      100.3289     270      "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm"                                         
JP5        "Jumper_Header 2x1 Fitted"     TopLayer    CON_SAMTEC_TSW-102-07-G-S                                  33.7260      93.9790      180      "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm - Shunt Fitted by default"               
L1         BEAD                           TopLayer    L0603                                                      30.7660      33.8539      180      "Ferrite bead, 600R@100MHz, +/-25%, 500mA, 380mR, 0603, T=0.8mm"                            
LD1        LED_green                      TopLayer    LED_0603_OSRAM_LG-Q396-PS-35_GREEN_1A2K_H0P4               40.1410      106.4969     90       "LED Green, 0603 SMD, Forward Voltage Typ=2V, Max=2.5V"                                     
LD5        LED_green                      TopLayer    LED_0603_OSRAM_LG-Q396-PS-35_GREEN_1A2K_H0P4               62.5125      122.3125     0        "LED Green, 0603 SMD, Forward Voltage Typ=2V, Max=2.5V"                                     
LD4        LED_BICOLOR                    TopLayer    LED_BI-GR_WE-150141SV73110                                 62.7160      129.4790     180      "LED Bicolor, Green/Red, 2V, 20mA,  4-PLCC"                                                 
LD7        LED_green                      TopLayer    LED_0603_OSRAM_LG-Q396-PS-35_GREEN_1A2K_H0P4               32.2410      2.7290       90       "LED Green, 0603 SMD, Forward Voltage Typ=2V, Max=2.5V"                                     
Q2         9013-SOT23                     BottomLayer NPN_SOT23                                                  40.1410      106.1469     180      "NPN Bipolar Transistor"                                                                    
R24        Resistor                       TopLayer    R0402                                                      40.1410      104.1789     270      Resistor,270R,0402,1%,1/16W                                                                 
R70        Resistor                       BottomLayer R0603                                                      40.4140      101.9669     0        Resistor,47K,0603,1%,1/10W                                                                  
R65        Resistor                       BottomLayer R0603                                                      40.4110      103.3849     0        Resistor,100K,0603,1%,1/10W                                                                 
R39        Resistor                       TopLayer    R0402                                                      38.2910      42.8539      90       Resistor,10K,0402,1%,1/16W                                                                  
R42        Resistor                       TopLayer    R0402                                                      41.4410      42.8539      90       Resistor,10K,0402,1%,1/16W                                                                  
R36        Resistor                       TopLayer    R0402                                                      32.4660      42.8539      90       Resistor,10K,0402,1%,1/16W                                                                  
R43        Resistor                       TopLayer    R0402                                                      33.1910      41.4789      180      Resistor,1K5,0402,1%,1/16W                                                                  
R44        Resistor                       TopLayer    R0402                                                      33.1910      40.4289      180      Resistor,10K,0402,1%,1/16W                                                                  
R73        Resistor                       BottomLayer R0402                                                      38.1910      34.3789      270      Resistor,49R9,0402,1%,1/16W                                                                 
R72        Resistor                       BottomLayer R0402                                                      39.1910      34.3789      270      Resistor,49R9,0402,1%,1/16W                                                                 
R75        Resistor                       BottomLayer R0402                                                      36.1910      34.3789      270      Resistor,49R9,0402,1%,1/16W                                                                 
R74        Resistor                       BottomLayer R0402                                                      37.1910      34.3789      270      Resistor,49R9,0402,1%,1/16W                                                                 
R40        Resistor                       TopLayer    R0402                                                      39.3410      42.8539      270      Resistor,33R,0402,1%,1/16W                                                                  
R38        Resistor                       TopLayer    R0402                                                      35.5660      42.8539      90       Resistor,10K,0402,1%,1/16W                                                                  
R41        Resistor                       TopLayer    R0402                                                      40.3910      42.8539      270      Resistor,33R,0402,1%,1/16W                                                                  
R51        Resistor                       TopLayer    R0402                                                      34.1910      19.4039      90       Resistor,75R,0402,1%,1/16W                                                                  
R52        Resistor                       TopLayer    R0402                                                      48.5160      19.4039      90       Resistor,75R,0402,1%,1/16W                                                                  
R53        Resistor                       TopLayer    R0402                                                      32.0910      18.5039      270      Resistor,75R,0402,1%,1/16W                                                                  
R54        Resistor                       TopLayer    R0402                                                      33.1410      18.5039      270      Resistor,75R,0402,1%,1/16W                                                                  
R37        Resistor                       TopLayer    R0402                                                      33.5160      42.8539      270      Resistor,33R,0402,1%,1/16W                                                                  
R47        Resistor                       TopLayer    R0402                                                      41.2160      34.8789      0        Resistor,12K1,0402,1%,1/16W                                                                 
R45        Resistor                       TopLayer    R0402                                                      33.1910      39.3789      0        Resistor,33R,0402,1%,1/16W                                                                  
R58        Resistor                       TopLayer    R0402                                                      53.8660      11.1289      90       Resistor,270R,0402,1%,1/16W                                                                 
R57        Resistor                       TopLayer    R0402                                                      34.8412      12.9727      90       Resistor,10K,0402,1%,1/16W                                                                  
R59        Resistor                       TopLayer    R0402                                                      34.8660      11.0790      270      Resistor,270R,0402,1%,1/16W                                                                 
R46        Resistor                       TopLayer    R0402                                                      41.5660      38.8789      180      Resistor,0R,0402,5%,1/16W                                                                   
R12        Resistor                       TopLayer    R0603                                                      60.0125      122.3125     180      Resistor,620R,0603,1%,1/10W                                                                 
R23        Resistor                       TopLayer    R0402                                                      49.4160      96.7789      270      Resistor,10K,0402,1%,1/16W                                                                  
R64        Resistor                       TopLayer    R0402                                                      42.0000      123.2500     270      "Resistor, 100K, 0402, +/-1%, 1/16W"                                                        
R11        Resistor                       TopLayer    R0402                                                      50.3750      120.6250     0        "Resistor, 5K1, 0402, +/-1%, 1/16W"                                                         
R19        Resistor                       TopLayer    R0402                                                      13.2500      113.5000     90       Resistor,100K,0402,1%,1/16W                                                                 
R22        Resistor                       TopLayer    R0402                                                      12.5000      120.2500     90       Resistor,100K,0402,1%,1/16W                                                                 
R3         Resistor                       TopLayer    R0402                                                      57.1500      126.0750     270      "Resistor, 330R, 0402, +/-1%, 1/16W"                                                        
R21        Resistor                       TopLayer    R0402                                                      14.7500      107.5000     270      Resistor,100K,0402,1%,1/16W                                                                 
R18        Resistor                       TopLayer    R0402                                                      35.8500      114.2250     0        "Resistor, 10K, 0402, +/-1%, 1/16W"                                                         
R17        Resistor                       TopLayer    R0402                                                      35.8500      115.2750     0        "Resistor, 10K, 0402, +/-1%, 1/16W"                                                         
R15        Resistor                       TopLayer    R0402                                                      37.9000      117.9500     90       "Resistor, 10K, 0402, +/-1%, 1/16W"                                                         
R14        Resistor                       TopLayer    R0402                                                      39.0000      117.9500     90       "Resistor, 5K1, 0402, +/-1%, 1/16W"                                                         
R20        Resistor                       TopLayer    R0402                                                      13.7500      107.5000     270      Resistor,100K,0402,1%,1/16W                                                                 
R5         Resistor                       TopLayer    R0402                                                      25.4660      126.4289     90       "Resistor, 0R, 0402, +/-5%, 1/16W"                                                          
R27        Resistor                       TopLayer    R0402                                                      50.3750      119.5750     0        "Resistor, 100K, 0402, +/-1%, 1/16W"                                                        
R6         Resistor                       TopLayer    R0402                                                      29.4660      126.4289     90       Resistor,3K,0402,1%,1/16W                                                                   
R16        Resistor                       TopLayer    R0402                                                      14.2500      113.5000     90       Resistor,100K,0402,1%,1/16W                                                                 
R10        Resistor                       TopLayer    R0402                                                      22.5500      114.7500     180      Resistor,10K,0402,1%,1/16W                                                                  
R13        Resistor                       TopLayer    R0402                                                      15.2500      113.5000     90       Resistor,100K,0402,1%,1/16W                                                                 
R2         Resistor                       TopLayer    R0402                                                      45.0000      108.5000     180      "Resistor, 3K, 0402, +/-1%, 1/16W"                                                          
R1         Resistor                       TopLayer    R0402                                                      37.3250      129.7750     90       Resistor,100K,0402,1%,1/16W                                                                 
R7         Resistor                       TopLayer    R0402                                                      39.4250      126.4250     180      Resistor,100K,0402,1%,1/16W                                                                 
R9         Resistor                       TopLayer    R0402                                                      63.4910      126.0769     270      "Resistor, 1K, 0402, +/-0.1%, 1/16W, +/-25ppm/°C"                                           
R8         Resistor                       TopLayer    R0402                                                      61.9410      126.1023     90       "Resistor, 330R, 0402, +/-1%, 1/16W"                                                        
R71        Resistor                       BottomLayer R0603                                                      29.8000      55.5000      270      Resistor,330R,0603,1%,1/10W                                                                 
R62        Resistor                       TopLayer    R0603                                                      14.5660      5.7289       270      Resistor,100K,0603,1%,1/10W                                                                 
R31        Resistor                       TopLayer    R0603                                                      20.7250      67.2250      180      Resistor,10K,0603,1%,1/10W                                                                  
R49        Resistor                       TopLayer    R0603                                                      16.1500      26.7250      90       Resistor,330K,0603,1%,1/10W                                                                 
R48        Resistor                       TopLayer    R0603                                                      18.9599      26.7314      270      Resistor,49K9,0603,1%                                                                       
R34        Resistor                       TopLayer    R0603                                                      29.2250      57.1750      270      Resistor,0R,0603,5%,1/10W                                                                   
R35        Resistor                       TopLayer    R0603                                                      30.6250      57.1750      270      Resistor,0R,0603,5%,1/10W                                                                   
R33        Resistor                       TopLayer    R0603                                                      47.2250      58.1750      180      Resistor,0R,0603,5%,1/10W                                                                   
R32        Resistor                       TopLayer    R0603                                                      44.8750      58.1750      180      Resistor,0R,0603,5%,1/10W                                                                   
R63        Resistor                       TopLayer    R0603                                                      33.6250      2.7250       90       Resistor,510R,0603,1%,1/10W                                                                 
R60        Resistor                       TopLayer    R0603                                                      28.7500      8.5500       0        Resistor,47K,0603,1%,1/10W                                                                  
R61        Resistor                       TopLayer    R0603                                                      28.7500      7.1000       0        Resistor,22K,0603,1%,1/10W                                                                  
R50        Resistor                       TopLayer    R0402                                                      12.5250      21.4250      270      Resistor,10K,0402,1%,1/16W                                                                  
SB25       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                     17.8750      85.3750      180      "Solder Bridge ON"                                                                          
SB16       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                     17.8750      86.8750      180      "Solder Bridge ON"                                                                          
SB46       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                     41.9500      63.8500      270      "Solder Bridge ON"                                                                          
SB20       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     32.8500      85.5375      90       "Solder Bridge 0402 ON"                                                                     
SB19       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                     35.0500      86.0000      0        "Solder Bridge ON"                                                                          
SB45       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     28.9750      64.6125      270      "Solder Bridge 0402 ON"                                                                     
SB44       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     30.2500      64.6125      270      "Solder Bridge 0402 ON"                                                                     
SB50       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                     34.3500      63.9500      90       "Solder Bridge ON"                                                                          
SB48       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                     37.1500      63.9500      90       "Solder Bridge ON"                                                                          
SB51       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                     45.7750      63.6750      0        "Solder Bridge ON"                                                                          
SB43       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                     45.9500      65.0750      0        "Solder Bridge ON"                                                                          
SB72       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                     32.7410      38.8789      0        "Solder Bridge ON"                                                                          
SB76       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                     54.8750      6.3500       0        "Solder Bridge ON"                                                                          
SB77       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                     34.0000      6.3500       180      "Solder Bridge ON"                                                                          
SB1        SB_ON                          TopLayer    SOLDER-BRIDGE_R0603-0R                                     40.7000      97.0000      180      "Solder Bridge ON"                                                                          
SB11       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                     25.3910      95.8789      180      "Solder Bridge ON"                                                                          
SB58       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                     44.4250      57.9500      270      "Solder Bridge ON"                                                                          
SB39       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                     20.4500      71.2000      0        "Solder Bridge ON"                                                                          
SB38       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     32.2125      71.2750      180      "Solder Bridge 0402 ON"                                                                     
SB52       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     18.4375      62.0500      0        "Solder Bridge 0402 ON"                                                                     
SB54       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     29.8000      57.5625      270      "Solder Bridge 0402 ON"                                                                     
SB17       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                     51.8000      85.0000      90       "Solder Bridge ON"                                                                          
SB27       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     29.0000      81.7125      270      "Solder Bridge 0402 ON"                                                                     
SB28       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     28.0000      81.7125      270      "Solder Bridge 0402 ON"                                                                     
SB59       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                     42.8750      58.0500      90       "Solder Bridge ON"                                                                          
SB62       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                     41.2250      54.5500      90       "Solder Bridge ON"                                                                          
SB42       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                     46.0000      66.4750      180      "Solder Bridge ON"                                                                          
SB36       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     32.2875      72.6750      0        "Solder Bridge 0402 ON"                                                                     
SB49       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                     35.7500      63.9500      90       "Solder Bridge ON"                                                                          
SB22       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     28.0000      84.9125      270      "Solder Bridge 0402 ON"                                                                     
SB56       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     51.0875      59.8250      180      "Solder Bridge 0402 ON"                                                                     
SB3        SB_ON                          TopLayer    SOLDER-BRIDGE_R0603-0R                                     36.6500      56.9250      270      "Solder Bridge ON"                                                                          
SB24       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                     47.8750      85.0000      90       "Solder Bridge ON"                                                                          
SB18       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                     45.4750      85.0000      90       "Solder Bridge ON"                                                                          
SB4        SB_ON                          TopLayer    SOLDER-BRIDGE_R0603-0R                                     38.0500      56.9250      270      "Solder Bridge ON"                                                                          
SB34       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                     20.4500      74.0000      0        "Solder Bridge ON"                                                                          
SB37       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                     20.4500      72.6000      0        "Solder Bridge ON"                                                                          
SB67       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     18.3625      51.7000      180      "Solder Bridge 0402 ON"                                                                     
SB15       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                     47.8750      87.8000      90       "Solder Bridge ON"                                                                          
SB40       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                     20.4500      69.0750      0        "Solder Bridge ON"                                                                          
SB14       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                     49.2750      87.8000      90       "Solder Bridge ON"                                                                          
SB55       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     28.7000      61.6375      90       "Solder Bridge 0402 ON"                                                                     
SB47       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                     40.5500      63.8500      270      "Solder Bridge ON"                                                                          
SB74       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                     59.5250      18.1750      270      "Solder Bridge ON"                                                                          
SB5        SB_ON                          TopLayer    SOLDER-BRIDGE_R0402-0R                                     14.9750      21.4125      270      "Solder Bridge 0402 ON"                                                                     
SB23       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                     49.2750      85.0000      90       "Solder Bridge ON"                                                                          
SB12       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                     47.2500      95.0500      90       "Solder Bridge ON"                                                                          
SB30       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                     45.7750      80.7250      0        "Solder Bridge ON"                                                                          
SB71       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     28.2000      59.3375      90       "Solder Bridge 0402 ON"                                                                     
SB57       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     18.3625      59.3500      180      "Solder Bridge 0402 ON"                                                                     
SB61       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     51.1625      56.3750      0        "Solder Bridge 0402 ON"                                                                     
SB41       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                     30.7250      68.4750      180      "Solder Bridge ON"                                                                          
SB33       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     32.2875      74.3250      0        "Solder Bridge 0402 ON"                                                                     
SB35       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     51.0875      72.9439      180      "Solder Bridge 0402 ON"                                                                     
SB53       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     18.4375      60.9500      0        "Solder Bridge 0402 ON"                                                                     
SB10       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                     47.2500      98.0500      90       "Solder Bridge ON"                                                                          
SB66       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     18.3625      53.3000      180      "Solder Bridge 0402 ON"                                                                     
SB64       SB_ON                          TopLayer    SOLDER-BRIDGE_R0402-0R                                     23.1750      57.8875      90       "Solder Bridge 0402 ON"                                                                     
SB68       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     27.2000      59.3375      90       "Solder Bridge 0402 ON"                                                                     
SB73       SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R                                     51.1625      38.1000      0        "Solder Bridge 0402 ON"                                                                     
T1         9013-SOT23                     TopLayer    NPN_SOT23                                                  28.7916      3.9517       180      "NPN Bipolar Transistor"                                                                    
TP1        "Test Point"                   TopLayer    TP_SMD_1MM                                                 28.7500      97.1750      270      "Test Point 1mm"                                                                            
TP2        "Test Point"                   TopLayer    TP_SMD_1MM                                                 26.0410      94.0039      180      "Test Point 1mm"                                                                            
U16        USBLC6-4SC6                    TopLayer    ESD_SOT23-6L                                               37.6910      32.2789      180      "Very low capacitance ESD protection , 4 lines"                                             
U17        KMS-1102NL                     TopLayer    TRS_DGKYD_KMS-1102NL                                       41.3460      22.8589      180      "Discrete Magnetic Transformer Module, 16 pins, SMT, 100 Base-TX"                           
U15        LAN8742A-CZ-TR                 TopLayer    ICC_VQFN24-EPAD_4X4_P050                                   37.6910      38.6289      180      "10/100M RMII Ethernet transceiver"                                                         
U7         STLINK-V3EC                    TopLayer    ICC_UFBGA201_176+25_10X10_P065                             29.0661      119.9039     90       "MCU, Arm Cortex-M7 32-bit MCU, 512KB Flash, 276KB RAM, With Crypto"                        
U11        ST1L05CPU33R                   TopLayer    ICC_DFN6-EPAD_3X3_P095                                     45.7500      97.7500      180      "LDO, 3.3V, 1.3A, Very low quiescent current BiCMOS voltage regulator"                      
U13        ST1L05BPUR                     TopLayer    ICC_DFN6-EPAD_3X3_P095                                     20.6660      94.9289      270      "LDO Linear Voltage Regulator IC Positive Adjustable 1 Output Adjustable 1.3A 6-DFN (3x3)"  
U8         TPS259535DSG                   TopLayer    ICC_WSON8-EPAD_2X2_P050                                    47.7500      108.0000     180      "eFuse with Fast Overvoltage Protection 2.7V to 18V 4A 34mOhm 8-Pin WSON"                   
U23        ESD-TRANSIL                    TopLayer    ESD_ST0201                                                 10.0000      117.7500     0        "ESD protection 6V1"                                                                        
U6         ESD-TRANSIL                    TopLayer    ESD_QFN1610_2N_1K_2A                                       53.1500      120.6000     270      "High power Transient voltage suppressor:25V/35A EOS and ESD transients protection."        
U2         STMPS2151STR                   TopLayer    MOS_SOT23-5L                                               39.9250      128.9250     180      "500mA, Enhanced single channel power switches with active high enable pin"                 
U10        74AVC4TD245BQ                  TopLayer    ICC_DHVQFN16-EPAD_SOT763-1_2P5X3P5_H0P85_P050              14.7500      110.5000     270      "4-bit dual supply translating transceiver with configurable voltage translation; 3-state"  
U9         ST730M33R                      TopLayer    ICC_SOT23-5L_H1P45                                         44.2500      114.7500     180      "LDO, 3.3V, 300mA, High input voltage: 2.5V to 28V, SOT23-5L"                               
U22        ESD-TRANSIL                    TopLayer    ESD_ST0201                                                 14.5660      3.7039       270      "ESD protection 6V1"                                                                        
U21        ESD-TRANSIL                    TopLayer    ESD_ST0201                                                 55.7478      8.5227       270      "ESD protection 6V1"                                                                        
U20        ESD-TRANSIL                    TopLayer    ESD_QFN1610_2N_1K_2A                                       24.3250      12.2500      0        "High power Transient voltage suppressor:25V/35A EOS and ESD transients protection."        
U18        TCPP01-M12                     TopLayer    ICC_QFN12L-EPAD_3X3_P050                                   12.5250      18.1250      270      "USB Type-C Port Protection for USB Power Delivery, PPS compliant"                          
U19        USBLC6-2SC6                    TopLayer    ESD_SOT23-6L                                               20.9000      15.8500      180      "Very low capacitance ESD protection"                                                       
X4         XTAL_4_PINS                    TopLayer    CRY_NX2016SA_4P                                            43.6660      39.3789      90       "Crystal 25MHz, 6pF, +-20ppm, 80ohms max, SMD"                                              
X1         XTAL_4_PINS                    TopLayer    CRY_NX2016SA_4P                                            28.4750      110.7750     0        "Crystal, 24MHz, 6pF, +/-20ppm, 80R, 2x1.6mm"                                               
X3         XTAL_4_PINS                    TopLayer    CRY_NX2016SA_4P                                            37.3500      54.4250      0        "Crystal 25MHz, 6pF, +-20ppm, 80ohms max, SMD"                                              
X2         XTAL_2_PINS                    TopLayer    CRY_NX1610SE_2P                                            29.9250      54.9000      180      "Crystal, 32.768kHz, 9pF, +/-20ppm, 70KR, 1.6x1mm"                                          
C55        Capacitor                      TopLayer    C0603                                                      20.8750      64.1000      0        "Capacitor, MLCC, 2.2uF, 10V, X5R, 10%, 0603, T=0,8mm"                                      
C50        Capacitor                      TopLayer    C0603                                                      48.9250      79.8750      180      "Capacitor, MLCC, 2.2uF, 10V, X5R, 10%, 0603, T=0,8mm"                                      
C62        Capacitor                      TopLayer    C0603                                                      26.5250      56.3250      90       "Capacitor, MLCC, 1uF, 6V3, X5R, 10%, 0603, T=0,8mm"                                        
SB32       SB_ON                          BottomLayer SOLDER-BRIDGE_R0603-0R                                     26.2500      77.9500      270      "Solder Bridge ON"                                                                          
U1         74AVC4TD245BQ                  TopLayer    ICC_DHVQFN16-EPAD_SOT763-1_2P5X3P5_H0P85_P050              15.0000      123.2500     270      "4-bit dual supply translating transceiver with configurable voltage translation; 3-state"  
C4         Capacitor                      TopLayer    C0402                                                      17.7500      124.2500     270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                      
C2         Capacitor                      TopLayer    C0402                                                      17.7500      122.5000     270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                      
R28        Resistor                       TopLayer    R0402                                                      20.6660      98.7039      0        Resistor,10K,0402,1%,1/16W                                                                  
R29        Resistor                       TopLayer    R0402                                                      23.1000      94.4500      270      Resistor,27K,0402,1%,1/16W                                                                  
R4         Resistor                       TopLayer    R0402                                                      58.6750      126.0750     270      "Resistor, 1K, 0402, +/-0.1%, 1/16W, +/-25ppm/°C"                                           
R30        Resistor                       TopLayer    R0402                                                      24.1500      94.4500      90       Resistor,56K,0402,1%,1/16W                                                                  
TP3        "Test Point"                   TopLayer    TP_SMD_1MM                                                 17.8250      92.9089      270      "Test Point 1mm"                                                                            
