Altium Designer Pick and Place Locations
E:\items\MB1508项目\ST 硬件资料\02-Manufacturing\MB1508C_PCB\Assembly\MB1508C_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       14/01/21
Time:       16:20
Revision:   Not in VersionControl
Variant:    L462RE
Units used: mm

Designator   Comment                       Layer       Footprint                                       Center-X(mm) Center-Y(mm) Rotation Description                                                                                              
CN13         "Header 25x2"                 BottomLayer CON_SAMTEC_TSM-125-01-F-DV-A                    41.7000      71.5200      180      "Header, 25x2, 2,54mm, VR, TH, Height 5.84mm/2.54mm, with alignment Pin"                                 
CN12         "Header 25x2"                 BottomLayer CON_SAMTEC_TSM-125-01-F-DV-A                    41.7000      5.4800       180      "Header, 25x2, 2,54mm, VR, TH, Height 5.84mm/2.54mm, with alignment Pin"                                 
CN2          MUP-C792                      TopLayer    CON_MICRO-SIMCARD_MUP_MUP-C792                  26.5000      67.6475      180      "Socket_microsim 17.17*16.75, height 1.5mm, 6PIN"                                                        
JP4          "Jumper_Header 2x1"           TopLayer    CON_SAMTEC_TSW-102-07-G-S                       64.0042      60.6184      90       "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm"                                                      
R21          Resistor                      TopLayer    R0603                                           52.6467      27.5904      360      Resistor,10K,0603,1%,1/10W                                                                               
Q6           BSN20                         BottomLayer MOS_SOT23                                       43.9228      60.0779      180      "MOSFET, N-Channel , Vds: 20V, Id: 2A, Vgs(th): 1.5V, Vgs(max): +/-8V, Rdson:120mohm@Vgs=1.8V, Qg=6.3nC" 
JP1          "Jumper_Header 2x1 Fitted"    TopLayer    CON_SAMTEC_TSW-102-07-G-S                       43.9039      56.3085      360      "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm - Shunt Fitted by default"                            
SB37         SB_ON                         BottomLayer SOLDER-BRIDGE_R0603-0R                          54.6510      42.3765      90       "Solder Bridge ON"                                                                                       
R80          Resistor                      BottomLayer R0603                                           45.8201      43.5773      270      Resistor,10K,0603,1%,1/10W                                                                               
SB8          SB_ON                         TopLayer    SOLDER-BRIDGE_R0603-0R                          52.8560      73.4616      270      "Solder Bridge ON"                                                                                       
SB45         SB_ON                         BottomLayer SOLDER-BRIDGE_R0603-0R                          46.9867      58.4452      180      "Solder Bridge ON"                                                                                       
R3           Resistor                      TopLayer    R0603                                           21.7247      12.4760      360      Resistor,10K,0603,1%,1/10W                                                                               
T1           9013-SOT23                    TopLayer    NPN_SOT23                                       74.3302      43.3212      270      "NPN Bipolar Transistor"                                                                                 
SB16         SB_ON                         TopLayer    SOLDER-BRIDGE_R0603-0R                          57.3193      13.3824      270      "Solder Bridge ON"                                                                                       
SB11         SB_ON                         TopLayer    SOLDER-BRIDGE_R0603-0R                          52.4900      21.2872      270      "Solder Bridge ON"                                                                                       
SB1          SB_ON                         TopLayer    SOLDER-BRIDGE_R0603-0R                          34.7848      41.2524      360      "Solder Bridge ON"                                                                                       
SB10         SB_ON                         TopLayer    SOLDER-BRIDGE_R0603-0R                          52.6243      26.2442      360      "Solder Bridge ON"                                                                                       
SB12         SB_ON                         TopLayer    SOLDER-BRIDGE_R0603-0R                          52.5460      13.0684      270      "Solder Bridge ON"                                                                                       
SB27         SB_ON                         TopLayer    SOLDER-BRIDGE_R0603-0R                          71.9867      24.2220      360      "Solder Bridge ON"                                                                                       
SB7          SB_ON                         TopLayer    SOLDER-BRIDGE_R0603-0R                          50.5633      24.3818      90       "Solder Bridge ON"                                                                                       
SB36         SB_ON                         TopLayer    SOLDER-BRIDGE_R0603-0R                          96.8747      36.3204      180      "Solder Bridge ON"                                                                                       
SB30         SB_ON                         TopLayer    SOLDER-BRIDGE_R0603-0R                          87.8176      16.5501      90       "Solder Bridge ON"                                                                                       
SB17         SB_ON                         TopLayer    SOLDER-BRIDGE_R0603-0R                          69.0479      40.9164      360      "Solder Bridge ON"                                                                                       
SB22         SB_ON                         TopLayer    SOLDER-BRIDGE_R0603-0R                          64.2992      44.6005      180      "Solder Bridge ON"                                                                                       
SB19         SB_ON                         TopLayer    SOLDER-BRIDGE_R0603-0R                          69.9160      46.4968      90       "Solder Bridge ON"                                                                                       
SB20         SB_ON                         TopLayer    SOLDER-BRIDGE_R0603-0R                          70.2449      52.2816      90       "Solder Bridge ON"                                                                                       
SB18         SB_ON                         TopLayer    SOLDER-BRIDGE_R0603-0R                          68.3928      52.2532      270      "Solder Bridge ON"                                                                                       
SB9          SB_ON                         TopLayer    SOLDER-BRIDGE_R0603-0R                          52.4477      18.4656      180      "Solder Bridge ON"                                                                                       
SB15         SB_ON                         TopLayer    SOLDER-BRIDGE_R0603-0R                          56.6931      20.7846      90       "Solder Bridge ON"                                                                                       
SB34         SB_ON                         TopLayer    SOLDER-BRIDGE_R0603-0R                          96.7974      37.9235      180      "Solder Bridge ON"                                                                                       
SB61         SB_ON                         BottomLayer SOLDER-BRIDGE_R0603-0R                          11.2468      27.1016      180      "Solder Bridge ON"                                                                                       
SB58         SB_ON                         BottomLayer SOLDER-BRIDGE_R0603-0R                          11.3056      24.2456      180      "Solder Bridge ON"                                                                                       
SB60         SB_ON                         BottomLayer SOLDER-BRIDGE_R0603-0R                          11.2802      25.6284      180      "Solder Bridge ON"                                                                                       
SB5          SB_ON                         TopLayer    SOLDER-BRIDGE_R0603-0R                          38.0474      58.9024      270      "Solder Bridge ON"                                                                                       
SB42         SB_ON                         BottomLayer SOLDER-BRIDGE_R0603-0R                          50.7223      35.8215      270      "Solder Bridge ON"                                                                                       
SB46         SB_ON                         BottomLayer SOLDER-BRIDGE_R0603-0R                          46.5601      29.5508      90       "Solder Bridge ON"                                                                                       
SB38         SB_ON                         BottomLayer SOLDER-BRIDGE_R0603-0R                          51.5505      38.1866      360      "Solder Bridge ON"                                                                                       
SB57         SB_ON                         BottomLayer SOLDER-BRIDGE_R0603-0R                          11.3064      18.5838      180      "Solder Bridge ON"                                                                                       
SB4          SB_ON                         TopLayer    SOLDER-BRIDGE_R0603-0R                          34.6569      39.7156      180      "Solder Bridge ON"                                                                                       
SB53         SB_ON                         BottomLayer SOLDER-BRIDGE_R0603-0R                          14.3020      20.4380      180      "Solder Bridge ON"                                                                                       
SB40         SB_ON                         BottomLayer SOLDER-BRIDGE_R0603-0R                          51.5334      17.0362      360      "Solder Bridge ON"                                                                                       
SB2          SB_ON                         TopLayer    SOLDER-BRIDGE_R0603-0R                          35.7210      49.4508      180      "Solder Bridge ON"                                                                                       
SB3          SB_ON                         TopLayer    SOLDER-BRIDGE_R0603-0R                          35.7581      46.3774      180      "Solder Bridge ON"                                                                                       
R72          Resistor                      BottomLayer R0603                                           52.7086      19.0636      90       Resistor,10K,0603,1%,1/10W                                                                               
R100         Resistor                      BottomLayer R0603                                           24.7676      32.8509      180      Resistor,0R,0603,5%,1/10W                                                                                
R99          Resistor                      BottomLayer R0603                                           24.7930      34.2390      180      Resistor,0R,0603,5%,1/10W                                                                                
R56          Resistor                      TopLayer    R0603                                           87.5614      54.1528      180      Resistor,10K,0603,1%,1/10W                                                                               
R54          Resistor                      TopLayer    R0603                                           87.5106      55.4990      360      Resistor,100K,0603,1%,1/10W                                                                              
R96          Resistor                      BottomLayer R0603                                           26.9178      28.9050      90       Resistor,0R,0603,5%,1/10W                                                                                
R66          Resistor                      TopLayer    R0603                                           92.7938      41.8632      90       Resistor,100K,0603,1%,1/10W                                                                              
R59          Resistor                      TopLayer    R0603                                           87.8058      39.9662      270      Resistor,100K,0603,1%,1/10W                                                                              
R58          Resistor                      TopLayer    R0603                                           87.6933      36.1452      90       Resistor,100K,0603,1%,1/10W                                                                              
R53          Resistor                      TopLayer    R0603                                           88.6670      13.3097      270      Resistor,10K,0603,1%,1/10W                                                                               
R65          Resistor                      TopLayer    R0603                                           93.6800      12.6097      90       Resistor,10K,0603,1%,1/10W                                                                               
R67          Resistor                      TopLayer    R0603                                           101.1620     6.4617       360      Resistor,100K,0603,1%,1/10W                                                                              
R50          Resistor                      TopLayer    R0603                                           84.4690      32.2832      90       Resistor,330R,0603,1%,1/10W                                                                              
R52          Resistor                      TopLayer    R0603                                           86.0492      32.2476      90       Resistor,330R,0603,1%,1/10W                                                                              
R48          Resistor                      TopLayer    R0603                                           87.5800      70.5900      360      Resistor,100K,0603,1%,1/10W                                                                              
R63          Resistor                      TopLayer    R0603                                           91.8169      69.1489      180      Resistor,47K,0603,1%,1/10W                                                                               
R36          Resistor                      TopLayer    R0603                                           71.6886      40.2528      90       Resistor,36K,0603,1%,1/10W                                                                               
R43          Resistor                      TopLayer    R0603                                           76.3114      47.0154      180      Resistor,1K5,0603,1%,1/10W                                                                               
R57          Resistor                      TopLayer    R0603                                           95.5437      71.5230      270      Resistor,47K,0603,1%,1/10W                                                                               
R37          Resistor                      TopLayer    R0603                                           71.6886      42.8578      270      Resistor,100R,0603,1%,1/10W                                                                              
R64          Resistor                      TopLayer    R0603                                           93.9845      71.5230      270      Resistor,1K,0603,1%,1/10W                                                                                
R39          Resistor                      TopLayer    R0603                                           73.1110      46.2280      90       Resistor,10K,0603,1%,1/10W                                                                               
R55          Resistor                      TopLayer    R0603                                           87.5509      52.6730      360      Resistor,4K7,0603,1%,1/10W                                                                               
R42          Resistor                      TopLayer    R0603                                           75.1552      48.4636      180      Resistor,100R,0603,1%,1/10W                                                                              
R33          Resistor                      TopLayer    R0603                                           64.1218      51.0795      360      Resistor,22R,0603,1%,1/10W                                                                               
R31          Resistor                      TopLayer    R0603                                           64.1430      48.2713      360      Resistor,22R,0603,1%,1/10W                                                                               
R32          Resistor                      TopLayer    R0603                                           64.1265      49.6911      360      Resistor,22R,0603,1%,1/10W                                                                               
R60          Resistor                      TopLayer    R0603                                           87.8938      42.5982      90       Resistor,10K,0603,1%,1/10W                                                                               
R34          Resistor                      TopLayer    R0603                                           69.7928      49.4426      270      Resistor,22R,0603,1%,1/10W                                                                               
R29          [N/A]                         TopLayer    R0603                                           68.2721      43.3369      270      Resistor,22R,0603,1%,1/10W                                                                               
R30          Resistor                      TopLayer    R0603                                           68.3928      49.4792      90       Resistor,10K,0603,1%,1/10W                                                                               
R51          Resistor                      TopLayer    R0603                                           84.8446      40.9042      90       Resistor,100K,0603,1%,1/10W                                                                              
R49          Resistor                      TopLayer    R0603                                           81.9725      40.7296      270      Resistor,4K7,0603,1%,1/10W                                                                               
R47          Resistor                      TopLayer    R0603                                           80.5478      40.7296      90       Resistor,2K7,0603,1%,1/10W                                                                               
R23          Resistor                      TopLayer    R0603                                           58.0780      18.4078      180      Resistor,0R,0603,5%,1/10W                                                                                
R24          Resistor                      TopLayer    R0603                                           58.1288      16.9391      180      Resistor,0R,0603,5%,1/10W                                                                                
R38          Resistor                      TopLayer    R0603                                           69.5403      18.8476      360      Resistor,0R,0603,5%,1/10W                                                                                
R35          Resistor                      TopLayer    R0603                                           69.4925      20.6256      360      Resistor,0R,0603,5%,1/10W                                                                                
R25          Resistor                      TopLayer    R0603                                           58.5689      25.9126      180      Resistor,0R,0603,5%,1/10W                                                                                
R28          Resistor                      TopLayer    R0603                                           58.6548      21.4797      180      Resistor,0R,0603,5%,1/10W                                                                                
R68          Resistor                      TopLayer    R0603                                           98.8216      44.2753      270      Resistor,43K,0603,1%,1/10W                                                                               
R69          Resistor                      TopLayer    R0603                                           98.8354      41.7495      270      Resistor,20K5,0603,1%,1/10W                                                                              
R95          Resistor                      BottomLayer R0603                                           26.4182      47.9882      180      Resistor,11K8,0603,1%,1/10W                                                                              
R104         Resistor                      BottomLayer R0603                                           24.1710      47.9931      180      Resistor,20K5,0603,1%,1/10W                                                                              
R75          Resistor                      BottomLayer R0603                                           51.2327      15.4141      360      Resistor,22R,0603,1%,1/10W                                                                               
R83          Resistor                      BottomLayer R0603                                           43.3089      29.3594      270      Resistor,22R,0603,1%,1/10W                                                                               
R81          Resistor                      BottomLayer R0603                                           44.8837      29.3340      270      Resistor,22R,0603,1%,1/10W                                                                               
R46          Resistor                      TopLayer    R0603                                           84.2800      6.7600       180      Resistor,100K,0603,1%,1/10W                                                                              
R40          Resistor                      TopLayer    R0603                                           68.2116      33.4534      90       Resistor,10K,0603,1%,1/10W                                                                               
R94          Resistor                      BottomLayer R0603                                           27.1822      41.9643      360      Resistor,100K,0603,1%,1/10W                                                                              
R107         Resistor                      BottomLayer R0603                                           22.3498      41.9779      360      Resistor,100K,0603,1%,1/10W                                                                              
R116         Resistor                      BottomLayer R0603                                           17.3395      41.9948      360      Resistor,100K,0603,1%,1/10W                                                                              
R90          Resistor                      BottomLayer R0603                                           29.4712      41.9135      360      Resistor,47K,0603,1%,1/10W                                                                               
R101         Resistor                      BottomLayer R0603                                           24.6204      41.9779      360      Resistor,47K,0603,1%,1/10W                                                                               
R113         Resistor                      BottomLayer R0603                                           19.8304      41.9779      360      Resistor,47K,0603,1%,1/10W                                                                               
R88          Resistor                      BottomLayer R0603                                           30.7270      39.3989      270      Resistor,510R,0603,1%,1/10W                                                                              
R98          Resistor                      BottomLayer R0603                                           25.5962      39.5513      270      Resistor,510R,0603,1%,1/10W                                                                              
R118         Resistor                      BottomLayer R0603                                           16.4663      39.3956      270      Resistor,510R,0603,1%,1/10W                                                                              
R19          Resistor                      TopLayer    R0603                                           52.3449      16.9806      360      Resistor,0R,0603,5%,1/10W                                                                                
R105         Resistor                      BottomLayer R0603                                           23.2474      12.4086      360      Resistor,10K,0603,1%,1/10W                                                                               
R103         Resistor                      BottomLayer R0603                                           24.2500      27.5246      360      Resistor,10K,0603,1%,1/10W                                                                               
R45          Resistor                      TopLayer    R0603                                           74.3655      19.8786      270      Resistor,0R,0603,5%,1/10W                                                                                
R26          Resistor                      TopLayer    R0603                                           58.5727      24.5760      360      Resistor,0R,0603,5%,1/10W                                                                                
R27          Resistor                      TopLayer    R0603                                           58.6489      22.8631      360      Resistor,0R,0603,5%,1/10W                                                                                
R106         Resistor                      BottomLayer R0603                                           22.7610      21.8858      360      Resistor,10K,0603,1%,1/10W                                                                               
R108         Resistor                      BottomLayer R0603                                           22.4982      32.2832      90       Resistor,4K7,0603,1%,1/10W                                                                               
R109         Resistor                      BottomLayer R0603                                           22.4728      34.6962      270      Resistor,4K7,0603,1%,1/10W                                                                               
R71          Resistor                      BottomLayer R0603                                           55.9548      60.0620      270      Resistor,100K,0603,1%,1/10W                                                                              
R70          Resistor                      BottomLayer R0603                                           57.3701      60.0748      90       Resistor,47K,0603,1%,1/10W                                                                               
R79          Resistor                      BottomLayer R0603                                           46.3802      60.8974      270      Resistor,100K,0603,1%,1/10W                                                                              
R17          Resistor                      TopLayer    R0603                                           49.1827      64.6085      180      Resistor,510R,0603,1%,1/10W                                                                              
R13          Resistor                      TopLayer    R0603                                           36.5952      44.4634      90       Resistor,10K,0603,1%,1/10W                                                                               
R10          Resistor                      TopLayer    R0603                                           35.1474      44.4888      90       Resistor,10K,0603,1%,1/10W                                                                               
R82          Resistor                      BottomLayer R0603                                           44.4621      43.4990      90       Resistor,10K,0603,1%,1/10W                                                                               
R76          Resistor                      BottomLayer R0603                                           51.3251      42.8915      270      Resistor,1K,0603,1%,1/10W                                                                                
R2           Resistor                      TopLayer    R0603                                           21.1221      4.5840       90       Resistor,100R,0603,1%,1/10W                                                                              
R11          Resistor                      TopLayer    R0603                                           35.7224      48.1300      360      Resistor,10K,0603,1%,1/10W                                                                               
R1           Resistor                      TopLayer    R0603                                           21.7410      10.6680      360      Resistor,10K,0603,1%,1/10W                                                                               
Q7           9013-SOT23                    BottomLayer NPN_SOT23                                       28.2124      39.2211      360      "NPN Bipolar Transistor"                                                                                 
Q8           9013-SOT23                    BottomLayer NPN_SOT23                                       23.0308      39.3481      360      "NPN Bipolar Transistor"                                                                                 
Q9           9013-SOT23                    BottomLayer NPN_SOT23                                       18.9668      39.3227      360      "NPN Bipolar Transistor"                                                                                 
Q4           9013-SOT23                    BottomLayer NPN_SOT23                                       53.3721      60.5868      180      "NPN Bipolar Transistor"                                                                                 
LD5          LED_green                     TopLayer    LED_0603_GREEN_H0P8                             51.9401      64.6085      360      "LED, Green, 0603"                                                                                       
D8           BAT60JFILM                    TopLayer    DIO_SOD323                                      101.3933     53.2767      180      BAT60JFILM                                                                                               
D7           BAT60JFILM                    TopLayer    DIO_SOD323                                      96.6391      55.1447      360      BAT60JFILM                                                                                               
D11          BAT60JFILM                    TopLayer    DIO_SOD323                                      101.3933     55.1447      180      BAT60JFILM                                                                                               
D9           BAT60JFILM                    TopLayer    DIO_SOD323                                      96.6391      56.8947      360      BAT60JFILM                                                                                               
D1           BAT60JFILM                    TopLayer    DIO_SOD323                                      68.3082      46.3550      270      BAT60JFILM                                                                                               
D2           BAT60JFILM                    TopLayer    DIO_SOD323                                      81.5024      38.3824      180      BAT60JFILM                                                                                               
D4           BAT60JFILM                    TopLayer    DIO_SOD323                                      92.4510      55.1447      180      BAT60JFILM                                                                                               
D12          BAT60JFILM                    TopLayer    DIO_SOD323                                      101.3711     56.9781      180      BAT60JFILM                                                                                               
D5           BAT60JFILM                    TopLayer    DIO_SOD323                                      96.6391      58.6947      360      BAT60JFILM                                                                                               
D3           BAT60JFILM                    TopLayer    DIO_SOD323                                      101.4011     58.8153      180      BAT60JFILM                                                                                               
C14          Capacitor                     TopLayer    C0603                                           58.0018      15.4510      180      "Capacitor, MLCC, 100nF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                   
C61          Capacitor                     BottomLayer C0603                                           25.5066      36.5250      180      "Capacitor, MLCC, 100nF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                   
C24          Capacitor                     TopLayer    C0603                                           79.9324      56.0284      360      "Capacitor, MLCC, 100nF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                   
C29          Capacitor                     TopLayer    C0603                                           87.4852      56.8706      360      "Capacitor, MLCC, 100nF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                   
C50          Capacitor                     BottomLayer C0603                                           75.3142      5.8936       360      "Capacitor, MLCC, 1uF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                     
C51          Capacitor                     BottomLayer C0603                                           43.1500      36.2736      180      "Capacitor, MLCC, 1uF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                     
C35          Capacitor                     TopLayer    C0603                                           94.7010      16.4001      270      "Capacitor, MLCC, 470nF, 16V, X7R, 10%, 0603, T=0.8mm"                                                   
C49          Capacitor                     TopLayer    C0603                                           105.8300     6.4487       180      "Capacitor, MLCC, 100nF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                   
C27          Capacitor                     TopLayer    C0603                                           85.9290      21.9240      270      "Capacitor, MLCC, 470nF, 16V, X7R, 10%, 0603, T=0.8mm"                                                   
C33          Capacitor                     TopLayer    C0603                                           93.7086      25.7181      270      "Capacitor, MLCC, 100nF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                   
C47          Capacitor                     TopLayer    C0603                                           100.9817     20.8041      360      "Capacitor, MLCC, 1uF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                     
C20          Capacitor                     TopLayer    C0603                                           84.0300      70.5900      360      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0603, T=0,8mm"                                                   
C26          Capacitor                     TopLayer    C0603                                           97.6779      67.8950      270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0603, T=0,8mm"                                                   
C32          Capacitor                     TopLayer    C0603                                           91.7942      67.3063      180      "Capacitor, MLCC, 1uF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                     
C43          Capacitor                     TopLayer    C0603                                           93.6641      49.9773      270      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0603, T=0,8mm"                                                   
C44          Capacitor                     TopLayer    C0603                                           94.9849      49.9773      270      "Capacitor, MLCC, 1uF, 16V, X5R, 10%, 0603, T=0,8mm"                                                     
C34          Capacitor                     TopLayer    C0603                                           94.0197      51.7457      360      "Capacitor, MLCC, 10nF, 50V, X7R, 10%, 0603, T=0.8mm"                                                    
C40          Capacitor                     TopLayer    C0603                                           101.3261     50.7634      180      "Capacitor, MLCC, 1uF, 16V, X5R, 10%, 0603, T=0,8mm"                                                     
C30          Capacitor                     TopLayer    C0603                                           90.1843      49.2011      360      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0603, T=0,8mm"                                                   
C37          Capacitor                     TopLayer    C0603                                           92.7684      47.0416      90       "Capacitor, MLCC, 10pF, 50V, NPO, 5%, 0603, T=0,8mm"                                                     
C36          Capacitor                     TopLayer    C0603                                           92.7626      44.6906      90       "Capacitor, MLCC, 10pF, 50V, NPO, 5%, 0603, T=0,8mm"                                                     
C31          Capacitor                     TopLayer    C0603                                           90.1843      50.5898      180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0603, T=0,8mm"                                                   
C23          Capacitor                     TopLayer    C0603                                           79.9244      54.5368      180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0603, T=0,8mm"                                                   
C19          Capacitor                     TopLayer    C0603                                           76.5146      44.7932      360      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0603, T=0,8mm"                                                   
C28          Capacitor                     TopLayer    C0603                                           86.2670      40.9296      90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0603, T=0,8mm"                                                   
C11          Capacitor                     TopLayer    C0603                                           53.9176      12.9981      270      "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                                                   
C13          Capacitor                     TopLayer    C0603                                           55.2917      12.9981      90       "Capacitor, MLCC, 100nF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                   
C17          Capacitor                     TopLayer    C0603                                           72.0399      22.8911      180      "Capacitor, MLCC, 2.2uF, 10V, X5R, 10%, 0603, T=0,8mm"                                                   
C16          Capacitor                     TopLayer    C0603                                           72.0287      21.6312      360      "Capacitor, MLCC, 100nF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                   
C74          Capacitor                     BottomLayer C0603                                           21.2258      29.3280      180      "Capacitor, MLCC, 1uF, 16V, X5R, 10%, 0603, T=0,8mm"                                                     
C63          Capacitor                     BottomLayer C0603                                           24.2048      28.8200      360      "Capacitor, MLCC, 1uF, 16V, X5R, 10%, 0603, T=0,8mm"                                                     
C12          Capacitor                     TopLayer    C0402                                           55.3872      26.4089      180      "Capacitor, MLCC, 220nF, 16V, 0402, X7R, 10%, T=0,5mm"                                                   
C83          Capacitor                     BottomLayer C0603                                           18.8098      29.3280      360      "Capacitor, MLCC, 1uF, 16V, X5R, 10%, 0603, T=0,8mm"                                                     
C85          Capacitor                     BottomLayer C0603                                           16.4395      29.3280      180      "Capacitor, MLCC, 1uF, 16V, X5R, 10%, 0603, T=0,8mm"                                                     
C9           Capacitor                     TopLayer    C0603                                           52.0082      24.3308      270      "Capacitor, MLCC, 10uF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                    
C10          Capacitor                     TopLayer    C0603                                           53.3132      24.2998      270      "Capacitor, MLCC, 100nF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                   
C8           Capacitor                     TopLayer    C0603                                           50.6866      22.0940      360      "Capacitor, MLCC, 100nF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                   
C39          Capacitor                     TopLayer    C0805                                           96.8641      39.6130      180      "Capacitor, MLCC, 10uF, 25V, X5R, 10%, 0805, T=0,85mm"                                                   
C42          Capacitor                     TopLayer    C0603                                           96.9327      41.1624      360      "Capacitor, MLCC, 100nF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                   
C90          Capacitor                     BottomLayer C0603                                           6.8224       42.1238      90       "Capacitor, MLCC, 100nF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                   
C84          Cap_POL_TANA                  BottomLayer CPOL_TAJ-A_1206_H180                            13.7415      41.7529      270      "Capacitor, Tantalum, 4.7uF, 16V, 10%, 4ohms, pkg Type_A (3216 metric), T=1.6mm"                         
C70          Capacitor                     BottomLayer C0805                                           23.1667      45.4510      270      "Capacitor, MLCC, 10uF, 25V, X5R, 10%, 0805, T=0,85mm"                                                   
C75          Capacitor                     BottomLayer C0603                                           21.6494      45.1508      90       "Capacitor, MLCC, 100nF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                   
C25          Capacitor                     TopLayer    C0603                                           88.6300      6.7600       180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0603, T=0,8mm"                                                   
C15          Capacitor                     TopLayer    C0603                                           68.2500      30.6755      270      "Capacitor, MLCC, 100nF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                   
C68          Capacitor                     BottomLayer C0603                                           23.2220      17.6156      360      "Capacitor, MLCC, 100nF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                   
C87          Capacitor                     BottomLayer C0603                                           11.3744      16.9806      360      "Capacitor, MLCC, 100nF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                   
C69          Capacitor                     BottomLayer C0603                                           22.9300      36.4742      360      "Capacitor, MLCC, 100nF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                   
C88          Capacitor                     BottomLayer C0603                                           11.3730      36.0424      360      "Capacitor, MLCC, 100nF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                   
C64          Capacitor                     BottomLayer C0603                                           24.1540      30.0646      360      "Capacitor, MLCC, 100nF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                   
C89          Capacitor                     BottomLayer C0603                                           11.3222      28.7272      360      "Capacitor, MLCC, 100nF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                   
C6           Capacitor                     TopLayer    C0402                                           33.0209      9.7398       90       "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                                                   
C21          Capacitor                     TopLayer    C0603                                           78.5847      38.4235      90       "Capacitor, MLCC, 100nF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                   
C22          Capacitor                     TopLayer    C0603                                           78.5847      40.7137      90       "Capacitor, MLCC, 100nF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                   
C1           Capacitor                     TopLayer    C0402                                           21.5378      9.2202       180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0,5mm"                                                   
B2           SW-PUSH-CMS                   TopLayer    SWI_WEALTHMETAL_TD-0341_4P_BLUE                 14.0000      5.2500       270      "Non-Open Push-Button 0.1A 24V"                                                                          
X1           XTAL_2_PINS                   TopLayer    CRY_NX3225GD_2P                                 90.5549      46.4319      90       "Crystal 8MHz, 8pF, +-20ppm, 500ohms max,  SMD"                                                          
U23          M24128-DFMN6TP                BottomLayer ICC_SO8_5X4_P127                                30.0294      33.4008      270      "I2C memory"                                                                                             
U14          SN74LVC2T45DCUT               TopLayer    ICC_VSSOP8_DCU_R-PDSO-G8_2X2P30_P050            83.7006      55.2958      270      "Dual bit dual supply bus transceiver"                                                                   
U18          CY7C65215-32LTXI              TopLayer    ICC_QFN32-EPAD_5X5_P050                         96.2968      21.4788      270      "USB-Serial Dual Channel (UART/I2C/SPI) Bridge"                                                          
U17          TS5A2066YZPR                  TopLayer    ICC_DSBGA8_YZP_0P88X1P88_H0P50_P050             92.7492      16.3995      360      "Dual-Channel 10-Ω SPST Analog Switch"                                                                   
U15          74LVC541ABQ                   TopLayer    ICC_DHVQFN20-EPAD_SOT764-1_2P5X4P5_H0P85_P050   89.5060      22.6581      90       "Octal buffer/line driver with 5 V tolerant inputs/outputs; 3-state"                                     
U13          USBLC6-2SC6                   TopLayer    ESD_SOT23-6L                                    85.7884      66.8744      360      "Very low capacitance ESD protection"                                                                    
U16          STMPS2141STR                  TopLayer    MOS_SOT23-5L                                    94.8873      68.1759      90       "Enhanced single channel power switches with active low enable pin"                                      
U20          LD3985M33R                    TopLayer    REG_SOT23-5L                                    97.7027      50.2171      90       "Ultra low drop-low noise BiCMOS voltage, regulators low ESR capacitors compatible"                      
U12          STM32F103CBT6                 TopLayer    ICC_LQFP48_7X7_P050                             82.7690      48.0876      90       "Medium-density performance line ARM-based 32-bit MCU with 128KB Flash"                                  
U6           LPS22HH                       TopLayer    ICC_HLGA10_2X2_P050                             54.9805      16.1766      180      "High-performance MEMS nano pressure sensor:260-1260 hPa absolute digital output barometer"              
U10          HTS221                        TopLayer    ICC_HLGA6_2X2_P075-1                            72.1961      19.7366      270      "Capacitive digital sensor for relative humidity and temperature"                                        
U7           LSM303AGR                     TopLayer    ICC_LGA12_2X2_P050                              55.6090      24.3464      180      "3D accelerometer and 3D magnetometer"                                                                   
U19          ST1L05BPUR                    TopLayer    ICC_DFN6-EPAD_3X3_P095                          96.2726      43.5288      270      "LDO Linear Voltage Regulator IC Positive Adjustable 1 Output Adjustable 1.3A 6-DFN (3x3)"               
U30          ST1L05BPUR                    BottomLayer ICC_DFN6-EPAD_3X3_P095                          10.8661      41.6434      180      "LDO Linear Voltage Regulator IC Positive Adjustable 1 Output Adjustable 1.3A 6-DFN (3x3)"               
U25          ST1L05BPUR                    BottomLayer ICC_DFN6-EPAD_3X3_P095                          25.8090      45.5227      180      "LDO Linear Voltage Regulator IC Positive Adjustable 1 Output Adjustable 1.3A 6-DFN (3x3)"               
U9           USBLC6-2SC6                   TopLayer    ESD_SOT23-6L                                    81.9336      9.9250       270      "Very low capacitance ESD protection"                                                                    
U8           MT25QU512ABB1EW9-0SIT         TopLayer    ICC_W-PDFN-8_8X6_P127                           64.2860      33.6136      270      "512Mb, 1.8V Multiple I/O Serial Flash Memory"                                                           
U27          TXS0108EPWR                   BottomLayer ICC_TSSOP20_6P50X4P40_P065                      17.5532      15.0786      270      "8bits_bidirectionnal level shifter, Delay 312ns/1V8"                                                    
U29          TXS0108EPWR                   BottomLayer ICC_TSSOP20_6P50X4P40_P065                      17.3214      33.7730      270      "8bits_bidirectionnal level shifter, Delay 312ns/1V8"                                                    
U11          SN74LVC2T45DCUT               TopLayer    ICC_VSSOP8_DCU_R-PDSO-G8_2X2P30_P050            76.4488      39.4508      180      "Dual bit dual supply bus transceiver"                                                                   
U2           ESD-TRANSIL                   TopLayer    ESD_QFN2_1P6X1_P125                             21.0967      6.9208       270      "High power transient voltage suppressor, 7V breakdown"                                                  
T2           STS5PF30L                     BottomLayer ICC_SO8_5X4_P127                                47.0695      38.0401      360      "Power MOSFET - P-channel 30V - 0.045 OHM - 5A SO-8 - STripFET"                                          
SB43         SB_ON                         BottomLayer SOLDER-BRIDGE_R0603-0R                          49.8056      29.5046      270      "Solder Bridge ON"                                                                                       
R8           Resistor                      TopLayer    R0402                                           33.6319      58.3576      360      Resistor,15K,0402,5%,1/16W                                                                               
R6           Resistor                      TopLayer    R0402                                           30.6592      55.1176      180      Resistor,18R,0402,5%,1/16W                                                                               
R7           Resistor                      TopLayer    R0402                                           30.6592      54.0731      180      Resistor,18R,0402,5%,1/16W                                                                               
R92          Resistor                      BottomLayer R0603                                           28.4418      28.8938      270      Resistor,620K,0603,1%,1/10W                                                                              
Q3           BSN20                         TopLayer    MOS_SOT23                                       90.6662      35.8332      270      "MOSFET, N-Channel , Vds: 20V, Id: 2A, Vgs(th): 1.5V, Vgs(max): +/-8V, Rdson:120mohm@Vgs=1.8V, Qg=6.3nC" 
Q2           MOSFET_FDN304P                TopLayer    MOS_SOT23                                       90.5060      39.7296      270      "MOSFET, P-Channel , Vds: -20V, Id: -2.4A, Vgs(th): -1.5V, Vgs(max): +/-8V, Rdson:100mohm@Vgs=-1.8V"     
Q5           9013-SOT23                    BottomLayer NPN_SOT23                                       48.5887      43.5519      90       "NPN Bipolar Transistor"                                                                                 
P1           "Socket 10X2 STMod+"          TopLayer    CON_SAMTEC_SQT-110-01-F-D-RA__STMOD+            7.1500       29.2456      270      "Socket 10x2, 2.00mm, RA, TH, Height 6.35mm/2.29mm"                                                      
LD6          LD_BICOLOR_CMS                TopLayer    LED_BI-GR_HSMF-A201-A00J1                       85.2080      35.9196      180      "LED Bicolor"                                                                                            
LD7          LED_red                       TopLayer    LED_0603_RED                                    94.6542      74.3678      360      "LED, Red, 0603"                                                                                         
LD4          LED_green                     TopLayer    LED_0603_GREEN_H0P8                             43.7732      64.6085      180      "LED, Green, 0603"                                                                                       
LD3          LED_blue                      TopLayer    LED_0603_OSRAM_LB-Q39G-L2OO-35-1_BLUE_1A2K_H0P4 30.8590      39.7250      180      "LED Blue, 0603 SMD, Forward Voltage Min=2,8V, Max=3,8V"                                                 
LD2          LED_red                       TopLayer    LED_0603_RED_H0P4                               24.6090      39.7250      180      "LED, Red, 0603"                                                                                         
LD1          LED_green                     TopLayer    LED_0603_GREEN_H0P8                             18.3590      39.7250      360      "LED, Green, 0603"                                                                                       
JP2          "Jumper_Header 2x1 Fitted"    TopLayer    CON_SAMTEC_TSW-102-07-G-S                       60.4641      43.9590      270      "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm - Shunt Fitted by default"                            
JP3          "Jumper_Header 2x1"           TopLayer    CON_SAMTEC_TSW-102-07-G-S                       64.0042      54.7484      90       "Header, 2x1, 2,54mm, VR, TH, Height 5.84mm/2.54mm"                                                      
D10          BAT60JFILM                    TopLayer    DIO_SOD323                                      96.6343      53.2767      360      BAT60JFILM                                                                                               
CN4          "Header 4x1"                  TopLayer    CON_988-JIUBABA_PHFS25-11-04-G0B115-T-1         52.2139      56.3085      360      "Header, 4x1, 2.54mm, VR, TH, Height 6mm/3mm"                                                            
C46          Capacitor                     TopLayer    C0603                                           100.9293     23.9769      360      "Capacitor, MLCC, 4.7uF, 16V, X5R, 10%, 0603, T=0.8mm"                                                   
C5           Capacitor                     TopLayer    C0402                                           29.2553      54.6440      90       "Capacitor, MLCC, 33pF, 50V, NPO, 5%, 0402, T=0,5mm"                                                     
C4           Capacitor                     TopLayer    C0402                                           29.2553      56.4206      270      "Capacitor, MLCC, 33pF, 50V, NPO, 5%, 0402, T=0,5mm"                                                     
C2           Capacitor                     TopLayer    C0402                                           23.2812      58.1507      180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0402, T=0.5mm"                                                   
C55          Cap_POL_TANA                  BottomLayer CPOL_TAJ-A_1206_H180                            31.3120      28.7526      360      "Capacitor, Tantalum, 4.7uF, 16V, 10%, 4ohms, pkg Type_A (3216 metric), T=1.6mm"                         
C52          Cap_POL_TANA                  BottomLayer CPOL_TAJ-A_1206_H180                            35.6046      28.7845      360      "Capacitor, Tantalum, 4.7uF, 16V, 10%, 4ohms, pkg Type_A (3216 metric), T=1.6mm"                         
C38          Cap_POL_TANA                  TopLayer    CPOL_TAJ-A_1206_H180                            96.4750      46.3911      180      "Capacitor, Tantalum, 4.7uF, 16V, 10%, 4ohms, pkg Type_A (3216 metric), T=1.6mm"                         
C86          Capacitor                     BottomLayer C0805                                           8.3511       42.0468      270      "Capacitor, MLCC, 10uF, 25V, X5R, 10%, 0805, T=0,85mm"                                                   
C58          Cap_POL_TANA                  BottomLayer CPOL_TAJ-A_1206_H180                            28.8122      45.5134      270      "Capacitor, Tantalum, 4.7uF, 16V, 10%, 4ohms, pkg Type_A (3216 metric), T=1.6mm"                         
B5           SW-PUSH-CMS_EVQP2_BLACK       TopLayer    SWI_PANASONIC_EVQP2F02K                         94.6800      3.9000       90       "EVQP2 - 4.7mm x 3.5 mm SMD Light Touch Switch"                                                          
B1           SW-PUSH-CMS                   TopLayer    SWI_WEALTHMETAL_TD-0341_4P_BLACK                28.5000      5.2500       270      "Non-Open Push-Button 0.1A 24V BLACK"                                                                    
U1           OLED_RITDISPLAY_9OL9935701000 TopLayer    OLED_RITDISPLAY_9OL9935701000-MB1378B-01        24.6000      22.7486      360      "128*64 20-pin OLED display driver SSD1306BZ Parallel or SPI interface"                                  
R15          Resistor                      TopLayer    R0603                                           46.4290      64.6085      360      Resistor,510R,0603,1%,1/10W                                                                              
CN11         USB_uB_105164-0001            TopLayer    CON_USBMICROB_MOLEX_105164-0001_H2P45           103.1300     73.8450      270      "Micro-USB B Receptacle without Flange, Top Mount, Surface Mount, Lead-Free"                             
CN9          USB_uB_105164-0001            TopLayer    CON_USBMICROB_MOLEX_105164-0001_H2P45           86.1300      73.8450      270      "Micro-USB B Receptacle without Flange, Top Mount, Surface Mount, Lead-Free"                             
CN8          USB_uB_105164-0001            TopLayer    CON_USBMICROB_MOLEX_105164-0001_H2P45           86.1300      3.1550       90       "Micro-USB B Receptacle without Flange, Top Mount, Surface Mount, Lead-Free"                             
SB49         SB_ON                         BottomLayer SOLDER-BRIDGE_R0603-0R                          24.8486      31.4362      180      "Solder Bridge ON"                                                                                       
CN6          U.FL-R-SMT-1                  TopLayer    CON_HRS_U.FL-R-SMT-1                            65.6230      9.8312       270      "U.FL RF connector"                                                                                      
U21          ESD-TRANSIL                   TopLayer    ESD_QFN2_1P6X1_P125                             101.1183     69.8158      180      "High power transient voltage suppressor, 7V breakdown"                                                  
B4           SW-PUSH-CMS_EVQP2_BLACK       TopLayer    SWI_PANASONIC_EVQP2F02K                         58.5000      73.2500      360      "EVQP2 - 4.7mm x 3.5 mm SMD Light Touch Switch"                                                          
CN10         USB_uB_105164-0001            TopLayer    CON_USBMICROB_MOLEX_105164-0001_H2P45           103.1300     3.1550       90       "Micro-USB B Receptacle without Flange, Top Mount, Surface Mount, Lead-Free"                             
U4           ESD-TRANSIL                   TopLayer    ESD_QFN2_1P6X1_P125                             34.2784      9.5946       270      "High power transient voltage suppressor, 7V breakdown"                                                  
SB44         SB_ON                         BottomLayer SOLDER-BRIDGE_R0603-0R                          48.0916      29.5342      90       "Solder Bridge ON"                                                                                       
U28          TXS0108EPWR                   BottomLayer ICC_TSSOP20_6P50X4P40_P065                      17.3314      24.8322      270      "8bits_bidirectionnal level shifter, Delay 312ns/1V8"                                                    
L1           BEAD                          BottomLayer L0603                                           54.4571      38.2508      180      "SMD Chip ferrite bead, 600R@100MHz +/-25%, 350mA, 500mohm DC, 0603, T=0.8mm"                            
U22          USBLC6-2SC6                   TopLayer    ESD_SOT23-6L                                    103.4550     9.2649       180      "Very low capacitance ESD protection"                                                                    
R117         Resistor                      BottomLayer R0603                                           11.5064      44.1834      180      Resistor,10K2,0603,1%,1/10W                                                                              
Designator15 Comment                       TopLayer    MARK                                            1.4136       11.5958      0        ""                                                                                                       
R122         Resistor                      TopLayer    R0603                                           49.9454      73.6753      90       Resistor,10K,0603,1%,1/10W                                                                               
BT1          "BATTERY HOLDER 3 x AAA"      BottomLayer BAT_KEYSTONE_PC-MOUNT-2479_HOLDER_AAA_X3        89.1000      62.2186      90       "3xAAA ECONOMICAL PLASTIC BATTERY HOLDER"                                                                
CN14         PJ-31060                      BottomLayer CON_PHONE-JACK-3P5_TAIYI_PJ31060                3.5292       69.4688      270      "Connector Jack socket Stereo 3.5mm, SMT"                                                                
Designator14 Comment                       TopLayer    MARK                                            70.6052      61.0552      0        ""                                                                                                       
Designator57 Comment                       TopLayer    Label                                           -1805.9160   -1413.9764   270      ""                                                                                                       
C48          Capacitor                     TopLayer    C0603                                           100.9833     22.1382      180      "Capacitor, MLCC, 100nF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                   
C3           Capacitor                     TopLayer    C0402                                           25.7179      54.8619      360      "Capacitor, MLCC, 33pF, 50V, NPO, 5%, 0402, T=0,5mm"                                                     
R4           Resistor                      TopLayer    R0402                                           25.7074      53.9758      180      Resistor,15K,0402,5%,1/16W                                                                               
R12          Resistor                      TopLayer    R0603                                           34.2782      11.8292      270      Resistor,22R,0603,1%,1/10W                                                                               
D6           BAT60JFILM                    TopLayer    DIO_SOD323                                      92.5208      53.2767      180      BAT60JFILM                                                                                               
Q1           MOSFET_FDN304P                TopLayer    MOS_SOT23                                       91.2078      13.1615      360      "MOSFET, P-Channel , Vds: -20V, Id: -2.4A, Vgs(th): -1.5V, Vgs(max): +/-8V, Rdson:100mohm@Vgs=-1.8V"     
Designator7  Comment                       TopLayer    预留天线                                            123.8000     49.2500      0        ""                                                                                                       
R119         Resistor                      BottomLayer R0603                                           9.2655       44.1990      180      Resistor,20K5,0603,1%,1/10W                                                                              
C66          Capacitor                     BottomLayer C0603                                           13.4126      47.7088      360      "Capacitor, MLCC, 100nF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                   
R97          Resistor                      BottomLayer R0603                                           15.2599      48.5988      90       Resistor,10K,0603,1%,1/10W                                                                               
C81          Capacitor                     BottomLayer C0603                                           9.4337       56.5300      360      "Capacitor, MLCC, 1uF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                     
SB52         SB_OFF                        BottomLayer SOLDER-BRIDGE_R0603-0R                          11.6130      62.2122      180      "Solder Bridge OFF"                                                                                      
SB50         SB_ON                         BottomLayer SOLDER-BRIDGE_R0603-0R                          14.4436      62.2122      180      "Solder Bridge ON"                                                                                       
L2           BEAD                          BottomLayer L0603_H0P8                                      13.8840      45.6914      270      "Ferrite bead, 1000R @ 100MHz,  600mA, 350mOhm, 0603"                                                    
U26          ESDA6V1BC6                    BottomLayer ESD_SOT23-6L                                    6.0354       60.8932      270      "Quad Bidir ESD protection"                                                                              
U24          MAX9867ETJ+                   BottomLayer ICC_TQFN32-EPAD_5X5_H0P75_P050                  14.9132      54.6501      180      "Ultra-Low Power Stereo Audio Codec"                                                                     
C73          Capacitor                     BottomLayer C0603                                           16.6946      45.6110      90       "Capacitor, MLCC, 1uF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                     
C72          Capacitor                     BottomLayer C0603                                           18.0168      45.6260      270      "Capacitor, MLCC, 100nF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                   
C57          Capacitor                     BottomLayer C0603                                           18.6090      57.0316      90       "Capacitor, MLCC, 1uF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                     
C60          Capacitor                     BottomLayer C0603                                           17.5308      59.8534      90       "Capacitor, MLCC, 1uF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                     
C76          Capacitor                     BottomLayer C0603                                           9.6257       58.1048      180      "Capacitor, MLCC, 1uF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                     
C77          Capacitor                     BottomLayer C0603                                           10.0163      48.0296      90       "Capacitor, MLCC, 1uF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                     
C71          Capacitor                     BottomLayer C0603                                           11.3305      48.0296      90       "Capacitor, MLCC, 2.2uF, 10V, X5R, 10%, 0603, T=0,8mm"                                                   
C82          Capacitor                     BottomLayer C0603                                           8.7337       48.0296      90       "Capacitor, MLCC, 1uF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                     
C80          Capacitor                     BottomLayer C0603                                           9.4663       51.1906      360      "Capacitor, MLCC, 1uF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                     
R110         Resistor                      BottomLayer R0603                                           11.5271      60.0098      90       Resistor,0R,0603,5%,1/10W                                                                                
R91          Resistor                      BottomLayer R0603                                           17.4800      49.5268      180      Resistor,0R,0603,5%,1/10W                                                                                
R93          Resistor                      BottomLayer R0603                                           17.4800      48.2314      180      Resistor,0R,0603,5%,1/10W                                                                                
R114         Resistor                      BottomLayer R0603                                           6.9610       56.9300      180      Resistor,2K15,0603,1%,1/10W                                                                              
R111         Resistor                      BottomLayer R0603                                           9.6105       59.4396      360      Resistor,0R,0603,5%,1/10W                                                                                
SB48         SB_ON                         BottomLayer SOLDER-BRIDGE_R0603-0R                          23.4299      56.6140      180      "Solder Bridge ON"                                                                                       
SB47         SB_ON                         BottomLayer SOLDER-BRIDGE_R0603-0R                          23.5548      54.7362      360      "Solder Bridge ON"                                                                                       
C59          Capacitor                     BottomLayer C0603                                           17.4800      50.7999      180      "Capacitor, MLCC, 1uF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                     
C65          Capacitor                     BottomLayer C0603                                           13.4014      48.9788      180      "Capacitor, MLCC, 1uF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                     
R102         Resistor                      BottomLayer R0603                                           16.0322      59.9804      90       Resistor,0R,0603,5%,1/10W                                                                                
U3           ESDA6V8V6-6/TR                TopLayer    ESD_SOT563-6L_P050                              27.1234      56.1938      270      "ESD protection"                                                                                         
R5           Resistor                      TopLayer    R0402                                           30.6592      56.1051      180      Resistor,18R,0402,5%,1/16W                                                                               
Designator58 Comment                       TopLayer    Label                                           -1805.9160   -1413.9764   270      ""                                                                                                       
U5           NBIoT_Mod_Type1SE             TopLayer    MOD_BOARD_MURATA_TYPE-1SE_ES3                   47.8129      43.2936      0        "NBIoT Module"                                                                                           
CN5          "Header 6x1"                  TopLayer    CON_988-JIUBABA_PHFS25-11-06-G0B115-T-1         60.4641      55.0384      270      "Header, 6x1, 2.54mm, VR, TH, Height 6mm/3mm"                                                            
R62          Resistor                      TopLayer    R0603                                           89.5388      52.9253      90       Resistor,4K7,0603,1%,1/10W                                                                               
C41          Capacitor                     TopLayer    C0603                                           101.3349     49.1634      180      "Capacitor, MLCC, 100nF, 16V, X7R, 10%, 0603, T=0,8mm"                                                   
C45          Capacitor                     TopLayer    C0603                                           100.5902     18.6177      360      "Capacitor, MLCC, 1uF, 6V3, X5R, 10%, 0603, T=0,8mm"                                                     
CN1          SLC-100180065                 TopLayer    CON_ROHO_SMA_RFSMARA-7053                       123.0000     5.0000       180      "RF Coxial Cable to uFL"                                                                                 
