customize

# Variant Report

Date: |  | 27/02/2023
Time: |  | 14:18:54
Elapsed Time: |  | 00:00:01

## Variations

Physical | Document | Parameter Name | Original Value | U5G9ZJQ_No_Display
--- | --- | --- | --- | ---
B1 | MCU_System.SchDoc |  | Fitted | Fitted
|  | Comment | SW-PB | SW-PB
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | France | France
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Misc/C&K_switch_button_KSS221GLFS/C&K_SWITCH_KSS221GLFS.pdf | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Misc/C&K_switch_button_KSS221GLFS/C&K_SWITCH_KSS221GLFS.pdf
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Subminiature Side Actuated Tact Switch for SMT - KSS series - 2.0 Newtons - Gull wing, SPST | Subminiature Side Actuated Tact Switch for SMT - KSS series - 2.0 Newtons - Gull wing, SPST
|  | Footprint | SWI_C&K_ITT_KSS221G__JIUBABA_TD-26EA__DI | SWI_C&K_ITT_KSS221G__JIUBABA_TD-26EA__DI
|  | Ibis Model |  |
|  | ID | 3435 | 3435
|  | Internal_Part_Number | MCD-01335 | MCD-01335
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01335 | MCD-01335
|  | Manufacturer | C&K | C&K
|  | Manufacturer_Part_Number | KSS221GLFS | KSS221GLFS
|  | Order_Code_Digikey | NA | NA
|  | Order_Code_Farnell | NA | NA
|  | Order_Code_RS | NA | NA
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Misc | Misc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Checked | Checked
|  | Value | KSS221GLFS | KSS221GLFS
B2 | User_Interface.SchDoc |  | Fitted | Fitted
|  | Comment | SW_BLUE_KSC721JLFS | SW_BLUE_KSC721JLFS
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | France | France
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Misc/C&K_tactile_switch_KSC_series | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Misc/C&K_tactile_switch_KSC_series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Switch HW BLUE High4.3mm 2.25 Newtons, BEND type | Switch HW BLUE High4.3mm 2.25 Newtons, BEND type
|  | Footprint | SWI_C&K_KSC721JLFS_BLUE | SWI_C&K_KSC721JLFS_BLUE
|  | Ibis Model |  |
|  | ID | 3900 | 3900
|  | Internal_Part_Number | MCD-01800 | MCD-01800
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01800 | MCD-01800
|  | Manufacturer | C&K | C&K
|  | Manufacturer_Part_Number | KSC721JLFS | KSC721JLFS
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Misc | Misc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | KSC721JLFS | KSC721JLFS
C1 | MCU_System.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C2 | MCU_System.SchDoc |  | Fitted | Fitted
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_NP0_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_NP0_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 3.3pF, 50V, NPO, +/-0.1pF, 0402, T=0.5mm | Capacitor, MLCC, 3.3pF, 50V, NPO, +/-0.1pF, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 3875 | 3875
|  | Internal_Part_Number | MCD-01775 | MCD-01775
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01775 | MCD-01775
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402BRNPO9BN3R3 | CC0402BRNPO9BN3R3
|  | Order_Code_Digikey | 311-1621-1-ND | 311-1621-1-ND
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 3.3pF | 3.3pF
C3 | MCU_System.SchDoc |  | Fitted | Fitted
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_NP0_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_NP0_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 3.3pF, 50V, NPO, +/-0.1pF, 0402, T=0.5mm | Capacitor, MLCC, 3.3pF, 50V, NPO, +/-0.1pF, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 3875 | 3875
|  | Internal_Part_Number | MCD-01775 | MCD-01775
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01775 | MCD-01775
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402BRNPO9BN3R3 | CC0402BRNPO9BN3R3
|  | Order_Code_Digikey | 311-1621-1-ND | 311-1621-1-ND
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 3.3pF | 3.3pF
C4 | MCU_System.SchDoc |  | Fitted | Fitted
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_NP0_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_NP0_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 8.2pF, 50V, NPO, +/-0.25pF, 0402, T=0.5mm | Capacitor, MLCC, 8.2pF, 50V, NPO, +/-0.25pF, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 4032 | 4032
|  | Internal_Part_Number | MCD-01932 | MCD-01932
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01932 | MCD-01932
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402CRNPO9BN8R2 | CC0402CRNPO9BN8R2
|  | Order_Code_Digikey | 311-1635-1-ND | 311-1635-1-ND
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 8.2pF | 8.2pF
C5 | MCU_System.SchDoc |  | Fitted | Fitted
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_NP0_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_NP0_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 8.2pF, 50V, NPO, +/-0.25pF, 0402, T=0.5mm | Capacitor, MLCC, 8.2pF, 50V, NPO, +/-0.25pF, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 4032 | 4032
|  | Internal_Part_Number | MCD-01932 | MCD-01932
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01932 | MCD-01932
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402CRNPO9BN8R2 | CC0402CRNPO9BN8R2
|  | Order_Code_Digikey | 311-1635-1-ND | 311-1635-1-ND
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 8.2pF | 8.2pF
C6 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 4.7uF, 6.3V, X5R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 4.7uF, 6.3V, X5R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 4714 | 4714
|  | Internal_Part_Number | MCD-02608 | MCD-02608
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-02608 | MCD-02608
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX5R5BB475 | CC0402KRX5R5BB475
|  | Order_Code_Digikey | 311-3476-2-ND | 311-3476-2-ND
|  | Order_Code_Farnell | 3366432 | 3366432
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Checked | Checked
|  | Value | 4.7uF | 4.7uF
C7 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C8 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C9 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 10uF, 6V3, X5R, +/-20%, 0402, T=0.5mm | Capacitor, MLCC, 10uF, 6V3, X5R, +/-20%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 3816 | 3816
|  | Internal_Part_Number | MCD-01716 | MCD-01716
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01716 | MCD-01716
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402MRX5R5BB106 | CC0402MRX5R5BB106
|  | Order_Code_Digikey | 311-1729-1-ND | 311-1729-1-ND
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 10uF | 10uF
C10 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C11 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C12 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C13 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C14 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C15 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C16 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C17 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C18 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C19 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C20 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C21 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C22 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | Japan | Japan
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/MURATA_GRM_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/MURATA_GRM_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 10uF, 10V, X5R, +/-10%, 0603, T=0.8mm | Capacitor, MLCC, 10uF, 10V, X5R, +/-10%, 0603, T=0.8mm
|  | Footprint | C0603 | C0603
|  | Ibis Model |  |
|  | ID | 2770 | 2770
|  | Internal_Part_Number | MCD-00099 | MCD-00099
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00099 | MCD-00099
|  | Manufacturer | MURATA | MURATA
|  | Manufacturer_Part_Number | GRM188R61A106KE69D | GRM188R61A106KE69D
|  | Order_Code_Digikey | 490-10474-1-ND | 490-10474-1-ND
|  | Order_Code_Farnell | 2494233 | 2494233
|  | Order_Code_RS | 170-6168 | 170-6168
|  | Package | 0603 | 0603
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 10uF | 10uF
C23 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C25 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 2.2uF, 6.3V, X5R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 2.2uF, 6.3V, X5R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 4712 | 4712
|  | Internal_Part_Number | MCD-02606 | MCD-02606
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-02606 | MCD-02606
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX5R5BB225 | CC0402KRX5R5BB225
|  | Order_Code_Digikey | 311-1682-2-ND | 311-1682-2-ND
|  | Order_Code_Farnell | 3366429 | 3366429
|  | Order_Code_RS | 1992205 | 1992205
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Checked | Checked
|  | Value | 2.2uF | 2.2uF
C26 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 2.2uF, 6.3V, X5R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 2.2uF, 6.3V, X5R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 4712 | 4712
|  | Internal_Part_Number | MCD-02606 | MCD-02606
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-02606 | MCD-02606
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX5R5BB225 | CC0402KRX5R5BB225
|  | Order_Code_Digikey | 311-1682-2-ND | 311-1682-2-ND
|  | Order_Code_Farnell | 3366429 | 3366429
|  | Order_Code_RS | 1992205 | 1992205
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Checked | Checked
|  | Value | 2.2uF | 2.2uF
C27 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C28 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C29 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C30 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 3822 | 3822
|  | Internal_Part_Number | MCD-01722 | MCD-01722
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01722 | MCD-01722
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX5R6BB105 | CC0402KRX5R6BB105
|  | Order_Code_Digikey | 311-1439-1-ND | 311-1439-1-ND
|  | Order_Code_Farnell | 1458896 | 1458896
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 1uF | 1uF
C31 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C32 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 3822 | 3822
|  | Internal_Part_Number | MCD-01722 | MCD-01722
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01722 | MCD-01722
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX5R6BB105 | CC0402KRX5R6BB105
|  | Order_Code_Digikey | 311-1439-1-ND | 311-1439-1-ND
|  | Order_Code_Farnell | 1458896 | 1458896
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 1uF | 1uF
C33 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C35 | Display.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C36 | Display.SchDoc |  | Fitted | Fitted
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 10uF, 25V, X5R, +/-10%, 0805, T=0.85mm | Capacitor, MLCC, 10uF, 25V, X5R, +/-10%, 0805, T=0.85mm
|  | Footprint | C0805 | C0805
|  | Full_Alternate_Internal_Part_Number | MCD-02385 | MCD-02385
|  | Ibis Model |  |
|  | ID | 2468 | 2468
|  | Internal_Part_Number | MCD-00014 | MCD-00014
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00014 | MCD-00014
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0805KRX5R8BB106 | CC0805KRX5R8BB106
|  | Order_Code_Digikey | 311-3503-1-ND | 311-3503-1-ND
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Package | 0805 | 0805
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03053 | MCD-03053
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 10uF | 10uF
C37 | Display.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C38 | USB_TYPE_C .SchDoc |  | Fitted | Fitted
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 1uF, 25V, X5R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 1uF, 25V, X5R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 4715 | 4715
|  | Internal_Part_Number | MCD-02609 | MCD-02609
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-02609 | MCD-02609
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX5R8BB105 | CC0402KRX5R8BB105
|  | Order_Code_Digikey | 311-1698-2-ND | 311-1698-2-ND
|  | Order_Code_Farnell | 3366440 | 3366440
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Checked | Checked
|  | Value | 1uF | 1uF
C39 | USB_TYPE_C .SchDoc |  | Fitted | Fitted
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_NP0_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_NP0_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 470pF, 50V, NPO, +/-5%, 0402, T=0.5mm | Capacitor, MLCC, 470pF, 50V, NPO, +/-5%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 3023 | 3023
|  | Internal_Part_Number | MCD-00724 | MCD-00724
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00724 | MCD-00724
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402JRNPO9BN471 | CC0402JRNPO9BN471
|  | Order_Code_Digikey | 311-1671-1-ND | 311-1671-1-ND
|  | Order_Code_Farnell | 3366416 | 3366416
|  | Order_Code_RS | 199-2186 | 199-2186
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 470pF | 470pF
C40 | USB_TYPE_C .SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C41 | Board_Power.SchDoc |  | Fitted | Fitted
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 4.7uF, 16V, X5R, +/-10%, 0603, T=0.8mm | Capacitor, MLCC, 4.7uF, 16V, X5R, +/-10%, 0603, T=0.8mm
|  | Footprint | C0603 | C0603
|  | Ibis Model |  |
|  | ID | 2471 | 2471
|  | Internal_Part_Number | MCD-00009 | MCD-00009
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00009 | MCD-00009
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0603KRX5R7BB475 | CC0603KRX5R7BB475
|  | Order_Code_Digikey | 311-1785-1-ND | 311-1785-1-ND
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Package | 0603 | 0603
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 4.7uF | 4.7uF
C42 | USB_TYPE_C .SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M, M | M, M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | Unknown | Unknown
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/WALSIN_Monolithic_Series/ | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/WALSIN_Monolithic_Series/
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 25V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 25V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 4461 | 4461
|  | Internal_Part_Number | MCD-02355 | MCD-02355
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-02355 | MCD-02355
|  | Manufacturer | WALSIN | WALSIN
|  | Manufacturer_Part_Number | 0402B104K250CT | 0402B104K250CT
|  | Order_Code_Digikey | 1292-1175-1-ND | 1292-1175-1-ND
|  | Order_Code_Farnell | 2496772 | 2496772
|  | Order_Code_RS | 176-3114 | 176-3114
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03302, MCD-03304 | MCD-03302, MCD-03304
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C43 | USB_TYPE_C .SchDoc |  | Fitted | Fitted
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_NP0_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_NP0_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100pF, 50V, NPO, +/-5%, 0402, T=0.5mm | Capacitor, MLCC, 100pF, 50V, NPO, +/-5%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2658 | 2658
|  | Internal_Part_Number | MCD-00205 | MCD-00205
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00205 | MCD-00205
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402JRNPO9BN101 | CC0402JRNPO9BN101
|  | Order_Code_Digikey | 311-1024-1-ND | 311-1024-1-ND
|  | Order_Code_Farnell | 3019226RL | 3019226RL
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100pF | 100pF
C45 | Board_Power.SchDoc |  | Fitted | Fitted
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 4.7uF, 16V, X5R, +/-10%, 0603, T=0.8mm | Capacitor, MLCC, 4.7uF, 16V, X5R, +/-10%, 0603, T=0.8mm
|  | Footprint | C0603 | C0603
|  | Ibis Model |  |
|  | ID | 2471 | 2471
|  | Internal_Part_Number | MCD-00009 | MCD-00009
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00009 | MCD-00009
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0603KRX5R7BB475 | CC0603KRX5R7BB475
|  | Order_Code_Digikey | 311-1785-1-ND | 311-1785-1-ND
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Package | 0603 | 0603
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 4.7uF | 4.7uF
C46 | Arduino.SchDoc |  | Fitted | Fitted
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 10uF, 25V, X5R, +/-10%, 0805, T=0.85mm | Capacitor, MLCC, 10uF, 25V, X5R, +/-10%, 0805, T=0.85mm
|  | Footprint | C0805 | C0805
|  | Full_Alternate_Internal_Part_Number | MCD-02385 | MCD-02385
|  | Ibis Model |  |
|  | ID | 2468 | 2468
|  | Internal_Part_Number | MCD-00014 | MCD-00014
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00014 | MCD-00014
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0805KRX5R8BB106 | CC0805KRX5R8BB106
|  | Order_Code_Digikey | 311-3503-1-ND | 311-3503-1-ND
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Package | 0805 | 0805
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03053 | MCD-03053
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 10uF | 10uF
C47 | Arduino.SchDoc |  | Fitted | Fitted
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 10uF, 25V, X5R, +/-10%, 0805, T=0.85mm | Capacitor, MLCC, 10uF, 25V, X5R, +/-10%, 0805, T=0.85mm
|  | Footprint | C0805 | C0805
|  | Full_Alternate_Internal_Part_Number | MCD-02385 | MCD-02385
|  | Ibis Model |  |
|  | ID | 2468 | 2468
|  | Internal_Part_Number | MCD-00014 | MCD-00014
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00014 | MCD-00014
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0805KRX5R8BB106 | CC0805KRX5R8BB106
|  | Order_Code_Digikey | 311-3503-1-ND | 311-3503-1-ND
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Package | 0805 | 0805
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03053 | MCD-03053
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 10uF | 10uF
C48 | Board_Power.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C49 | Flash_Memory.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C50 | Flash_Memory.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C51 | Flash_Memory.SchDoc |  | Fitted | Fitted
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 4.7uF, 16V, X5R, +/-10%, 0603, T=0.8mm | Capacitor, MLCC, 4.7uF, 16V, X5R, +/-10%, 0603, T=0.8mm
|  | Footprint | C0603 | C0603
|  | Ibis Model |  |
|  | ID | 2471 | 2471
|  | Internal_Part_Number | MCD-00009 | MCD-00009
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00009 | MCD-00009
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0603KRX5R7BB475 | CC0603KRX5R7BB475
|  | Order_Code_Digikey | 311-1785-1-ND | 311-1785-1-ND
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Package | 0603 | 0603
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 4.7uF | 4.7uF
C52 | Flash_Memory.SchDoc |  | Fitted | Fitted
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 4.7uF, 16V, X5R, +/-10%, 0603, T=0.8mm | Capacitor, MLCC, 4.7uF, 16V, X5R, +/-10%, 0603, T=0.8mm
|  | Footprint | C0603 | C0603
|  | Ibis Model |  |
|  | ID | 2471 | 2471
|  | Internal_Part_Number | MCD-00009 | MCD-00009
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00009 | MCD-00009
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0603KRX5R7BB475 | CC0603KRX5R7BB475
|  | Order_Code_Digikey | 311-1785-1-ND | 311-1785-1-ND
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Package | 0603 | 0603
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 4.7uF | 4.7uF
C53 | Flash_Memory.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C54 | Flash_Memory.SchDoc |  | Fitted | Fitted
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 4.7uF, 16V, X5R, +/-10%, 0603, T=0.8mm | Capacitor, MLCC, 4.7uF, 16V, X5R, +/-10%, 0603, T=0.8mm
|  | Footprint | C0603 | C0603
|  | Ibis Model |  |
|  | ID | 2471 | 2471
|  | Internal_Part_Number | MCD-00009 | MCD-00009
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00009 | MCD-00009
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0603KRX5R7BB475 | CC0603KRX5R7BB475
|  | Order_Code_Digikey | 311-1785-1-ND | 311-1785-1-ND
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Package | 0603 | 0603
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 4.7uF | 4.7uF
C58 | Arduino.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C59 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_NP0_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_NP0_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100pF, 50V, NPO, +/-5%, 0402, T=0.5mm | Capacitor, MLCC, 100pF, 50V, NPO, +/-5%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2658 | 2658
|  | Internal_Part_Number | MCD-00205 | MCD-00205
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00205 | MCD-00205
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402JRNPO9BN101 | CC0402JRNPO9BN101
|  | Order_Code_Digikey | 311-1024-1-ND | 311-1024-1-ND
|  | Order_Code_Farnell | 3019226RL | 3019226RL
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100pF | 100pF
C60 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_NP0_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_NP0_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 20pF, 50V, NPO, +/- 5%, 0402, T=0.5mm | Capacitor, MLCC, 20pF, 50V, NPO, +/- 5%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2479 | 2479
|  | Internal_Part_Number | MCD-00016 | MCD-00016
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00016 | MCD-00016
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402JRNPO9BN200 | CC0402JRNPO9BN200
|  | Order_Code_Digikey | 311-1417-1-ND | 311-1417-1-ND
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 20pF | 20pF
C61 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 10nF, 50V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 10nF, 50V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 4298 | 4298
|  | Internal_Part_Number | MCD-02198 | MCD-02198
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-02198 | MCD-02198
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R9BB103 | CC0402KRX7R9BB103
|  | Order_Code_Digikey | N/A | N/A
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | 6169644 | 6169644
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Checked | Checked
|  | Value | 10nF | 10nF
C62 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 10nF, 50V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 10nF, 50V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 4298 | 4298
|  | Internal_Part_Number | MCD-02198 | MCD-02198
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-02198 | MCD-02198
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R9BB103 | CC0402KRX7R9BB103
|  | Order_Code_Digikey | N/A | N/A
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | 6169644 | 6169644
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Checked | Checked
|  | Value | 10nF | 10nF
C63 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_NP0_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_NP0_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 2.7pF, 50V, NPO, +/-0.1pF, 0402, T=0.5mm | Capacitor, MLCC, 2.7pF, 50V, NPO, +/-0.1pF, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 3874 | 3874
|  | Internal_Part_Number | MCD-01774 | MCD-01774
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01774 | MCD-01774
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402BRNPO9BN2R7 | CC0402BRNPO9BN2R7
|  | Order_Code_Digikey | 311-1619-1-ND | 311-1619-1-ND
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 2.7pF | 2.7pF
C64 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_NP0_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_NP0_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 2.7pF, 50V, NPO, +/-0.1pF, 0402, T=0.5mm | Capacitor, MLCC, 2.7pF, 50V, NPO, +/-0.1pF, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 3874 | 3874
|  | Internal_Part_Number | MCD-01774 | MCD-01774
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01774 | MCD-01774
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402BRNPO9BN2R7 | CC0402BRNPO9BN2R7
|  | Order_Code_Digikey | 311-1619-1-ND | 311-1619-1-ND
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 2.7pF | 2.7pF
C65 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 2.2uF, 6.3V, X5R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 2.2uF, 6.3V, X5R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 4712 | 4712
|  | Internal_Part_Number | MCD-02606 | MCD-02606
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-02606 | MCD-02606
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX5R5BB225 | CC0402KRX5R5BB225
|  | Order_Code_Digikey | 311-1682-2-ND | 311-1682-2-ND
|  | Order_Code_Farnell | 3366429 | 3366429
|  | Order_Code_RS | 1992205 | 1992205
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Checked | Checked
|  | Value | 2.2uF | 2.2uF
C66 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C67 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | Japan | Japan
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/MURATA_GRM_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/MURATA_GRM_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 10uF, 10V, X5R, +/-10%, 0603, T=0.8mm | Capacitor, MLCC, 10uF, 10V, X5R, +/-10%, 0603, T=0.8mm
|  | Footprint | C0603 | C0603
|  | Ibis Model |  |
|  | ID | 2770 | 2770
|  | Internal_Part_Number | MCD-00099 | MCD-00099
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00099 | MCD-00099
|  | Manufacturer | MURATA | MURATA
|  | Manufacturer_Part_Number | GRM188R61A106KE69D | GRM188R61A106KE69D
|  | Order_Code_Digikey | 490-10474-1-ND | 490-10474-1-ND
|  | Order_Code_Farnell | 2494233 | 2494233
|  | Order_Code_RS | 170-6168 | 170-6168
|  | Package | 0603 | 0603
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 10uF | 10uF
C68 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M, M | M, M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | Unknown | Unknown
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/WALSIN_Monolithic_Series/ | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/WALSIN_Monolithic_Series/
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 25V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 25V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 4461 | 4461
|  | Internal_Part_Number | MCD-02355 | MCD-02355
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-02355 | MCD-02355
|  | Manufacturer | WALSIN | WALSIN
|  | Manufacturer_Part_Number | 0402B104K250CT | 0402B104K250CT
|  | Order_Code_Digikey | 1292-1175-1-ND | 1292-1175-1-ND
|  | Order_Code_Farnell | 2496772 | 2496772
|  | Order_Code_RS | 176-3114 | 176-3114
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03302, MCD-03304 | MCD-03302, MCD-03304
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C69 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 10nF, 50V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 10nF, 50V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 4298 | 4298
|  | Internal_Part_Number | MCD-02198 | MCD-02198
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-02198 | MCD-02198
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R9BB103 | CC0402KRX7R9BB103
|  | Order_Code_Digikey | N/A | N/A
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | 6169644 | 6169644
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Checked | Checked
|  | Value | 10nF | 10nF
C70 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C71 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C72 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C73 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C74 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C75 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C76 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C77 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C78 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C79 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C80 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C81 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C82 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C83 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C84 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C85 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C86 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 2474 | 2474
|  | Internal_Part_Number | MCD-00006 | MCD-00006
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00006 | MCD-00006
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX7R7BB104 | CC0402KRX7R7BB104
|  | Order_Code_Digikey | 311-1338-1-ND | 311-1338-1-ND
|  | Order_Code_Farnell | 9402047 | 9402047
|  | Order_Code_RS | 616-9701 | 616-9701
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | Partial_Alternate_Internal_Part_Number | MCD-03299 | MCD-03299
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100nF | 100nF
C87 | STLINK-V3EC.SchDoc |  | Fitted | Not Fitted
|  | Alternate_EMS | M, M |
|  | Comment | Capacitor |
|  | Component Kind | Standard |
|  | Component_Country_Of_Origin | Unknown |
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/WALSIN_Monolithic_Series/ |
|  | Database Table Name | MCD_PARTS$ |
|  | Description | Capacitor, MLCC, 100nF, 25V, X7R, +/-10%, 0402, T=0.5mm |
|  | Footprint | C0402 |
|  | Ibis Model |  |
|  | ID | 4461 |
|  | Internal_Part_Number | MCD-02355 |
|  | Library Name | MCD_PARTS_database.DbLib |
|  | Library Reference | MCD-02355 |
|  | Manufacturer | WALSIN |
|  | Manufacturer_Part_Number | 0402B104K250CT |
|  | Order_Code_Digikey | 1292-1175-1-ND |
|  | Order_Code_Farnell | 2496772 |
|  | Order_Code_RS | 176-3114 |
|  | Package | 0402 |
|  | Part_Preference | Recommended |
|  | Part_Type | Capacitor |
|  | Partial_Alternate_Internal_Part_Number | MCD-03302, MCD-03304 |
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES |
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released |
|  | Value | 100nF |
C88 | STLINK-V3EC.SchDoc |  | Fitted | Not Fitted
|  | Comment | Capacitor |
|  | Component Kind | Standard |
|  | Component_Country_Of_Origin | Japan |
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/MURATA_GRM_Series |
|  | Database Table Name | MCD_PARTS$ |
|  | Description | Capacitor, MLCC, 10uF, 10V, X5R, +/-10%, 0603, T=0.8mm |
|  | Footprint | C0603 |
|  | Ibis Model |  |
|  | ID | 2770 |
|  | Internal_Part_Number | MCD-00099 |
|  | Library Name | MCD_PARTS_database.DbLib |
|  | Library Reference | MCD-00099 |
|  | Manufacturer | MURATA |
|  | Manufacturer_Part_Number | GRM188R61A106KE69D |
|  | Order_Code_Digikey | 490-10474-1-ND |
|  | Order_Code_Farnell | 2494233 |
|  | Order_Code_RS | 170-6168 |
|  | Package | 0603 |
|  | Part_Preference | Recommended |
|  | Part_Type | Capacitor |
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES |
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released |
|  | Value | 10uF |
C89 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 2.2uF, 6.3V, X5R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 2.2uF, 6.3V, X5R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 4712 | 4712
|  | Internal_Part_Number | MCD-02606 | MCD-02606
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-02606 | MCD-02606
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX5R5BB225 | CC0402KRX5R5BB225
|  | Order_Code_Digikey | 311-1682-2-ND | 311-1682-2-ND
|  | Order_Code_Farnell | 3366429 | 3366429
|  | Order_Code_RS | 1992205 | 1992205
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Checked | Checked
|  | Value | 2.2uF | 2.2uF
C90 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 2.2uF, 6.3V, X5R, +/-10%, 0402, T=0.5mm | Capacitor, MLCC, 2.2uF, 6.3V, X5R, +/-10%, 0402, T=0.5mm
|  | Footprint | C0402 | C0402
|  | Ibis Model |  |
|  | ID | 4712 | 4712
|  | Internal_Part_Number | MCD-02606 | MCD-02606
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-02606 | MCD-02606
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | CC0402KRX5R5BB225 | CC0402KRX5R5BB225
|  | Order_Code_Digikey | 311-1682-2-ND | 311-1682-2-ND
|  | Order_Code_Farnell | 3366429 | 3366429
|  | Order_Code_RS | 1992205 | 1992205
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Checked | Checked
|  | Value | 2.2uF | 2.2uF
C91 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | Japan | Japan
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/MURATA_GRM_Series/GRM21BR71E225KE11 | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/MURATA_GRM_Series/GRM21BR71E225KE11
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 2.2uF, 25V, X7R, +/-10%, 0805, T=1,25mm | Capacitor, MLCC, 2.2uF, 25V, X7R, +/-10%, 0805, T=1,25mm
|  | Footprint | C0805 | C0805
|  | Ibis Model |  |
|  | ID | 4478 | 4478
|  | Internal_Part_Number | MCD-02372 | MCD-02372
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-02372 | MCD-02372
|  | Manufacturer | MURATA | MURATA
|  | Manufacturer_Part_Number | GRM21BR71E225KE11L | GRM21BR71E225KE11L
|  | Order_Code_Digikey | 490-14467 | 490-14467
|  | Order_Code_Farnell | 2688538 | 2688538
|  | Order_Code_RS | N/A | N/A
|  | Package | 0805 | 0805
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 2.2uF | 2.2uF
C92 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | Capacitor | Capacitor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | Japan | Japan
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/MURATA_GRM_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/MURATA_GRM_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Capacitor, MLCC, 10uF, 10V, X5R, +/-10%, 0603, T=0.8mm | Capacitor, MLCC, 10uF, 10V, X5R, +/-10%, 0603, T=0.8mm
|  | Footprint | C0603 | C0603
|  | Ibis Model |  |
|  | ID | 2770 | 2770
|  | Internal_Part_Number | MCD-00099 | MCD-00099
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00099 | MCD-00099
|  | Manufacturer | MURATA | MURATA
|  | Manufacturer_Part_Number | GRM188R61A106KE69D | GRM188R61A106KE69D
|  | Order_Code_Digikey | 490-10474-1-ND | 490-10474-1-ND
|  | Order_Code_Farnell | 2494233 | 2494233
|  | Order_Code_RS | 170-6168 | 170-6168
|  | Package | 0603 | 0603
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Capacitor | Capacitor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 10uF | 10uF
CN1 | MCU_Interfaces.SchDoc |  | Fitted | Fitted
|  | Comment | Header 20x2 | Header 20x2
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | USA | USA
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Connector/SAMTEC_TSW_Series/ | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Connector/SAMTEC_TSW_Series/
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Header, 20x2, 2.54mm, RA, TH, T=5.84mm/2.29mm | Header, 20x2, 2.54mm, RA, TH, T=5.84mm/2.29mm
|  | Footprint | CON_SAMTEC_TSW-120-08-F-D-RA | CON_SAMTEC_TSW-120-08-F-D-RA
|  | Ibis Model |  |
|  | ID | 5261 | 5261
|  | Internal_Part_Number | MCD-03145 | MCD-03145
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-03145 | MCD-03145
|  | Manufacturer | SAMTEC | SAMTEC
|  | Manufacturer_Part_Number | TSW-120-08-F-D-RA | TSW-120-08-F-D-RA
|  | Order_Code_Digikey | TSW-120-08-F-D-RA-ND | TSW-120-08-F-D-RA-ND
|  | Order_Code_Farnell | 3664253 | 3664253
|  | Order_Code_RS | 208-5661 | 208-5661
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Connector | Connector
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Checked | Checked
|  | Value | Header 20x2 | Header 20x2
CN2 | USB_TYPE_C .SchDoc |  | Fitted | Fitted
|  | Comment | USB_TYPE_C_Receptacle | USB_TYPE_C_Receptacle
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Connectors/WURTH_ELEKTRONIK_USB_TYPE-C_632723300011 | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Connectors/WURTH_ELEKTRONIK_USB_TYPE-C_632723300011
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Connector_USB_TypeC, 24pins, RA, TH, T=1.9mm (USB certified) | Connector_USB_TypeC, 24pins, RA, TH, T=1.9mm (USB certified)
|  | Footprint | CON_USB-TYPEC_WE_632723300011 | CON_USB-TYPEC_WE_632723300011
|  | Ibis Model |  |
|  | ID | 4373 | 4373
|  | Internal_Part_Number | MCD-02273 | MCD-02273
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-02273 | MCD-02273
|  | Manufacturer | WURTH ELEKTRONIK | WURTH ELEKTRONIK
|  | Manufacturer_Part_Number | 632723300011 | 632723300011
|  | Order_Code_Digikey | 732-9618-1-ND | 732-9618-1-ND
|  | Order_Code_Farnell | 2984404 | 2984404
|  | Order_Code_RS | N/A | N/A
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Connector | Connector
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | USB_C_632723300011 | USB_C_632723300011
CN3 | Display.SchDoc |  | Fitted | Fitted
|  | Comment | Header 25x2 | Header 25x2
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China, Costa Rica, Malaysia, United States, Vietnam | China, Costa Rica, Malaysia, United States, Vietnam
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Connector/SAMTEC_FLE_Series/ | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Connector/SAMTEC_FLE_Series/
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Header, 25x2, 1.27mm, SMD, VR, T=4.55mm | Header, 25x2, 1.27mm, SMD, VR, T=4.55mm
|  | Footprint | CON_SAMTEC_FLE-125-01-G-DV | CON_SAMTEC_FLE-125-01-G-DV
|  | Ibis Model |  |
|  | ID | 3274 | 3274
|  | Internal_Part_Number | MCD-01222 | MCD-01222
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01222 | MCD-01222
|  | Manufacturer | SAMTEC | SAMTEC
|  | Manufacturer_Part_Number | FLE-125-01-G-DV | FLE-125-01-G-DV
|  | Order_Code_Digikey | N/A | N/A
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | 766-8965 | 766-8965
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Connector | Connector
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Checked | Checked
|  | Value | Header 25x2 | Header 25x2
CN4 | Arduino.SchDoc |  | Fitted | Fitted
|  | Comment | Socket 10x1 | Socket 10x1
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China, Costa Rica, Malaysia, United States, Vietnam | China, Costa Rica, Malaysia, United States, Vietnam
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Connector/SAMTEC_SSW-SSQ(TH)_Series/ | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Connector/SAMTEC_SSW-SSQ(TH)_Series/
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Socket, 10x1, 2.54mm, VR, TH, T=8.51/2.64mm | Socket, 10x1, 2.54mm, VR, TH, T=8.51/2.64mm
|  | Footprint | CON_SAMTEC_SSW-110-01-X-S | CON_SAMTEC_SSW-110-01-X-S
|  | Ibis Model |  |
|  | ID | 4180 | 4180
|  | Internal_Part_Number | MCD-02080 | MCD-02080
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-02080 | MCD-02080
|  | Manufacturer | SAMTEC | SAMTEC
|  | Manufacturer_Part_Number | SSW-110-01-G-S | SSW-110-01-G-S
|  | Order_Code_Digikey | SSW-110-01-G-S-LL-ND | SSW-110-01-G-S-LL-ND
|  | Order_Code_Farnell | 1668374 | 1668374
|  | Order_Code_RS | 765-5736 | 765-5736
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Connector | Connector
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Checked | Checked
|  | Value | Socket 10x1 | Socket 10x1
CN5 | Arduino.SchDoc |  | Fitted | Fitted
|  | Comment | Socket 8x1 | Socket 8x1
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China, Costa Rica, Malaysia, United States, Vietnam | China, Costa Rica, Malaysia, United States, Vietnam
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Connector/SAMTEC_SSW-SSQ(TH)_Series/ | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Connector/SAMTEC_SSW-SSQ(TH)_Series/
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Socket, 8x1, 2.54mm, VR, TH, T=8.51/2.64mm | Socket, 8x1, 2.54mm, VR, TH, T=8.51/2.64mm
|  | Footprint | CON_SAMTEC_SSW-108-01-X-S | CON_SAMTEC_SSW-108-01-X-S
|  | Ibis Model |  |
|  | ID | 3843 | 3843
|  | Internal_Part_Number | MCD-01743 | MCD-01743
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01743 | MCD-01743
|  | Manufacturer | SAMTEC | SAMTEC
|  | Manufacturer_Part_Number | SSW-108-01-G-S | SSW-108-01-G-S
|  | Order_Code_Digikey | SAM1209-08-ND | SAM1209-08-ND
|  | Order_Code_Farnell | 1668363 | 1668363
|  | Order_Code_RS | 765-5698 | 765-5698
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Connector | Connector
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | Socket 8x1 | Socket 8x1
CN6 | Arduino.SchDoc |  | Fitted | Fitted
|  | Comment | Socket 8x1 | Socket 8x1
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China, Costa Rica, Malaysia, United States, Vietnam | China, Costa Rica, Malaysia, United States, Vietnam
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Connector/SAMTEC_SSW-SSQ(TH)_Series/ | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Connector/SAMTEC_SSW-SSQ(TH)_Series/
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Socket, 8x1, 2.54mm, VR, TH, T=8.51/2.64mm | Socket, 8x1, 2.54mm, VR, TH, T=8.51/2.64mm
|  | Footprint | CON_SAMTEC_SSW-108-01-X-S | CON_SAMTEC_SSW-108-01-X-S
|  | Ibis Model |  |
|  | ID | 3843 | 3843
|  | Internal_Part_Number | MCD-01743 | MCD-01743
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01743 | MCD-01743
|  | Manufacturer | SAMTEC | SAMTEC
|  | Manufacturer_Part_Number | SSW-108-01-G-S | SSW-108-01-G-S
|  | Order_Code_Digikey | SAM1209-08-ND | SAM1209-08-ND
|  | Order_Code_Farnell | 1668363 | 1668363
|  | Order_Code_RS | 765-5698 | 765-5698
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Connector | Connector
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | Socket 8x1 | Socket 8x1
CN7 | Arduino.SchDoc |  | Fitted | Fitted
|  | Comment | Socket 6x1 | Socket 6x1
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China, Costa Rica, Malaysia, United States, Vietnam | China, Costa Rica, Malaysia, United States, Vietnam
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Connector/SAMTEC_SSW-SSQ(TH)_Series/ | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Connector/SAMTEC_SSW-SSQ(TH)_Series/
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Socket, 6x1, 2.54mm, VR, TH, T=8.51/2.64mm | Socket, 6x1, 2.54mm, VR, TH, T=8.51/2.64mm
|  | Footprint | CON_SAMTEC_SSW-106-01-X-S | CON_SAMTEC_SSW-106-01-X-S
|  | Ibis Model |  |
|  | ID | 4179 | 4179
|  | Internal_Part_Number | MCD-02079 | MCD-02079
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-02079 | MCD-02079
|  | Manufacturer | SAMTEC | SAMTEC
|  | Manufacturer_Part_Number | SSW-106-01-G-S | SSW-106-01-G-S
|  | Order_Code_Digikey | SSW-106-01-G-S-LL-ND | SSW-106-01-G-S-LL-ND
|  | Order_Code_Farnell | 1668352 | 1668352
|  | Order_Code_RS | 765-5666 | 765-5666
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Connector | Connector
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Checked | Checked
|  | Value | Socket 6x1 | Socket 6x1
CN8 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | USB_TYPE_C_Receptacle | USB_TYPE_C_Receptacle
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Connectors/WURTH_ELEKTRONIK_USB_TYPE-C_632723300011 | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Connectors/WURTH_ELEKTRONIK_USB_TYPE-C_632723300011
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Connector_USB_TypeC, 24pins, RA, TH, T=1.9mm (USB certified) | Connector_USB_TypeC, 24pins, RA, TH, T=1.9mm (USB certified)
|  | Footprint | CON_USB-TYPEC_WE_632723300011 | CON_USB-TYPEC_WE_632723300011
|  | Ibis Model |  |
|  | ID | 4373 | 4373
|  | Internal_Part_Number | MCD-02273 | MCD-02273
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-02273 | MCD-02273
|  | Manufacturer | WURTH ELEKTRONIK | WURTH ELEKTRONIK
|  | Manufacturer_Part_Number | 632723300011 | 632723300011
|  | Order_Code_Digikey | 732-9618-1-ND | 732-9618-1-ND
|  | Order_Code_Farnell | 2984404 | 2984404
|  | Order_Code_RS | N/A | N/A
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Connector | Connector
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | USB_C_632723300011 | USB_C_632723300011
CN9 | STLINK-V3EC.SchDoc |  | Fitted | Not Fitted
|  | Comment | Header 4x1 |
|  | Component Kind | Standard |
|  | Component_Country_Of_Origin | China, Costa Rica, Malaysia, United States, Vietnam |
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Connector/SAMTEC_TSW_Series/ |
|  | Database Table Name | MCD_PARTS$ |
|  | Description | Header, 4x1, 2.54mm, VR, TH, T=5.84mm/2.54mm |
|  | Footprint | CON_SAMTEC_TSW-104-07-G-S |
|  | Ibis Model |  |
|  | ID | 2487 |
|  | Internal_Part_Number | MCD-00029 |
|  | Library Name | MCD_PARTS_database.DbLib |
|  | Library Reference | MCD-00029 |
|  | Manufacturer | SAMTEC |
|  | Manufacturer_Part_Number | TSW-104-07-G-S |
|  | Order_Code_Digikey | TSW-104-07-G-S-ND |
|  | Order_Code_Farnell | 2667450 |
|  | Order_Code_RS | 161-2261 |
|  | Part_Preference | Recommended |
|  | Part_Type | Connector |
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES |
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released |
|  | Value | Header 4x1 |
CN10 | External_Debug_Connectors.SchDoc |  | Fitted | Not Fitted
|  | Comment | Tag-10-C |
|  | Component Kind | Standard (No BOM) |
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Connector/TAG-CONNECT_TC2050-IDC-NL-FP/ |
|  | Database Table Name | MCD_PARTS$ |
|  | Description | Header_Plug-of-nails, 5x2, 1.27mm, No legs |
|  | Footprint | CON_TAG-C_TC2050-IDC-NL |
|  | Ibis Model |  |
|  | ID | 2486 |
|  | Internal_Part_Number | MCD-00031 |
|  | Library Name | MCD_PARTS_database.DbLib |
|  | Library Reference | MCD-00031 |
|  | Manufacturer | N/A |
|  | Manufacturer_Part_Number | N/A |
|  | Order_Code_Digikey | N/A |
|  | Order_Code_Farnell | N/A |
|  | Order_Code_RS | N/A |
|  | Part_Preference | Recommended |
|  | Part_Type | Connector |
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES |
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released |
|  | Value | Header 5x2 |
CN11 | External_Debug_Connectors.SchDoc |  | Fitted | Fitted
|  | Comment | Header 7x2 | Header 7x2
|  | Component Kind | Standard | Standard
|  | ComponentLink1Description | Datasheet | Datasheet
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Connectors/Samtec_FTSH_smt_series | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Connectors/Samtec_FTSH_smt_series
|  | Description | Header 5x2, 1.27mm, Dual row, Straight, Surface mount, vertical male connector. 3.05mm lead. Mates with FFSD connector. Footprint compatible with FTSH-107-01-L-DV,-K,-A,-P,-ES (STDC14 MEDIUM) | Header 5x2, 1.27mm, Dual row, Straight, Surface mount, vertical male connector. 3.05mm lead. Mates with FFSD connector. Footprint compatible with FTSH-107-01-L-DV,-K,-A,-P,-ES (STDC14 MEDIUM)
|  | Footprint | CON_STDC14_Receiver_MEDIUM_WITH_MIPI10_3D | CON_STDC14_Receiver_MEDIUM_WITH_MIPI10_3D
|  | Ibis Model |  |
|  | Initial_Board_Reference | MCD16-052 | MCD16-052
|  | Internal_Part_Number | MCD-01226 | MCD-01226
|  | Library Name | Remy.SchLib | Remy.SchLib
|  | Library Reference | MCD-01226 | MCD-01226
|  | Manufacturer | SAMTEC | SAMTEC
|  | Manufacturer_Part_Number | FTSH-105-01-L-DV-K | FTSH-105-01-L-DV-K
|  | Part_Type | Connector | Connector
|  | PCB3D |  |
|  | Pin Info |  |
|  | Provided_By | Subcon | Subcon
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Checked | Checked
|  | Value | MIPI10 on STDC14 footprint | MIPI10 on STDC14 footprint
D1 | USB_TYPE_C .SchDoc |  | Fitted | Fitted
|  | BMS_Part_Number | 9151123 | 9151123
|  | Comment | SCHOTTKY_1A_2K | SCHOTTKY_1A_2K
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Diodes/STM_SCHOTTKY_DOUBLE_BAT54SWFILM/STM_SCHOTTKY_DOUBLE_BAT54SWFILM.pdf | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Diodes/STM_SCHOTTKY_DOUBLE_BAT54SWFILM/STM_SCHOTTKY_DOUBLE_BAT54SWFILM.pdf
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Small signal Schottky diodes | Small signal Schottky diodes
|  | Footprint | DIO_SOD523_1A_2K | DIO_SOD523_1A_2K
|  | Ibis Model |  |
|  | ID | 3777 | 3777
|  | Internal_Part_Number | MCD-01677 | MCD-01677
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01677 | MCD-01677
|  | Manufacturer | STMICROELECTRONICS | STMICROELECTRONICS
|  | Manufacturer_HQ_COO | EU | EU
|  | Manufacturer_Part_Number | BAT54KFILM | BAT54KFILM
|  | Package | SOD-523 | SOD-523
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Diode | Diode
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Checked | Checked
|  | Value | BAT54KFILM | BAT54KFILM
D2 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | SCHOTTKY_1A_2K | SCHOTTKY_1A_2K
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Diode/STMICROELECTRONICS_BAT20J | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Diode/STMICROELECTRONICS_BAT20J
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Diode, Schottky, 0V54, 1A, 23V, SOD-323 | Diode, Schottky, 0V54, 1A, 23V, SOD-323
|  | Footprint | DIO_SOD323_1A_2K | DIO_SOD323_1A_2K
|  | Ibis Model |  |
|  | ID | 5127 | 5127
|  | Internal_Part_Number | MCD-03011 | MCD-03011
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-03011 | MCD-03011
|  | Manufacturer | STMICROELECTRONICS | STMICROELECTRONICS
|  | Manufacturer_Part_Number | BAT20JFILM | BAT20JFILM
|  | Order_Code_Digikey | 497-3381-2-ND | 497-3381-2-ND
|  | Order_Code_Farnell | 2354440 | 2354440
|  | Order_Code_RS | 165-7545 | 165-7545
|  | Package | SOD-323 | SOD-323
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Diode | Diode
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Checked | Checked
|  | Value | BAT20JFILM | BAT20JFILM
D3 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | SCHOTTKY_1A_2K | SCHOTTKY_1A_2K
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Diode/STMICROELECTRONICS_BAT20J | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Diode/STMICROELECTRONICS_BAT20J
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Diode, Schottky, 0V54, 1A, 23V, SOD-323 | Diode, Schottky, 0V54, 1A, 23V, SOD-323
|  | Footprint | DIO_SOD323_1A_2K | DIO_SOD323_1A_2K
|  | Ibis Model |  |
|  | ID | 5127 | 5127
|  | Internal_Part_Number | MCD-03011 | MCD-03011
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-03011 | MCD-03011
|  | Manufacturer | STMICROELECTRONICS | STMICROELECTRONICS
|  | Manufacturer_Part_Number | BAT20JFILM | BAT20JFILM
|  | Order_Code_Digikey | 497-3381-2-ND | 497-3381-2-ND
|  | Order_Code_Farnell | 2354440 | 2354440
|  | Order_Code_RS | 165-7545 | 165-7545
|  | Package | SOD-323 | SOD-323
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Diode | Diode
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Checked | Checked
|  | Value | BAT20JFILM | BAT20JFILM
H1 | Display.SchDoc |  | Fitted | Fitted
|  | Comment | MB1860_HOLES | MB1860_HOLES
|  | Component Kind | Standard (No BOM) | Standard (No BOM)
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Misc/STMICROELECTRONICS_MB1860 | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Misc/STMICROELECTRONICS_MB1860
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Footprint 1: MB1860 (5 inches LCD) Position Holes. Footprint 2: MB1860 (5 inches LCD) Position Holes + MB1860 3D + 7mm Spacers (8mm up and 15mm down) | Footprint 1: MB1860 (5 inches LCD) Position Holes. Footprint 2: MB1860 (5 inches LCD) Position Holes + MB1860 3D + 7mm Spacers (8mm up and 15mm down)
|  | Footprint | MOD_LCD_MB1860 | MOD_LCD_MB1860_DRAWING
|  | Ibis Model |  |
|  | ID | 5246 | 5246
|  | Internal_Part_Number | MCD-03130 | MCD-03130
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-03130 | MCD-03130
|  | Manufacturer | N/A | N/A
|  | Manufacturer_Part_Number | N/A | N/A
|  | Order_Code_Digikey | N/A | N/A
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Misc | Misc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | New | New
|  | Value | N/A | N/A
H5 | Display.SchDoc |  | Fitted | Fitted
|  | Comment | POSITION HOLE | POSITION HOLE
|  | Component Kind | Standard (No BOM) | Standard (No BOM)
|  | ComponentLink1URL | N/A | N/A
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | POSITION HOLE C9D4R5 | POSITION HOLE C9D4R5
|  | Footprint | PTH_450_900 | PTH_450_900
|  | Ibis Model |  |
|  | ID | 3712 | 3712
|  | Internal_Part_Number | MCD-01612 | MCD-01612
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01612 | MCD-01612
|  | Manufacturer | N/A | N/A
|  | Manufacturer_Part_Number | N/A | N/A
|  | Order_Code_Digikey | N/A | N/A
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Package | N/A | N/A
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Misc | Misc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | New | New
|  | Value | N/A | N/A
H6 | Display.SchDoc |  | Fitted | Fitted
|  | Comment | POSITION HOLE | POSITION HOLE
|  | Component Kind | Standard (No BOM) | Standard (No BOM)
|  | ComponentLink1URL | N/A | N/A
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | POSITION HOLE C9D4R5 | POSITION HOLE C9D4R5
|  | Footprint | PTH_450_900 | PTH_450_900
|  | Ibis Model |  |
|  | ID | 3712 | 3712
|  | Internal_Part_Number | MCD-01612 | MCD-01612
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01612 | MCD-01612
|  | Manufacturer | N/A | N/A
|  | Manufacturer_Part_Number | N/A | N/A
|  | Order_Code_Digikey | N/A | N/A
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Package | N/A | N/A
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Misc | Misc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | New | New
|  | Value | N/A | N/A
HW1 | MB1918_TOP.SchDoc |  | Fitted | Fitted
|  | Comment | STICKER_BOARD | STICKER_BOARD
|  | Component Kind | Standard (No BOM) | Standard (No BOM)
|  | ComponentLink1URL | N/A | N/A
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Sticker Board 25x9 mm | Sticker Board 25x9 mm
|  | Footprint | STICKER_BOARD_25X9 | STICKER_BOARD_25X9
|  | Ibis Model |  |
|  | ID | 2632 | 2632
|  | Internal_Part_Number | MCD-00235 | MCD-00235
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00235 | MCD-00235
|  | Manufacturer | N/A | N/A
|  | Manufacturer_Part_Number | N/A | N/A
|  | Order_Code_Digikey | N/A | N/A
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Misc | Misc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | Sticker board | Sticker board
HW2 | MB1918_TOP.SchDoc |  | Fitted | Fitted
|  | Comment | STICKER_PRODUCT | STICKER_PRODUCT
|  | Component Kind | Standard (No BOM) | Standard (No BOM)
|  | ComponentLink1URL | N/A | N/A
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Sticker product 25x5 mm | Sticker product 25x5 mm
|  | Footprint | STICKER_PRODUCT_25X5 | STICKER_PRODUCT_25X5
|  | Ibis Model |  |
|  | ID | 4289 | 4289
|  | Internal_Part_Number | MCD-02189 | MCD-02189
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-02189 | MCD-02189
|  | Manufacturer | N/A | N/A
|  | Manufacturer_Part_Number | N/A | N/A
|  | Order_Code_Digikey | N/A | N/A
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Misc | Misc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | Sticker product | Sticker product
HW3 | Board_Power.SchDoc |  | Fitted | Fitted
|  | Comment | Shunt Black 2.54mm | Shunt Black 2.54mm
|  | Component Kind | Mechanical | Mechanical
|  | Component_Country_Of_Origin | China, Costa Rica, Malaysia, United States, Vietnam | China, Costa Rica, Malaysia, United States, Vietnam
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Connectors/Samtec_Shunt_Jumper_SNT100 | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Connectors/Samtec_Shunt_Jumper_SNT100
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | SHUNT 2.54mm BLACK | SHUNT 2.54mm BLACK
|  | Footprint |  |
|  | Full_Alternate_Internal_Part_Number | MCD-02388 | MCD-02388
|  | Ibis Model |  |
|  | ID | 2551 | 2551
|  | Internal_Part_Number | MCD-00043 | MCD-00043
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00043 | MCD-00043
|  | Manufacturer | SAMTEC | SAMTEC
|  | Manufacturer_Part_Number | SNT-100-BK-G | SNT-100-BK-G
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Misc | Misc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | SNT-100-BK-G | SNT-100-BK-G
HW4 | MCU_System.SchDoc |  | Fitted | Not Fitted
|  | Comment | SOCKET_LQFP144 |
|  | Component Kind | Mechanical |
|  | Component_Country_Of_Origin | Unknown |
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Misc/Yamaichi_LQFP_socket_IC149_144_145_B5 |
|  | Database Table Name | MCD_PARTS$ |
|  | Description | Socket_IC, LQFP144, IC149 series, pitch 0.5mm, without positionning pin |
|  | Footprint |  |
|  | Ibis Model |  |
|  | ID | 3005 |
|  | Internal_Part_Number | MCD-01015 |
|  | Library Name | MCD_PARTS_database.DbLib |
|  | Library Reference | MCD-01015 |
|  | Manufacturer | YAMAICHI |
|  | Manufacturer_Part_Number | IC149-144-145-B5 |
|  | Order_Code_Digikey | N/A |
|  | Order_Code_Farnell | N/A |
|  | Order_Code_RS | N/A |
|  | Package | LQFP144 |
|  | Part_Preference | Recommended |
|  | Part_Type | Socket_IC |
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES |
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released |
|  | Value | LQFP144_socket |
HW5 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Comment | Shunt Black 2.54mm | Shunt Black 2.54mm
|  | Component Kind | Mechanical | Mechanical
|  | Component_Country_Of_Origin | China, Costa Rica, Malaysia, United States, Vietnam | China, Costa Rica, Malaysia, United States, Vietnam
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Connectors/Samtec_Shunt_Jumper_SNT100 | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Connectors/Samtec_Shunt_Jumper_SNT100
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | SHUNT 2.54mm BLACK | SHUNT 2.54mm BLACK
|  | Footprint |  |
|  | Full_Alternate_Internal_Part_Number | MCD-02388 | MCD-02388
|  | Ibis Model |  |
|  | ID | 2551 | 2551
|  | Internal_Part_Number | MCD-00043 | MCD-00043
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00043 | MCD-00043
|  | Manufacturer | SAMTEC | SAMTEC
|  | Manufacturer_Part_Number | SNT-100-BK-G | SNT-100-BK-G
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Misc | Misc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | SNT-100-BK-G | SNT-100-BK-G
JP1 | Board_Power.SchDoc |  | Fitted | Fitted
|  | Comment | Header 3x2 | Header 3x2
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China, Costa Rica, Malaysia, United States, Vietnam | China, Costa Rica, Malaysia, United States, Vietnam
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Connector/SAMTEC_TSW_Series/ | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Connector/SAMTEC_TSW_Series/
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Header, 3x2, 2.54mm, VR, TH, T=5.84mm/2.54mm | Header, 3x2, 2.54mm, VR, TH, T=5.84mm/2.54mm
|  | Footprint | CON_SAMTEC_TSW-103-07-X-D | CON_SAMTEC_TSW-103-07-X-D
|  | Ibis Model |  |
|  | ID | 2638 | 2638
|  | Internal_Part_Number | MCD-00233 | MCD-00233
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00233 | MCD-00233
|  | Manufacturer | SAMTEC | SAMTEC
|  | Manufacturer_Part_Number | TSW-103-07-G-D | TSW-103-07-G-D
|  | Order_Code_Digikey | SAM1028-03-ND | SAM1028-03-ND
|  | Order_Code_Farnell | 2748590 | 2748590
|  | Order_Code_RS | 161-2249 | 161-2249
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Connector | Connector
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | Header 3x2 | Header 3x2
JP3 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | Jumper_Header 2x1 | Jumper_Header 2x1
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China, Costa Rica, Malaysia, United States, Vietnam | China, Costa Rica, Malaysia, United States, Vietnam
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Connector/SAMTEC_TSW_Series/ | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Connector/SAMTEC_TSW_Series/
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Header, 2x1, 2.54mm, VR, TH, T=5.84mm/2.54mm | Header, 2x1, 2.54mm, VR, TH, T=5.84mm/2.54mm
|  | Footprint | CON_SAMTEC_TSW-102-07-G-S | CON_SAMTEC_TSW-102-07-G-S
|  | Full_Alternate_Internal_Part_Number | MCD-02390 | MCD-02390
|  | Ibis Model |  |
|  | ID | 2545 | 2545
|  | Internal_Part_Number | MCD-00045 | MCD-00045
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00045 | MCD-00045
|  | Manufacturer | SAMTEC | SAMTEC
|  | Manufacturer_Part_Number | TSW-102-07-G-S | TSW-102-07-G-S
|  | Order_Code_Digikey | SAM1029-02-ND | SAM1029-02-ND
|  | Order_Code_Farnell | 2505044 | 2505044
|  | Order_Code_RS | 155-5312 | 155-5312
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Connector | Connector
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | Header 2x1 | Header 2x1
JP4 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Comment | Jumper_Header 2x1 Fitted | Jumper_Header 2x1 Fitted
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China, Costa Rica, Malaysia, United States, Vietnam | China, Costa Rica, Malaysia, United States, Vietnam
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Connector/SAMTEC_TSW_Series/ | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Connector/SAMTEC_TSW_Series/
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Header, 2x1, 2.54mm, VR, TH, T=5.84mm/2.54mm | Header, 2x1, 2.54mm, VR, TH, T=5.84mm/2.54mm
|  | Footprint | CON_SAMTEC_TSW-102-07-G-S | CON_SAMTEC_TSW-102-07-G-S
|  | Full_Alternate_Internal_Part_Number | MCD-02389 | MCD-02389
|  | Ibis Model |  |
|  | ID | 3057 | 3057
|  | Internal_Part_Number | MCD-00683 | MCD-00683
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00683 | MCD-00683
|  | Manufacturer | SAMTEC | SAMTEC
|  | Manufacturer_Part_Number | TSW-102-07-G-S | TSW-102-07-G-S
|  | Order_Code_Digikey | SAM1029-02-ND | SAM1029-02-ND
|  | Order_Code_Farnell | 2505044 | 2505044
|  | Order_Code_RS | 155-5312 | 155-5312
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Connector | Connector
|  | Partial_Alternate_Internal_Part_Number | MCD-02957 | MCD-02957
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | Header 2x1 | Header 2x1
L1 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Comment | Inductor | Inductor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | Japan | Japan
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Inductor/MURATA_LQM_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Inductor/MURATA_LQM_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Inductor, 2.2uH, +/-20%, 0.7A, 0R156, 0805, T=0.9mm | Inductor, 2.2uH, +/-20%, 0.7A, 0R156, 0805, T=0.9mm
|  | Footprint | L0805_H0P9 | L0805_H0P9
|  | Ibis Model |  |
|  | ID | 2963 | 2963
|  | Internal_Part_Number | MCD-01060 | MCD-01060
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01060 | MCD-01060
|  | Manufacturer | MURATA | MURATA
|  | Manufacturer_Part_Number | LQM21PN2R2MGH | LQM21PN2R2MGH
|  | Order_Code_Digikey | 490-9573-2-ND | 490-9573-2-ND
|  | Order_Code_Farnell | 3471402 | 3471402
|  | Order_Code_RS | 166-9883 | 166-9883
|  | Package | 0805 | 0805
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Inductor | Inductor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 2.2uH | 2.2uH
LD1 | User_Interface.SchDoc |  | Fitted | Fitted
|  | Comment | LED_green | LED_green
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | Unknown | Unknown
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Display/OSRAM_LED_GREEN_LG Q396-PS-35 | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Display/OSRAM_LED_GREEN_LG Q396-PS-35
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | LED Green, 0603 SMD, Forward Voltage Typ=2V, Max=2.5V | LED Green, 0603 SMD, Forward Voltage Typ=2V, Max=2.5V
|  | Footprint | LED_0603_OSRAM_LG-Q396-PS-35_GREEN_1A2K_H0P4 | LED_0603_OSRAM_LG-Q396-PS-35_GREEN_1A2K_H0P4
|  | Full_Alternate_Internal_Part_Number | MCD-02400 | MCD-02400
|  | Ibis Model |  |
|  | ID | 3155 | 3155
|  | Internal_Part_Number | MCD-00588 | MCD-00588
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00588 | MCD-00588
|  | Manufacturer | OSRAM OPTO SEMICONDUCTORS | OSRAM OPTO SEMICONDUCTORS
|  | Manufacturer_Part_Number | LG Q396-PS-35 | LG Q396-PS-35
|  | Order_Code_Digikey | LG Q396-PS-35-ND | LG Q396-PS-35-ND
|  | Package | LED 0603 | LED 0603
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Display | Display
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | GREEN | GREEN
LD2 | User_Interface.SchDoc |  | Fitted | Fitted
|  | Comment | LED_red | LED_red
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | Unknown | Unknown
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Display/OSRAM_LED_RED_LS Q976-NR-1 | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Display/OSRAM_LED_RED_LS Q976-NR-1
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | LED Red, 0603 SMD, Forward Voltage Typ=2V, Max=2.5V | LED Red, 0603 SMD, Forward Voltage Typ=2V, Max=2.5V
|  | Footprint | LED_0603_OSRAM_LS-Q976-NR-1_RED_1A2K_H0P8 | LED_0603_OSRAM_LS-Q976-NR-1_RED_1A2K_H0P8
|  | Ibis Model |  |
|  | ID | 3158 | 3158
|  | Internal_Part_Number | MCD-00586 | MCD-00586
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00586 | MCD-00586
|  | Manufacturer | OSRAM OPTO SEMICONDUCTORS | OSRAM OPTO SEMICONDUCTORS
|  | Manufacturer_Part_Number | LS Q976-NR-1 | LS Q976-NR-1
|  | Order_Code_Digikey | 475-2512-1-ND | 475-2512-1-ND
|  | Package | LED 0603 | LED 0603
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Display | Display
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | RED | RED
LD3 | User_Interface.SchDoc |  | Fitted | Fitted
|  | Comment | LED_green | LED_green
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | Unknown | Unknown
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Display/OSRAM_LED_GREEN_LG Q396-PS-35 | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Display/OSRAM_LED_GREEN_LG Q396-PS-35
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | LED Green, 0603 SMD, Forward Voltage Typ=2V, Max=2.5V | LED Green, 0603 SMD, Forward Voltage Typ=2V, Max=2.5V
|  | Footprint | LED_0603_OSRAM_LG-Q396-PS-35_GREEN_1A2K_H0P4 | LED_0603_OSRAM_LG-Q396-PS-35_GREEN_1A2K_H0P4
|  | Full_Alternate_Internal_Part_Number | MCD-02400 | MCD-02400
|  | Ibis Model |  |
|  | ID | 3155 | 3155
|  | Internal_Part_Number | MCD-00588 | MCD-00588
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00588 | MCD-00588
|  | Manufacturer | OSRAM OPTO SEMICONDUCTORS | OSRAM OPTO SEMICONDUCTORS
|  | Manufacturer_Part_Number | LG Q396-PS-35 | LG Q396-PS-35
|  | Order_Code_Digikey | LG Q396-PS-35-ND | LG Q396-PS-35-ND
|  | Package | LED 0603 | LED 0603
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Display | Display
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | GREEN | GREEN
LD5 | User_Interface.SchDoc |  | Fitted | Fitted
|  | Comment | LED_green | LED_green
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | Unknown | Unknown
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Display/OSRAM_LED_GREEN_LG Q396-PS-35 | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Display/OSRAM_LED_GREEN_LG Q396-PS-35
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | LED Green, 0603 SMD, Forward Voltage Typ=2V, Max=2.5V | LED Green, 0603 SMD, Forward Voltage Typ=2V, Max=2.5V
|  | Footprint | LED_0603_OSRAM_LG-Q396-PS-35_GREEN_1A2K_H0P4 | LED_0603_OSRAM_LG-Q396-PS-35_GREEN_1A2K_H0P4
|  | Full_Alternate_Internal_Part_Number | MCD-02400 | MCD-02400
|  | Ibis Model |  |
|  | ID | 3155 | 3155
|  | Internal_Part_Number | MCD-00588 | MCD-00588
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00588 | MCD-00588
|  | Manufacturer | OSRAM OPTO SEMICONDUCTORS | OSRAM OPTO SEMICONDUCTORS
|  | Manufacturer_Part_Number | LG Q396-PS-35 | LG Q396-PS-35
|  | Order_Code_Digikey | LG Q396-PS-35-ND | LG Q396-PS-35-ND
|  | Package | LED 0603 | LED 0603
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Display | Display
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | GREEN | GREEN
LD6 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | LED_BICOLOR | LED_BICOLOR
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Display/WURTH_ELEKTRONIK_150141SV73110 | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Display/WURTH_ELEKTRONIK_150141SV73110
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | LED Bicolor, Green/Red, 2V, 20mA, 4-PLCC | LED Bicolor, Green/Red, 2V, 20mA, 4-PLCC
|  | Footprint | LED_BI-GR_WE-150141SV73110 | LED_BI-GR_WE-150141SV73110
|  | Ibis Model |  |
|  | ID | 4737 | 4737
|  | Internal_Part_Number | MCD-02631 | MCD-02631
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-02631 | MCD-02631
|  | Manufacturer | WURTH ELEKTRONIK | WURTH ELEKTRONIK
|  | Manufacturer_Part_Number | 150141SV73110 | 150141SV73110
|  | Order_Code_Digikey | 732-13404-2-ND | 732-13404-2-ND
|  | Order_Code_Farnell | 2990869 | 2990869
|  | Order_Code_RS | 184-6963 | 184-6963
|  | Package | 4-PLCC | 4-PLCC
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Display | Display
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Checked | Checked
|  | Value | Green / Red | Green / Red
LD7 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | LED_BICOLOR | LED_BICOLOR
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Display/WURTH_ELEKTRONIK_150141SV73110 | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Display/WURTH_ELEKTRONIK_150141SV73110
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | LED Bicolor, Green/Red, 2V, 20mA, 4-PLCC | LED Bicolor, Green/Red, 2V, 20mA, 4-PLCC
|  | Footprint | LED_BI-GR_WE-150141SV73110 | LED_BI-GR_WE-150141SV73110
|  | Ibis Model |  |
|  | ID | 4737 | 4737
|  | Internal_Part_Number | MCD-02631 | MCD-02631
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-02631 | MCD-02631
|  | Manufacturer | WURTH ELEKTRONIK | WURTH ELEKTRONIK
|  | Manufacturer_Part_Number | 150141SV73110 | 150141SV73110
|  | Order_Code_Digikey | 732-13404-2-ND | 732-13404-2-ND
|  | Order_Code_Farnell | 2990869 | 2990869
|  | Order_Code_RS | 184-6963 | 184-6963
|  | Package | 4-PLCC | 4-PLCC
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Display | Display
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Checked | Checked
|  | Value | Green / Red | Green / Red
LNK1 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | link_200 | link_200
|  | Component Kind | Standard (No BOM) | Standard (No BOM)
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Track link on PCB 200um width for layout routing | Track link on PCB 200um width for layout routing
|  | Footprint | LINK200 | LINK200
|  | Ibis Model |  |
|  | ID | 4889 | 4889
|  | Internal_Part_Number | MCD-02777 | MCD-02777
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-02777 | MCD-02777
|  | Manufacturer | N/A | N/A
|  | Manufacturer_Part_Number | link_200 | link_200
|  | Order_Code_Digikey | N/A | N/A
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Misc | Misc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Checked | Checked
|  | Value | link_200 | link_200
Q1 | User_Interface.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M, M | M, M
|  | Comment | 9013-SOT23 | 9013-SOT23
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | Unknown | Unknown
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/IC/NXP_Transistor_BSR14 | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/IC/NXP_Transistor_BSR14
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | NPN Bipolar Transistor | NPN Bipolar Transistor
|  | Footprint | NPN_SOT23 | NPN_SOT23
|  | Ibis Model |  |
|  | ID | 2519 | 2519
|  | Internal_Part_Number | MCD-00073 | MCD-00073
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00073 | MCD-00073
|  | Manufacturer | ON SEMICONDUCTOR | ON SEMICONDUCTOR
|  | Manufacturer_Part_Number | BSR14 | BSR14
|  | Package | SOT23 | SOT23
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | IC | IC
|  | Partial_Alternate_Internal_Part_Number | MCD-01737, MCD-03305 | MCD-01737, MCD-03305
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | NPN SOT23 | NPN SOT23
Q2 | USB_TYPE_C .SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | A, | A,
|  | BMS_Part_Number | 9153561 | 9153561
|  | Comment | STL11N3LLH6 | STL11N3LLH6
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/IC/STM_POWER_MOSFET_STL11N3LLH6 | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/IC/STM_POWER_MOSFET_STL11N3LLH6
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | N-channel 30 V, 6 mO typ, 11 A STripFET™ H6, Power MOSFET in a PowerFLAT™ 3.3x3.3 package | N-channel 30 V, 6 mO typ, 11 A STripFET™ H6, Power MOSFET in a PowerFLAT™ 3.3x3.3 package
|  | Footprint | MOS_POWERFLAT_3P3X3P3_P065 | MOS_POWERFLAT_3P3X3P3_P065
|  | Ibis Model |  |
|  | ID | 3910 | 3910
|  | Internal_Part_Number | MCD-01810 | MCD-01810
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01810 | MCD-01810
|  | Manufacturer | STMICROELECTRONICS | STMICROELECTRONICS
|  | Manufacturer_HQ_COO | EU | EU
|  | Manufacturer_Part_Number | STL11N3LLH6 | STL11N3LLH6
|  | Package | PowerFLAT 3.3x3.3 | PowerFLAT 3.3x3.3
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | IC | IC
|  | Partial_Alternate_Internal_Part_Number | MCD-03269, MCD-03325 | MCD-03269, MCD-03325
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | STL11N3LLH6 | STL11N3LLH6
Q3 | User_Interface.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M, M | M, M
|  | Comment | 9013-SOT23 | 9013-SOT23
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | Unknown | Unknown
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/IC/NXP_Transistor_BSR14 | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/IC/NXP_Transistor_BSR14
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | NPN Bipolar Transistor | NPN Bipolar Transistor
|  | Footprint | NPN_SOT23 | NPN_SOT23
|  | Ibis Model |  |
|  | ID | 2519 | 2519
|  | Internal_Part_Number | MCD-00073 | MCD-00073
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00073 | MCD-00073
|  | Manufacturer | ON SEMICONDUCTOR | ON SEMICONDUCTOR
|  | Manufacturer_Part_Number | BSR14 | BSR14
|  | Package | SOT23 | SOT23
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | IC | IC
|  | Partial_Alternate_Internal_Part_Number | MCD-01737, MCD-03305 | MCD-01737, MCD-03305
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | NPN SOT23 | NPN SOT23
Q4 | User_Interface.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M, M | M, M
|  | Comment | 9013-SOT23 | 9013-SOT23
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | Unknown | Unknown
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/IC/NXP_Transistor_BSR14 | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/IC/NXP_Transistor_BSR14
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | NPN Bipolar Transistor | NPN Bipolar Transistor
|  | Footprint | NPN_SOT23 | NPN_SOT23
|  | Ibis Model |  |
|  | ID | 2519 | 2519
|  | Internal_Part_Number | MCD-00073 | MCD-00073
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00073 | MCD-00073
|  | Manufacturer | ON SEMICONDUCTOR | ON SEMICONDUCTOR
|  | Manufacturer_Part_Number | BSR14 | BSR14
|  | Package | SOT23 | SOT23
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | IC | IC
|  | Partial_Alternate_Internal_Part_Number | MCD-01737, MCD-03305 | MCD-01737, MCD-03305
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | NPN SOT23 | NPN SOT23
R1 | MCU_System.SchDoc |  | Fitted | Fitted
|  | BMS_Part_Number | 9131590 | 9131590
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 10K, 0402, +/-1%, 1/16W | Resistor, 10K, 0402, +/-1%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2539 | 2539
|  | Internal_Part_Number | MCD-00053 | MCD-00053
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00053 | MCD-00053
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402FR-0710KL | RC0402FR-0710KL
|  | Order_Code_Digikey | 311-10.0KLRCT-ND | 311-10.0KLRCT-ND
|  | Order_Code_Farnell | 9239359 | 9239359
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 10K | 10K
R2 | MCU_System.SchDoc |  | Fitted | Not Fitted
|  | Comment | Resistor |
|  | Component Kind | Standard |
|  | Component_Country_Of_Origin | China |
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series |
|  | Database Table Name | MCD_PARTS$ |
|  | Description | Resistor, 0R, 0402, +/-5%, 1/16W |
|  | Footprint | R0402 |
|  | Ibis Model |  |
|  | ID | 2540 |
|  | Internal_Part_Number | MCD-00052 |
|  | Library Name | MCD_PARTS_database.DbLib |
|  | Library Reference | MCD-00052 |
|  | Manufacturer | YAGEO |
|  | Manufacturer_Part_Number | RC0402JR-070RL |
|  | Order_Code_Digikey | 311-0.0JRCT-ND |
|  | Order_Code_Farnell | 9232516RL |
|  | Order_Code_RS | 618-5804 |
|  | Package | 0402 |
|  | Part_Preference | Recommended |
|  | Part_Type | Resistor |
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES |
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released |
|  | Value | 0R |
R3 | MCU_System.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 0R, 0402, +/-5%, 1/16W | Resistor, 0R, 0402, +/-5%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2540 | 2540
|  | Internal_Part_Number | MCD-00052 | MCD-00052
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00052 | MCD-00052
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402JR-070RL | RC0402JR-070RL
|  | Order_Code_Digikey | 311-0.0JRCT-ND | 311-0.0JRCT-ND
|  | Order_Code_Farnell | 9232516RL | 9232516RL
|  | Order_Code_RS | 618-5804 | 618-5804
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 0R | 0R
R4 | MCU_System.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 0R, 0402, +/-5%, 1/16W | Resistor, 0R, 0402, +/-5%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2540 | 2540
|  | Internal_Part_Number | MCD-00052 | MCD-00052
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00052 | MCD-00052
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402JR-070RL | RC0402JR-070RL
|  | Order_Code_Digikey | 311-0.0JRCT-ND | 311-0.0JRCT-ND
|  | Order_Code_Farnell | 9232516RL | 9232516RL
|  | Order_Code_RS | 618-5804 | 618-5804
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 0R | 0R
R5 | Display.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 0R, 0402, +/-5%, 1/16W | Resistor, 0R, 0402, +/-5%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2540 | 2540
|  | Internal_Part_Number | MCD-00052 | MCD-00052
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00052 | MCD-00052
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402JR-070RL | RC0402JR-070RL
|  | Order_Code_Digikey | 311-0.0JRCT-ND | 311-0.0JRCT-ND
|  | Order_Code_Farnell | 9232516RL | 9232516RL
|  | Order_Code_RS | 618-5804 | 618-5804
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 0R | 0R
R6 | Display.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 0R, 0402, +/-5%, 1/16W | Resistor, 0R, 0402, +/-5%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2540 | 2540
|  | Internal_Part_Number | MCD-00052 | MCD-00052
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00052 | MCD-00052
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402JR-070RL | RC0402JR-070RL
|  | Order_Code_Digikey | 311-0.0JRCT-ND | 311-0.0JRCT-ND
|  | Order_Code_Farnell | 9232516RL | 9232516RL
|  | Order_Code_RS | 618-5804 | 618-5804
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 0R | 0R
R7 | Display.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 0R, 0603, +/-5%, 1/10W | Resistor, 0R, 0603, +/-5%, 1/10W
|  | Footprint | R0603 | R0603
|  | Ibis Model |  |
|  | ID | 2536 | 2536
|  | Internal_Part_Number | MCD-00056 | MCD-00056
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00056 | MCD-00056
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0603JR-070RL | RC0603JR-070RL
|  | Order_Code_Digikey | 311-0.0GRCT-ND | 311-0.0GRCT-ND
|  | Order_Code_Farnell | 9233130RL | 9233130RL
|  | Order_Code_RS | N/A | N/A
|  | Package | 0603 | 0603
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 0R | 0R
R8 | Display.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 0R, 0603, +/-5%, 1/10W | Resistor, 0R, 0603, +/-5%, 1/10W
|  | Footprint | R0603 | R0603
|  | Ibis Model |  |
|  | ID | 2536 | 2536
|  | Internal_Part_Number | MCD-00056 | MCD-00056
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00056 | MCD-00056
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0603JR-070RL | RC0603JR-070RL
|  | Order_Code_Digikey | 311-0.0GRCT-ND | 311-0.0GRCT-ND
|  | Order_Code_Farnell | 9233130RL | 9233130RL
|  | Order_Code_RS | N/A | N/A
|  | Package | 0603 | 0603
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 0R | 0R
R9 | User_Interface.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 2K2, 0402, +/-1%, 1/16W | Resistor, 2K2, 0402, +/-1%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2534 | 2534
|  | Internal_Part_Number | MCD-00057 | MCD-00057
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00057 | MCD-00057
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402FR-072K2L | RC0402FR-072K2L
|  | Order_Code_Digikey | 311-2.20KLRCT-ND | 311-2.20KLRCT-ND
|  | Order_Code_Farnell | 9239278 | 9239278
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 2K2 | 2K2
R10 | User_Interface.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | Taiwan | Taiwan
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RT_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RT_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 390R, 0402, +/-0.1%, 1/16W, +/-25ppm/°C | Resistor, 390R, 0402, +/-0.1%, 1/16W, +/-25ppm/°C
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 5130 | 5130
|  | Internal_Part_Number | MCD-03014 | MCD-03014
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-03014 | MCD-03014
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RT0402BRD07390RL | RT0402BRD07390RL
|  | Order_Code_Digikey | YAG1417CT-ND | YAG1417CT-ND
|  | Order_Code_Farnell | 3496504 | 3496504
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Checked | Checked
|  | Value | 390R | 390R
R11 | User_Interface.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 47K, 0603, 1%, 1/10W | Resistor, 47K, 0603, 1%, 1/10W
|  | Footprint | R0603 | R0603
|  | Ibis Model |  |
|  | ID | 2645 | 2645
|  | Internal_Part_Number | MCD-00222 | MCD-00222
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00222 | MCD-00222
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0603FR-0747KL | RC0603FR-0747KL
|  | Order_Code_Digikey | 311-47.0KHRCT-ND | 311-47.0KHRCT-ND
|  | Order_Code_Farnell | 9238689 | 9238689
|  | Order_Code_RS | N/A | N/A
|  | Package | 0603 | 0603
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 47K | 47K
R12 | User_Interface.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 22K, 0603, +/-1%, 1/10W | Resistor, 22K, 0603, +/-1%, 1/10W
|  | Footprint | R0603 | R0603
|  | Ibis Model |  |
|  | ID | 2847 | 2847
|  | Internal_Part_Number | MCD-00430 | MCD-00430
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00430 | MCD-00430
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0603FR-0722KL | RC0603FR-0722KL
|  | Order_Code_Digikey | 311-22.0KHRCT-ND | 311-22.0KHRCT-ND
|  | Order_Code_Farnell | 9238646 | 9238646
|  | Order_Code_RS | N/A | N/A
|  | Package | 0603 | 0603
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 22K | 22K
R13 | Board_Power.SchDoc |  | Fitted | Fitted
|  | BMS_Part_Number | 9131590 | 9131590
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 10K, 0402, +/-1%, 1/16W | Resistor, 10K, 0402, +/-1%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2539 | 2539
|  | Internal_Part_Number | MCD-00053 | MCD-00053
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00053 | MCD-00053
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402FR-0710KL | RC0402FR-0710KL
|  | Order_Code_Digikey | 311-10.0KLRCT-ND | 311-10.0KLRCT-ND
|  | Order_Code_Farnell | 9239359 | 9239359
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 10K | 10K
R14 | USB_TYPE_C .SchDoc |  | Fitted | Fitted
|  | BMS_Part_Number | 9131590 | 9131590
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 10K, 0402, +/-1%, 1/16W | Resistor, 10K, 0402, +/-1%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2539 | 2539
|  | Internal_Part_Number | MCD-00053 | MCD-00053
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00053 | MCD-00053
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402FR-0710KL | RC0402FR-0710KL
|  | Order_Code_Digikey | 311-10.0KLRCT-ND | 311-10.0KLRCT-ND
|  | Order_Code_Farnell | 9239359 | 9239359
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 10K | 10K
R15 | USB_TYPE_C .SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 2K4, 0402, +/-1%, 1/16W | Resistor, 2K4, 0402, +/-1%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2843 | 2843
|  | Internal_Part_Number | MCD-00433 | MCD-00433
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00433 | MCD-00433
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402FR-072K4L | RC0402FR-072K4L
|  | Order_Code_Digikey | 311-2.40KLRCT-ND | 311-2.40KLRCT-ND
|  | Order_Code_Farnell | 1458767 | 1458767
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 2K4 | 2K4
R18 | User_Interface.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 270R, 0402, +/-1%, 1/16W | Resistor, 270R, 0402, +/-1%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2838 | 2838
|  | Internal_Part_Number | MCD-00441 | MCD-00441
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00441 | MCD-00441
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402FR-07270RL | RC0402FR-07270RL
|  | Order_Code_Digikey | 311-270LRCT-ND | 311-270LRCT-ND
|  | Order_Code_Farnell | 9239162 | 9239162
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 270R | 270R
R19 | User_Interface.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | Taiwan | Taiwan
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RT_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RT_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 390R, 0402, +/-0.1%, 1/16W, +/-25ppm/°C | Resistor, 390R, 0402, +/-0.1%, 1/16W, +/-25ppm/°C
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 5130 | 5130
|  | Internal_Part_Number | MCD-03014 | MCD-03014
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-03014 | MCD-03014
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RT0402BRD07390RL | RT0402BRD07390RL
|  | Order_Code_Digikey | YAG1417CT-ND | YAG1417CT-ND
|  | Order_Code_Farnell | 3496504 | 3496504
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Checked | Checked
|  | Value | 390R | 390R
R20 | User_Interface.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 47K, 0603, 1%, 1/10W | Resistor, 47K, 0603, 1%, 1/10W
|  | Footprint | R0603 | R0603
|  | Ibis Model |  |
|  | ID | 2645 | 2645
|  | Internal_Part_Number | MCD-00222 | MCD-00222
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00222 | MCD-00222
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0603FR-0747KL | RC0603FR-0747KL
|  | Order_Code_Digikey | 311-47.0KHRCT-ND | 311-47.0KHRCT-ND
|  | Order_Code_Farnell | 9238689 | 9238689
|  | Order_Code_RS | N/A | N/A
|  | Package | 0603 | 0603
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 47K | 47K
R21 | User_Interface.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 47K, 0603, 1%, 1/10W | Resistor, 47K, 0603, 1%, 1/10W
|  | Footprint | R0603 | R0603
|  | Ibis Model |  |
|  | ID | 2645 | 2645
|  | Internal_Part_Number | MCD-00222 | MCD-00222
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00222 | MCD-00222
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0603FR-0747KL | RC0603FR-0747KL
|  | Order_Code_Digikey | 311-47.0KHRCT-ND | 311-47.0KHRCT-ND
|  | Order_Code_Farnell | 9238689 | 9238689
|  | Order_Code_RS | N/A | N/A
|  | Package | 0603 | 0603
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 47K | 47K
R22 | User_Interface.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 100K, 0603, +/- 1%, 1/10W | Resistor, 100K, 0603, +/- 1%, 1/10W
|  | Footprint | R0603 | R0603
|  | Ibis Model |  |
|  | ID | 2647 | 2647
|  | Internal_Part_Number | MCD-00223 | MCD-00223
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00223 | MCD-00223
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0603FR-07100KL | RC0603FR-07100KL
|  | Order_Code_Digikey | 311-100KHRTR-ND | 311-100KHRTR-ND
|  | Order_Code_Farnell | 2421851 | 2421851
|  | Order_Code_RS | N/A | N/A
|  | Package | 0603 | 0603
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100K | 100K
R23 | User_Interface.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 100K, 0603, +/- 1%, 1/10W | Resistor, 100K, 0603, +/- 1%, 1/10W
|  | Footprint | R0603 | R0603
|  | Ibis Model |  |
|  | ID | 2647 | 2647
|  | Internal_Part_Number | MCD-00223 | MCD-00223
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00223 | MCD-00223
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0603FR-07100KL | RC0603FR-07100KL
|  | Order_Code_Digikey | 311-100KHRTR-ND | 311-100KHRTR-ND
|  | Order_Code_Farnell | 2421851 | 2421851
|  | Order_Code_RS | N/A | N/A
|  | Package | 0603 | 0603
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100K | 100K
R24 | MCU_Interfaces.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 1K5, 0402, +/-1%, 1/16W | Resistor, 1K5, 0402, +/-1%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2524 | 2524
|  | Internal_Part_Number | MCD-00068 | MCD-00068
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00068 | MCD-00068
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402FR-071K5L | RC0402FR-071K5L
|  | Order_Code_Digikey | 311-1.50KLRCT-ND | 311-1.50KLRCT-ND
|  | Order_Code_Farnell | 9239251 | 9239251
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 1K5 | 1K5
R25 | MCU_Interfaces.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 1K5, 0402, +/-1%, 1/16W | Resistor, 1K5, 0402, +/-1%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2524 | 2524
|  | Internal_Part_Number | MCD-00068 | MCD-00068
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00068 | MCD-00068
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402FR-071K5L | RC0402FR-071K5L
|  | Order_Code_Digikey | 311-1.50KLRCT-ND | 311-1.50KLRCT-ND
|  | Order_Code_Farnell | 9239251 | 9239251
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 1K5 | 1K5
R26 | Flash_Memory.SchDoc |  | Fitted | Fitted
|  | BMS_Part_Number | 9131590 | 9131590
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 10K, 0402, +/-1%, 1/16W | Resistor, 10K, 0402, +/-1%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2539 | 2539
|  | Internal_Part_Number | MCD-00053 | MCD-00053
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00053 | MCD-00053
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402FR-0710KL | RC0402FR-0710KL
|  | Order_Code_Digikey | 311-10.0KLRCT-ND | 311-10.0KLRCT-ND
|  | Order_Code_Farnell | 9239359 | 9239359
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 10K | 10K
R27 | Flash_Memory.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 33R, 0402, +/-1%, 1/16W | Resistor, 33R, 0402, +/-1%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2821 | 2821
|  | Internal_Part_Number | MCD-00455 | MCD-00455
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00455 | MCD-00455
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402FR-0733RL | RC0402FR-0733RL
|  | Order_Code_Digikey | 311-33.0LRCT-ND | 311-33.0LRCT-ND
|  | Order_Code_Farnell | 9239057 | 9239057
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 33R | 33R
R28 | Flash_Memory.SchDoc |  | Fitted | Fitted
|  | BMS_Part_Number | 9131590 | 9131590
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 10K, 0402, +/-1%, 1/16W | Resistor, 10K, 0402, +/-1%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2539 | 2539
|  | Internal_Part_Number | MCD-00053 | MCD-00053
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00053 | MCD-00053
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402FR-0710KL | RC0402FR-0710KL
|  | Order_Code_Digikey | 311-10.0KLRCT-ND | 311-10.0KLRCT-ND
|  | Order_Code_Farnell | 9239359 | 9239359
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 10K | 10K
R29 | Flash_Memory.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 33R, 0402, +/-1%, 1/16W | Resistor, 33R, 0402, +/-1%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2821 | 2821
|  | Internal_Part_Number | MCD-00455 | MCD-00455
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00455 | MCD-00455
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402FR-0733RL | RC0402FR-0733RL
|  | Order_Code_Digikey | 311-33.0LRCT-ND | 311-33.0LRCT-ND
|  | Order_Code_Farnell | 9239057 | 9239057
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 33R | 33R
R39 | Arduino.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 1K, 0402, +/-1%,1/16W | Resistor, 1K, 0402, +/-1%,1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2532 | 2532
|  | Internal_Part_Number | MCD-00061 | MCD-00061
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00061 | MCD-00061
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402FR-071KL | RC0402FR-071KL
|  | Order_Code_Digikey | 311-1.00KLRCT-ND | 311-1.00KLRCT-ND
|  | Order_Code_Farnell | 9239235 | 9239235
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 1K | 1K
R41 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 5K1, 0402, +/-1%, 1/16W | Resistor, 5K1, 0402, +/-1%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2944 | 2944
|  | Internal_Part_Number | MCD-00333 | MCD-00333
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00333 | MCD-00333
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402FR-075K1L | RC0402FR-075K1L
|  | Order_Code_Digikey | 311-5.10KLRCT-ND | 311-5.10KLRCT-ND
|  | Order_Code_Farnell | 1458805 | 1458805
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 5K1 | 5K1
R42 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 100R, 0402, +/- 1%, 1/16W | Resistor, 100R, 0402, +/- 1%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2527 | 2527
|  | Internal_Part_Number | MCD-00067 | MCD-00067
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00067 | MCD-00067
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402FR-07100RL | RC0402FR-07100RL
|  | Order_Code_Digikey | 311-100LRCT-ND | 311-100LRCT-ND
|  | Order_Code_Farnell | 9239111 | 9239111
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100R | 100R
R43 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 100K, 0402, +/-1%, 1/16W | Resistor, 100K, 0402, +/-1%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2533 | 2533
|  | Internal_Part_Number | MCD-00059 | MCD-00059
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00059 | MCD-00059
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402FR-07100KL | RC0402FR-07100KL
|  | Order_Code_Digikey | 311-100KLRTR-ND | 311-100KLRTR-ND
|  | Order_Code_Farnell | 2421891 | 2421891
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | Partial_Alternate_Internal_Part_Number | MCD-03301 | MCD-03301
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100K | 100K
R44 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 100K, 0402, +/-1%, 1/16W | Resistor, 100K, 0402, +/-1%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2533 | 2533
|  | Internal_Part_Number | MCD-00059 | MCD-00059
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00059 | MCD-00059
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402FR-07100KL | RC0402FR-07100KL
|  | Order_Code_Digikey | 311-100KLRTR-ND | 311-100KLRTR-ND
|  | Order_Code_Farnell | 2421891 | 2421891
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | Partial_Alternate_Internal_Part_Number | MCD-03301 | MCD-03301
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100K | 100K
R45 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 5K1, 0402, +/-1%, 1/16W | Resistor, 5K1, 0402, +/-1%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2944 | 2944
|  | Internal_Part_Number | MCD-00333 | MCD-00333
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00333 | MCD-00333
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402FR-075K1L | RC0402FR-075K1L
|  | Order_Code_Digikey | 311-5.10KLRCT-ND | 311-5.10KLRCT-ND
|  | Order_Code_Farnell | 1458805 | 1458805
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 5K1 | 5K1
R46 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 33R, 0402, +/-1%, 1/16W | Resistor, 33R, 0402, +/-1%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2821 | 2821
|  | Internal_Part_Number | MCD-00455 | MCD-00455
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00455 | MCD-00455
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402FR-0733RL | RC0402FR-0733RL
|  | Order_Code_Digikey | 311-33.0LRCT-ND | 311-33.0LRCT-ND
|  | Order_Code_Farnell | 9239057 | 9239057
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 33R | 33R
R47 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 0R, 0402, +/-5%, 1/16W | Resistor, 0R, 0402, +/-5%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2540 | 2540
|  | Internal_Part_Number | MCD-00052 | MCD-00052
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00052 | MCD-00052
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402JR-070RL | RC0402JR-070RL
|  | Order_Code_Digikey | 311-0.0JRCT-ND | 311-0.0JRCT-ND
|  | Order_Code_Farnell | 9232516RL | 9232516RL
|  | Order_Code_RS | 618-5804 | 618-5804
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 0R | 0R
R48 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 33R, 0402, +/-1%, 1/16W | Resistor, 33R, 0402, +/-1%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2821 | 2821
|  | Internal_Part_Number | MCD-00455 | MCD-00455
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00455 | MCD-00455
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402FR-0733RL | RC0402FR-0733RL
|  | Order_Code_Digikey | 311-33.0LRCT-ND | 311-33.0LRCT-ND
|  | Order_Code_Farnell | 9239057 | 9239057
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 33R | 33R
R49 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 33R, 0402, +/-1%, 1/16W | Resistor, 33R, 0402, +/-1%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2821 | 2821
|  | Internal_Part_Number | MCD-00455 | MCD-00455
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00455 | MCD-00455
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402FR-0733RL | RC0402FR-0733RL
|  | Order_Code_Digikey | 311-33.0LRCT-ND | 311-33.0LRCT-ND
|  | Order_Code_Farnell | 9239057 | 9239057
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 33R | 33R
R50 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 0R, 0402, +/-5%, 1/16W | Resistor, 0R, 0402, +/-5%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2540 | 2540
|  | Internal_Part_Number | MCD-00052 | MCD-00052
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00052 | MCD-00052
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402JR-070RL | RC0402JR-070RL
|  | Order_Code_Digikey | 311-0.0JRCT-ND | 311-0.0JRCT-ND
|  | Order_Code_Farnell | 9232516RL | 9232516RL
|  | Order_Code_RS | 618-5804 | 618-5804
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 0R | 0R
R51 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 33R, 0402, +/-1%, 1/16W | Resistor, 33R, 0402, +/-1%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2821 | 2821
|  | Internal_Part_Number | MCD-00455 | MCD-00455
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00455 | MCD-00455
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402FR-0733RL | RC0402FR-0733RL
|  | Order_Code_Digikey | 311-33.0LRCT-ND | 311-33.0LRCT-ND
|  | Order_Code_Farnell | 9239057 | 9239057
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 33R | 33R
R52 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 0R, 0402, +/-5%, 1/16W | Resistor, 0R, 0402, +/-5%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2540 | 2540
|  | Internal_Part_Number | MCD-00052 | MCD-00052
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00052 | MCD-00052
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402JR-070RL | RC0402JR-070RL
|  | Order_Code_Digikey | 311-0.0JRCT-ND | 311-0.0JRCT-ND
|  | Order_Code_Farnell | 9232516RL | 9232516RL
|  | Order_Code_RS | 618-5804 | 618-5804
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 0R | 0R
R53 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 3K, 0402, +/-1%, 1/16W | Resistor, 3K, 0402, +/-1%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2682 | 2682
|  | Internal_Part_Number | MCD-00185 | MCD-00185
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00185 | MCD-00185
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402FR-073KL | RC0402FR-073KL
|  | Order_Code_Digikey | 311-3KLRCT-ND | 311-3KLRCT-ND
|  | Order_Code_Farnell | 1458777 | 1458777
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 3K | 3K
R54 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | BMS_Part_Number | 9131590 | 9131590
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 10K, 0402, +/-1%, 1/16W | Resistor, 10K, 0402, +/-1%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2539 | 2539
|  | Internal_Part_Number | MCD-00053 | MCD-00053
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00053 | MCD-00053
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402FR-0710KL | RC0402FR-0710KL
|  | Order_Code_Digikey | 311-10.0KLRCT-ND | 311-10.0KLRCT-ND
|  | Order_Code_Farnell | 9239359 | 9239359
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 10K | 10K
R55 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | BMS_Part_Number | 9131590 | 9131590
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 10K, 0402, +/-1%, 1/16W | Resistor, 10K, 0402, +/-1%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2539 | 2539
|  | Internal_Part_Number | MCD-00053 | MCD-00053
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00053 | MCD-00053
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402FR-0710KL | RC0402FR-0710KL
|  | Order_Code_Digikey | 311-10.0KLRCT-ND | 311-10.0KLRCT-ND
|  | Order_Code_Farnell | 9239359 | 9239359
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 10K | 10K
R56 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | BMS_Part_Number | 9131590 | 9131590
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 10K, 0402, +/-1%, 1/16W | Resistor, 10K, 0402, +/-1%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2539 | 2539
|  | Internal_Part_Number | MCD-00053 | MCD-00053
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00053 | MCD-00053
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402FR-0710KL | RC0402FR-0710KL
|  | Order_Code_Digikey | 311-10.0KLRCT-ND | 311-10.0KLRCT-ND
|  | Order_Code_Farnell | 9239359 | 9239359
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 10K | 10K
R57 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 3K, 0402, +/-1%, 1/16W | Resistor, 3K, 0402, +/-1%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2682 | 2682
|  | Internal_Part_Number | MCD-00185 | MCD-00185
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00185 | MCD-00185
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402FR-073KL | RC0402FR-073KL
|  | Order_Code_Digikey | 311-3KLRCT-ND | 311-3KLRCT-ND
|  | Order_Code_Farnell | 1458777 | 1458777
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 3K | 3K
R58 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 5K1, 0402, +/-1%, 1/16W | Resistor, 5K1, 0402, +/-1%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2944 | 2944
|  | Internal_Part_Number | MCD-00333 | MCD-00333
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00333 | MCD-00333
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402FR-075K1L | RC0402FR-075K1L
|  | Order_Code_Digikey | 311-5.10KLRCT-ND | 311-5.10KLRCT-ND
|  | Order_Code_Farnell | 1458805 | 1458805
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 5K1 | 5K1
R59 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 1K8, 0402, +/-1%, 1/16W | Resistor, 1K8, 0402, +/-1%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2871 | 2871
|  | Internal_Part_Number | MCD-00409 | MCD-00409
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00409 | MCD-00409
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402FR-071K8L | RC0402FR-071K8L
|  | Order_Code_Digikey | 311-1.80KLRCT-ND | 311-1.80KLRCT-ND
|  | Order_Code_Farnell | 9239260 | 9239260
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 1K8 | 1K8
R60 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 1K3, 0402, +/-1%, 1/16W | Resistor, 1K3, 0402, +/-1%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2898 | 2898
|  | Internal_Part_Number | MCD-00381 | MCD-00381
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00381 | MCD-00381
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402FR-071K3L | RC0402FR-071K3L
|  | Order_Code_Digikey | YAG3036CT-ND | YAG3036CT-ND
|  | Order_Code_Farnell | 1799176 | 1799176
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 1K3 | 1K3
R61 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC0402_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC0402_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 3K9, 0402, +/-1%, 1/16W, +/-100ppm/°C | Resistor, 3K9, 0402, +/-1%, 1/16W, +/-100ppm/°C
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 4561 | 4561
|  | Internal_Part_Number | MCD-02455 | MCD-02455
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-02455 | MCD-02455
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402FR-073K9L | RC0402FR-073K9L
|  | Order_Code_Digikey | 311-3.90KLRTR-ND | 311-3.90KLRTR-ND
|  | Order_Code_Farnell | 9239308 | 9239308
|  | Order_Code_RS | 198-7783 | 198-7783
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 3K9 | 3K9
R62 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 5K1, 0402, +/-1%, 1/16W | Resistor, 5K1, 0402, +/-1%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2944 | 2944
|  | Internal_Part_Number | MCD-00333 | MCD-00333
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00333 | MCD-00333
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402FR-075K1L | RC0402FR-075K1L
|  | Order_Code_Digikey | 311-5.10KLRCT-ND | 311-5.10KLRCT-ND
|  | Order_Code_Farnell | 1458805 | 1458805
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 5K1 | 5K1
R63 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS | M | M
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 100K, 0402, +/-1%, 1/16W | Resistor, 100K, 0402, +/-1%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2533 | 2533
|  | Internal_Part_Number | MCD-00059 | MCD-00059
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00059 | MCD-00059
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402FR-07100KL | RC0402FR-07100KL
|  | Order_Code_Digikey | 311-100KLRTR-ND | 311-100KLRTR-ND
|  | Order_Code_Farnell | 2421891 | 2421891
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | Partial_Alternate_Internal_Part_Number | MCD-03301 | MCD-03301
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100K | 100K
R64 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | BMS_Part_Number | 9131590 | 9131590
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 10K, 0402, +/-1%, 1/16W | Resistor, 10K, 0402, +/-1%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2539 | 2539
|  | Internal_Part_Number | MCD-00053 | MCD-00053
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00053 | MCD-00053
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402FR-0710KL | RC0402FR-0710KL
|  | Order_Code_Digikey | 311-10.0KLRCT-ND | 311-10.0KLRCT-ND
|  | Order_Code_Farnell | 9239359 | 9239359
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 10K | 10K
R65 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RT_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RT_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 1K, 0402, +/-0.1%, 1/16W, +/-25ppm/°C | Resistor, 1K, 0402, +/-0.1%, 1/16W, +/-25ppm/°C
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 4771 | 4771
|  | Internal_Part_Number | MCD-02665 | MCD-02665
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-02665 | MCD-02665
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RT0402BRD071KL | RT0402BRD071KL
|  | Order_Code_Digikey | YAG1386TR-ND | YAG1386TR-ND
|  | Order_Code_Farnell | 3496475 | 3496475
|  | Order_Code_RS | 199-1298 | 199-1298
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Checked | Checked
|  | Value | 1K | 1K
R66 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RT_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RT_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 1K, 0402, +/-0.1%, 1/16W, +/-25ppm/°C | Resistor, 1K, 0402, +/-0.1%, 1/16W, +/-25ppm/°C
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 4771 | 4771
|  | Internal_Part_Number | MCD-02665 | MCD-02665
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-02665 | MCD-02665
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RT0402BRD071KL | RT0402BRD071KL
|  | Order_Code_Digikey | YAG1386TR-ND | YAG1386TR-ND
|  | Order_Code_Farnell | 3496475 | 3496475
|  | Order_Code_RS | 199-1298 | 199-1298
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Checked | Checked
|  | Value | 1K | 1K
R67 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 330R, 0402, +/-1%, 1/16W | Resistor, 330R, 0402, +/-1%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2529 | 2529
|  | Internal_Part_Number | MCD-00062 | MCD-00062
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00062 | MCD-00062
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402FR-07330RL | RC0402FR-07330RL
|  | Order_Code_Digikey | 311-330LRCT-ND | 311-330LRCT-ND
|  | Order_Code_Farnell | 9239170 | 9239170
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 330R | 330R
R68 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 330R, 0402, +/-1%, 1/16W | Resistor, 330R, 0402, +/-1%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2529 | 2529
|  | Internal_Part_Number | MCD-00062 | MCD-00062
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00062 | MCD-00062
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402FR-07330RL | RC0402FR-07330RL
|  | Order_Code_Digikey | 311-330LRCT-ND | 311-330LRCT-ND
|  | Order_Code_Farnell | 9239170 | 9239170
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 330R | 330R
R69 | STLINK-V3EC.SchDoc |  | Fitted | Not Fitted
|  | Alternate_EMS | M |
|  | Comment | Resistor |
|  | Component Kind | Standard |
|  | Component_Country_Of_Origin | China |
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series |
|  | Database Table Name | MCD_PARTS$ |
|  | Description | Resistor, 100K, 0402, +/-1%, 1/16W |
|  | Footprint | R0402 |
|  | Ibis Model |  |
|  | ID | 2533 |
|  | Internal_Part_Number | MCD-00059 |
|  | Library Name | MCD_PARTS_database.DbLib |
|  | Library Reference | MCD-00059 |
|  | Manufacturer | YAGEO |
|  | Manufacturer_Part_Number | RC0402FR-07100KL |
|  | Order_Code_Digikey | 311-100KLRTR-ND |
|  | Order_Code_Farnell | 2421891 |
|  | Order_Code_RS | N/A |
|  | Package | 0402 |
|  | Part_Preference | Recommended |
|  | Part_Type | Resistor |
|  | Partial_Alternate_Internal_Part_Number | MCD-03301 |
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES |
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released |
|  | Value | 100K |
R70 | STLINK-V3EC.SchDoc |  | Fitted | Not Fitted
|  | Alternate_EMS | M |
|  | Comment | Resistor |
|  | Component Kind | Standard |
|  | Component_Country_Of_Origin | China |
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series |
|  | Database Table Name | MCD_PARTS$ |
|  | Description | Resistor, 100K, 0402, +/-1%, 1/16W |
|  | Footprint | R0402 |
|  | Ibis Model |  |
|  | ID | 2533 |
|  | Internal_Part_Number | MCD-00059 |
|  | Library Name | MCD_PARTS_database.DbLib |
|  | Library Reference | MCD-00059 |
|  | Manufacturer | YAGEO |
|  | Manufacturer_Part_Number | RC0402FR-07100KL |
|  | Order_Code_Digikey | 311-100KLRTR-ND |
|  | Order_Code_Farnell | 2421891 |
|  | Order_Code_RS | N/A |
|  | Package | 0402 |
|  | Part_Preference | Recommended |
|  | Part_Type | Resistor |
|  | Partial_Alternate_Internal_Part_Number | MCD-03301 |
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES |
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released |
|  | Value | 100K |
R71 | External_Debug_Connectors.SchDoc |  | Fitted | Fitted
|  | Comment | Resistor | Resistor
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Resistor, 100R, 0402, +/- 1%, 1/16W | Resistor, 100R, 0402, +/- 1%, 1/16W
|  | Footprint | R0402 | R0402
|  | Ibis Model |  |
|  | ID | 2527 | 2527
|  | Internal_Part_Number | MCD-00067 | MCD-00067
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00067 | MCD-00067
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402FR-07100RL | RC0402FR-07100RL
|  | Order_Code_Digikey | 311-100LRCT-ND | 311-100LRCT-ND
|  | Order_Code_Farnell | 9239111 | 9239111
|  | Order_Code_RS | N/A | N/A
|  | Package | 0402 | 0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Resistor | Resistor
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 100R | 100R
SB1 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Comment | SB_ON | SB_ON
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Resistors/Yageo_Resistor_RC0402-series | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Resistors/Yageo_Resistor_RC0402-series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Solder Bridge 0402 ON | Solder Bridge 0402 ON
|  | Footprint | SOLDER-BRIDGE_R0402-0R | SOLDER-BRIDGE_R0402-0R
|  | Ibis Model |  |
|  | ID | 3718 | 3718
|  | Internal_Part_Number | MCD-01618 | MCD-01618
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01618 | MCD-01618
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402JR-070RL | RC0402JR-070RL
|  | Order_Code_Digikey | 311-0.0JRTR-ND | 311-0.0JRTR-ND
|  | Order_Code_Farnell | 2363467 | 2363467
|  | Order_Code_RS | 618-5804 | 618-5804
|  | Package | SB0402 | SB0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Misc | Misc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
SB2 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Comment | SB_ON | SB_ON
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Resistors/Yageo_Resistor_RC0402-series | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Resistors/Yageo_Resistor_RC0402-series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Solder Bridge 0402 ON | Solder Bridge 0402 ON
|  | Footprint | SOLDER-BRIDGE_R0402-0R | SOLDER-BRIDGE_R0402-0R
|  | Ibis Model |  |
|  | ID | 3718 | 3718
|  | Internal_Part_Number | MCD-01618 | MCD-01618
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01618 | MCD-01618
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402JR-070RL | RC0402JR-070RL
|  | Order_Code_Digikey | 311-0.0JRTR-ND | 311-0.0JRTR-ND
|  | Order_Code_Farnell | 2363467 | 2363467
|  | Order_Code_RS | 618-5804 | 618-5804
|  | Package | SB0402 | SB0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Misc | Misc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
SB3 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Comment | SB_ON | SB_ON
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Resistors/Yageo_Resistor_RC0402-series | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Resistors/Yageo_Resistor_RC0402-series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Solder Bridge 0402 ON | Solder Bridge 0402 ON
|  | Footprint | SOLDER-BRIDGE_R0402-0R | SOLDER-BRIDGE_R0402-0R
|  | Ibis Model |  |
|  | ID | 3718 | 3718
|  | Internal_Part_Number | MCD-01618 | MCD-01618
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01618 | MCD-01618
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402JR-070RL | RC0402JR-070RL
|  | Order_Code_Digikey | 311-0.0JRTR-ND | 311-0.0JRTR-ND
|  | Order_Code_Farnell | 2363467 | 2363467
|  | Order_Code_RS | 618-5804 | 618-5804
|  | Package | SB0402 | SB0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Misc | Misc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
SB4 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Comment | SB_ON | SB_ON
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Resistors/Yageo_Resistor_RC0402-series | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Resistors/Yageo_Resistor_RC0402-series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Solder Bridge 0402 ON | Solder Bridge 0402 ON
|  | Footprint | SOLDER-BRIDGE_R0402-0R | SOLDER-BRIDGE_R0402-0R
|  | Ibis Model |  |
|  | ID | 3718 | 3718
|  | Internal_Part_Number | MCD-01618 | MCD-01618
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01618 | MCD-01618
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402JR-070RL | RC0402JR-070RL
|  | Order_Code_Digikey | 311-0.0JRTR-ND | 311-0.0JRTR-ND
|  | Order_Code_Farnell | 2363467 | 2363467
|  | Order_Code_RS | 618-5804 | 618-5804
|  | Package | SB0402 | SB0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Misc | Misc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
SB5 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Comment | SB_ON | SB_ON
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Resistors/Yageo_Resistor_RC0402-series | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Resistors/Yageo_Resistor_RC0402-series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Solder Bridge 0402 ON | Solder Bridge 0402 ON
|  | Footprint | SOLDER-BRIDGE_R0402-0R | SOLDER-BRIDGE_R0402-0R
|  | Ibis Model |  |
|  | ID | 3718 | 3718
|  | Internal_Part_Number | MCD-01618 | MCD-01618
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01618 | MCD-01618
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402JR-070RL | RC0402JR-070RL
|  | Order_Code_Digikey | 311-0.0JRTR-ND | 311-0.0JRTR-ND
|  | Order_Code_Farnell | 2363467 | 2363467
|  | Order_Code_RS | 618-5804 | 618-5804
|  | Package | SB0402 | SB0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Misc | Misc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
SB6 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Comment | SB_ON | SB_ON
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Resistors/Yageo_Resistor_RC0402-series | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Resistors/Yageo_Resistor_RC0402-series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Solder Bridge 0402 ON | Solder Bridge 0402 ON
|  | Footprint | SOLDER-BRIDGE_R0402-0R | SOLDER-BRIDGE_R0402-0R
|  | Ibis Model |  |
|  | ID | 3718 | 3718
|  | Internal_Part_Number | MCD-01618 | MCD-01618
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01618 | MCD-01618
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402JR-070RL | RC0402JR-070RL
|  | Order_Code_Digikey | 311-0.0JRTR-ND | 311-0.0JRTR-ND
|  | Order_Code_Farnell | 2363467 | 2363467
|  | Order_Code_RS | 618-5804 | 618-5804
|  | Package | SB0402 | SB0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Misc | Misc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
SB7 | Display.SchDoc |  | Fitted | Fitted
|  | Comment | SB_ON | SB_ON
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Resistors/Yageo_Resistor_RC0402-series | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Resistors/Yageo_Resistor_RC0402-series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Solder Bridge 0402 ON | Solder Bridge 0402 ON
|  | Footprint | SOLDER-BRIDGE_R0402-0R | SOLDER-BRIDGE_R0402-0R
|  | Ibis Model |  |
|  | ID | 3718 | 3718
|  | Internal_Part_Number | MCD-01618 | MCD-01618
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01618 | MCD-01618
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402JR-070RL | RC0402JR-070RL
|  | Order_Code_Digikey | 311-0.0JRTR-ND | 311-0.0JRTR-ND
|  | Order_Code_Farnell | 2363467 | 2363467
|  | Order_Code_RS | 618-5804 | 618-5804
|  | Package | SB0402 | SB0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Misc | Misc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
SB8 | Board_Power.SchDoc |  | Fitted | Fitted
|  | Comment | SB_ON | SB_ON
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Resistors/Yageo_Resistor_RC0402-series | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Resistors/Yageo_Resistor_RC0402-series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Solder Bridge 0402 ON | Solder Bridge 0402 ON
|  | Footprint | SOLDER-BRIDGE_R0402-0R | SOLDER-BRIDGE_R0402-0R
|  | Ibis Model |  |
|  | ID | 3718 | 3718
|  | Internal_Part_Number | MCD-01618 | MCD-01618
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01618 | MCD-01618
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402JR-070RL | RC0402JR-070RL
|  | Order_Code_Digikey | 311-0.0JRTR-ND | 311-0.0JRTR-ND
|  | Order_Code_Farnell | 2363467 | 2363467
|  | Order_Code_RS | 618-5804 | 618-5804
|  | Package | SB0402 | SB0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Misc | Misc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
SB9 | Display.SchDoc |  | Fitted | Fitted
|  | Comment | SB_ON | SB_ON
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Resistors/Yageo_Resistor_RC0402-series | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Resistors/Yageo_Resistor_RC0402-series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Solder Bridge 0402 ON | Solder Bridge 0402 ON
|  | Footprint | SOLDER-BRIDGE_R0402-0R | SOLDER-BRIDGE_R0402-0R
|  | Ibis Model |  |
|  | ID | 3718 | 3718
|  | Internal_Part_Number | MCD-01618 | MCD-01618
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01618 | MCD-01618
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402JR-070RL | RC0402JR-070RL
|  | Order_Code_Digikey | 311-0.0JRTR-ND | 311-0.0JRTR-ND
|  | Order_Code_Farnell | 2363467 | 2363467
|  | Order_Code_RS | 618-5804 | 618-5804
|  | Package | SB0402 | SB0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Misc | Misc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
SB10 | Flash_Memory.SchDoc |  | Fitted | Fitted
|  | Comment | SB_ON | SB_ON
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Resistors/Yageo_Resistor_RC0402-series | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Resistors/Yageo_Resistor_RC0402-series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Solder Bridge 0402 ON | Solder Bridge 0402 ON
|  | Footprint | SOLDER-BRIDGE_R0402-0R | SOLDER-BRIDGE_R0402-0R
|  | Ibis Model |  |
|  | ID | 3718 | 3718
|  | Internal_Part_Number | MCD-01618 | MCD-01618
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01618 | MCD-01618
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402JR-070RL | RC0402JR-070RL
|  | Order_Code_Digikey | 311-0.0JRTR-ND | 311-0.0JRTR-ND
|  | Order_Code_Farnell | 2363467 | 2363467
|  | Order_Code_RS | 618-5804 | 618-5804
|  | Package | SB0402 | SB0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Misc | Misc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
SB11 | MCU_System.SchDoc |  | Fitted | Fitted
|  | Comment | SB_ON | SB_ON
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Resistors/Yageo_Resistor_RC0402-series | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Resistors/Yageo_Resistor_RC0402-series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Solder Bridge 0402 ON | Solder Bridge 0402 ON
|  | Footprint | SOLDER-BRIDGE_R0402-0R | SOLDER-BRIDGE_R0402-0R
|  | Ibis Model |  |
|  | ID | 3718 | 3718
|  | Internal_Part_Number | MCD-01618 | MCD-01618
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01618 | MCD-01618
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402JR-070RL | RC0402JR-070RL
|  | Order_Code_Digikey | 311-0.0JRTR-ND | 311-0.0JRTR-ND
|  | Order_Code_Farnell | 2363467 | 2363467
|  | Order_Code_RS | 618-5804 | 618-5804
|  | Package | SB0402 | SB0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Misc | Misc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
SB12 | MCU_Power.SchDoc |  | Fitted | Not Fitted
|  | Comment | SB_ON |
|  | Component Kind | Standard |
|  | Component_Country_Of_Origin | China |
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Resistors/Yageo_Resistor_RC0402-series |
|  | Database Table Name | MCD_PARTS$ |
|  | Description | Solder Bridge 0402 ON |
|  | Footprint | SOLDER-BRIDGE_R0402-0R |
|  | Ibis Model |  |
|  | ID | 3718 |
|  | Internal_Part_Number | MCD-01618 |
|  | Library Name | MCD_PARTS_database.DbLib |
|  | Library Reference | MCD-01618 |
|  | Manufacturer | YAGEO |
|  | Manufacturer_Part_Number | RC0402JR-070RL |
|  | Order_Code_Digikey | 311-0.0JRTR-ND |
|  | Order_Code_Farnell | 2363467 |
|  | Order_Code_RS | 618-5804 |
|  | Package | SB0402 |
|  | Part_Preference | Recommended |
|  | Part_Type | Misc |
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES |
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released |
SB13 | External_Debug_Connectors.SchDoc |  | Fitted | Fitted
|  | Comment | SB_ON | SB_ON
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Resistors/Yageo_Resistor_RC0402-series | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Resistors/Yageo_Resistor_RC0402-series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Solder Bridge 0402 ON | Solder Bridge 0402 ON
|  | Footprint | SOLDER-BRIDGE_R0402-0R | SOLDER-BRIDGE_R0402-0R
|  | Ibis Model |  |
|  | ID | 3718 | 3718
|  | Internal_Part_Number | MCD-01618 | MCD-01618
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01618 | MCD-01618
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402JR-070RL | RC0402JR-070RL
|  | Order_Code_Digikey | 311-0.0JRTR-ND | 311-0.0JRTR-ND
|  | Order_Code_Farnell | 2363467 | 2363467
|  | Order_Code_RS | 618-5804 | 618-5804
|  | Package | SB0402 | SB0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Misc | Misc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
SB14 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Comment | SB_ON | SB_ON
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Resistors/Yageo_Resistor_RC0402-series | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Resistors/Yageo_Resistor_RC0402-series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Solder Bridge 0402 ON | Solder Bridge 0402 ON
|  | Footprint | SOLDER-BRIDGE_R0402-0R | SOLDER-BRIDGE_R0402-0R
|  | Ibis Model |  |
|  | ID | 3718 | 3718
|  | Internal_Part_Number | MCD-01618 | MCD-01618
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01618 | MCD-01618
|  | Manufacturer | YAGEO | YAGEO
|  | Manufacturer_Part_Number | RC0402JR-070RL | RC0402JR-070RL
|  | Order_Code_Digikey | 311-0.0JRTR-ND | 311-0.0JRTR-ND
|  | Order_Code_Farnell | 2363467 | 2363467
|  | Order_Code_RS | 618-5804 | 618-5804
|  | Package | SB0402 | SB0402
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Misc | Misc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
SW1 | MCU_System.SchDoc |  | Fitted | Fitted
|  | Comment | SW_MECA_1K2 | SW_MECA_1K2
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | Switzerland | Switzerland
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Misc/EAO_SWITCH_09.03290.01 | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Misc/EAO_SWITCH_09.03290.01
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Mechanical Slide Switches 1K2 BLK ACT GOLD STRT MNT | Mechanical Slide Switches 1K2 BLK ACT GOLD STRT MNT
|  | Footprint | SWI_EAO_09-03290-01_EXTENDED_STRAIGHT_BLACK | SWI_EAO_09-03290-01_EXTENDED_STRAIGHT_BLACK
|  | Ibis Model |  |
|  | ID | 3181 | 3181
|  | Internal_Part_Number | MCD-00566 | MCD-00566
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00566 | MCD-00566
|  | Manufacturer | EAO | EAO
|  | Manufacturer_Part_Number | 09.03290.01 | 09.03290.01
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Misc | Misc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | Mechanical Slide Switch 1K2 | Mechanical Slide Switch 1K2
TP1 | Flash_Memory.SchDoc |  | Fitted | Fitted
|  | Comment | Test Point | Test Point
|  | Component Kind | Standard (No BOM) | Standard (No BOM)
|  | ComponentLink1URL | http://na | http://na
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Test Point 1mm | Test Point 1mm
|  | Footprint | TP_SMD_1MM | TP_SMD_1MM
|  | Ibis Model |  |
|  | ID | 2518 | 2518
|  | Internal_Part_Number | MCD-00074 | MCD-00074
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00074 | MCD-00074
|  | Manufacturer | N/A | N/A
|  | Manufacturer_Part_Number | N/A | N/A
|  | Order_Code_Digikey | N/A | N/A
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Misc | Misc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
TP2 | Flash_Memory.SchDoc |  | Fitted | Fitted
|  | Comment | Test Point | Test Point
|  | Component Kind | Standard (No BOM) | Standard (No BOM)
|  | ComponentLink1URL | http://na | http://na
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Test Point 1mm | Test Point 1mm
|  | Footprint | TP_SMD_1MM | TP_SMD_1MM
|  | Ibis Model |  |
|  | ID | 2518 | 2518
|  | Internal_Part_Number | MCD-00074 | MCD-00074
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00074 | MCD-00074
|  | Manufacturer | N/A | N/A
|  | Manufacturer_Part_Number | N/A | N/A
|  | Order_Code_Digikey | N/A | N/A
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Misc | Misc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
TP3 | Flash_Memory.SchDoc |  | Fitted | Fitted
|  | Comment | Test Point | Test Point
|  | Component Kind | Standard (No BOM) | Standard (No BOM)
|  | ComponentLink1URL | http://na | http://na
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Test Point 1mm | Test Point 1mm
|  | Footprint | TP_SMD_1MM | TP_SMD_1MM
|  | Ibis Model |  |
|  | ID | 2518 | 2518
|  | Internal_Part_Number | MCD-00074 | MCD-00074
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00074 | MCD-00074
|  | Manufacturer | N/A | N/A
|  | Manufacturer_Part_Number | N/A | N/A
|  | Order_Code_Digikey | N/A | N/A
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Misc | Misc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
TP4 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | Test Point | Test Point
|  | Component Kind | Standard (No BOM) | Standard (No BOM)
|  | ComponentLink1URL | http://na | http://na
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Test Point 1mm | Test Point 1mm
|  | Footprint | TP_SMD_1MM | TP_SMD_1MM
|  | Ibis Model |  |
|  | ID | 2518 | 2518
|  | Internal_Part_Number | MCD-00074 | MCD-00074
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00074 | MCD-00074
|  | Manufacturer | N/A | N/A
|  | Manufacturer_Part_Number | N/A | N/A
|  | Order_Code_Digikey | N/A | N/A
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Misc | Misc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
TP5 | Flash_Memory.SchDoc |  | Fitted | Fitted
|  | Comment | Test Point | Test Point
|  | Component Kind | Standard (No BOM) | Standard (No BOM)
|  | ComponentLink1URL | http://na | http://na
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Test Point 1mm | Test Point 1mm
|  | Footprint | TP_SMD_1MM | TP_SMD_1MM
|  | Ibis Model |  |
|  | ID | 2518 | 2518
|  | Internal_Part_Number | MCD-00074 | MCD-00074
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00074 | MCD-00074
|  | Manufacturer | N/A | N/A
|  | Manufacturer_Part_Number | N/A | N/A
|  | Order_Code_Digikey | N/A | N/A
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Misc | Misc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
TP6 | Flash_Memory.SchDoc |  | Fitted | Fitted
|  | Comment | Test Point | Test Point
|  | Component Kind | Standard (No BOM) | Standard (No BOM)
|  | ComponentLink1URL | http://na | http://na
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Test Point 1mm | Test Point 1mm
|  | Footprint | TP_SMD_1MM | TP_SMD_1MM
|  | Ibis Model |  |
|  | ID | 2518 | 2518
|  | Internal_Part_Number | MCD-00074 | MCD-00074
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00074 | MCD-00074
|  | Manufacturer | N/A | N/A
|  | Manufacturer_Part_Number | N/A | N/A
|  | Order_Code_Digikey | N/A | N/A
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Misc | Misc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
TP7 | Flash_Memory.SchDoc |  | Fitted | Fitted
|  | Comment | Test Point | Test Point
|  | Component Kind | Standard (No BOM) | Standard (No BOM)
|  | ComponentLink1URL | http://na | http://na
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Test Point 1mm | Test Point 1mm
|  | Footprint | TP_SMD_1MM | TP_SMD_1MM
|  | Ibis Model |  |
|  | ID | 2518 | 2518
|  | Internal_Part_Number | MCD-00074 | MCD-00074
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00074 | MCD-00074
|  | Manufacturer | N/A | N/A
|  | Manufacturer_Part_Number | N/A | N/A
|  | Order_Code_Digikey | N/A | N/A
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Misc | Misc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
TP8 | Flash_Memory.SchDoc |  | Fitted | Fitted
|  | Comment | Test Point | Test Point
|  | Component Kind | Standard (No BOM) | Standard (No BOM)
|  | ComponentLink1URL | http://na | http://na
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Test Point 1mm | Test Point 1mm
|  | Footprint | TP_SMD_1MM | TP_SMD_1MM
|  | Ibis Model |  |
|  | ID | 2518 | 2518
|  | Internal_Part_Number | MCD-00074 | MCD-00074
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00074 | MCD-00074
|  | Manufacturer | N/A | N/A
|  | Manufacturer_Part_Number | N/A | N/A
|  | Order_Code_Digikey | N/A | N/A
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Misc | Misc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
TP9 | Flash_Memory.SchDoc |  | Fitted | Fitted
|  | Comment | Test Point | Test Point
|  | Component Kind | Standard (No BOM) | Standard (No BOM)
|  | ComponentLink1URL | http://na | http://na
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Test Point 1mm | Test Point 1mm
|  | Footprint | TP_SMD_1MM | TP_SMD_1MM
|  | Ibis Model |  |
|  | ID | 2518 | 2518
|  | Internal_Part_Number | MCD-00074 | MCD-00074
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00074 | MCD-00074
|  | Manufacturer | N/A | N/A
|  | Manufacturer_Part_Number | N/A | N/A
|  | Order_Code_Digikey | N/A | N/A
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Misc | Misc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
TP10 | Flash_Memory.SchDoc |  | Fitted | Fitted
|  | Comment | Test Point | Test Point
|  | Component Kind | Standard (No BOM) | Standard (No BOM)
|  | ComponentLink1URL | http://na | http://na
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Test Point 1mm | Test Point 1mm
|  | Footprint | TP_SMD_1MM | TP_SMD_1MM
|  | Ibis Model |  |
|  | ID | 2518 | 2518
|  | Internal_Part_Number | MCD-00074 | MCD-00074
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00074 | MCD-00074
|  | Manufacturer | N/A | N/A
|  | Manufacturer_Part_Number | N/A | N/A
|  | Order_Code_Digikey | N/A | N/A
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Misc | Misc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
TP11 | Flash_Memory.SchDoc |  | Fitted | Fitted
|  | Comment | Test Point | Test Point
|  | Component Kind | Standard (No BOM) | Standard (No BOM)
|  | ComponentLink1URL | http://na | http://na
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Test Point 1mm | Test Point 1mm
|  | Footprint | TP_SMD_1MM | TP_SMD_1MM
|  | Ibis Model |  |
|  | ID | 2518 | 2518
|  | Internal_Part_Number | MCD-00074 | MCD-00074
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00074 | MCD-00074
|  | Manufacturer | N/A | N/A
|  | Manufacturer_Part_Number | N/A | N/A
|  | Order_Code_Digikey | N/A | N/A
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Misc | Misc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
TP12 | Flash_Memory.SchDoc |  | Fitted | Fitted
|  | Comment | Test Point | Test Point
|  | Component Kind | Standard (No BOM) | Standard (No BOM)
|  | ComponentLink1URL | http://na | http://na
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Test Point 1mm | Test Point 1mm
|  | Footprint | TP_SMD_1MM | TP_SMD_1MM
|  | Ibis Model |  |
|  | ID | 2518 | 2518
|  | Internal_Part_Number | MCD-00074 | MCD-00074
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00074 | MCD-00074
|  | Manufacturer | N/A | N/A
|  | Manufacturer_Part_Number | N/A | N/A
|  | Order_Code_Digikey | N/A | N/A
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Misc | Misc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
TP13 | Flash_Memory.SchDoc |  | Fitted | Fitted
|  | Comment | Test Point | Test Point
|  | Component Kind | Standard (No BOM) | Standard (No BOM)
|  | ComponentLink1URL | http://na | http://na
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Test Point 1mm | Test Point 1mm
|  | Footprint | TP_SMD_1MM | TP_SMD_1MM
|  | Ibis Model |  |
|  | ID | 2518 | 2518
|  | Internal_Part_Number | MCD-00074 | MCD-00074
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00074 | MCD-00074
|  | Manufacturer | N/A | N/A
|  | Manufacturer_Part_Number | N/A | N/A
|  | Order_Code_Digikey | N/A | N/A
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Misc | Misc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
U1 | MCU_System.SchDoc |  | Fitted | Fitted
|  | BMS_Part_Number | 9151132 | 9151132
|  | Comment | ESD-TRANSIL | ESD-TRANSIL
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Diodes/STM_ESD_ESDALC6V1-1U2 | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Diodes/STM_ESD_ESDALC6V1-1U2
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | ESD protection 6V1 | ESD protection 6V1
|  | Footprint | ESD_ST0201 | ESD_ST0201
|  | Ibis Model |  |
|  | ID | 2696 | 2696
|  | Internal_Part_Number | MCD-00170 | MCD-00170
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00170 | MCD-00170
|  | Manufacturer | STMICROELECTRONICS | STMICROELECTRONICS
|  | Manufacturer_HQ_COO | EU | EU
|  | Manufacturer_Part_Number | ESDALC6V1-1U2 | ESDALC6V1-1U2
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Diode | Diode
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | ESDALC6V1-1U2 | ESDALC6V1-1U2
U2 | MCU_Power.SchDoc |  | Fitted | Fitted
|  | Comment | STM32U5G9ZJT6Q | STM32U5G9ZJT6Q
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | Unknown | Unknown
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/IC/STMICROELECTRONICS_STM32U5F9ZJT6Q | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/IC/STMICROELECTRONICS_STM32U5F9ZJT6Q
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Ultra-low-power microcontroller, Arm Cortex M33 - Up to 160 MHz. | Ultra-low-power microcontroller, Arm Cortex M33 - Up to 160 MHz.
|  | Footprint | ICC_LQFP144_20X20_P050_SOCKET_YAMAICHI_IC149-144-145-B5_NM | ICC_LQFP144_20X20_P050_SOCKET_YAMAICHI_IC149-144-145-B5_NM
|  | Ibis Model |  |
|  | ID | 5389 | 5389
|  | Internal_Part_Number | MCD-03273 | MCD-03273
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-03273 | MCD-03273
|  | Manufacturer | STMICROELECTRONICS | STMICROELECTRONICS
|  | Manufacturer_Part_Number | STM32U5G9ZJT6Q | STM32U5G9ZJT6Q
|  | Order_Code_Digikey | N/A | N/A
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Package | LQFP144 | LQFP144
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | IC | IC
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Checked | Checked
|  | Value | STM32U5G9ZJT6Q | STM32U5G9ZJT6Q
U3 | USB_TYPE_C .SchDoc |  | Fitted | Fitted
|  | BMS_Part_Number | 9151145 | 9151145
|  | Comment | TCPP01-M12 | TCPP01-M12
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | Malaysia | Malaysia
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/IC/STM_UCPD_Protection_TCPP01-M12 | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/IC/STM_UCPD_Protection_TCPP01-M12
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | USB Type-C Port Protection for USB Power Delivery, PPS compliant | USB Type-C Port Protection for USB Power Delivery, PPS compliant
|  | Footprint | ICC_QFN12L-EPAD_3X3_P050 | ICC_QFN12L-EPAD_3X3_P050
|  | Ibis Model |  |
|  | ID | 3909 | 3909
|  | Internal_Part_Number | MCD-01809 | MCD-01809
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01809 | MCD-01809
|  | Manufacturer | STMICROELECTRONICS | STMICROELECTRONICS
|  | Manufacturer_HQ_COO | EU | EU
|  | Manufacturer_Part_Number | TCPP01-M12 | TCPP01-M12
|  | Package | QFN-12L | QFN-12L
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | IC | IC
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | TCPP01-M12 | TCPP01-M12
U4 | USB_TYPE_C .SchDoc |  | Fitted | Fitted
|  | BMS_Part_Number | 9179045 | 9179045
|  | Comment | ESD-TRANSIL | ESD-TRANSIL
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Diodes/STM_ESD_ESDA25P35-1U1M | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Diodes/STM_ESD_ESDA25P35-1U1M
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | High power Transient voltage suppressor:25V/35A EOS and ESD transients protection. | High power Transient voltage suppressor:25V/35A EOS and ESD transients protection.
|  | Footprint | ESD_QFN1610_2N_1K_2A | ESD_QFN1610_2N_1K_2A
|  | Ibis Model |  |
|  | ID | 3289 | 3289
|  | Internal_Part_Number | MCD-01207 | MCD-01207
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01207 | MCD-01207
|  | Manufacturer | STMICROELECTRONICS | STMICROELECTRONICS
|  | Manufacturer_HQ_COO | EU | EU
|  | Manufacturer_Part_Number | ESDA25P35-1U1M | ESDA25P35-1U1M
|  | Package | QFN1610 | QFN1610
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Diode | Diode
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | ESDA25P35-1U1M | ESDA25P35-1U1M
U5 | USB_TYPE_C .SchDoc |  | Fitted | Fitted
|  | BMS_Part_Number | 9151138 | 9151138
|  | Comment | ECMF02-2AMX6 | ECMF02-2AMX6
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Diodes/STM_ESD_ECMF02-2AMX6 | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Diodes/STM_ESD_ECMF02-2AMX6
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Common mode filter with ESD protection for USB 2.0 interface | Common mode filter with ESD protection for USB 2.0 interface
|  | Footprint | ESD_QFN-6L_1P7X1P5_P050 | ESD_QFN-6L_1P7X1P5_P050
|  | Ibis Model |  |
|  | ID | 3094 | 3094
|  | Internal_Part_Number | MCD-00649 | MCD-00649
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00649 | MCD-00649
|  | Manufacturer | STMICROELECTRONICS | STMICROELECTRONICS
|  | Manufacturer_HQ_COO | EU | EU
|  | Manufacturer_Part_Number | ECMF02-2AMX6 | ECMF02-2AMX6
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Diode | Diode
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | ECMF02-2AMX6 | ECMF02-2AMX6
U6 | User_Interface.SchDoc |  | Fitted | Fitted
|  | BMS_Part_Number | 9151132 | 9151132
|  | Comment | ESD-TRANSIL | ESD-TRANSIL
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Diodes/STM_ESD_ESDALC6V1-1U2 | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Diodes/STM_ESD_ESDALC6V1-1U2
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | ESD protection 6V1 | ESD protection 6V1
|  | Footprint | ESD_ST0201 | ESD_ST0201
|  | Ibis Model |  |
|  | ID | 2696 | 2696
|  | Internal_Part_Number | MCD-00170 | MCD-00170
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00170 | MCD-00170
|  | Manufacturer | STMICROELECTRONICS | STMICROELECTRONICS
|  | Manufacturer_HQ_COO | EU | EU
|  | Manufacturer_Part_Number | ESDALC6V1-1U2 | ESDALC6V1-1U2
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Diode | Diode
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | ESDALC6V1-1U2 | ESDALC6V1-1U2
U7 | Board_Power.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS |  |
|  | BMS_Part_Number | 9176246 | 9176246
|  | Comment | ST1L05CPU33R | ST1L05CPU33R
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | Malaysia | Malaysia
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/IC/STM_LDO_ST1L05CPU33R | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/IC/STM_LDO_ST1L05CPU33R
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | LDO, 3.3V, 1.3A, Very low quiescent current BiCMOS voltage regulator | LDO, 3.3V, 1.3A, Very low quiescent current BiCMOS voltage regulator
|  | Footprint | ICC_DFN6-EPAD_3X3_P095 | ICC_DFN6-EPAD_3X3_P095
|  | Full_Alternate_Internal_Part_Number |  |
|  | Ibis Model |  |
|  | ID | 2998 | 2998
|  | Internal_Part_Number | MCD-01025 | MCD-01025
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01025 | MCD-01025
|  | Manufacturer | STMICROELECTRONICS | STMICROELECTRONICS
|  | Manufacturer_HQ_COO | EU | EU
|  | Manufacturer_Part_Number | ST1L05CPU33R | ST1L05CPU33R
|  | Order_Code_Digikey |  |
|  | Order_Code_Farnell |  |
|  | Order_Code_RS |  |
|  | Package | DFN6-3x3 | DFN6-3x3
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | IC | IC
|  | Partial_Alternate_Internal_Part_Number |  |
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | ST1L05CPU33R 3.3V 1.3A | ST1L05CPU33R 3.3V 1.3A
U8 | Board_Power.SchDoc |  | Fitted | Fitted
|  | BMS_Part_Number | 9179046 | 9179046
|  | Comment | ESD-TRANSIL | ESD-TRANSIL
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Diodes/STM_ESD_ESDA7P120-1U1M | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Diodes/STM_ESD_ESDA7P120-1U1M
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | High power transient voltage suppressor | High power transient voltage suppressor
|  | Footprint | ESD_QFN1610_2N_1K_2A | ESD_QFN1610_2N_1K_2A
|  | Ibis Model |  |
|  | ID | 2997 | 2997
|  | Internal_Part_Number | MCD-01026 | MCD-01026
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01026 | MCD-01026
|  | Manufacturer | STMICROELECTRONICS | STMICROELECTRONICS
|  | Manufacturer_HQ_COO | EU | EU
|  | Manufacturer_Part_Number | ESDA7P120-1U1M | ESDA7P120-1U1M
|  | Package | QFN1610 | QFN1610
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Diode | Diode
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | ESDA7P120-1U1M | ESDA7P120-1U1M
U9 | Arduino.SchDoc |  | Fitted | Fitted
|  | BMS_Part_Number | 9176133 | 9176133
|  | Comment | LD1117S50TR | LD1117S50TR
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/IC/STM_LDO_LD1117 | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/IC/STM_LDO_LD1117
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | IC REG LDO 5V 0.8A SOT223 | IC REG LDO 5V 0.8A SOT223
|  | Footprint | REG_SOT223-TAB | REG_SOT223-TAB
|  | Ibis Model |  |
|  | ID | 2503 | 2503
|  | Internal_Part_Number | MCD-00088 | MCD-00088
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00088 | MCD-00088
|  | Manufacturer | STMICROELECTRONICS | STMICROELECTRONICS
|  | Manufacturer_HQ_COO | EU | EU
|  | Manufacturer_Part_Number | LD1117S50TR | LD1117S50TR
|  | Package | SOT-223 | SOT-223
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | IC | IC
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | LD1117S50TR | LD1117S50TR
U11 | Flash_Memory.SchDoc |  | Fitted | Fitted
|  | Alternate_EMS |  |
|  | BMS_Part_Number |  |
|  | Comment | MX66LM1G45GXDI00 | MX66LM1G45GXDI00
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | Taiwan° | Taiwan°
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/IC/MACRONIX_MX66LM1G45GXDI00 | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/IC/MACRONIX_MX66LM1G45GXDI00
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Memory, Octo-SPI-NOR, 1Gb, 133MHz, 3V, DTR, SFDP, BGA24 | Memory, Octo-SPI-NOR, 1Gb, 133MHz, 3V, DTR, SFDP, BGA24
|  | Footprint | ICC_BGA24_5X5-BALL-ARRAY_6X8_P1 | ICC_BGA24_5X5-BALL-ARRAY_6X8_P1
|  | Full_Alternate_Internal_Part_Number |  |
|  | Ibis Model |  |
|  | ID | 5125 | 5125
|  | Internal_Part_Number | MCD-03009 | MCD-03009
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-03009 | MCD-03009
|  | Manufacturer | MACRONIX | MACRONIX
|  | Manufacturer_HQ_COO |  |
|  | Manufacturer_Part_Number | MX66LM1G45GXDI00 | MX66LM1G45GXDI00
|  | Order_Code_Digikey | 1092-1257-ND | 1092-1257-ND
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Package | BGA24 | BGA24
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | IC | IC
|  | Partial_Alternate_Internal_Part_Number |  |
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Checked | Checked
|  | Value | MX66LM1G45GXDI00 | MX66LM1G45GXDI00
U13 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | BMS_Part_Number | 9175300 | 9175300
|  | Comment | STLINK-V3EC | STLINK-V3EC
|  | Component Kind | Standard | Standard
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/IC/STMICROELECTRONICS_STM32F723IEK6 | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/IC/STMICROELECTRONICS_STM32F723IEK6
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | MCU, Arm Cortex-M7 32-bit MCU, 512KB Flash, 276KB RAM, With Crypto | MCU, Arm Cortex-M7 32-bit MCU, 512KB Flash, 276KB RAM, With Crypto
|  | Footprint | ICC_UFBGA201_176+25_10X10_P065 | ICC_UFBGA201_176+25_10X10_P065
|  | Ibis Model |  |
|  | ID | 4812 | 4812
|  | Internal_Part_Number | MCD-02706 | MCD-02706
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-02706 | MCD-02706
|  | Manufacturer | STMICROELECTRONICS | STMICROELECTRONICS
|  | Manufacturer_Part_Number | STM32F723IEK6 | STM32F723IEK6
|  | Order_Code_Digikey | 497-17186-ND | 497-17186-ND
|  | Order_Code_Farnell | 2725149 | 2725149
|  | Order_Code_RS | 135-8241 | 135-8241
|  | Package | BGA176 | BGA176
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | IC | IC
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Checked | Checked
|  | Value | STM32F723IEK6 | STM32F723IEK6
U14 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | BMS_Part_Number | 9179045 | 9179045
|  | Comment | ESD-TRANSIL | ESD-TRANSIL
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Diodes/STM_ESD_ESDA25P35-1U1M | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Diodes/STM_ESD_ESDA25P35-1U1M
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | High power Transient voltage suppressor:25V/35A EOS and ESD transients protection. | High power Transient voltage suppressor:25V/35A EOS and ESD transients protection.
|  | Footprint | ESD_QFN1610_2N_1K_2A | ESD_QFN1610_2N_1K_2A
|  | Ibis Model |  |
|  | ID | 3289 | 3289
|  | Internal_Part_Number | MCD-01207 | MCD-01207
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01207 | MCD-01207
|  | Manufacturer | STMICROELECTRONICS | STMICROELECTRONICS
|  | Manufacturer_HQ_COO | EU | EU
|  | Manufacturer_Part_Number | ESDA25P35-1U1M | ESDA25P35-1U1M
|  | Package | QFN1610 | QFN1610
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Diode | Diode
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | ESDA25P35-1U1M | ESDA25P35-1U1M
U15 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | BMS_Part_Number | 9151138 | 9151138
|  | Comment | ? | ?
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Diodes/STM_ESD_ECMF02-2AMX6 | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Diodes/STM_ESD_ECMF02-2AMX6
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Common mode filter with ESD protection for USB 2.0 interface | Common mode filter with ESD protection for USB 2.0 interface
|  | Footprint | ESD_QFN-6L_1P7X1P5_P050 | ESD_QFN-6L_1P7X1P5_P050
|  | Ibis Model |  |
|  | ID | 3094 | 3094
|  | Internal_Part_Number | MCD-00649 | MCD-00649
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00649 | MCD-00649
|  | Manufacturer | STMICROELECTRONICS | STMICROELECTRONICS
|  | Manufacturer_HQ_COO | EU | EU
|  | Manufacturer_Part_Number | ECMF02-2AMX6 | ECMF02-2AMX6
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Diode | Diode
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | ECMF02-2AMX6 | ECMF02-2AMX6
U16 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | TPS259535DSG | TPS259535DSG
|  | Component Kind | Standard | Standard
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/IC/TEXAS_INSTRUMENTS_TPS259535DSG | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/IC/TEXAS_INSTRUMENTS_TPS259535DSG
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | IC, eFuse with Fast Overvoltage Protection 2.7V to 18V 4A 34mOhm 8-Pin WSON | IC, eFuse with Fast Overvoltage Protection 2.7V to 18V 4A 34mOhm 8-Pin WSON
|  | Footprint | ICC_WSON8-EPAD_2X2_P050 | ICC_WSON8-EPAD_2X2_P050
|  | Ibis Model |  |
|  | ID | 4638 | 4638
|  | Internal_Part_Number | MCD-02532 | MCD-02532
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-02532 | MCD-02532
|  | Manufacturer | TEXAS INSTRUMENTS | TEXAS INSTRUMENTS
|  | Manufacturer_Part_Number | TPS259535DSG | TPS259535DSG
|  | Order_Code_Digikey | N/A | N/A
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Package | WSON8 | WSON8
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | IC | IC
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Checked | Checked
|  | Value | TPS259535DSG | TPS259535DSG
U17 | STLINK-V3EC.SchDoc |  | Fitted | Not Fitted
|  | BMS_Part_Number | 9159009 |
|  | Comment | STMPS2151STR |
|  | Component Kind | Standard |
|  | Component_Country_Of_Origin | Malaysia |
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/IC/STMICROELECTRONICS_STMPS2151STR |
|  | Database Table Name | MCD_PARTS$ |
|  | Description | 500mA, Enhanced single channel power switches with active high enable pin |
|  | Footprint | MOS_SOT23-5L |
|  | Ibis Model |  |
|  | ID | 2708 |
|  | Internal_Part_Number | MCD-00159 |
|  | Library Name | MCD_PARTS_database.DbLib |
|  | Library Reference | MCD-00159 |
|  | Manufacturer | STMICROELECTRONICS |
|  | Manufacturer_HQ_COO | EU |
|  | Manufacturer_Part_Number | STMPS2151STR |
|  | Order_Code_Digikey | 497-6934-2-ND |
|  | Order_Code_Farnell | 1842616 |
|  | Order_Code_RS | 880-5415 |
|  | Part_Preference | Recommended |
|  | Part_Type | IC |
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES |
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released |
|  | Value | STMPS2151STR |
U18 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | Comment | ST730M33R | ST730M33R
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | Malaysia | Malaysia
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/IC/STMICROELECTRONICS_ST730M33R | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/IC/STMICROELECTRONICS_ST730M33R
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | LDO, 3.3V, 300mA, High input voltage: 2.5V to 28V, SOT23-5L | LDO, 3.3V, 300mA, High input voltage: 2.5V to 28V, SOT23-5L
|  | Footprint | ICC_SOT23-5L_H1P45 | ICC_SOT23-5L_H1P45
|  | Ibis Model |  |
|  | ID | 4620 | 4620
|  | Internal_Part_Number | MCD-02514 | MCD-02514
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-02514 | MCD-02514
|  | Manufacturer | STMICROELECTRONICS | STMICROELECTRONICS
|  | Manufacturer_Part_Number | ST730M33R | ST730M33R
|  | Order_Code_Digikey | N/A | N/A
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Package | SOT23-5L | SOT23-5L
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | IC | IC
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | ST730M33R | ST730M33R
U19 | External_Debug_Connectors.SchDoc |  | Fitted | Fitted
|  | BMS_Part_Number | 9151112 | 9151112
|  | Comment | ESDALC6V1W5 | ESDALC6V1W5
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Diodes/STM_ESD_ESDALC6V1W5 | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Diodes/STM_ESD_ESDALC6V1W5
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Dual Transil array for ESD protection | Dual Transil array for ESD protection
|  | Footprint | ESD_SOT323-5L | ESD_SOT323-5L
|  | Ibis Model |  |
|  | ID | 2731 | 2731
|  | Internal_Part_Number | MCD-00136 | MCD-00136
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00136 | MCD-00136
|  | Manufacturer | STMICROELECTRONICS | STMICROELECTRONICS
|  | Manufacturer_HQ_COO | EU | EU
|  | Manufacturer_Part_Number | ESDALC6V1W5 | ESDALC6V1W5
|  | Order_Code_Digikey | N/A | N/A
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Diode | Diode
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | ESDALC6V1W5 | ESDALC6V1W5
U20 | External_Debug_Connectors.SchDoc |  | Fitted | Fitted
|  | BMS_Part_Number | 9151112 | 9151112
|  | Comment | ESDALC6V1W5 | ESDALC6V1W5
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | China | China
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Diodes/STM_ESD_ESDALC6V1W5 | http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Diodes/STM_ESD_ESDALC6V1W5
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Dual Transil array for ESD protection | Dual Transil array for ESD protection
|  | Footprint | ESD_SOT323-5L | ESD_SOT323-5L
|  | Ibis Model |  |
|  | ID | 2731 | 2731
|  | Internal_Part_Number | MCD-00136 | MCD-00136
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-00136 | MCD-00136
|  | Manufacturer | STMICROELECTRONICS | STMICROELECTRONICS
|  | Manufacturer_HQ_COO | EU | EU
|  | Manufacturer_Part_Number | ESDALC6V1W5 | ESDALC6V1W5
|  | Order_Code_Digikey | N/A | N/A
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Diode | Diode
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | ESDALC6V1W5 | ESDALC6V1W5
X1 | MCU_System.SchDoc |  | Fitted | Fitted
|  | BMS_Part_Number | 9157049 | 9157049
|  | Comment | XTAL_2_PINS | XTAL_2_PINS
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | Unknown | Unknown
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Crytal_Oscillator/NDK_NX2012SA_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Crytal_Oscillator/NDK_NX2012SA_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Crystal, 32.768kHz, 6pF, +/-20ppm, 80K, 2.05x1.2mm | Crystal, 32.768kHz, 6pF, +/-20ppm, 80K, 2.05x1.2mm
|  | Footprint | CRY_NX2012SA_2P | CRY_NX2012SA_2P
|  | Ibis Model |  |
|  | ID | 3579 | 3579
|  | Internal_Part_Number | MCD-01479 | MCD-01479
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01479 | MCD-01479
|  | Manufacturer | NDK | NDK
|  | Manufacturer_Part_Number | NX2012SA-32.768KHZ-EXS00A-MU00527 | NX2012SA-32.768KHZ-EXS00A-MU00527
|  | Order_Code_Digikey | 644-1352 | 644-1352
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Package | 2.05x1.2mm | 2.05x1.2mm
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Crystal_Osc | Crystal_Osc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 32.768KHz | 32.768KHz
X2 | MCU_System.SchDoc |  | Fitted | Fitted
|  | BMS_Part_Number | 9157046 | 9157046
|  | Comment | XTAL_4_PINS | XTAL_4_PINS
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | Unknown | Unknown
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Crytal_Oscillator/NDK_NX2016SA_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Crytal_Oscillator/NDK_NX2016SA_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Crystal, 16 MHz, 8pF, +/-20ppm, 200R, 2x1.6mm | Crystal, 16 MHz, 8pF, +/-20ppm, 200R, 2x1.6mm
|  | Footprint | CRY_NX2016SA_4P | CRY_NX2016SA_4P
|  | Ibis Model |  |
|  | ID | 3576 | 3576
|  | Internal_Part_Number | MCD-01476 | MCD-01476
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01476 | MCD-01476
|  | Manufacturer | NDK | NDK
|  | Manufacturer_Part_Number | NX2016SA-16MHZ-EXS00A-CS07826 | NX2016SA-16MHZ-EXS00A-CS07826
|  | Order_Code_Digikey | 644-1360 | 644-1360
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Package | 2x1.6mm | 2x1.6mm
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Crystal_Osc | Crystal_Osc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 16MHz | 16MHz
X3 | STLINK-V3EC.SchDoc |  | Fitted | Fitted
|  | BMS_Part_Number | 9157045 | 9157045
|  | Comment | XTAL_4_PINS | XTAL_4_PINS
|  | Component Kind | Standard | Standard
|  | Component_Country_Of_Origin | Unknown | Unknown
|  | ComponentLink1URL | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Crytal_Oscillator/NDK_NX2016SA_Series | http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Crytal_Oscillator/NDK_NX2016SA_Series
|  | Database Table Name | MCD_PARTS$ | MCD_PARTS$
|  | Description | Crystal, 24MHz, 6pF, +/-20ppm, 80R, 2x1.6mm | Crystal, 24MHz, 6pF, +/-20ppm, 80R, 2x1.6mm
|  | Footprint | CRY_NX2016SA_4P | CRY_NX2016SA_4P
|  | Ibis Model |  |
|  | ID | 2989 | 2989
|  | Internal_Part_Number | MCD-01036 | MCD-01036
|  | Library Name | MCD_PARTS_database.DbLib | MCD_PARTS_database.DbLib
|  | Library Reference | MCD-01036 | MCD-01036
|  | Manufacturer | NDK | NDK
|  | Manufacturer_Part_Number | NX2016SA-24MHZ-EXS00A-CS10820 | NX2016SA-24MHZ-EXS00A-CS10820
|  | Order_Code_Digikey | 644-1365 | 644-1365
|  | Order_Code_Farnell | N/A | N/A
|  | Order_Code_RS | N/A | N/A
|  | Package | 2x1.6mm | 2x1.6mm
|  | Part_Preference | Recommended | Recommended
|  | Part_Type | Crystal_Osc | Crystal_Osc
|  | PCB3D |  |
|  | Pin Info |  |
|  | ShowFields | YES | YES
|  | Signal Integrity |  |
|  | Simulation |  |
|  | Status | Released | Released
|  | Value | 24MHz | 24MHz

Back to top