Removed Pin From Net: NetName=PA1 Pin=CN1-4
Removed Pin From Net: NetName=PA4 Pin=CN1-6
Removed Pin From Net: NetName=GND Pin=Q3-2
Removed Pin From Net: NetName=GND Pin=Q4-2
Removed Pin From Net: NetName=LED_RED Pin=R20-1
Removed Pin From Net: NetName=LED_GREEN Pin=R21-1
Removed Pin From Net: NetName=GND Pin=R22-1
Removed Pin From Net: NetName=GND Pin=R23-1
Removed Member From Class: ClassName=User Interface Member=Q3
Removed Member From Class: ClassName=User Interface Member=Q4
Removed Member From Class: ClassName=User Interface Member=R20
Removed Member From Class: ClassName=User Interface Member=R21
Removed Member From Class: ClassName=User Interface Member=R22
Removed Member From Class: ClassName=User Interface Member=R23
Added Component: Designator=R16(R0402)
Add component (AddParameter): Name = "Component_Country_Of_Origin"; Value = "China"; VariantName = "[No Variations]"
Add component (AddParameter): Name = "ComponentLink1URL"; Value = "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series"; VariantName = "[No Variations]"
Add component (AddParameter): Name = "ID"; Value = "2912"; VariantName = "[No Variations]"
Add component (AddParameter): Name = "Internal_Part_Number"; Value = "MCD-00367"; VariantName = "[No Variations]"
Add component (AddParameter): Name = "Manufacturer"; Value = "YAGEO"; VariantName = "[No Variations]"
Add component (AddParameter): Name = "Manufacturer_Part_Number"; Value = "RC0402FR-07110KL"; VariantName = "[No Variations]"
Add component (AddParameter): Name = "Order_Code_Digikey"; Value = "311-110KLRCT-ND"; VariantName = "[No Variations]"
Add component (AddParameter): Name = "Order_Code_Farnell"; Value = "1458740"; VariantName = "[No Variations]"
Add component (AddParameter): Name = "Order_Code_RS"; Value = "N/A"; VariantName = "[No Variations]"
Add component (AddParameter): Name = "Package"; Value = "0402"; VariantName = "[No Variations]"
Add component (AddParameter): Name = "Part_Preference"; Value = "Recommended"; VariantName = "[No Variations]"
Add component (AddParameter): Name = "Part_Type"; Value = "Resistor"; VariantName = "[No Variations]"
Add component (AddParameter): Name = "ShowFields"; Value = "YES"; VariantName = "[No Variations]"
Add component (AddParameter): Name = "Status"; Value = "Released"; VariantName = "[No Variations]"
Add component (AddParameter): Name = "Value"; Value = "110K"; VariantName = "[No Variations]"
Added Component: Designator=R17(R0402)
Add component (AddParameter): Name = "Component_Country_Of_Origin"; Value = "China"; VariantName = "[No Variations]"
Add component (AddParameter): Name = "ComponentLink1URL"; Value = "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series"; VariantName = "[No Variations]"
Add component (AddParameter): Name = "ID"; Value = "2852"; VariantName = "[No Variations]"
Add component (AddParameter): Name = "Internal_Part_Number"; Value = "MCD-00423"; VariantName = "[No Variations]"
Add component (AddParameter): Name = "Manufacturer"; Value = "YAGEO"; VariantName = "[No Variations]"
Add component (AddParameter): Name = "Manufacturer_Part_Number"; Value = "RC0402FR-07200KL"; VariantName = "[No Variations]"
Add component (AddParameter): Name = "Order_Code_Digikey"; Value = "311-200KLRCT-ND"; VariantName = "[No Variations]"
Add component (AddParameter): Name = "Order_Code_Farnell"; Value = "1458761"; VariantName = "[No Variations]"
Add component (AddParameter): Name = "Order_Code_RS"; Value = "N/A"; VariantName = "[No Variations]"
Add component (AddParameter): Name = "Package"; Value = "0402"; VariantName = "[No Variations]"
Add component (AddParameter): Name = "Part_Preference"; Value = "Recommended"; VariantName = "[No Variations]"
Add component (AddParameter): Name = "Part_Type"; Value = "Resistor"; VariantName = "[No Variations]"
Add component (AddParameter): Name = "ShowFields"; Value = "YES"; VariantName = "[No Variations]"
Add component (AddParameter): Name = "Status"; Value = "Released"; VariantName = "[No Variations]"
Add component (AddParameter): Name = "Value"; Value = "200K"; VariantName = "[No Variations]"
Added Pin To Net: NetName=VDD Pin=CN1-4
Added Pin To Net: NetName=VDD Pin=CN1-6
Add Pin To Net: Unknown Pin: Pin H1-GND1
Add Pin To Net: Unknown Pin: Pin H1-GND2
Add Pin To Net: Unknown Pin: Pin H1-GND3
Add Pin To Net: Unknown Pin: Pin H1-GND4
Added Pin To Net: NetName=LED_RED Pin=LD2-2
Added Pin To Net: NetName=LED_GREEN Pin=LD3-2
Added Pin To Net: NetName=PA1 Pin=R16-1
Added Pin To Net: NetName=5V_USB Pin=R16-2
Added Pin To Net: NetName=GND Pin=R17-1
Added Pin To Net: NetName=PA1 Pin=R17-2
Added Pin To Net: NetName=PA4 Pin=U3-11
Change Net Name : Old Net Name=PA1 New Net Name=PA1 (USBC_DETECT)
Change Net Name : Old Net Name=PA4 New Net Name=PA4 (USBC_FLT)
Added Member To Class: ClassName=USB Type C Member=Component R16 Resistor
Added Member To Class: ClassName=USB Type C Member=Component R17 Resistor
