Altium Designer Pick and Place Locations
D:\CAD_Activity\Altium_Projects\STM_LEMANS\MB2032B\02-Manufacturing\MB2032B_PCB\Assembly\MB2032B_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       09/06/23
Time:       11:23
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator  Comment                        Layer       Footprint                           Center-X(mm) Center-Y(mm) Rotation Description                                                                                  
SB57        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2875      2.5000       0        "Solder Bridge 0402 ON"                                                                      
SB56        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2875      3.7500       0        "Solder Bridge 0402 ON"                                                                      
SB55        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2875      7.5000       0        "Solder Bridge 0402 ON"                                                                      
SB54        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2875      6.2500       0        "Solder Bridge 0402 ON"                                                                      
SB53        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2125      16.0000      180      "Solder Bridge 0402 ON"                                                                      
SB52        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2125      22.2500      180      "Solder Bridge 0402 ON"                                                                      
SB51        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              9.9625       5.2500       180      "Solder Bridge 0402 ON"                                                                      
SB49        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              27.7125      22.2500      180      "Solder Bridge 0402 ON"                                                                      
SB48        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              10.0375      30.5000      0        "Solder Bridge 0402 ON"                                                                      
SB47        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2125      21.0000      180      "Solder Bridge 0402 ON"                                                                      
SB46        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              10.0375      1.5000       0        "Solder Bridge 0402 ON"                                                                      
SB45        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              9.9625       29.2500      180      "Solder Bridge 0402 ON"                                                                      
SB44        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2125      13.5000      180      "Solder Bridge 0402 ON"                                                                      
SB43        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2125      24.7500      180      "Solder Bridge 0402 ON"                                                                      
SB42        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2875      14.7500      0        "Solder Bridge 0402 ON"                                                                      
SB41        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2125      26.0000      180      "Solder Bridge 0402 ON"                                                                      
SB40        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2875      17.2500      0        "Solder Bridge 0402 ON"                                                                      
SB39        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2125      18.5000      180      "Solder Bridge 0402 ON"                                                                      
SB38        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              10.0375      2.7500       0        "Solder Bridge 0402 ON"                                                                      
SB37        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2875      8.5000       0        "Solder Bridge 0402 ON"                                                                      
SB36        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2875      9.7500       0        "Solder Bridge 0402 ON"                                                                      
SB35        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              28.2875      3.5000       0        "Solder Bridge 0402 ON"                                                                      
SB34        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2875      29.7500      0        "Solder Bridge 0402 ON"                                                                      
SB33        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              28.2875      8.5000       0        "Solder Bridge 0402 ON"                                                                      
SB32        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2875      31.0000      0        "Solder Bridge 0402 ON"                                                                      
SB31        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              28.2875      2.5000       0        "Solder Bridge 0402 ON"                                                                      
SB30        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              10.0375      14.0000      0        "Solder Bridge 0402 ON"                                                                      
SB29        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              28.2875      7.5000       0        "Solder Bridge 0402 ON"                                                                      
SB28        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              9.9625       4.0000       180      "Solder Bridge 0402 ON"                                                                      
SB25        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              10.0375      9.0000       0        "Solder Bridge 0402 ON"                                                                      
SB24        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2875      11.0000      0        "Solder Bridge 0402 ON"                                                                      
SB23        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              10.0375      6.5000       0        "Solder Bridge 0402 ON"                                                                      
SB22        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2875      23.5000      0        "Solder Bridge 0402 ON"                                                                      
SB21        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              9.9625       10.2500      180      "Solder Bridge 0402 ON"                                                                      
SB20        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2875      12.2500      0        "Solder Bridge 0402 ON"                                                                      
SB19        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              10.0375      12.5750      0        "Solder Bridge 0402 ON"                                                                      
SB18        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              9.9625       7.7500       180      "Solder Bridge 0402 ON"                                                                      
SB17        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              10.0375      25.2500      0        "Solder Bridge 0402 ON"                                                                      
SB16        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              9.9625       17.7500      180      "Solder Bridge 0402 ON"                                                                      
SB15        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              9.9625       21.5000      180      "Solder Bridge 0402 ON"                                                                      
SB14        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2875      27.2500      0        "Solder Bridge 0402 ON"                                                                      
SB13        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              9.9625       19.0000      180      "Solder Bridge 0402 ON"                                                                      
SB12        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2125      19.7500      180      "Solder Bridge 0402 ON"                                                                      
SB11        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              10.0375      26.5000      0        "Solder Bridge 0402 ON"                                                                      
SB10        SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              9.9625       16.5000      180      "Solder Bridge 0402 ON"                                                                      
SB9         SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2875      28.5000      0        "Solder Bridge 0402 ON"                                                                      
SB8         SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              9.9625       11.5000      180      "Solder Bridge 0402 ON"                                                                      
R10         Resistor                       TopLayer    R0402                               19.5000      45.0000      90       "Resistor, 0R, 0402, +/-5%, 1/16W"                                                           
SB1         SB_ON                          TopLayer    SOLDER-BRIDGE_R0402-0R              12.3000      33.2125      270      "Solder Bridge 0402 ON"                                                                      
R1          Resistor                       TopLayer    R0402                               19.5000      42.4500      90       "Resistor, 0R, 0402, +/-5%, 1/16W"                                                           
R2          Resistor                       TopLayer    r0402                               19.0500      42.0000      180      "Resistor, 0R, 0402, +/-5%, 1/16W"                                                           
MIRE3       Comment                        TopLayer    MIRE_PLACE_SMD_0P8MM                2.2500       1.5000       0        ""                                                                                           
MIRE1       Comment                        TopLayer    MIRE_PLACE_SMD_0P8MM                1.5000       39.7500      0        ""                                                                                           
MIRE6       Comment                        BottomLayer MIRE_PLACE_SMD_0P8MM                2.2500       1.5000       0        ""                                                                                           
MIRE4       Comment                        BottomLayer MIRE_PLACE_SMD_0P8MM                1.5000       39.7500      0        ""                                                                                           
MIRE5       Comment                        BottomLayer MIRE_PLACE_SMD_0P8MM                39.2500      1.7500       0        ""                                                                                           
MIRE2       Comment                        TopLayer    MIRE_PLACE_SMD_0P8MM                39.2500      1.7500       0        ""                                                                                           
SC2         Shield-clip_S0951-46R          TopLayer    CLIP_HARWIN_S0981-46R               24.0000      38.4500      90       "shield clip Harwin S0981-46R to fix RF shielded cavity - SMT RFI Shield Clip, Corner (T+R)" 
SC3         Shield-clip_S0951-46R          TopLayer    CLIP_HARWIN_S0951-46R               11.0000      33.2000      90       "shield clip Harwin S0951-46R to fix RF shielded cavity"                                     
SC1         Shield-clip_S0951-46R          TopLayer    CLIP_HARWIN_S0981-46R               13.0000      38.4500      180      "shield clip Harwin S0981-46R to fix RF shielded cavity - SMT RFI Shield Clip, Corner (T+R)" 
SC7         Shield-clip_S0951-46R          TopLayer    CLIP_HARWIN_S0981-46R               13.0000      22.4500      270      "shield clip Harwin S0981-46R to fix RF shielded cavity - SMT RFI Shield Clip, Corner (T+R)" 
SC8         Shield-clip_S0951-46R          TopLayer    CLIP_HARWIN_S0981-46R               24.0000      22.4500      0        "shield clip Harwin S0981-46R to fix RF shielded cavity - SMT RFI Shield Clip, Corner (T+R)" 
U2          MLPF-WB55-01E3                 TopLayer    ICC_CSPG_6BUMPS_1X1P60_P050-P0577   19.7500      37.3720      0        "2.4 GHz low pass filter matched to BLUENRG-LP-LPS"                                          
SC5         Shield-clip_S0951-46R          TopLayer    CLIP_HARWIN_S0951-46R               11.0000      27.7000      90       "shield clip Harwin S0951-46R to fix RF shielded cavity"                                     
SC4         Shield-clip_S0951-46R          TopLayer    CLIP_HARWIN_S0951-46R               26.0000      33.2000      90       "shield clip Harwin S0951-46R to fix RF shielded cavity"                                     
SC6         Shield-clip_S0951-46R          TopLayer    CLIP_HARWIN_S0951-46R               26.0000      27.7000      90       "shield clip Harwin S0951-46R to fix RF shielded cavity"                                     
SB7         SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2875      1.5000       0        "Solder Bridge 0402 ON"                                                                      
L2          Inductor                       TopLayer    C0402                               18.0000      27.7500      90       "Inductor, MLCC, 22nH, ±2%, 350mA, 0.58R, 0402, T=1.45mm"                                    
L3          Inductor                       TopLayer    IND_0805_MURATA_LQM21               19.0000      25.7500      180      "Inductor, MLCC, 10uH, ±20%, 300mA, 845mR, 0805, T=1.45mm"                                   
JP1         "Jumper_Header 3x1 Fitted 2-3" TopLayer    CON_SAMTEC_TSW-103-07-F-S           30.7500      32.5000      270      "Header, 3x1, 2.54mm, VR, TH, T=5.84mm/2.54mm"                                               
HW1         S02-20150300                   TopLayer    SHIELD_HARWIN_S02-20150300_15X20_H3 -275.4530    -237.3752    0        "RFI shield can, 20x15x3mm"                                                                  
C2          Capacitor                      TopLayer    C0402_MURATA_GRM155_H0P5            19.9500      43.6500      180      "Capacitor, MLCC, 0.9pF, 25V, +/-0.05pF, 0402, T=0.5mm"                                      
ANT1        2.4GHz_BT_ANT                  TopLayer    ANT_BT_BNRG_2P4GHZ_MB2032           19.5200      47.2500      90       "2.4 GHZ Bluetooth BNRG PCB antenna"                                                         
CN4         U.FL-R-SMT-1                   TopLayer    CON_HRS_U.FL-R-SMT-1                15.2500      42.7500      0        "Connector_RF, 0Hz to 6GHz, 50R, VR, SMD, T= 1.25mm"                                         
Designator1 Comment                        TopLayer    IMPEDANCE_TABLE                     -275.4530    -237.3752    0        ""                                                                                           
Designator3 Comment                        TopLayer    Sheetbox_4L2S                       96.9858      -7.8310      0        ""                                                                                           
Designator2 Comment                        TopLayer    PCB_SPECIFICATIONS                  -275.4530    -237.3752    0        ""                                                                                           
SB6         SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              33.2125      5.0000       180      "Solder Bridge 0402 ON"                                                                      
SB2         SB_ON                          TopLayer    SOLDER-BRIDGE_R0402-0R              12.3000      30.7875      90       "Solder Bridge 0402 ON"                                                                      
CN3         "Header 7x2"                   TopLayer    CON_SAMTEC_FTSH-107-01-L-DV-K-A     22.1014      4.5794       0        "Header, 7x2, 1.27mm, VR, T=5.97mm, FTSH series STDC14 without Alignment Pin"                
CN2         FTSH-125-02-L-DV               BottomLayer CON_SAMTEC_FTSH-125-02-L-DV         38.6564      18.5484      270      "Header, 25x2, 12.7mm, VR, SMD, T=4.83mm"                                                    
CN1         FTSH-125-02-L-DV               BottomLayer CON_SAMTEC_FTSH-125-02-L-DV         4.3664       18.5484      270      "Header, 25x2, 12.7mm, VR, SMD, T=4.83mm"                                                    
U1          STM32WB09                      TopLayer    ICC_QFN32-EPAD_5X5_P050             20.2500      32.2500      90       "Bluetooth® Low Energy wireless SoC"                                                         
SB4         SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              10.0375      20.2500      0        "Solder Bridge 0402 ON"                                                                      
SB3         SB_ON                          TopLayer    SOLDER-BRIDGE_R0402-0R              19.0314      24.2500      180      "Solder Bridge 0402 ON"                                                                      
C5          Capacitor                      TopLayer    C0402                               21.7500      36.5000      270      "Capacitor, MLCC, 3pF, COG, 50V, 0402, ±0.1pF, T=0.5mm"                                      
C6          Capacitor                      TopLayer    C0402                               22.5500      36.5000      270      "Capacitor, MLCC, 100nF, ±10%, X7R, 25V, 0402, T=0.5mm"                                      
C16         Capacitor                      TopLayer    C0402                               21.2500      26.7500      90       "Capacitor, MLCC, 0.22uF, X5R, 6.3V, +/-10%, 0402, T=0.5mm"                                  
C13         Capacitor                      TopLayer    C0402                               23.2500      27.7500      180      "Capacitor, MLCC, 1uF, X7R, 6.3V, 0402, ± 10%, T=0.5mm"                                      
C4          Capacitor                      TopLayer    C0402                               18.0000      36.5000      270      "Capacitor, MLCC, 3pF, COG, 50V, +/-0.1pF, 0402, T=0.5mm"                                    
C3          Capacitor                      TopLayer    C0402                               17.2000      36.5000      270      "Capacitor, MLCC, 100nF, ±10%, X7R, 25V, 0402, T=0.5mm"                                      
X1          XTAL_4_PINS                    TopLayer    CRY_NX2016SA_4P                     15.0000      35.0000      90       "Crystal, 32MHz, 8pF, +/-10ppm, 60R, 2x1.6mm"                                                
X2          XTAL_2_PINS                    TopLayer    CRY_NX2012SA_2P                     14.5000      32.0000      90       "Crystal, 32.768kHz, 7pF, +/-20ppm, 80K, 2.05x1.2mm"                                         
SB5         SB_ON                          BottomLayer SOLDER-BRIDGE_R0402-0R              9.9625       15.2500      180      "Solder Bridge 0402 ON"                                                                      
R4          Resistor                       BottomLayer R0402                               25.9091      9.9474       90       "Resistor, 47R, 0402, +/-1%, 1/16W"                                                          
R8          Resistor                       BottomLayer R0402                               26.7500      5.0000       270      "Resistor, 47R, 0402, +/-1%, 1/16W"                                                          
R5          Resistor                       BottomLayer R0402                               24.6510      9.9474       90       "Resistor, 47R, 0402, +/-1%, 1/16W"                                                          
R9          Resistor                       BottomLayer R0402                               23.0000      5.0000       270      "Resistor, 100R, 0402, +/- 1%, 1/16W"                                                        
R6          Resistor                       BottomLayer R0402                               20.8874      9.8779       90       "Resistor, 47R, 0402, +/-1%, 1/16W"                                                          
R7          Resistor                       BottomLayer R0402                               19.6054      9.8779       90       "Resistor, 47R, 0402, +/-1%, 1/16W"                                                          
R3          Resistor                       TopLayer    R0402                               30.7500      27.5000      90       "Resistor, 100K, 0402, +/-1%, 1/16W"                                                         
HW2         STICKER_PRODUCT                TopLayer    STICKER_PRODUCT_25X5                -275.4530    -237.3752    90       "Sticker product 25x5 mm"                                                                    
HW3         STICKER_BOARD                  TopLayer    STICKER_BOARD_25X5                  -275.4530    -237.3752    90       "Sticker board 25x5 mm"                                                                      
C10         Capacitor                      TopLayer    C0402                               23.2500      28.7500      180      "Capacitor, MLCC, 100nF, ±10%, X7R, 25V, 0402, T=0.5mm"                                      
C12         Capacitor                      TopLayer    C0402                               19.5000      28.2500      0        "Capacitor, MLCC, 100nF, ±10%, X7R, 25V, 0402, T=0.5mm"                                      
C15         Capacitor                      TopLayer    C0402                               19.5000      27.2500      0        "Capacitor, MLCC, 4.7uF, X5R, 10 V, 0402, ± 20%, T=0.5mm"                                    
C11         Capacitor                      TopLayer    C0402                               16.0000      28.7500      180      "Capacitor, MLCC, 100nF, ±10%, X7R, 25V, 0402, T=0.5mm"                                      
C14         Capacitor                      TopLayer    C0402                               16.0000      27.7500      180      "Capacitor, MLCC, 4.7uF, X5R, 10 V, 0402, ± 20%, T=0.5mm"                                    
C7          Capacitor                      TopLayer    C0201_H0P3                          19.5000      35.8500      90       "Capacitor, MLCC, 20pF, 25V, COG, +/-2%, 0201, T=0.33mm"                                     
C9          Capacitor                      TopLayer    C0402                               13.2500      30.7500      270      "Capacitor, MLCC, 10pF, 50V, NPO, +/-5%, 0402, T=0.5mm"                                      
C8          Capacitor                      TopLayer    C0402                               13.2500      33.2500      270      "Capacitor, MLCC, 10pF, 50V, NPO, +/-5%, 0402, T=0.5mm"                                      
C1          Capacitor                      TopLayer    C0402                               19.9500      46.3500      180      "Capacitor, MLCC, 6.8pF, 50V, C0G, +/-0.05pF, 0402, T=0.5mm"                                 
