Altium Designer Pick and Place Locations
C:\Reference_design\boards\02-Manufacturing\MB2157A_PCB\Assembly\MB2157A_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       05/08/24
Time:       08:28
Revision:   Not in VersionControl
Variant:    Variant A
Units used: mm

Designator   Comment               Layer    Footprint                           Center-X(mm) Center-Y(mm) Rotation Description                                                               
HW1          S02-20150300          TopLayer SHIELD_HARWIN_S02-20150300_15X20_H3 -63.8710     -61.9050     90       "RFI shield can, 20x15x3mm"                                               
SC1          Shield-clip_S0951-46R TopLayer CLIP_HARWIN_S0981-46R               31.6754      21.3582      90       "Shield clip Harwin S0981-46R to fix RF shielded cavity"                  
SC2          Shield-clip_S0951-46R TopLayer CLIP_HARWIN_S0981-46R               15.6754      21.3582      180      "Shield clip Harwin S0981-46R to fix RF shielded cavity"                  
SC3          Shield-clip_S0951-46R TopLayer CLIP_HARWIN_S0981-46R               31.6754      10.3582      0        "Shield clip Harwin S0981-46R to fix RF shielded cavity"                  
SC4          Shield-clip_S0951-46R TopLayer CLIP_HARWIN_S0981-46R               15.6754      10.3582      270      "Shield clip Harwin S0981-46R to fix RF shielded cavity"                  
SC5          Shield-clip_S0951-46R TopLayer CLIP_HARWIN_S0951-46R               20.9254      23.3582      180      "RFI shield clip mini TIN SMD"                                            
SC6          Shield-clip_S0951-46R TopLayer CLIP_HARWIN_S0951-46R               26.4254      23.3582      180      "RFI shield clip mini TIN SMD"                                            
SC9          Shield-clip_S0951-46R TopLayer CLIP_HARWIN_S0951-46R               20.9254      8.3582       180      "RFI shield clip mini TIN SMD"                                            
SC8          Shield-clip_S0951-46R TopLayer CLIP_HARWIN_S0951-46R               26.4254      8.3582       180      "RFI shield clip mini TIN SMD"                                            
SC7          Shield-clip_S0951-46R TopLayer CLIP_HARWIN_S0951-46R               13.6754      15.9324      270      "RFI shield clip mini TIN SMD"                                            
L2           Inductor              TopLayer C0402                               22.4000      17.5500      0        "Inductor, MLCC, 22nH, +/-2%, 350mA, 0.58R, 0402, T=1.45mm"               
Designator16 Comment               TopLayer IMPEDANCE_TABLE                     -63.8710     -61.9050     0        ""                                                                        
C11          Capacitor             TopLayer C0402                               22.6500      15.9500      270      "Capacitor, MLCC, 100nF, +/-10%, X7R, 25V, 0402, T=0.5mm"                 
C6           Capacitor             TopLayer 20p_capacitor_SMD_0201              30.1132      15.5024      90       "Capacitor, MLCC, 20pF, 25V, COG, +/-2%, 0201, T=0.3mm"                   
U2           MLPF-WB55-01E3        TopLayer ICC_CSPG_6BUMPS_1X1P60_P050-P0577   31.7372      15.2500      270      "2.4 GHz low pass filter matched to BLUENRG-LP-LPS"                       
C3           Capacitor             TopLayer C0402                               23.4550      19.1045      0        "Capacitor, MLCC, 4.7uF, X5R, 10V, +/-20%, 0402, T=0.5mm"                 
L1           Inductor              TopLayer IND_0805_MURATA_LQM21               20.5077      16.6020      90       "Inductor, MLCC, 10uH, +/-20%, 300mA, 845mR, 0805, T=1.45mm"              
C4           Capacitor             TopLayer C0201_H0P3                          23.6510      18.3044      0        "Capacitor, MLCC,100nF, 10V, X5R, +/-10%, 0201, T=0.3mm"                  
C5           Capacitor             TopLayer C0402                               31.3500      17.4500      135      "Capacitor, MLCC, 1uF, X7R, 6.3V,+/- 10%, 0402, T=0.5mm"                  
J1           SMA_connector         TopLayer SMA_AMPHENOL_132415                 38.5909      15.5000      180      "Rf Connector, Sma End Launch Recept Jack For .032" Pcb / Individual Bag" 
X2           XTAL_4_PINS           TopLayer CRY_NX2016SA_4P                     30.3000      20.0000      270      "Crystal, 32MHz, 8pF, +/-10ppm, 60R, 2x1.6mm"                             
X1           XTAL_2_PINS           TopLayer CRY_NX2012SA_2P                     26.6000      20.4000      0        "Crystal, 32.768kHz, 7pF, +/-20ppm, 80K, 2.05x1.2mm"                      
U1           STM32WB09             TopLayer ICC_QFN32-EPAD_5X5_P050             26.6160      14.7500      0        "Bluetooth® Low Energy wireless SoC"                                      
C10          Capacitor             TopLayer C0402                               22.4500      14.7000      0        "Capacitor, MLCC, 0.22uF, X5R, 6.3V, +/-10%, 0402, T=0.5mm"               
C9           Capacitor             TopLayer C0402                               31.7500      13.4500      225      "Capacitor, MLCC, 1uF, X7R, 6.3V,+/- 10%, 0402, T=0.5mm"                  
C8           Capacitor             TopLayer C0402                               23.0000      12.2500      90       "Capacitor, MLCC, 1uF, X7R, 6.3V,+/- 10%, 0402, T=0.5mm"                  
C7           Capacitor             TopLayer C0402                               21.8500      15.9500      270      "Capacitor, MLCC, 4.7uF, X5R, 10V, +/-20%, 0402, T=0.5mm"                 
C2           Capacitor             TopLayer C0402                               27.6000      22.2500      180      "Capacitor, MLCC, 10pF, 50V, NPO, +/-5%, 0402, T=0.5mm"                   
C1           Capacitor             TopLayer C0402                               25.4500      22.2500      180      "Capacitor, MLCC, 10pF, 50V, NPO, +/-5%, 0402, T=0.5mm"                   
