Altium Designer Pick and Place Locations
C:\Reference_design\boards\02-Manufacturing\MB2172A_PCB\Assembly\MB2172A_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       05/08/24
Time:       08:53
Revision:   Not in VersionControl
Variant:    Variant A
Units used: mm

Designator   Comment               Layer    Footprint                           Center-X(mm) Center-Y(mm) Rotation Description                                                               
HW1          S02-20150300          TopLayer SHIELD_HARWIN_S02-20150300_15X20_H3 -49.3709     -61.9050     90       "RFI shield can, 20x15x3mm"                                               
Designator16 Comment               TopLayer IMPEDANCE_TABLE                     -49.3709     -61.9050     0        ""                                                                        
J1           SMA_connector         TopLayer SMA_AMPHENOL_132415                 53.2375      15.5000      180      "Rf Connector, Sma End Launch Recept Jack For .032" Pcb / Individual Bag" 
C8           Capacitor             TopLayer 20p_capacitor_SMD_0201              45.6407      15.5024      90       "Capacitor, MLCC, 20pF, 25V, COG, +/-2%, 0201, T=0.3mm"                   
U2           MLPF-WB55-01E3        TopLayer ICC_CSPG_6BUMPS_1X1P60_P050-P0577   47.2650      15.2500      270      "2.4 GHz low pass filter matched to BLUENRG-LP-LPS"                       
C6           Capacitor             TopLayer C0402                               34.5240      15.5500      270      "Capacitor, MLCC, 10nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                  
X2           XTAL_4_PINS           TopLayer CRY_NX2016SA_4P                     46.0111      19.8314      90       "Crystal, 32MHz, 8pF, +/-10ppm, 60R, 2x1.6mm"                             
SC12         Shield-clip_S0951-46R TopLayer CLIP_HARWIN_S0951-46R               42.1981      23.4180      180      "RFI shield clip mini TIN SMD"                                            
SC11         Shield-clip_S0951-46R TopLayer CLIP_HARWIN_S0951-46R               36.4481      23.4180      180      "RFI shield clip mini TIN SMD"                                            
SC4          Shield-clip_S0951-46R TopLayer CLIP_HARWIN_S0981-46R               31.3371      21.4180      180      "Shield clip Harwin S0981-46R to fix RF shielded cavity"                  
SC10         Shield-clip_S0951-46R TopLayer CLIP_HARWIN_S0951-46R               36.4481      8.5001       180      "RFI shield clip mini TIN SMD"                                            
SC9          Shield-clip_S0951-46R TopLayer CLIP_HARWIN_S0951-46R               42.1981      8.5001       180      "RFI shield clip mini TIN SMD"                                            
SC8          Shield-clip_S0951-46R TopLayer CLIP_HARWIN_S0951-46R               29.3371      15.9930      270      "RFI shield clip mini TIN SMD"                                            
SC3          Shield-clip_S0951-46R TopLayer CLIP_HARWIN_S0981-46R               31.3371      10.5001      270      "Shield clip Harwin S0981-46R to fix RF shielded cavity"                  
SC2          Shield-clip_S0951-46R TopLayer CLIP_HARWIN_S0981-46R               47.3371      10.5001      0        "Shield clip Harwin S0981-46R to fix RF shielded cavity"                  
SC1          Shield-clip_S0951-46R TopLayer CLIP_HARWIN_S0981-46R               47.3371      21.4184      90       "Shield clip Harwin S0981-46R to fix RF shielded cavity"                  
C10          Capacitor             TopLayer C0402                               37.3411      14.5000      225      "Capacitor, MLCC, 100nF, 25V, X7R, +/-10%, 0402, T=0.5mm"                 
L3           Inductor              TopLayer C0402                               39.3500      18.5500      270      "Inductor, MLCC, 22nH, +/-2%, 350mA, 0.58R, 0402, T=1.45mm"               
L2           Inductor              TopLayer IND_0805_MURATA_LQM21               39.2990      20.9000      180      "Inductor, MLCC, 10uH, +/-20%, 300mA, 845mR, 0805, T=1.45mm"              
C13          Capacitor             TopLayer C0402                               40.5000      19.1000      90       "Capacitor, MLCC, 4.7uF, X5R, 10V, +/-20%, 0402, T=0.5mm"                 
C1           Capacitor             TopLayer C0402                               41.6911      22.2000      180      "Capacitor, MLCC, 10pF, 50V, NPO, +/-5%, 0402, T=0.5mm"                   
C2           Capacitor             TopLayer C0402                               43.3411      22.2000      180      "Capacitor, MLCC, 10pF, 50V, NPO, +/-5%, 0402, T=0.5mm"                   
X1           XTAL_2_PINS           TopLayer CRY_NX2012SA_2P                     42.4911      21.0500      0        "Crystal, 32.768kHz, 7pF, +/-20ppm, 80K, 2.05x1.2mm"                      
U1           STM32WB07             TopLayer ICC_QFN48-EPAD-4P5X4P5_6X6_P040     41.7935      14.0999      90       "IC, Bluetooth Low Energy wireless SoC, QFN48"                            
C21          Capacitor             TopLayer C0402                               44.1740      18.4000      180      "Capacitor, MLCC, 1uF, X7R, 6.3V,+/- 10%, 0402, T=0.5mm"                  
C19          Capacitor             TopLayer C0402                               41.8611      18.6500      270      "Capacitor, MLCC, 0.22uF, X5R, 6.3V, +/-10%, 0402, T=0.5mm"               
C18          Capacitor             TopLayer C0402                               37.4000      16.9500      270      "Capacitor, MLCC, 1uF, X7R, 6.3V,+/- 10%, 0402, T=0.5mm"                  
C16          Capacitor             TopLayer C0402                               47.2500      13.6500      225      "Capacitor, MLCC, 1uF, X7R, 6.3V,+/- 10%, 0402, T=0.5mm"                  
C12          Capacitor             TopLayer C0402                               36.7911      15.1500      45       "Capacitor, MLCC, 1uF, X7R, 6.3V,+/- 10%, 0402, T=0.5mm"                  
C7           Capacitor             TopLayer C0402                               46.8000      17.0500      135      "Capacitor, MLCC, 1uF, X7R, 6.3V,+/- 10%, 0402, T=0.5mm"                  
C4           Capacitor             TopLayer C0201_H0P3                          38.0411      18.7000      270      "Capacitor, MLCC,100nF, 10V, X5R, +/-10%, 0201, T=0.3mm"                  
C3           Capacitor             TopLayer C0402                               37.2911      18.8500      270      "Capacitor, MLCC, 4.7uF, X5R, 10V, +/-20%, 0402, T=0.5mm"                 
