Altium Designer Pick and Place Locations
C:\Reference_design\boards\02-Manufacturing\MB2173A_PCB\Assembly\MB2173A_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       05/08/24
Time:       09:07
Revision:   Not in VersionControl
Variant:    Variant A
Units used: mm

Designator   Comment               Layer    Footprint                           Center-X(mm) Center-Y(mm) Rotation Description                                                                                 
C9           Capacitor             TopLayer 0_8p_capacitor_SMD_0201             43.5933      15.7583      0        "Multilayer Ceramic Capacitor, 0.8 pF, 25 V, ± 0.05pF, C0G (NP0), 0201 [0603 Metric]"       
HW1          S02-20150300          TopLayer SHIELD_HARWIN_S02-20150300_15X20_H3 -49.3709     -61.9050     90       "RFI shield can, 20x15x3mm"                                                                 
Designator16 Comment               TopLayer IMPEDANCE_TABLE                     -49.3709     -61.9050     0        ""                                                                                          
J1           SMA_connector         TopLayer SMA_AMPHENOL_132415                 53.2375      15.5000      180      "Rf Connector, Sma End Launch Recept Jack For .032" Pcb / Individual Bag"                   
C6           Capacitor             TopLayer C0402                               32.4500      15.5500      270      "Capacitor, MLCC, 10nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                    
X2           XTAL_4_PINS           TopLayer CRY_NX2016SA_4P                     43.9371      19.8314      90       "Crystal, 32MHz, 8pF, +/-10ppm, 60R, 2x1.6mm"                                               
C11          Capacitor             TopLayer 1_5p_capacitor_SMD_0201             45.5969      15.8032      0        "Multilayer Ceramic Capacitor, 1.5 pF, 25 V, ± 0.1pF, C0G (NP0), 0201 [0603 Metric]"        
L4           Inductor              TopLayer 3n3_inductor_SMD_0201               46.5888      15.5023      90       "Inductor RF Chip Thin Film 3.3nH 0.1nH 500MHz 14Q-Factor 450mA 250mOhm DCR 0201 Paper T/R" 
L1           Inductor              TopLayer 2n4_inductor_SMD_0201               44.5907      15.1488      90       "Inductor RF Chip Thin Film 2.4nH 0.1nH 500MHz 14Q-Factor 500mA 200mOhm DCR 0201 Paper T/R" 
C14          Capacitor             TopLayer 0_8p_capacitor_SMD_0201             47.5708      15.2317      180      "Multilayer Ceramic Capacitor, 0.8 pF, 25 V, ± 0.05pF, C0G (NP0), 0201 [0603 Metric]"       
C5           Capacitor             TopLayer 0_5p_capacitor_SMD_0201             44.5896      15.8732      90       "0201 0.3 pF 25 V ±0.05 pF Tolerance C0G SMT Multilayer Ceramic Capacitor"                  
C8           Capacitor             TopLayer 20p_capacitor_SMD_0201              48.5349      15.5023      90       "Capacitor, MLCC, 20pF, 25V, COG, +/-2%, 0201, T=0.3mm"                                     
SC12         Shield-clip_S0951-46R TopLayer CLIP_HARWIN_S0951-46R               42.1981      23.4180      180      "RFI shield clip mini TIN SMD"                                                              
SC11         Shield-clip_S0951-46R TopLayer CLIP_HARWIN_S0951-46R               36.4481      23.4180      180      "RFI shield clip mini TIN SMD"                                                              
SC4          Shield-clip_S0951-46R TopLayer CLIP_HARWIN_S0981-46R               31.3371      21.4180      180      "Shield clip Harwin S0981-46R to fix RF shielded cavity"                                    
SC10         Shield-clip_S0951-46R TopLayer CLIP_HARWIN_S0951-46R               36.4481      8.5001       180      "RFI shield clip mini TIN SMD"                                                              
SC9          Shield-clip_S0951-46R TopLayer CLIP_HARWIN_S0951-46R               42.1981      8.5001       180      "RFI shield clip mini TIN SMD"                                                              
SC8          Shield-clip_S0951-46R TopLayer CLIP_HARWIN_S0951-46R               29.3371      15.9930      270      "RFI shield clip mini TIN SMD"                                                              
SC3          Shield-clip_S0951-46R TopLayer CLIP_HARWIN_S0981-46R               31.3371      10.5001      270      "Shield clip Harwin S0981-46R to fix RF shielded cavity"                                    
SC2          Shield-clip_S0951-46R TopLayer CLIP_HARWIN_S0981-46R               47.3371      10.5001      0        "Shield clip Harwin S0981-46R to fix RF shielded cavity"                                    
SC1          Shield-clip_S0951-46R TopLayer CLIP_HARWIN_S0981-46R               47.3371      21.4184      90       "Shield clip Harwin S0981-46R to fix RF shielded cavity"                                    
C10          Capacitor             TopLayer C0402                               35.2671      14.5000      225      "Capacitor, MLCC, 100nF, 25V, X7R, +/-10%, 0402, T=0.5mm"                                   
L3           Inductor              TopLayer C0402                               37.2500      18.6500      270      "Inductor, MLCC, 22nH, +/-2%, 350mA, 0.58R, 0402, T=1.45mm"                                 
L2           Inductor              TopLayer IND_0805_MURATA_LQM21               37.2250      20.9000      180      "Inductor, MLCC, 10uH, +/-20%, 300mA, 845mR, 0805, T=1.45mm"                                
C13          Capacitor             TopLayer C0402                               38.4500      19.2000      90       "Capacitor, MLCC, 4.7uF, X5R, 10V, +/-20%, 0402, T=0.5mm"                                   
C1           Capacitor             TopLayer C0402                               39.6171      22.2000      180      "Capacitor, MLCC, 10pF, 50V, NPO, +/-5%, 0402, T=0.5mm"                                     
C2           Capacitor             TopLayer C0402                               41.2671      22.2000      180      "Capacitor, MLCC, 10pF, 50V, NPO, +/-5%, 0402, T=0.5mm"                                     
X1           XTAL_2_PINS           TopLayer CRY_NX2012SA_2P                     40.4171      21.0500      0        "Crystal, 32.768kHz, 7pF, +/-20ppm, 80K, 2.05x1.2mm"                                        
U1           STM32WB07             TopLayer ICC_QFN48-EPAD-4P5X4P5_6X6_P040     39.7195      14.0999      90       "IC, Bluetooth Low Energy wireless SoC, QFN48"                                              
C21          Capacitor             TopLayer C0402                               42.1000      18.4000      180      "Capacitor, MLCC, 1uF, X7R, 6.3V,+/- 10%, 0402, T=0.5mm"                                    
C19          Capacitor             TopLayer C0402                               39.7871      18.6500      270      "Capacitor, MLCC, 0.22uF, X5R, 6.3V, +/-10%, 0402, T=0.5mm"                                 
C18          Capacitor             TopLayer C0402                               35.1671      16.9500      270      "Capacitor, MLCC, 1uF, X7R, 6.3V,+/- 10%, 0402, T=0.5mm"                                    
C16          Capacitor             TopLayer C0402                               44.8371      14.0000      225      "Capacitor, MLCC, 1uF, X7R, 6.3V,+/- 10%, 0402, T=0.5mm"                                    
C12          Capacitor             TopLayer C0402                               34.7171      15.1500      45       "Capacitor, MLCC, 1uF, X7R, 6.3V,+/- 10%, 0402, T=0.5mm"                                    
C7           Capacitor             TopLayer C0402                               44.7456      17.1681      135      "Capacitor, MLCC, 1uF, X7R, 6.3V,+/- 10%, 0402, T=0.5mm"                                    
C4           Capacitor             TopLayer C0201_H0P3                          35.9671      18.7000      270      "Capacitor, MLCC,100nF, 10V, X5R, +/-10%, 0201, T=0.3mm"                                    
C3           Capacitor             TopLayer C0402                               35.2171      18.8500      270      "Capacitor, MLCC, 4.7uF, X5R, 10V, +/-20%, 0402, T=0.5mm"                                   
