Altium Designer Pick and Place Locations
C:\Users\jorda\Documents\Projets\STM Le Mans\MB2293B\BASE\MB2293B\02-Manufacturing\MB2293B_PCB\Assembly\MB2293B_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       27/01/26
Time:       09:09
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator Comment                     Layer       Footprint                          Center-X(mm) Center-Y(mm) Rotation Description                                                                                  
SB6        SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             9.7875       25.5000      0        "Solder Bridge 0402 ON"                                                                      
SB5        SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             9.7875       27.0000      0        "Solder Bridge 0402 ON"                                                                      
SB18       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             24.7125      23.0000      180      "Solder Bridge 0402 ON"                                                                      
SB14       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             24.7125      21.0000      180      "Solder Bridge 0402 ON"                                                                      
SB12       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             24.7125      22.0000      180      "Solder Bridge 0402 ON"                                                                      
SB10       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             33.5375      4.2500       0        "Solder Bridge 0402 ON"                                                                      
SB9        SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             33.5375      5.2500       0        "Solder Bridge 0402 ON"                                                                      
SB8        SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             33.5375      7.2500       0        "Solder Bridge 0402 ON"                                                                      
SB7        SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             33.5375      6.2500       0        "Solder Bridge 0402 ON"                                                                      
SB3        SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             33.4625      3.2500       180      "Solder Bridge 0402 ON"                                                                      
SB19       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             33.4625      21.5000      180      "Solder Bridge 0402 ON"                                                                      
SB17       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             33.5375      30.2500      0        "Solder Bridge 0402 ON"                                                                      
SB15       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             33.4625      20.5000      180      "Solder Bridge 0402 ON"                                                                      
SB13       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             33.5375      18.0000      0        "Solder Bridge 0402 ON"                                                                      
SB2        SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             26.2621      28.2741      90       "Solder Bridge 0402 ON"                                                                      
SB1        SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             26.2500      26.2125      270      "Solder Bridge 0402 ON"                                                                      
SC2        Shield-clip_S0951-46R       TopLayer    CLIP_HARWIN_S0981-46R              11.1948      18.5354      270      "shield clip Harwin S0981-46R to fix RF shielded cavity - SMT RFI Shield Clip, Corner (T+R)" 
SC1        Shield-clip_S0951-46R       TopLayer    CLIP_HARWIN_S0981-46R              29.3945      18.5354      0        "shield clip Harwin S0981-46R to fix RF shielded cavity - SMT RFI Shield Clip, Corner (T+R)" 
U3         IC_MX25xxx3xFMxI            BottomLayer ICC_SOIC8_3P91X4P90_P127_H1P75     29.2500      32.7500      90       "Memory, Serial NOR Flash, 1.65V to 3.6V, 32Mbits, 80MHz, SOP-8"                             
SH1        "RF Shield (22.2x19.2x2mm)" TopLayer    SHIELD_RF_ST-CUSTOM_22P2X19P2_H2   -275.4530    -237.3752    180      "RF Shield, 22.2x19.2x2mm"                                                                   
SC8        Shield-clip_S0951-46R       TopLayer    CLIP_HARWIN_S0981-46R              29.3944      33.7290      90       "shield clip Harwin S0981-46R to fix RF shielded cavity - SMT RFI Shield Clip, Corner (T+R)" 
SC7        Shield-clip_S0951-46R       TopLayer    CLIP_HARWIN_S0981-46R              11.1947      33.7290      180      "shield clip Harwin S0981-46R to fix RF shielded cavity - SMT RFI Shield Clip, Corner (T+R)" 
SB47       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             33.2875      34.2500      0        "Solder Bridge 0402 ON"                                                                      
SB46       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             22.1125      22.6500      0        "Resistor, 0R, SB0402, 5%, 0.063W"                                                           
SB45       SB_ON                       TopLayer    SOLDER-BRIDGE_R0402-0R             13.3096      27.2663      90       "Resistor, 0R, SB0402, 5%, 0.063W"                                                           
SB44       SB_ON                       TopLayer    SOLDER-BRIDGE_R0402-0R             12.1666      27.1913      270      "Resistor, 0R, SB0402, 5%, 0.063W"                                                           
SB43       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             12.2125      28.7500      180      "Solder Bridge 0402 ON"                                                                      
SB42       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             9.7875       28.7500      0        "Solder Bridge 0402 ON"                                                                      
SB41       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             33.5375      9.5000       0        "Solder Bridge 0402 ON"                                                                      
SB40       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             33.5375      8.5000       0        "Solder Bridge 0402 ON"                                                                      
SB39       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             33.4625      29.2500      180      "Solder Bridge 0402 ON"                                                                      
SB38       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             33.4625      14.5000      180      "Solder Bridge 0402 ON"                                                                      
SB37       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             33.4625      16.5000      180      "Solder Bridge 0402 ON"                                                                      
SB36       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             33.5375      2.0000       0        "Solder Bridge 0402 ON"                                                                      
SB35       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             9.7875       30.0000      0        "Solder Bridge 0402 ON"                                                                      
SB34       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             33.4625      26.2500      180      "Solder Bridge 0402 ON"                                                                      
SB33       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             33.5375      10.5000      0        "Solder Bridge 0402 ON"                                                                      
SB32       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             33.4625      11.5000      180      "Solder Bridge 0402 ON"                                                                      
SB31       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             9.7125       15.2500      180      "Solder Bridge 0402 ON"                                                                      
SB30       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             33.4625      25.0000      180      "Solder Bridge 0402 ON"                                                                      
SB29       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             33.4625      12.5000      180      "Solder Bridge 0402 ON"                                                                      
SB28       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             33.4625      27.2500      180      "Solder Bridge 0402 ON"                                                                      
SB27       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             9.7875       8.2500       0        "Solder Bridge 0402 ON"                                                                      
SB26       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             9.7875       19.0000      0        "Solder Bridge 0402 ON"                                                                      
SB25       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             33.4625      28.2500      180      "Solder Bridge 0402 ON"                                                                      
SB24       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             33.4625      15.5000      180      "Solder Bridge 0402 ON"                                                                      
SB23       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             33.4625      19.5000      180      "Solder Bridge 0402 ON"                                                                      
SB22       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             9.7875       6.5000       0        "Solder Bridge 0402 ON"                                                                      
SB21       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             9.7875       5.2500       0        "Solder Bridge 0402 ON"                                                                      
SB20       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             9.7875       11.0000      0        "Solder Bridge 0402 ON"                                                                      
SB11       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             9.7875       17.5000      0        "Solder Bridge 0402 ON"                                                                      
C21        Capacitor                   BottomLayer C0402                              33.2500      35.2500      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                    
U1         IC_STM32WBA25CEU6           TopLayer    ICC_UFQFPN48-EPAD_7X7_H0P55_P050   22.6500      28.0250      90       "MCU, ARM Cortex-M33 32-bit, 512KB Flash, 96KB RAM, Crypto"                                  
CN3        "Header 7x2"                TopLayer    CON_SAMTEC_FTSH-107-01-L-DV-K-A    21.5000      4.5790       0        "Header, 7x2, 1.27mm, VR, T=5.97mm, FTSH series STDC14 without Alignment Pin"                
ANT1       2.4GHz_BT_ANT               TopLayer    ANT_BT_BNRG_2P4GHZ_MB2032          17.7889      44.0656      90       "2.4 GHZ Bluetooth BNRG PCB antenna"                                                         
R9         Resistor                    TopLayer    R0402                              22.5000      9.7500       270      "Resistor, 100R, 0402, +/- 1%, 1/16W"                                                        
R8         Resistor                    TopLayer    R0402                              26.5000      9.7500       270      Resistor,47R,0402,1%,1/16W                                                                   
R7         Resistor                    TopLayer    R0402                              19.0000      9.7500       90       Resistor,47R,0402,1%,1/16W                                                                   
R6         Resistor                    TopLayer    R0402                              20.2500      9.7500       90       Resistor,47R,0402,1%,1/16W                                                                   
R5         Resistor                    TopLayer    R0402                              23.7500      9.7500       90       Resistor,47R,0402,1%,1/16W                                                                   
CN4        SMA-J-P-H-ST-EM1            TopLayer    CON_ROSENBERGER_32K141_40ML5       37.5926      39.0144      270      "Jack_SMA, VR, SMD, 50R, T=8.7mm"                                                            
CN1        FTSH-125-02-L-DV            BottomLayer CON_SAMTEC_FTSH-125-02-L-DV_INV    4.3664       18.5484      270      "Header, 25x2, 12.7mm, VR, SMD, T=4.83mm"                                                    
CN2        FTSH-125-02-L-DV            BottomLayer CON_SAMTEC_FTSH-125-02-L-DV_INV    38.6564      18.5484      270      "Header, 25x2, 12.7mm, VR, SMD, T=4.83mm"                                                    
C17        Capacitor                   TopLayer    C0402                              14.9860      24.7904      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                    
C15        Capacitor                   TopLayer    C0402                              19.1770      19.3876      270      "Capacitor, MLCC, 4.7uF, 6V3, X5R, +/-20%, 0402, T=0.5mm"                                    
C6         Capacitor                   TopLayer    C0402                              20.5500      33.6500      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                    
C7         Capacitor                   TopLayer    C0402                              27.9000      31.5750      180      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                    
C8         Capacitor                   TopLayer    C0402                              29.7500      26.5000      90       "Capacitor, MLCC, 6pF, 50V, NPO, +/-0,25pF, 0402, T=0.5mm"                                   
C14        Capacitor                   TopLayer    C0402                              23.3426      21.4772      90       "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                                      
L4         Inductor                    TopLayer    C0402                              20.7010      22.6388      270      "Inductor, 10nH, +/-2%, 0.5A, 260mR, 0402, T=0.5mm"                                          
L5         Inductor                    TopLayer    L0805_H0P9                         20.7010      20.2258      270      "Inductor, 2.2uH, +/-30%, 0.6A, 0R23, 0805, T=0.9mm"                                         
L3         Inductor                    TopLayer    IND_0402_MURATA_LQG15HSXXXX02_H0P5 17.7800      42.0116      90       "Inductor, 1.5nH, +/-0.3nH, 1A, 70mR, 0402, T=0.5mm"                                         
C19        Capacitor                   TopLayer    C0402                              15.2654      31.5976      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                    
C9         Capacitor                   TopLayer    C0402                              29.7500      28.5000      270      "Capacitor, MLCC, 6pF, 50V, NPO, +/-0,25pF, 0402, T=0.5mm"                                   
C16        Capacitor                   TopLayer    C0402                              18.2880      19.3876      270      "Capacitor, MLCC, 2.2uF, 6V3, X5R,+/-10%, 0402, T=0.5mm"                                     
L1         Resistor                    TopLayer    R0603                              12.5222      28.8544      180      "Resistor, 0R, 0603, +/-5%, 1/10W"                                                           
U2         MLPF-WB-04D3                TopLayer    ICC_CSPG_6BUMPS_1X1P60_P050-P0577  17.5188      32.4262      180      "IC, 2.4 GHz low pass filter matched to WBA mini board"                                      
C4         Capacitor                   TopLayer    C0603                              15.7987      33.4020      270      "Capacitor, MLCC, 470nF, 16V, X7R, +/-10%, 0603, T=0.8mm"                                    
C3         Capacitor                   TopLayer    C0402                              15.2654      30.4800      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                    
C20        Capacitor                   TopLayer    C0402                              19.7000      33.6500      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                    
X1         XTAL_4_PINS                 TopLayer    CRY_NX1612SA_4P                    15.2908      28.9814      180      "Crystal, 32MHz, 8pF, +/-10ppm, 40R, 1612(metric)"                                           
X2         XTAL_2_PINS                 TopLayer    CRY_NX1610SE_2P                    28.6500      27.5000      270      "Crystal, 32.768kHz, 6pF, +/-20ppm, 70KR, 1.6x1mm"                                           
SC3        Shield-clip_S0951-46R       TopLayer    CLIP_HARWIN_S0951-46R              9.1948       26.1500      90       "shield clip Harwin S0951-46R to fix RF shielded cavity"                                     
SC5        Shield-clip_S0951-46R       TopLayer    CLIP_HARWIN_S0951-46R              19.5000      16.5354      180      "shield clip Harwin S0951-46R to fix RF shielded cavity"                                     
SC4        Shield-clip_S0951-46R       TopLayer    CLIP_HARWIN_S0951-46R              31.3944      26.1500      90       "shield clip Harwin S0951-46R to fix RF shielded cavity"                                     
SB16       SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             33.4625      13.5000      180      "Solder Bridge 0402 ON"                                                                      
SB4        SB_ON                       BottomLayer SOLDER-BRIDGE_R0402-0R             31.7500      3.7125       270      "Solder Bridge 0402 ON"                                                                      
R10        Resistor                    BottomLayer R0402                              28.2000      22.6500      0        "Resistor, 10K, 0402, +/-1%, 1/16W"                                                          
R1         Resistor                    TopLayer    R0402                              17.7653      37.1510      90       "Resistor, 0R, 0402, +/-5%, 1/16W"                                                           
R3         Resistor                    TopLayer    R0402                              5.2500       29.2500      270      "Resistor, 100K, 0402, +/-1%, 1/16W"                                                         
R2         Resistor                    TopLayer    R0402                              18.2153      36.7010      0        "Resistor, 0R, 0402, +/-5%, 1/16W"                                                           
R4         Resistor                    TopLayer    R0402                              25.2500      9.7500       90       Resistor,47R,0402,1%,1/16W                                                                   
L2         Resistor                    TopLayer    R0603                              17.6784      22.2578      270      "Resistor, 0R, 0603, +/-5%, 1/10W"                                                           
C18        Capacitor                   TopLayer    C0402                              27.3456      22.2178      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                    
C5         Capacitor                   TopLayer    C0402                              15.6210      26.9240      270      "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                    
C13        Capacitor                   TopLayer    C0402                              17.7292      20.6322      0        "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm"                                      
C1         Capacitor                   TopLayer    C0402_H0P5                         17.3482      43.2308      0        "Capacitor, MLCC, 1.1pF, 50V, C0G, +/-0.05pF, 0402, T=0.5mm"                                 
C2         Capacitor                   TopLayer    C0402                              17.3228      40.8178      0        "Capacitor, MLCC, 1.5pF, 50V, C0G, +/-0.25pF, 0402, T=0.5mm"                                 
C11        Capacitor                   TopLayer    C0402                              14.9860      25.6032      0        "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                    
C12        Capacitor                   TopLayer    C0603                              18.9738      22.3340      270      "Capacitor, MLCC, 10uF, 6V3, X5R, +/-10%, 0603, T=0.8mm"                                     
C10        Capacitor                   TopLayer    C0402                              25.5000      22.2500      90       "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm"                                    
