# Design Rule Verification Report

Date: |  | 06/03/2025
Time: |  | 09:14:18
Elapsed Time: |  | 00:00:01
Filename: |  | C:\Users\jorda\Documents\Projets\STM Le Mans\MB2339A\BASE\MB2339A\01-Design-sources\Altium_Designer\MB2339.PcbDoc
Warnings: |  | 0
Rule Violations: |  | 0
Waived Violations: |  | 17

## Summary

Warnings | Count
--- | ---
Total | 0

Rule Violations | Count
--- | ---
Clearance Constraint (Gap=0.15mm) (All),(All) | 0
Clearance Constraint (Gap=0.5mm) (InNetClass('NC_RF-50R')),(All) | 0
Clearance Constraint (Gap=0.15mm) (All),(All) | 0
Clearance Constraint (Gap=0.15mm) (InNet('GND')),(All) | 0
Clearance Constraint (Gap=0.138mm) (WithinRoom('RoomDefinition_IPD')),(OnLayer('Top Layer')) | 0
Clearance Constraint (Gap=0.095mm) (touchesRoom('RoomDefinition_1')),(All) | 0
Clearance Constraint (Gap=0.15mm) (All),(IsKeepOut) | 0
Short-Circuit Constraint (Allowed=No) (All),(All) | 0
Un-Routed Net Constraint ( (All) ) | 0
Width Constraint (Min=0.15mm) (Max=10mm) (Preferred=0.2mm) (All) | 0
Width Constraint (Min=0.25mm) (Max=0.43mm) (Preferred=0.254mm) (InNetClass('NC_RF-50R')) | 0
Routing Layers(All) | 0
Routing Via (Templates Used To Check Via: v45h20m0mx0) (Disabled)(All) | 0
Differential Pairs Uncoupled Length using the Gap Constraints (Min=0.254mm) (Max=0.254mm) (Prefered=0.254mm) and Width Constraints (Min=0.381mm) (Max=0.381mm) (Prefered=0.381mm) (All) | 0
Power Plane Connect Rule(Relief Connect )(Expansion=0.508mm) (Conductor Width=0.21mm) (Air Gap=0.21mm) (Entries=4) (All) | 0
Hole To Hole Clearance (Gap=0.254mm) (All),(All) | 0
Net Antennae (Tolerance=0mm) (All) | 0
Vias Under SMD Constraint (Allowed=Allowed) (InPadClass('PC__VIAS-IN-PAD')) | 0
Component Clearance Constraint ( Horizontal Gap = 0.165mm, Vertical Gap = 0.165mm ) (All),(All) | 0
Height Constraint (Min=0mm) (Max=25.4mm) (Prefered=12.7mm) (All) | 0
Total | 0

Waived Violations | Count
--- | ---
Clearance Constraint (Gap=0.15mm) (All),(IsKeepOut) | 4
Component Clearance Constraint ( Horizontal Gap = 0.165mm, Vertical Gap = 0.165mm ) (All),(All) | 13
Total | 17

## Rule Violations

## Waived Violations

Clearance Constraint (Gap=0.15mm) (All),(IsKeepOut)
Clearance Constraint: (0.028mm < 0.15mm) Between Region (0 hole(s)) Top Layer And Region (0 hole(s)) Top Layer Waived by Jordane Gasnot at 24/02/2025 11:49:15 OK
Clearance Constraint: (0.138mm < 0.15mm) Between Region (0 hole(s)) Top Layer And Region (0 hole(s)) Top Layer Waived by Jordane Gasnot at 24/02/2025 11:49:15 OK
Clearance Constraint: (Collision < 0.15mm) Between Region (0 hole(s)) Top Layer And Region (0 hole(s)) Top Layer Waived by Jordane Gasnot at 24/02/2025 11:49:15 OK
Clearance Constraint: (Collision < 0.15mm) Between Region (0 hole(s)) Top Layer And Region (0 hole(s)) Top Layer Waived by Jordane Gasnot at 24/02/2025 11:49:15 OK

Back to top

Component Clearance Constraint ( Horizontal Gap = 0.165mm, Vertical Gap = 0.165mm ) (All),(All)
Component Clearance Constraint: (Collision < 0.165mm) Between SMT SIP Component SC12-Shield-clip_S0951-46R (24.09mm,11.775mm) on Top Layer And SMT Small Component HW1-S02-20150300 (21.5mm,24.275mm) on Top Layer Waived by Jordane Gasnot at 05/03/2025 09:02:27 Ok capot et clips en contact
Component Clearance Constraint: (Collision < 0.165mm) Between SMT SIP Component SC13-Shield-clip_S0951-46R (18.89mm,11.774mm) on Top Layer And SMT Small Component HW1-S02-20150300 (21.5mm,24.275mm) on Top Layer Waived by Jordane Gasnot at 05/03/2025 09:02:27 Ok capot et clips en contact
Component Clearance Constraint: (Collision < 0.165mm) Between SMT SIP Component SC1-Shield-clip_S0951-46R (18.65mm,36.775mm) on Top Layer And SMT Small Component HW1-S02-20150300 (21.5mm,24.275mm) on Top Layer Waived by Jordane Gasnot at 05/03/2025 09:02:27 Ok capot et clips en contact
Component Clearance Constraint: (Collision < 0.165mm) Between SMT SIP Component SC4-Shield-clip_S0951-46R (11.5mm,29.433mm) on Top Layer And SMT Small Component HW1-S02-20150300 (21.5mm,24.275mm) on Top Layer Waived by Jordane Gasnot at 05/03/2025 09:02:27 Ok capot et clips en contact
Component Clearance Constraint: (Collision < 0.165mm) Between SMT SIP Component SC5-Shield-clip_S0951-46R (31.5mm,29.433mm) on Top Layer And SMT Small Component HW1-S02-20150300 (21.5mm,24.275mm) on Top Layer Waived by Jordane Gasnot at 05/03/2025 09:02:27 Ok capot et clips en contact
Component Clearance Constraint: (Collision < 0.165mm) Between SMT SIP Component SC6-Shield-clip_S0951-46R (11.5mm,24.278mm) on Top Layer And SMT Small Component HW1-S02-20150300 (21.5mm,24.275mm) on Top Layer Waived by Jordane Gasnot at 05/03/2025 09:02:27 Ok capot et clips en contact
Component Clearance Constraint: (Collision < 0.165mm) Between SMT SIP Component SC7-Shield-clip_S0951-46R (31.5mm,24.278mm) on Top Layer And SMT Small Component HW1-S02-20150300 (21.5mm,24.275mm) on Top Layer Waived by Jordane Gasnot at 05/03/2025 09:02:27 Ok capot et clips en contact
Component Clearance Constraint: (Collision < 0.165mm) Between SMT SIP Component SC8-Shield-clip_S0951-46R (11.5mm,19.12mm) on Top Layer And SMT Small Component HW1-S02-20150300 (21.5mm,24.275mm) on Top Layer Waived by Jordane Gasnot at 05/03/2025 09:02:27 Ok capot et clips en contact
Component Clearance Constraint: (Collision < 0.165mm) Between SMT SIP Component SC9-Shield-clip_S0951-46R (31.5mm,19.12mm) on Top Layer And SMT Small Component HW1-S02-20150300 (21.5mm,24.275mm) on Top Layer Waived by Jordane Gasnot at 05/03/2025 09:02:27 Ok capot et clips en contact
Component Clearance Constraint: (Collision < 0.165mm) Between SMT Small Component HW1-S02-20150300 (21.5mm,24.275mm) on Top Layer And SMT Small Component SC10-Shield-clip_S0951-46R (11.5mm,11.775mm) on Top Layer Waived by Jordane Gasnot at 05/03/2025 09:02:27 Ok capot et clips en contact
Component Clearance Constraint: (Collision < 0.165mm) Between SMT Small Component HW1-S02-20150300 (21.5mm,24.275mm) on Top Layer And SMT Small Component SC11-Shield-clip_S0951-46R (31.5mm,11.775mm) on Top Layer Waived by Jordane Gasnot at 05/03/2025 09:02:27 Ok capot et clips en contact
Component Clearance Constraint: (Collision < 0.165mm) Between SMT Small Component HW1-S02-20150300 (21.5mm,24.275mm) on Top Layer And SMT Small Component SC2-Shield-clip_S0951-46R (11.5mm,36.775mm) on Top Layer Waived by Jordane Gasnot at 05/03/2025 09:02:27 Ok capot et clips en contact
Component Clearance Constraint: (Collision < 0.165mm) Between SMT Small Component HW1-S02-20150300 (21.5mm,24.275mm) on Top Layer And SMT Small Component SC3-Shield-clip_S0951-46R (31.5mm,36.775mm) on Top Layer Waived by Jordane Gasnot at 05/03/2025 09:02:27 Ok capot et clips en contact

Back to top