ACCEL_ASCII "MB2439.PrjPCB"
(asciiHeader
  (asciiVersion 3 0)
  (fileUnits Mil)
)
(netlist "Netlist_1"
  (globalAttrs
    (attr "Address1" "Not used" (textStyleRef "(Default)"))
    (attr "Address2" "Not used" (textStyleRef "(Default)"))
    (attr "Address3" "Not used" (textStyleRef "(Default)"))
    (attr "Address4" "Not used" (textStyleRef "(Default)"))
    (attr "Application_BuildNumber" "Not used" (textStyleRef "(Default)"))
    (attr "ApprovedBy" "Not used" (textStyleRef "(Default)"))
    (attr "Author" "Not used" (textStyleRef "(Default)"))
    (attr "CheckedBy" "Not used" (textStyleRef "(Default)"))
    (attr "CompanyName" "STMicroelectronics" (textStyleRef "(Default)"))
    (attr "CurrentDate" "12/02/2026" (textStyleRef "(Default)"))
    (attr "CurrentTime" "17:39:36" (textStyleRef "(Default)"))
    (attr "Date" "Not used" (textStyleRef "(Default)"))
    (attr "DocumentFullPathAndName" "C:\\Subversion\\_Boards\\MB2439_STM32WBA2_CSP37_SMPS_USB_IPD_4L\\Trunk\\01-Design_Source\\Altium_Designer\\Top.SchDoc" (textStyleRef "(Default)"))
    (attr "DocumentName" "Top.SchDoc" (textStyleRef "(Default)"))
    (attr "DocumentNumber" "Not used" (textStyleRef "(Default)"))
    (attr "DrawnBy" "Not used" (textStyleRef "(Default)"))
    (attr "Engineer" "Not used" (textStyleRef "(Default)"))
    (attr "ImagePath" "Not used" (textStyleRef "(Default)"))
    (attr "ModifiedDate" "08/12/2025" (textStyleRef "(Default)"))
    (attr "Organization" "Not used" (textStyleRef "(Default)"))
    (attr "ProjectName" "MB2439.PrjPCB" (textStyleRef "(Default)"))
    (attr "Revision" "Not used" (textStyleRef "(Default)"))
    (attr "SheetNumber" "2" (textStyleRef "(Default)"))
    (attr "SheetTotal" "4" (textStyleRef "(Default)"))
    (attr "Time" "Not used" (textStyleRef "(Default)"))
    (attr "Title" "Top Schematic" (textStyleRef "(Default)"))
  )
  (compInst "C2"
    (compRef "CAPACITOR")
    (originalName "CAPACITOR")
    (compValue "470nF")
    (attr "BMS_Part_Number" "9142003" (textStyleRef "(Default)"))
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Capacitor, MLCC, 470nF, 16V, X7R, +/-10%, 0603, T=0.8mm" (textStyleRef "(Default)"))
    (attr "ID" "3017" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01006" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "CC0603KRX7R7BB474" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-1428-1-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2370686" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "200-6576" (textStyleRef "(Default)"))
    (attr "Package" "0603" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Capacitor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "RF & Power Management Schematic" (textStyleRef "(Default)"))
  )
  (compInst "C3"
    (compRef "CAPACITOR")
    (originalName "CAPACITOR")
    (compValue "100nF")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm" (textStyleRef "(Default)"))
    (attr "ID" "2474" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-00006" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "CC0402KRX7R7BB104" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-1338-1-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "9402047" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "9402047" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Capacitor" (textStyleRef "(Default)"))
    (attr "Partial_Alternate_Internal_Part_Number" "MCD-03299" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "RF & Power Management Schematic" (textStyleRef "(Default)"))
  )
  (compInst "C4"
    (compRef "CAPACITOR")
    (originalName "CAPACITOR")
    (compValue "1uF")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm" (textStyleRef "(Default)"))
    (attr "ID" "3822" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01722" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "CC0402KRX5R6BB105" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-1439-1-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "1458896" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "N/A" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Capacitor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "C5"
    (compRef "CAPACITOR")
    (originalName "CAPACITOR")
    (compValue "1uF")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm" (textStyleRef "(Default)"))
    (attr "ID" "3822" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01722" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "CC0402KRX5R6BB105" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-1439-1-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "1458896" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "N/A" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Capacitor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "C6"
    (compRef "CAPACITOR")
    (originalName "CAPACITOR")
    (compValue "10uF")
    (attr "Component_Country_Of_Origin" "Japan" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/MURATA_GRM_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Capacitor, MLCC, 10uF, 10V, X6S, +/-20%, 0603, T=1mm" (textStyleRef "(Default)"))
    (attr "ID" "4845" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-02733" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "MURATA" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "GRM188C81A106MA73" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "490-7197-1-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "3581731" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "170-6242" (textStyleRef "(Default)"))
    (attr "Package" "0603" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Capacitor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Checked" (textStyleRef "(Default)"))
    (attr "Sheet" "RF & Power Management Schematic" (textStyleRef "(Default)"))
  )
  (compInst "C7"
    (compRef "CAPACITOR")
    (originalName "CAPACITOR")
    (compValue "100nF")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm" (textStyleRef "(Default)"))
    (attr "ID" "2474" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-00006" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "CC0402KRX7R7BB104" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-1338-1-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "9402047" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "9402047" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Capacitor" (textStyleRef "(Default)"))
    (attr "Partial_Alternate_Internal_Part_Number" "MCD-03299" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "C8"
    (compRef "CAPACITOR")
    (originalName "CAPACITOR")
    (compValue "6pF")
    (attr "Component_Country_Of_Origin" "Singapore" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/MURATA_GJM_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Capacitor, MLCC, 6pF, 50V, C0G/NP0, +/-0,25pF, 0402, T=0.5mm" (textStyleRef "(Default)"))
    (attr "ID" "5301" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-03185" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "MURATA" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "GJM1555C1H6R0CB01" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "490-3104-2-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2995032" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "170-6040" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Capacitor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Checked" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "C9"
    (compRef "CAPACITOR")
    (originalName "CAPACITOR")
    (compValue "6pF")
    (attr "Component_Country_Of_Origin" "Singapore" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/MURATA_GJM_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Capacitor, MLCC, 6pF, 50V, C0G/NP0, +/-0,25pF, 0402, T=0.5mm" (textStyleRef "(Default)"))
    (attr "ID" "5301" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-03185" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "MURATA" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "GJM1555C1H6R0CB01" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "490-3104-2-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2995032" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "170-6040" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Capacitor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Checked" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "C10"
    (compRef "CAPACITOR")
    (originalName "CAPACITOR")
    (compValue "1uF")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm" (textStyleRef "(Default)"))
    (attr "ID" "3822" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01722" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "CC0402KRX5R6BB105" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-1439-1-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "1458896" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "N/A" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Capacitor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "C11"
    (compRef "CAPACITOR")
    (originalName "CAPACITOR")
    (compValue "1uF")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm" (textStyleRef "(Default)"))
    (attr "ID" "3822" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01722" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "CC0402KRX5R6BB105" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-1439-1-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "1458896" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "N/A" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Capacitor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "C15"
    (compRef "CAPACITOR")
    (originalName "CAPACITOR")
    (compValue "1uF")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm" (textStyleRef "(Default)"))
    (attr "ID" "3822" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01722" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "CC0402KRX5R6BB105" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-1439-1-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "1458896" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "N/A" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Capacitor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "C16"
    (compRef "CAPACITOR")
    (originalName "CAPACITOR")
    (compValue "100nF")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm" (textStyleRef "(Default)"))
    (attr "ID" "2474" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-00006" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "CC0402KRX7R7BB104" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-1338-1-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "9402047" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "9402047" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Capacitor" (textStyleRef "(Default)"))
    (attr "Partial_Alternate_Internal_Part_Number" "MCD-03299" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "RF & Power Management Schematic" (textStyleRef "(Default)"))
  )
  (compInst "C17"
    (compRef "CAPACITOR")
    (originalName "CAPACITOR")
    (compValue "100nF")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm" (textStyleRef "(Default)"))
    (attr "ID" "2474" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-00006" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "CC0402KRX7R7BB104" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-1338-1-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "9402047" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "9402047" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Capacitor" (textStyleRef "(Default)"))
    (attr "Partial_Alternate_Internal_Part_Number" "MCD-03299" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "RF & Power Management Schematic" (textStyleRef "(Default)"))
  )
  (compInst "C18"
    (compRef "CAPACITOR")
    (originalName "CAPACITOR")
    (compValue "100nF")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm" (textStyleRef "(Default)"))
    (attr "ID" "2474" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-00006" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "CC0402KRX7R7BB104" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-1338-1-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "9402047" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "9402047" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Capacitor" (textStyleRef "(Default)"))
    (attr "Partial_Alternate_Internal_Part_Number" "MCD-03299" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "RF & Power Management Schematic" (textStyleRef "(Default)"))
  )
  (compInst "C19"
    (compRef "CAPACITOR")
    (originalName "CAPACITOR")
    (compValue "100nF")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm" (textStyleRef "(Default)"))
    (attr "ID" "2474" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-00006" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "CC0402KRX7R7BB104" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-1338-1-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "9402047" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "9402047" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Capacitor" (textStyleRef "(Default)"))
    (attr "Partial_Alternate_Internal_Part_Number" "MCD-03299" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "RF & Power Management Schematic" (textStyleRef "(Default)"))
  )
  (compInst "C20"
    (compRef "CAPACITOR")
    (originalName "CAPACITOR")
    (compValue "1uF")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm" (textStyleRef "(Default)"))
    (attr "ID" "3822" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01722" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "CC0402KRX5R6BB105" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-1439-1-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "1458896" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "N/A" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Capacitor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "RF & Power Management Schematic" (textStyleRef "(Default)"))
  )
  (compInst "C21"
    (compRef "CAPACITOR")
    (originalName "CAPACITOR")
    (compValue "1uF")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm" (textStyleRef "(Default)"))
    (attr "ID" "3822" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01722" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "CC0402KRX5R6BB105" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-1439-1-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "1458896" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "N/A" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Capacitor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "RF & Power Management Schematic" (textStyleRef "(Default)"))
  )
  (compInst "C22"
    (compRef "CAPACITOR")
    (originalName "CAPACITOR")
    (compValue "1uF")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm" (textStyleRef "(Default)"))
    (attr "ID" "3822" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01722" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "CC0402KRX5R6BB105" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-1439-1-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "1458896" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "N/A" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Capacitor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "RF & Power Management Schematic" (textStyleRef "(Default)"))
  )
  (compInst "C23"
    (compRef "CAPACITOR")
    (originalName "CAPACITOR")
    (compValue "4.7uF")
    (attr "Component_Country_Of_Origin" "Japan°°" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/MURATA_GRM_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Capacitor, MLCC, 4.7uF, 6V3, X5R, 20%, 0402, T=0.5mm" (textStyleRef "(Default)"))
    (attr "ID" "3456" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01356" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "MURATA" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "GRM155R60J475ME47" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "490-5915-1-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2666407" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "814-5230" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Capacitor" (textStyleRef "(Default)"))
    (attr "Partial_Alternate_Internal_Part_Number" "MCD-04455" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "RF & Power Management Schematic" (textStyleRef "(Default)"))
  )
  (compInst "C24"
    (compRef "CAPACITOR")
    (originalName "CAPACITOR")
    (compValue "100nF")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm" (textStyleRef "(Default)"))
    (attr "ID" "2474" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-00006" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "CC0402KRX7R7BB104" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-1338-1-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "9402047" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "9402047" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Capacitor" (textStyleRef "(Default)"))
    (attr "Partial_Alternate_Internal_Part_Number" "MCD-03299" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "RF & Power Management Schematic" (textStyleRef "(Default)"))
  )
  (compInst "C26"
    (compRef "CAPACITOR")
    (originalName "CAPACITOR")
    (compValue "100nF")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X7R_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Capacitor, MLCC, 100nF, 16V, X7R, +/-10%, 0402, T=0.5mm" (textStyleRef "(Default)"))
    (attr "ID" "2474" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-00006" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "CC0402KRX7R7BB104" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-1338-1-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "9402047" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "9402047" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Capacitor" (textStyleRef "(Default)"))
    (attr "Partial_Alternate_Internal_Part_Number" "MCD-03299" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "RF & Power Management Schematic" (textStyleRef "(Default)"))
  )
  (compInst "C27"
    (compRef "CAPACITOR")
    (originalName "CAPACITOR")
    (compValue "1uF")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm" (textStyleRef "(Default)"))
    (attr "ID" "3822" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01722" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "CC0402KRX5R6BB105" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-1439-1-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "1458896" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "N/A" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Capacitor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "C32"
    (compRef "CAPACITOR")
    (originalName "CAPACITOR")
    (compValue "1uF")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Capacitor/YAGEO_X5R_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Capacitor, MLCC, 1uF, 10V, X5R, +/-10%, 0402, T=0.5mm" (textStyleRef "(Default)"))
    (attr "ID" "3822" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01722" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "CC0402KRX5R6BB105" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-1439-1-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "1458896" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "N/A" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Capacitor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "CN1"
    (compRef "HEADER_25X2")
    (originalName "HEADER_25X2")
    (compValue "Header 25x2")
    (attr "Component_Country_Of_Origin" "China, Costa Rica, Malaysia, USA, Vietnam" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Connector/SAMTEC_FTSH_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Header, 25x2, 1.27mm, VR, SMD, T=4.83mm" (textStyleRef "(Default)"))
    (attr "ID" "4858" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-02746" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "SAMTEC" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "FTSH-125-02-L-DV" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "FTSH-125-02-L-DV-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "3751075" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "N/A" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Connector" (textStyleRef "(Default)"))
    (attr "Partial_Alternate_Internal_Part_Number" "MCD-03741" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "CN2"
    (compRef "HEADER_25X2")
    (originalName "HEADER_25X2")
    (compValue "Header 25x2")
    (attr "Component_Country_Of_Origin" "China, Costa Rica, Malaysia, USA, Vietnam" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Connector/SAMTEC_FTSH_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Header, 25x2, 1.27mm, VR, SMD, T=4.83mm" (textStyleRef "(Default)"))
    (attr "ID" "4858" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-02746" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "SAMTEC" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "FTSH-125-02-L-DV" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "FTSH-125-02-L-DV-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "3751075" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "N/A" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Connector" (textStyleRef "(Default)"))
    (attr "Partial_Alternate_Internal_Part_Number" "MCD-03741" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "CN3"
    (compRef "HEADER_7X2")
    (originalName "HEADER_7X2")
    (compValue "Header 7x2")
    (attr "Component_Country_Of_Origin" "China, Costa Rica, Malaysia, United States, Vietnam" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Connector/SAMTEC_FTSH_Series/" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Header, 7x2, 1.27mm, VR, T=5.97mm, FTSH series STDC14 without Alignment Pin" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01531" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "SAMTEC" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "FTSH-107-01-L-DV-K" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "SAM9449-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2856443" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "179-9021" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Connector" (textStyleRef "(Default)"))
    (attr "Status" "Checked" (textStyleRef "(Default)"))
    (attr "Sheet" "RF & Power Management Schematic" (textStyleRef "(Default)"))
  )
  (compInst "CN4"
    (compRef "SMA-J-P-H-ST-EM1")
    (originalName "SMA-J-P-H-ST-EM1")
    (compValue "Jack_SMA_142-0701-851")
    (attr "Component_Country_Of_Origin" "USA°°" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Connector/CINCH_142-0701-851" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Jack_SMA, VR, PCB edge, 50R, T=7.92mm" (textStyleRef "(Default)"))
    (attr "ID" "4172" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-02072" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "CINCH" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "142-0701-851" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "J658-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "1019325" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "885-7532" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Connector" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "RF & Power Management Schematic" (textStyleRef "(Default)"))
  )
  (compInst "D1"
    (compRef "SCHOTTKY_1A_2K")
    (originalName "SCHOTTKY_1A_2K")
    (compValue "BAT54KFILM")
    (attr "BMS_Part_Number" "9151123" (textStyleRef "(Default)"))
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Diode/STMICROELECTRONICS_BAT54_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Diode, Schottky, 0V9, 100mA, 40V, SOD-523" (textStyleRef "(Default)"))
    (attr "ID" "3777" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01677" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "STMICROELECTRONICS" (textStyleRef "(Default)"))
    (attr "Manufacturer_HQ_COO" "EU" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "BAT54KFILM" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "497-5561-2-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2341638" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "714-6869" (textStyleRef "(Default)"))
    (attr "Package" "SOD-523" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Diode" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "HW1"
    (compRef "SHIELD_COVER")
    (originalName "SHIELD_COVER")
    (compValue "36003200")
    (attr "Component_Country_Of_Origin" "Germany°" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Misc/WURTH_ELEKTRONIK_36003200" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "RF Shield cover, 21.5x21.5x3.3mm" (textStyleRef "(Default)"))
    (attr "ID" "6802" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-04686" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "WURTH ELEKTRONIK" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "36003200" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "732-2488-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "1909659" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "773-7282" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Misc" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Checked" (textStyleRef "(Default)"))
    (attr "Sheet" "RF & Power Management Schematic" (textStyleRef "(Default)"))
  )
  (compInst "HW2"
    (compRef "PCB")
    (originalName "PCB")
    (compValue "MB2439")
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/PCB/MB2439" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "PCB, MB2439, 47x43mm, 4L2S, 1.6mm, standard, FR4" (textStyleRef "(Default)"))
    (attr "ID" "7096" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-04980" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "PLOTEC" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "N/A" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "N/A" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "N/A" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "N/A" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "PCB" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Technically approved" (textStyleRef "(Default)"))
    (attr "Sheet" "Project_Overview" (textStyleRef "(Default)"))
  )
  (compInst "HW3"
    (compRef "STICKER_PRODUCT")
    (originalName "STICKER_PRODUCT")
    (compValue "Sticker Product")
    (attr "Component_Country_Of_Origin" "Unknown" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Sticker product, 25x9mm" (textStyleRef "(Default)"))
    (attr "ID" "3197" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-00547" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "N/A" (textStyleRef "(Default)"))
    (attr "Manufacturer_HQ_COO" "Unknown" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "N/A" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "N/A" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "N/A" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "N/A" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Misc" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "Project_Overview" (textStyleRef "(Default)"))
  )
  (compInst "HW4"
    (compRef "STICKER_ES")
    (originalName "STICKER_ES")
    (compValue "N/A")
    (attr "Component_Country_Of_Origin" "Unknown" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Sticker ES, 6x6mm" (textStyleRef "(Default)"))
    (attr "ID" "2634" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-00234" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "N/A" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "N/A" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "N/A" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "N/A" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "N/A" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Misc" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "Project_Overview" (textStyleRef "(Default)"))
  )
  (compInst "L4"
    (compRef "BEAD")
    (originalName "BEAD")
    (compValue "33R @ 100MHz")
    (attr "Component_Country_Of_Origin" "Japan, Thailand" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Inductor/MURATA_BLM_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Ferrite bead, 33R @ 100MHz, 3A, 22mR, 0402, T=0.5mm" (textStyleRef "(Default)"))
    (attr "ID" "6488" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-04372" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "MURATA" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "BLM15PX330SN1" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "490-10661-2-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "3471086" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "N/A" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Inductor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Checked" (textStyleRef "(Default)"))
    (attr "Sheet" "RF & Power Management Schematic" (textStyleRef "(Default)"))
  )
  (compInst "L5"
    (compRef "INDUCTOR")
    (originalName "INDUCTOR")
    (compValue "10nH")
    (attr "Component_Country_Of_Origin" "Japan" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Inductor/MURATA_LQG15HS10NJ02" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Inductor, 10nH, +/-2%, 0.5A, 260mR, 0402, T=0.5mm" (textStyleRef "(Default)"))
    (attr "ID" "5151" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-03035" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "MURATA" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "LQG15HS10NJ02D" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "490-2623-1-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2840111RL" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "124-8162" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Inductor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Checked" (textStyleRef "(Default)"))
    (attr "Sheet" "RF & Power Management Schematic" (textStyleRef "(Default)"))
  )
  (compInst "L6"
    (compRef "INDUCTOR")
    (originalName "INDUCTOR")
    (compValue "2.2uH")
    (attr "Component_Country_Of_Origin" "Japan" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Inductor/MURATA_LQM_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Inductor, 2.2uH, +/-30%, 0.6A, 0R23, 0805, T=0.9mm" (textStyleRef "(Default)"))
    (attr "ID" "6807" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-04691" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "MURATA" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "LQM21PN2R2NGC" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "490-7781-2-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2470293" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "167-4839" (textStyleRef "(Default)"))
    (attr "Package" "0805" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Inductor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Checked" (textStyleRef "(Default)"))
    (attr "Sheet" "RF & Power Management Schematic" (textStyleRef "(Default)"))
  )
  (compInst "L7"
    (compRef "BEAD")
    (originalName "BEAD")
    (compValue "33R @ 100MHz")
    (attr "Component_Country_Of_Origin" "Japan, Thailand" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Inductor/MURATA_BLM_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Ferrite bead, 33R @ 100MHz, 3A, 22mR, 0402, T=0.5mm" (textStyleRef "(Default)"))
    (attr "ID" "6488" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-04372" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "MURATA" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "BLM15PX330SN1" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "490-10661-2-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "3471086" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "N/A" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Inductor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Checked" (textStyleRef "(Default)"))
    (attr "Sheet" "RF & Power Management Schematic" (textStyleRef "(Default)"))
  )
  (compInst "R1"
    (compRef "RESISTOR")
    (originalName "RESISTOR")
    (compValue "100K")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Resistor, 100K, 0402, +/-1%, 1/16W" (textStyleRef "(Default)"))
    (attr "ID" "2533" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-00059" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "RC0402FR-07100KL" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-100KLRTR-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2421891" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "2421891" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Resistor" (textStyleRef "(Default)"))
    (attr "Partial_Alternate_Internal_Part_Number" "MCD-03301" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "R2"
    (compRef "RESISTOR")
    (originalName "RESISTOR")
    (compValue "47R")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Resistor, 47R, 0402, +/-1%, 1/16W" (textStyleRef "(Default)"))
    (attr "ID" "2796" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-00481" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "RC0402FR-0747RL" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-47.0LRCT-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "9239073" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "N/A" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Resistor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "RF & Power Management Schematic" (textStyleRef "(Default)"))
  )
  (compInst "R3"
    (compRef "RESISTOR")
    (originalName "RESISTOR")
    (compValue "47R")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Resistor, 47R, 0402, +/-1%, 1/16W" (textStyleRef "(Default)"))
    (attr "ID" "2796" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-00481" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "RC0402FR-0747RL" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-47.0LRCT-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "9239073" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "N/A" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Resistor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "RF & Power Management Schematic" (textStyleRef "(Default)"))
  )
  (compInst "R4"
    (compRef "RESISTOR")
    (originalName "RESISTOR")
    (compValue "47R")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Resistor, 47R, 0402, +/-1%, 1/16W" (textStyleRef "(Default)"))
    (attr "ID" "2796" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-00481" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "RC0402FR-0747RL" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-47.0LRCT-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "9239073" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "N/A" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Resistor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "RF & Power Management Schematic" (textStyleRef "(Default)"))
  )
  (compInst "R5"
    (compRef "RESISTOR")
    (originalName "RESISTOR")
    (compValue "47R")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Resistor, 47R, 0402, +/-1%, 1/16W" (textStyleRef "(Default)"))
    (attr "ID" "2796" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-00481" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "RC0402FR-0747RL" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-47.0LRCT-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "9239073" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "N/A" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Resistor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "RF & Power Management Schematic" (textStyleRef "(Default)"))
  )
  (compInst "R6"
    (compRef "RESISTOR")
    (originalName "RESISTOR")
    (compValue "47R")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Resistor, 47R, 0402, +/-1%, 1/16W" (textStyleRef "(Default)"))
    (attr "ID" "2796" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-00481" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "RC0402FR-0747RL" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-47.0LRCT-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "9239073" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "N/A" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Resistor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "RF & Power Management Schematic" (textStyleRef "(Default)"))
  )
  (compInst "R7"
    (compRef "RESISTOR")
    (originalName "RESISTOR")
    (compValue "47R")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Resistor, 47R, 0402, +/-1%, 1/16W" (textStyleRef "(Default)"))
    (attr "ID" "2796" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-00481" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "RC0402FR-0747RL" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-47.0LRCT-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "9239073" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "N/A" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Resistor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "RF & Power Management Schematic" (textStyleRef "(Default)"))
  )
  (compInst "R8"
    (compRef "RESISTOR")
    (originalName "RESISTOR")
    (compValue "47R")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Resistor, 47R, 0402, +/-1%, 1/16W" (textStyleRef "(Default)"))
    (attr "ID" "2796" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-00481" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "RC0402FR-0747RL" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-47.0LRCT-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "9239073" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "N/A" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Resistor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "RF & Power Management Schematic" (textStyleRef "(Default)"))
  )
  (compInst "R9"
    (compRef "RESISTOR")
    (originalName "RESISTOR")
    (compValue "47R")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC_L_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Resistor, 47R, 0402, +/-1%, 1/16W" (textStyleRef "(Default)"))
    (attr "ID" "2796" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-00481" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "RC0402FR-0747RL" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-47.0LRCT-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "9239073" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "N/A" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Resistor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "RF & Power Management Schematic" (textStyleRef "(Default)"))
  )
  (compInst "SB1"
    (compRef "SB_ON")
    (originalName "SB_ON")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC0402_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Resistor, 0R, SB0402, 5%, 0.063W" (textStyleRef "(Default)"))
    (attr "ID" "3718" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01618" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "RC0402JR-070RL" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-0.0JRTR-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2363467" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "618-5804" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Resistor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "SB2"
    (compRef "SB_ON")
    (originalName "SB_ON")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC0402_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Resistor, 0R, SB0402, 5%, 0.063W" (textStyleRef "(Default)"))
    (attr "ID" "3718" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01618" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "RC0402JR-070RL" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-0.0JRTR-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2363467" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "618-5804" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Resistor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "SB4"
    (compRef "SB_ON")
    (originalName "SB_ON")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC0402_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Resistor, 0R, SB0402, 5%, 0.063W" (textStyleRef "(Default)"))
    (attr "ID" "3718" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01618" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "RC0402JR-070RL" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-0.0JRTR-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2363467" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "618-5804" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Resistor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "SB5"
    (compRef "SB_ON")
    (originalName "SB_ON")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC0402_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Resistor, 0R, SB0402, 5%, 0.063W" (textStyleRef "(Default)"))
    (attr "ID" "3718" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01618" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "RC0402JR-070RL" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-0.0JRTR-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2363467" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "618-5804" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Resistor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "SB6"
    (compRef "SB_ON")
    (originalName "SB_ON")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC0402_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Resistor, 0R, SB0402, 5%, 0.063W" (textStyleRef "(Default)"))
    (attr "ID" "3718" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01618" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "RC0402JR-070RL" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-0.0JRTR-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2363467" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "618-5804" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Resistor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "RF & Power Management Schematic" (textStyleRef "(Default)"))
  )
  (compInst "SB9"
    (compRef "SB_ON")
    (originalName "SB_ON")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC0402_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Resistor, 0R, SB0402, 5%, 0.063W" (textStyleRef "(Default)"))
    (attr "ID" "3718" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01618" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "RC0402JR-070RL" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-0.0JRTR-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2363467" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "618-5804" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Resistor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "SB10"
    (compRef "SB_ON")
    (originalName "SB_ON")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC0402_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Resistor, 0R, SB0402, 5%, 0.063W" (textStyleRef "(Default)"))
    (attr "ID" "3718" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01618" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "RC0402JR-070RL" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-0.0JRTR-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2363467" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "618-5804" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Resistor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "SB11"
    (compRef "SB_ON")
    (originalName "SB_ON")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC0402_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Resistor, 0R, SB0402, 5%, 0.063W" (textStyleRef "(Default)"))
    (attr "ID" "3718" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01618" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "RC0402JR-070RL" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-0.0JRTR-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2363467" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "618-5804" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Resistor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "SB12"
    (compRef "SB_ON")
    (originalName "SB_ON")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC0402_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Resistor, 0R, SB0402, 5%, 0.063W" (textStyleRef "(Default)"))
    (attr "ID" "3718" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01618" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "RC0402JR-070RL" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-0.0JRTR-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2363467" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "618-5804" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Resistor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "SB15"
    (compRef "SB_ON")
    (originalName "SB_ON")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC0402_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Resistor, 0R, SB0402, 5%, 0.063W" (textStyleRef "(Default)"))
    (attr "ID" "3718" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01618" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "RC0402JR-070RL" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-0.0JRTR-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2363467" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "618-5804" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Resistor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "SB16"
    (compRef "SB_ON")
    (originalName "SB_ON")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC0402_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Resistor, 0R, SB0402, 5%, 0.063W" (textStyleRef "(Default)"))
    (attr "ID" "3718" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01618" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "RC0402JR-070RL" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-0.0JRTR-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2363467" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "618-5804" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Resistor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "SB18"
    (compRef "SB_ON")
    (originalName "SB_ON")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC0402_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Resistor, 0R, SB0402, 5%, 0.063W" (textStyleRef "(Default)"))
    (attr "ID" "3718" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01618" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "RC0402JR-070RL" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-0.0JRTR-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2363467" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "618-5804" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Resistor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "SB19"
    (compRef "SB_ON")
    (originalName "SB_ON")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC0402_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Resistor, 0R, SB0402, 5%, 0.063W" (textStyleRef "(Default)"))
    (attr "ID" "3718" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01618" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "RC0402JR-070RL" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-0.0JRTR-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2363467" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "618-5804" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Resistor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "SB20"
    (compRef "SB_ON")
    (originalName "SB_ON")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC0402_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Resistor, 0R, SB0402, 5%, 0.063W" (textStyleRef "(Default)"))
    (attr "ID" "3718" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01618" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "RC0402JR-070RL" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-0.0JRTR-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2363467" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "618-5804" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Resistor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "SB21"
    (compRef "SB_ON")
    (originalName "SB_ON")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC0402_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Resistor, 0R, SB0402, 5%, 0.063W" (textStyleRef "(Default)"))
    (attr "ID" "3718" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01618" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "RC0402JR-070RL" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-0.0JRTR-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2363467" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "618-5804" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Resistor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "SB22"
    (compRef "SB_ON")
    (originalName "SB_ON")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC0402_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Resistor, 0R, SB0402, 5%, 0.063W" (textStyleRef "(Default)"))
    (attr "ID" "3718" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01618" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "RC0402JR-070RL" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-0.0JRTR-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2363467" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "618-5804" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Resistor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "SB23"
    (compRef "SB_ON")
    (originalName "SB_ON")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC0402_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Resistor, 0R, SB0402, 5%, 0.063W" (textStyleRef "(Default)"))
    (attr "ID" "3718" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01618" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "RC0402JR-070RL" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-0.0JRTR-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2363467" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "618-5804" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Resistor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "SB24"
    (compRef "SB_ON")
    (originalName "SB_ON")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC0402_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Resistor, 0R, SB0402, 5%, 0.063W" (textStyleRef "(Default)"))
    (attr "ID" "3718" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01618" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "RC0402JR-070RL" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-0.0JRTR-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2363467" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "618-5804" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Resistor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "SB25"
    (compRef "SB_ON")
    (originalName "SB_ON")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC0402_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Resistor, 0R, SB0402, 5%, 0.063W" (textStyleRef "(Default)"))
    (attr "ID" "3718" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01618" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "RC0402JR-070RL" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-0.0JRTR-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2363467" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "618-5804" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Resistor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "SB27"
    (compRef "SB_ON")
    (originalName "SB_ON")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC0402_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Resistor, 0R, SB0402, 5%, 0.063W" (textStyleRef "(Default)"))
    (attr "ID" "3718" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01618" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "RC0402JR-070RL" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-0.0JRTR-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2363467" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "618-5804" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Resistor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "SB32"
    (compRef "SB_ON")
    (originalName "SB_ON")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC0402_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Resistor, 0R, SB0402, 5%, 0.063W" (textStyleRef "(Default)"))
    (attr "ID" "3718" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01618" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "RC0402JR-070RL" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-0.0JRTR-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2363467" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "618-5804" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Resistor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "SB37"
    (compRef "SB_ON")
    (originalName "SB_ON")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC0402_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Resistor, 0R, SB0402, 5%, 0.063W" (textStyleRef "(Default)"))
    (attr "ID" "3718" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01618" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "RC0402JR-070RL" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-0.0JRTR-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2363467" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "618-5804" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Resistor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "SB38"
    (compRef "SB_ON")
    (originalName "SB_ON")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC0402_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Resistor, 0R, SB0402, 5%, 0.063W" (textStyleRef "(Default)"))
    (attr "ID" "3718" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01618" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "RC0402JR-070RL" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-0.0JRTR-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2363467" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "618-5804" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Resistor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "SB39"
    (compRef "SB_ON")
    (originalName "SB_ON")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC0402_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Resistor, 0R, SB0402, 5%, 0.063W" (textStyleRef "(Default)"))
    (attr "ID" "3718" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01618" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "RC0402JR-070RL" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-0.0JRTR-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2363467" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "618-5804" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Resistor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "SB40"
    (compRef "SB_ON")
    (originalName "SB_ON")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC0402_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Resistor, 0R, SB0402, 5%, 0.063W" (textStyleRef "(Default)"))
    (attr "ID" "3718" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01618" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "RC0402JR-070RL" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-0.0JRTR-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2363467" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "618-5804" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Resistor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "SB41"
    (compRef "SB_ON")
    (originalName "SB_ON")
    (attr "Component_Country_Of_Origin" "China" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Resistor/YAGEO_RC0402_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Resistor, 0R, SB0402, 5%, 0.063W" (textStyleRef "(Default)"))
    (attr "ID" "3718" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01618" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "YAGEO" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "RC0402JR-070RL" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "311-0.0JRTR-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2363467" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "618-5804" (textStyleRef "(Default)"))
    (attr "Package" "0402" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Resistor" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "RF & Power Management Schematic" (textStyleRef "(Default)"))
  )
  (compInst "SC1"
    (compRef "SHIELD-CLIP_S0951-46R")
    (originalName "SHIELD-CLIP_S0951-46R")
    (compValue "S0951-46R")
    (attr "Component_Country_Of_Origin" "South Korea" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Connectors/Harwin_Shield-clip_S0951-46R" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "shield clip Harwin S0951-46R to fix RF shielded cavity" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01587" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "HARWIN" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "S0951-46R" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "952-2669-1-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2490970" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "N/A" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Misc" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "RF & Power Management Schematic" (textStyleRef "(Default)"))
  )
  (compInst "SC2"
    (compRef "SHIELD-CLIP_S0951-46R")
    (originalName "SHIELD-CLIP_S0951-46R")
    (compValue "S0951-46R")
    (attr "Component_Country_Of_Origin" "South Korea" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Connectors/Harwin_Shield-clip_S0951-46R" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "shield clip Harwin S0951-46R to fix RF shielded cavity" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01587" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "HARWIN" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "S0951-46R" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "952-2669-1-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2490970" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "N/A" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Misc" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "RF & Power Management Schematic" (textStyleRef "(Default)"))
  )
  (compInst "SC3"
    (compRef "SHIELD-CLIP_S0951-46R")
    (originalName "SHIELD-CLIP_S0951-46R")
    (compValue "S0951-46R")
    (attr "Component_Country_Of_Origin" "South Korea" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Connectors/Harwin_Shield-clip_S0951-46R" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "shield clip Harwin S0951-46R to fix RF shielded cavity" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01587" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "HARWIN" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "S0951-46R" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "952-2669-1-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2490970" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "N/A" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Misc" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "RF & Power Management Schematic" (textStyleRef "(Default)"))
  )
  (compInst "SC4"
    (compRef "SHIELD-CLIP_S0951-46R")
    (originalName "SHIELD-CLIP_S0951-46R")
    (compValue "S0951-46R")
    (attr "Component_Country_Of_Origin" "South Korea" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Connectors/Harwin_Shield-clip_S0951-46R" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "shield clip Harwin S0951-46R to fix RF shielded cavity" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01587" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "HARWIN" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "S0951-46R" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "952-2669-1-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2490970" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "N/A" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Misc" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "RF & Power Management Schematic" (textStyleRef "(Default)"))
  )
  (compInst "SC5"
    (compRef "SHIELD-CLIP_S0951-46R")
    (originalName "SHIELD-CLIP_S0951-46R")
    (compValue "S0951-46R")
    (attr "Component_Country_Of_Origin" "South Korea" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Datasheet_Library/Trunk/Connectors/Harwin_Shield-clip_S0951-46R" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "shield clip Harwin S0951-46R to fix RF shielded cavity" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-01587" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "HARWIN" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "S0951-46R" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "952-2669-1-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "2490970" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "N/A" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Misc" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "RF & Power Management Schematic" (textStyleRef "(Default)"))
  )
  (compInst "U1"
    (compRef "IC_STM32WBA25HEF6")
    (originalName "IC_STM32WBA25HEF6")
    (compValue "STM32WBA25HEF7")
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/IC/STMICROELECTRONICS_STM32WBA25HEF" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "MCU, ARM Cortex-M33 32-bit, 512KB Flash, 96KB RAM, Crypto" (textStyleRef "(Default)"))
    (attr "ID" "7054" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-04938" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "STMICROELECTRONICS" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "STM32WBA25HEF7" (textStyleRef "(Default)"))
    (attr "Order_code_Digikey" "N/A" (textStyleRef "(Default)"))
    (attr "Order_code_Farnell" "N/A" (textStyleRef "(Default)"))
    (attr "Order_code_RS" "N/A" (textStyleRef "(Default)"))
    (attr "Package" "WLCSP37" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "IC" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "New" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "U2"
    (compRef "IC_MLPF-WB-05D3")
    (originalName "IC_MLPF-WB-05D3")
    (compValue "MLPF-WB-05D3")
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/IC/STMICROELECTRONICS_MLPF-WB-05D3/" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "IC, 2.4GHz low pass filter matched to WBA CSP package mini board" (textStyleRef "(Default)"))
    (attr "ID" "7241" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-05125" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "STMICROELECTRONICS" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "MLPF-WB-05D3" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "497-MLPF-WB-05D3CT-ND" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "4785178" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "719-629" (textStyleRef "(Default)"))
    (attr "Package" "CSP6" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "IC" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Technically approved" (textStyleRef "(Default)"))
    (attr "Sheet" "RF & Power Management Schematic" (textStyleRef "(Default)"))
  )
  (compInst "X1"
    (compRef "XTAL_2_PINS")
    (originalName "XTAL_2_PINS")
    (compValue "32.768kHz")
    (attr "Component_Country_Of_Origin" "Japan" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Crystal_Oscillator/NDK_NX1610SE_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Crystal, 32.768kHz, 6pF, +/-20ppm, 70KR, 1.6x1mm" (textStyleRef "(Default)"))
    (attr "ID" "4685" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-02579" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "NDK" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "NX1610SE-32.768KHz-EXS00A-MU01501" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "N/A" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "N/A" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "N/A" (textStyleRef "(Default)"))
    (attr "Package" "1.6x1.0mm" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Crystal_Osc" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (compInst "X2"
    (compRef "XTAL_4_PINS")
    (originalName "XTAL_4_PINS")
    (compValue "32MHz")
    (attr "Component_Country_Of_Origin" "Japan" (textStyleRef "(Default)"))
    (attr "ComponentLink1URL" "http://tunmcdsvn.tun.st.com/Component_Documentation_Library/Trunk/Crystal_Oscillator/NDK_NX1612SA_Series" (textStyleRef "(Default)"))
    (attr "Database Table Name" "MCD_PARTS$" (textStyleRef "(Default)"))
    (attr "Description" "Crystal, 32MHz, 8pF, +/-10ppm, 40R, 1612(metric)" (textStyleRef "(Default)"))
    (attr "ID" "4684" (textStyleRef "(Default)"))
    (attr "Internal_Part_Number" "MCD-02578" (textStyleRef "(Default)"))
    (attr "Library Name" "MCD_PARTS_database.DbLib" (textStyleRef "(Default)"))
    (attr "Manufacturer" "NDK" (textStyleRef "(Default)"))
    (attr "Manufacturer_Part_Number" "NX1612SA-32MHz-EXS00A-CS09166" (textStyleRef "(Default)"))
    (attr "Order_Code_Digikey" "N/A" (textStyleRef "(Default)"))
    (attr "Order_Code_Farnell" "N/A" (textStyleRef "(Default)"))
    (attr "Order_Code_RS" "N/A" (textStyleRef "(Default)"))
    (attr "Package" "1612(metric)" (textStyleRef "(Default)"))
    (attr "Part_Preference" "Recommended" (textStyleRef "(Default)"))
    (attr "Part_Type" "Crystal_Osc" (textStyleRef "(Default)"))
    (attr "ShowFields" "YES" (textStyleRef "(Default)"))
    (attr "Status" "Released" (textStyleRef "(Default)"))
    (attr "Sheet" "STM32 microcontroller I/Os & Clock" (textStyleRef "(Default)"))
  )
  (net "VDDA"
    (node "C11" "2")
    (node "C20" "2")
    (node "CN1" "20")
    (node "SB11" "2")
    (node "U1" "H8")
  )
  (net "VDD15"
    (node "C15" "2")
    (node "C22" "1")
    (node "CN2" "49")
    (node "CN3" "3")
    (node "SB15" "2")
  )
  (net "VDD10"
    (node "C10" "2")
    (node "CN2" "1")
    (node "SB6" "1")
    (node "SB10" "2")
  )
  (net "VDD9"
    (node "C21" "1")
    (node "C27" "2")
    (node "CN2" "31")
    (node "L4" "1")
    (node "SB27" "2")
  )
  (net "VDD8"
    (node "C17" "1")
    (node "C32" "2")
    (node "CN1" "48")
    (node "SB32" "2")
    (node "U1" "L7")
  )
  (net "VDD5"
    (node "C3" "1")
    (node "C5" "2")
    (node "CN2" "3")
    (node "SB5" "2")
    (node "U1" "B4")
  )
  (net "VDD4"
    (node "C4" "2")
    (node "C18" "1")
    (node "C19" "1")
    (node "CN1" "30")
    (node "SB4" "2")
    (node "U1" "D6")
    (node "U1" "L5")
  )
  (net "USB_FS_P"
    (node "CN2" "16")
    (node "U1" "J7")
    (attr "ClassName" "DIFF90" (textStyleRef "(Default)"))
    (attr "DifferentialPair" "True" (textStyleRef "(Default)"))
    (attr "DifferentialPairClassName" "DIFF90" (textStyleRef "(Default)"))
    (attr "MinImpedance" "80.00"  (pt 0.0 0.0) (isVisible False) (textStyleRef "(Default)") )
    (attr "MaxImpedance" "100.0"  (pt 0.0 0.0) (isVisible False) (textStyleRef "(Default)") )
    (attr "Matched Net Lengths" "Tolerance = 2mm"  (pt 0.0 0.0) (isVisible False) (textStyleRef "(Default)") )
  )
  (net "USB_FS_N"
    (node "CN2" "18")
    (node "U1" "K8")
    (attr "ClassName" "DIFF90" (textStyleRef "(Default)"))
    (attr "DifferentialPair" "True" (textStyleRef "(Default)"))
    (attr "DifferentialPairClassName" "DIFF90" (textStyleRef "(Default)"))
    (attr "MinImpedance" "80.00"  (pt 0.0 0.0) (isVisible False) (textStyleRef "(Default)") )
    (attr "MaxImpedance" "100.0"  (pt 0.0 0.0) (isVisible False) (textStyleRef "(Default)") )
    (attr "Matched Net Lengths" "Tolerance = 2mm"  (pt 0.0 0.0) (isVisible False) (textStyleRef "(Default)") )
  )
  (net "OSC_OUT"
    (node "CN1" "41")
    (node "SB40" "2")
  )
  (net "OSC_IN"
    (node "CN1" "39")
    (node "SB39" "2")
  )
  (net "NRST"
    (node "CN1" "12")
    (node "D1" "2")
    (node "R7" "2")
  )
  (net "NetU1_F2"
    (node "U1" "F2")
    (node "U2" "A1")
    (attr "ClassName" "RF" (textStyleRef "(Default)"))
  )
  (net "NetSB40_1"
    (node "SB40" "1")
    (node "U1" "C5")
    (node "X2" "1")
  )
  (net "NetSB39_1"
    (node "SB39" "1")
    (node "U1" "A5")
    (node "X2" "3")
  )
  (net "NetSB24_2"
    (node "SB24" "2")
    (node "SB25" "2")
    (node "U1" "J3")
  )
  (net "NetSB21_2"
    (node "SB21" "2")
    (node "SB22" "2")
    (node "U1" "F6")
  )
  (net "NetSB19_1"
    (node "SB19" "1")
    (node "SB20" "1")
    (node "U1" "H6")
  )
  (net "NetSB16_1"
    (node "SB16" "1")
    (node "SB18" "1")
    (node "U1" "L3")
  )
  (net "NetSB9_2"
    (node "SB9" "2")
    (node "SB12" "2")
    (node "SB23" "2")
    (node "U1" "F8")
  )
  (net "NetSB4_1"
    (node "SB4" "1")
    (node "SB5" "1")
    (node "SB10" "1")
    (node "SB11" "1")
    (node "SB15" "1")
    (node "SB27" "1")
    (node "SB32" "1")
  )
  (net "NetSB1_2"
    (node "SB1" "2")
    (node "SB2" "2")
    (node "U1" "G5")
  )
  (net "NetL7_1"
    (node "L7" "1")
    (node "SB41" "2")
  )
  (net "NetL5_2"
    (node "L5" "2")
    (node "L6" "1")
  )
  (net "NetL5_1"
    (node "L5" "1")
    (node "U1" "D8")
  )
  (net "NetCN4_1"
    (node "CN4" "1")
    (node "U2" "A3")
    (attr "ClassName" "RF" (textStyleRef "(Default)"))
  )
  (net "NetCN3_14"
    (node "CN3" "14")
    (node "R8" "1")
  )
  (net "NetCN3_13"
    (node "CN3" "13")
    (node "R9" "2")
  )
  (net "NetCN3_12"
    (node "CN3" "12")
    (node "R7" "1")
  )
  (net "NetCN3_11"
    (node "CN3" "11")
    (node "R6" "2")
  )
  (net "NetCN3_10"
    (node "CN3" "10")
    (node "R5" "1")
  )
  (net "NetCN3_8"
    (node "CN3" "8")
    (node "R4" "1")
  )
  (net "NetCN3_6"
    (node "CN3" "6")
    (node "R3" "1")
  )
  (net "NetCN3_4"
    (node "CN3" "4")
    (node "R2" "1")
  )
  (net "NetC23_2"
    (node "C23" "2")
    (node "C24" "1")
    (node "C26" "1")
    (node "L6" "2")
    (node "L7" "2")
    (node "U1" "A7")
    (node "U1" "D4")
  )
  (net "NetC16_2"
    (node "C16" "2")
    (node "SB6" "2")
    (node "SB41" "1")
    (node "U1" "B6")
  )
  (net "NetC9_2"
    (node "C9" "2")
    (node "SB37" "1")
    (node "U1" "K4")
    (node "X1" "1")
  )
  (net "NetC8_2"
    (node "C8" "2")
    (node "SB38" "1")
    (node "U1" "J5")
    (node "X1" "2")
  )
  (net "NetC7_2"
    (node "C7" "2")
    (node "D1" "1")
    (node "U1" "E1")
  )
  (net "NetC6_1"
    (node "C6" "1")
    (node "L4" "2")
    (node "U1" "B8")
  )
  (net "NetC2_2"
    (node "C2" "2")
    (node "U1" "C3")
  )
  (net "GPIO56"
    (node "CN2" "46")
    (node "SB12" "1")
  )
  (net "GPIO42"
    (node "CN2" "27")
    (node "U1" "G3")
  )
  (net "GPIO38"
    (node "CN2" "22")
    (node "R5" "2")
    (node "SB24" "1")
  )
  (net "GPIO37"
    (node "CN2" "21")
    (node "SB1" "1")
  )
  (net "GPIO34"
    (node "CN2" "15")
    (node "SB22" "1")
  )
  (net "GPIO33"
    (node "CN2" "13")
    (node "SB18" "2")
  )
  (net "GPIO32"
    (node "CN2" "12")
    (node "R4" "2")
    (node "SB19" "2")
  )
  (net "GPIO31"
    (node "CN2" "11")
    (node "SB23" "1")
  )
  (net "GPIO30"
    (node "CN2" "10")
    (node "SB16" "2")
  )
  (net "GPIO29"
    (node "CN2" "9")
    (node "SB20" "2")
  )
  (net "GPIO28"
    (node "CN2" "7")
    (node "SB25" "1")
  )
  (net "GPIO24"
    (node "CN1" "47")
    (node "R8" "2")
    (node "SB21" "1")
  )
  (net "GPIO23"
    (node "CN1" "45")
    (node "R9" "1")
    (node "U1" "H2")
  )
  (net "GPIO22"
    (node "CN1" "44")
    (node "SB2" "1")
  )
  (net "GPIO16/OSC32_OUT"
    (node "CN1" "35")
    (node "SB38" "2")
  )
  (net "GPIO15/OSC32_IN"
    (node "CN1" "33")
    (node "SB37" "2")
  )
  (net "GPIO12"
    (node "CN1" "26")
    (node "SB9" "1")
  )
  (net "GPIO6/JTCK/SWCLK"
    (node "CN1" "15")
    (node "R3" "2")
    (node "U1" "K2")
  )
  (net "GPIO5/JTMS/SWDIO"
    (node "CN1" "13")
    (node "R2" "2")
    (node "U1" "H4")
  )
  (net "GPIO3/BOOT0"
    (node "CN1" "9")
    (node "R1" "1")
    (node "U1" "G1")
  )
  (net "GND"
    (node "C2" "1")
    (node "C3" "2")
    (node "C4" "1")
    (node "C5" "1")
    (node "C6" "2")
    (node "C7" "1")
    (node "C8" "1")
    (node "C9" "1")
    (node "C10" "1")
    (node "C11" "1")
    (node "C15" "1")
    (node "C16" "1")
    (node "C17" "2")
    (node "C18" "2")
    (node "C19" "2")
    (node "C20" "1")
    (node "C21" "2")
    (node "C22" "2")
    (node "C23" "1")
    (node "C24" "2")
    (node "C26" "2")
    (node "C27" "1")
    (node "C32" "1")
    (node "CN1" "1")
    (node "CN1" "6")
    (node "CN1" "7")
    (node "CN1" "14")
    (node "CN1" "17")
    (node "CN1" "22")
    (node "CN1" "25")
    (node "CN1" "28")
    (node "CN1" "31")
    (node "CN1" "34")
    (node "CN1" "37")
    (node "CN1" "40")
    (node "CN1" "46")
    (node "CN1" "49")
    (node "CN2" "2")
    (node "CN2" "8")
    (node "CN2" "14")
    (node "CN2" "20")
    (node "CN2" "26")
    (node "CN2" "32")
    (node "CN2" "38")
    (node "CN2" "44")
    (node "CN2" "50")
    (node "CN3" "5")
    (node "CN3" "7")
    (node "CN4" "2")
    (node "CN4" "3")
    (node "CN4" "4")
    (node "CN4" "5")
    (node "R1" "2")
    (node "R6" "1")
    (node "SC1" "1")
    (node "SC2" "1")
    (node "SC3" "1")
    (node "SC4" "1")
    (node "SC5" "1")
    (node "U1" "C7")
    (node "U1" "E3")
    (node "U1" "E5")
    (node "U1" "E7")
    (node "U1" "F4")
    (node "U1" "G7")
    (node "U1" "K6")
    (node "U2" "A2")
    (node "U2" "B1")
    (node "U2" "B2")
    (node "U2" "B3")
    (node "X2" "2")
    (node "X2" "4")
  )
)
