Altium Designer Pick and Place Locations
C:\Subversion\Boards\MB997-STM32F4-Manta1M-413-disc1\Trunk\02-Manufacturing\MB997E_PCB\Assembly\MB997E_PickandPlace.txt

========================================================================================================================
File Design Information:

Date:       23/04/20
Time:       11:21
Revision:   Not in VersionControl
Variant:    No variations
Units used: mm

Designator Comment                                   Layer       Footprint                Center-X(mm) Center-Y(mm) Rotation Description                                                                         
X3         "MC306-G-06Q-32.768 (manufacturer JFVNY)" TopLayer    MC306-CRYSTAL            44.2000      63.5000      0        ""                                                                                  
X2         8MHz                                      TopLayer    HC-49A                   30.6000      63.7000      0        "Crystal Oscillator"                                                                
X1         8MHz                                      TopLayer    HC-49A                   20.1222      79.1844      90       "Crystal Oscillator"                                                                
U9         IMP34DT05TR                               TopLayer    MIC_HCLGA_3X4X1_4LD_t    47.6685      8.9748       180      "MEMS audio sensor omnidirectional digital microphone for industrial applications"  
U8         EMIF02-USB03F2                            TopLayer    FLIPCHIP(11)             42.6520      15.4661      0        "2-line IPAD, EMI filter including ESD protection"                                  
U7         CS43L22_NEW                               TopLayer    QFN40(6_6)               27.0031      20.2920      0        "Low Power, Stereo DAC w/Headphone & Speaker Amps"                                  
U6         STMPS2141STR                              TopLayer    SOT-23-5L                40.7960      22.6796      180      "Enhanced single channel power switches"                                            
U5         LIS3DSHTR                                 TopLayer    LGA16_                   33.5080      31.1100      0        "MEMS motion sensor 3-axis - ±2g/±4g/±6g/±8g/±16g digital output accelerometer"     
U4         STM32F407VGT6                             TopLayer    QFP100-1414              32.6635      48.4619      180      "STM32 Manta (STM32F407VGT6)"                                                       
U3         LD3985M25R                                TopLayer    SOT-23-5L                14.4000      66.9000      270      "Ultra low drop-low noise BiCMOS voltage, regulators low ESR capacitors compatible" 
U2         STM32F103CBT6                             TopLayer    LQFP48$2F$0.5MM$5C$9X9B  31.2507      77.0890      0        "Medium-density performance line ARM-based 32-bit MCU with 128KB Flash"             
U1         LD3985M33R                                TopLayer    SOT-23-5L                48.5990      86.7210      0        "Ultra low drop-low noise BiCMOS voltage, regulators low ESR capacitors compatible" 
T1         9013                                      TopLayer    SOT23                    37.8260      10.8686      180      "NPN Bipolar Transistor"                                                            
SB9        "Circuit Breaker"                         BottomLayer JUMPER                   55.6490      72.5010      180      "Circuit Breaker"                                                                   
SB8        "Circuit Breaker"                         BottomLayer JUMPER                   39.8490      72.5010      180      "Circuit Breaker"                                                                   
SB7        "Circuit Breaker"                         BottomLayer JUMPER                   55.6490      75.0410      180      "Circuit Breaker"                                                                   
SB6        "Circuit Breaker"                         BottomLayer JUMPER                   39.8490      75.0410      180      "Circuit Breaker"                                                                   
SB5        "Circuit Breaker"                         BottomLayer JUMPER                   55.6490      77.5810      180      "Circuit Breaker"                                                                   
SB4        "Circuit Breaker"                         BottomLayer JUMPER                   39.8490      77.5810      180      "Circuit Breaker"                                                                   
SB3        "Circuit Breaker"                         BottomLayer JUMPER                   55.6490      80.1210      180      "Circuit Breaker"                                                                   
SB20       "Circuit Breaker"                         BottomLayer JUMPER                   18.8268      37.6664      270      "Circuit Breaker"                                                                   
SB2        "Circuit Breaker"                         BottomLayer JUMPER                   39.8490      80.1210      180      "Circuit Breaker"                                                                   
SB19       "Circuit Breaker"                         BottomLayer JUMPER                   19.8067      48.0167      270      "Circuit Breaker"                                                                   
SB18       "Circuit Breaker"                         BottomLayer JUMPER                   45.3937      51.6148      270      "Circuit Breaker"                                                                   
SB17       "Circuit Breaker"                         BottomLayer JUMPER                   13.6960      53.7700      270      "Circuit Breaker"                                                                   
SB16       "Circuit Breaker"                         BottomLayer JUMPER                   37.3172      63.4212      360      "Circuit Breaker"                                                                   
SB15       "Circuit Breaker"                         BottomLayer JUMPER                   37.3172      64.8436      360      "Circuit Breaker"                                                                   
SB14       "Circuit Breaker"                         BottomLayer JUMPER                   34.0495      66.6572      360      "Circuit Breaker"                                                                   
SB13       "Circuit Breaker"                         BottomLayer JUMPER                   34.0495      68.2563      360      "Circuit Breaker"                                                                   
SB12       "Circuit Breaker"                         BottomLayer JUMPER                   37.1979      69.4057      270      "Circuit Breaker"                                                                   
SB11       "Circuit Breaker"                         BottomLayer JUMPER                   29.7996      69.5942      270      "Circuit Breaker"                                                                   
SB10       "Circuit Breaker"                         BottomLayer JUMPER                   22.2000      70.5500      90       "Circuit Breaker"                                                                   
SB1        "Circuit Breaker"                         TopLayer    JUMPER                   46.7430      39.2711      180      "Circuit Breaker"                                                                   
R9         1K5                                       TopLayer    0402R                    31.2990      85.5210      270      Resistor                                                                            
R8         100K                                      TopLayer    0402R                    29.2990      85.0210      270      Resistor                                                                            
R7         100K                                      TopLayer    0402R                    27.6990      85.0210      270      Resistor                                                                            
R69        100                                       BottomLayer 0402R                    35.5987      74.8530      90       Resistor                                                                            
R68        100                                       BottomLayer 0603R                    33.1999      75.0529      270      Resistor                                                                            
R67        620                                       TopLayer    0603R                    46.4220      2.2580       90       Resistor                                                                            
R66        330                                       TopLayer    0603R                    26.6500      2.2580       90       Resistor                                                                            
R65        0                                         TopLayer    0603R                    24.8042      2.2900       90       Resistor                                                                            
R64        0                                         TopLayer    0402R                    44.5941      8.0871       270      Resistor                                                                            
R63        0                                         TopLayer    0402R                    43.1948      8.0871       90       Resistor                                                                            
R62        51                                        TopLayer    0603R                    27.2000      11.1000      90       Resistor                                                                            
R61        51                                        TopLayer    0603R                    24.7700      10.9880      90       Resistor                                                                            
R60        22                                        TopLayer    0402R                    43.8585      11.8465      0        Resistor                                                                            
R6         10K                                       TopLayer    0402R                    26.1990      85.0210      270      Resistor                                                                            
R59        0                                         TopLayer    0603R                    40.6200      12.2275      90       Resistor                                                                            
R58        22                                        TopLayer    0402R                    43.8585      13.1800      0        Resistor                                                                            
R57        [N/A]                                     TopLayer    0603R                    38.0800      13.6880      0        Resistor                                                                            
R56        47K                                       TopLayer    0402R                    40.5961      15.6832      90       Resistor                                                                            
R55        0                                         TopLayer    0603R                    37.9780      15.5600      180      Resistor                                                                            
R54        1.2K                                      TopLayer    0603R                    34.6760      15.5600      0        Resistor                                                                            
R53        100                                       TopLayer    0402R                    32.0005      17.6822      180      Resistor                                                                            
R52        100K                                      TopLayer    0402R                    35.8575      19.2760      0        Resistor                                                                            
R51        47K                                       TopLayer    0402R                    45.8016      21.7144      270      Resistor                                                                            
R50        0                                         TopLayer    0603R                    44.2776      22.0192      270      Resistor                                                                            
R5         10K                                       TopLayer    0402R                    24.6990      85.0210      270      Resistor                                                                            
R49        0                                         TopLayer    0603R                    36.1984      20.8805      180      Resistor                                                                            
R48        0                                         TopLayer    0603R                    37.4700      22.9260      0        Resistor                                                                            
R47        100                                       TopLayer    0402R                    31.6007      22.8795      180      Resistor                                                                            
R46        0                                         TopLayer    0603R                    43.7945      26.0779      90       Resistor                                                                            
R45        10K                                       TopLayer    0402R                    41.5956      25.8780      270      Resistor                                                                            
R44        100K                                      TopLayer    0402R                    36.2000      24.4500      0        Resistor                                                                            
R43        10K                                       TopLayer    0402R                    32.0005      24.4787      0        Resistor                                                                            
R42        680                                       TopLayer    0603R                    37.2926      26.7690      0        Resistor                                                                            
R41        680                                       TopLayer    0603R                    37.7244      29.4868      180      Resistor                                                                            
R40        510                                       TopLayer    0603R                    29.4018      34.0738      180      Resistor                                                                            
R4         100                                       TopLayer    0402R                    17.0990      85.5210      90       Resistor                                                                            
R39        220K                                      TopLayer    0603R                    22.7892      36.6496      270      Resistor                                                                            
R38        100                                       TopLayer    0402R                    18.2172      35.7352      180      Resistor                                                                            
R37        1K5                                       TopLayer    0402R                    44.1943      37.0723      180      Resistor                                                                            
R36        680                                       TopLayer    0603R                    33.3998      37.6720      180      Resistor                                                                            
R35        330                                       TopLayer    0603R                    19.8936      37.4116      0        Resistor                                                                            
R34        10K                                       TopLayer    0402R                    18.2076      47.0672      270      Resistor                                                                            
R33        4.7K                                      TopLayer    0402R                    47.7925      47.8668      180      Resistor                                                                            
R32        510                                       TopLayer    0603R                    19.8067      47.4670      90       Resistor                                                                            
R31        10K                                       TopLayer    0402R                    46.7930      50.2655      90       Resistor                                                                            
R30        510                                       TopLayer    0603R                    45.1938      50.6653      270      Resistor                                                                            
R3         100                                       TopLayer    0402R                    15.5990      85.5210      90       Resistor                                                                            
R29        4.7K                                      TopLayer    0402R                    49.3068      53.7184      90       Resistor                                                                            
R28        0                                         TopLayer    0603R                    46.7160      56.3092      90       Resistor                                                                            
R27        [N/A]                                     TopLayer    0603R                    45.0396      56.3092      90       Resistor                                                                            
R26        [N/A]                                     TopLayer    0603R                    37.8000      59.7000      270      Resistor                                                                            
R25        0                                         TopLayer    0603R                    32.6444      59.6874      90       Resistor                                                                            
R24        220                                       TopLayer    0603R                    30.5108      59.6874      270      Resistor                                                                            
R23        47                                        TopLayer    0603R                    21.8057      60.6602      270      Resistor                                                                            
R22        0                                         TopLayer    0603R                    38.2000      62.5000      0        Resistor                                                                            
R21        0                                         TopLayer    0603R                    38.2000      64.3000      0        Resistor                                                                            
R20        4.7K                                      TopLayer    0402R                    27.0280      71.6000      90       Resistor                                                                            
R2         100                                       TopLayer    0402R                    12.0000      85.9000      270      Resistor                                                                            
R19        4.7K                                      TopLayer    0402R                    25.6340      71.6000      90       Resistor                                                                            
R18        100K                                      TopLayer    0402R                    22.0000      71.7000      270      Resistor                                                                            
R17        22                                        TopLayer    0402R                    11.0000      72.9000      0        Resistor                                                                            
R16        22                                        TopLayer    0402R                    11.0000      75.5000      0        Resistor                                                                            
R15        22                                        TopLayer    0402R                    11.0000      78.1000      0        Resistor                                                                            
R14        1K                                        TopLayer    0402R                    41.4990      81.7210      270      Resistor                                                                            
R13        10K                                       TopLayer    0402R                    14.1786      81.1656      270      Resistor                                                                            
R12        22                                        TopLayer    0402R                    10.8000      83.1000      0        Resistor                                                                            
R11        0                                         TopLayer    0603R                    34.5990      85.2210      270      Resistor                                                                            
R10        0                                         TopLayer    0603R                    32.8990      85.2210      270      Resistor                                                                            
R1         0                                         TopLayer    0603R                    16.0990      92.8210      0        Resistor                                                                            
P2         "Header 25X2"                             TopLayer    HEAD25X2$2F$2.54         58.4000      32.7000      270      "Header, 25-Pin, Dual row"                                                          
P1         "Header 25X2"                             TopLayer    HEAD25X2$2F$2.54         7.6000       32.7000      270      "Header, 25-Pin, Dual row"                                                          
LD8        Red                                       TopLayer    LED0603                  44.4000      2.3000       90       "Typical RED, GREEN, YELLOW, AMBER GaAs LED"                                        
LD7        Green                                     TopLayer    LED0603                  29.1900      2.3000       90       "Typical RED, GREEN, YELLOW, AMBER GaAs LED"                                        
LD6        Blue                                      TopLayer    LED0603                  33.5080      26.8960      180      "Typical RED, GREEN, YELLOW, AMBER GaAs LED"                                        
LD5        Red                                       TopLayer    LED0603                  37.6482      31.0870      0        "Typical RED, GREEN, YELLOW, AMBER GaAs LED"                                        
LD4        Green                                     TopLayer    LED0603                  29.3424      31.0870      0        "Typical RED, GREEN, YELLOW, AMBER GaAs LED"                                        
LD3        Orange                                    TopLayer    LED0603                  33.5080      35.2780      0        "Typical RED, GREEN, YELLOW, AMBER GaAs LED"                                        
LD2        RED                                       TopLayer    LED0603                  41.5575      84.6625      90       ""                                                                                  
LD1        LD_BICOLOR_CMS                            TopLayer    AV02-0501EN              16.3490      89.5710      180      "Bicolor Led"                                                                       
L1         fcm1608-0603                              TopLayer    0603L                    19.8067      60.6602      270      Inductor                                                                            
JP3        ""                                        BottomLayer SIP2$2F$2.54             59.6700      92.3900      180      ""                                                                                  
JP2        ""                                        BottomLayer SIP2$2F$2.54             6.3300       92.3900      180      ""                                                                                  
JP1        ""                                        TopLayer    SIP2$2F$2.54             17.6079      54.4634      0        ""                                                                                  
D3         BAT60JFILM                                TopLayer    SOD323$2F$A              53.2990      83.1910      90       BAT60JFILM                                                                          
D2         BAT60JFILM                                TopLayer    SOD323$2F$A              10.2000      86.0300      270      BAT60JFILM                                                                          
D1         BAT60JFILM                                TopLayer    SOD323$2F$A              41.5990      88.4510      270      BAT60JFILM                                                                          
CN5        475900001                                 TopLayer    USB-MICRO-AB_new         36.8100      3.3878       90       ""                                                                                  
CN4        ST-225-02                                 TopLayer    PCBCOMPONENT_1$2F$2_new_ 17.7600      5.5600       90       "Connector Jack 35mm"                                                               
CN3        "Header 4"                                TopLayer    HEADER4$2F$2.54          47.2990      76.3110      270      "Header, 4-Pin"                                                                     
CN2        "Header 6"                                TopLayer    HEADER6$2F$2.54          6.3300       79.3500      270      "Header, 6-Pin"                                                                     
CN1        UBF-MINI5-03                              TopLayer    USB-MINI-B-SMD-A_        33.3563      93.0260      0        ""                                                                                  
C9         20pF                                      TopLayer    0402C                    15.9617      77.2032      270      Capacitor                                                                           
C8         100nF                                     TopLayer    0402C                    35.6000      81.9000      270      Capacitor                                                                           
C7         100nF                                     TopLayer    0402C                    26.6000      82.3000      270      Capacitor                                                                           
C61        20pF                                      BottomLayer 0603C                    33.1999      71.8545      270      Capacitor                                                                           
C60        100nF                                     TopLayer    0402C                    50.7800      8.6080       90       Capacitor                                                                           
C6         20pF                                      TopLayer    0402C                    15.9617      81.1656      90       Capacitor                                                                           
C59        1uF                                       TopLayer    CASE-A                   29.4000      12.3000      270      "Polarized Capacitor (Radial)"                                                      
C58        10uF                                      TopLayer    0603C                    47.6685      13.0587      0        Capacitor                                                                           
C57        1uF(X5R)                                  TopLayer    0603C                    33.2000      13.1000      90       Capacitor                                                                           
C56        1uF(X5R)                                  TopLayer    0603C                    31.4000      13.1000      90       Capacitor                                                                           
C55        0.022uF                                   TopLayer    0603C                    27.2000      14.1000      90       Capacitor                                                                           
C54        0.022uF                                   TopLayer    0603C                    24.7700      14.0360      90       Capacitor                                                                           
C53        0.1uF                                     TopLayer    0402C                    20.4000      15.5000      0        Capacitor                                                                           
C52        10nF                                      TopLayer    0603C                    37.9780      17.5920      0        Capacitor                                                                           
C51        1uF(X7R)                                  TopLayer    0603C                    34.6760      17.5920      0        Capacitor                                                                           
C50        "1uF (X7R)"                               TopLayer    0603C                    20.5540      17.2440      0        Capacitor                                                                           
C5         10nF_X7R_0603                             TopLayer    0603C                    44.7990      84.5210      0        "0603  X7R 10NF"                                                                    
C49        4.7uF                                     TopLayer    CASE-A                   42.1953      18.4817      0        "Polarized Capacitor (Radial)"                                                      
C48        150pF(COG)                                TopLayer    0603C                    32.2004      19.4812      180      Capacitor                                                                           
C47        1uF(X7R)                                  TopLayer    0603C                    20.5540      19.0220      180      Capacitor                                                                           
C46        150pF(COG)                                TopLayer    0603C                    32.2004      21.0804      180      Capacitor                                                                           
C45        0.1uF                                     TopLayer    0402C                    20.4040      21.3079      0        Capacitor                                                                           
C44        1uF(X7R)                                  TopLayer    0603C                    34.4220      22.9260      0        Capacitor                                                                           
C43        0.1uF                                     TopLayer    0402C                    20.4000      22.7000      0        Capacitor                                                                           
C42        0.1uF                                     TopLayer    0402C                    29.0020      25.6781      270      Capacitor                                                                           
C41        0.1uF                                     TopLayer    0402C                    27.6028      25.6781      270      Capacitor                                                                           
C40        0.1uF                                     TopLayer    0402C                    26.2035      25.6781      270      Capacitor                                                                           
C4         100nF                                     TopLayer    0402C                    53.3835      86.9035      270      Capacitor                                                                           
C39        100nF                                     TopLayer    0402C                    29.8016      29.0763      0        Capacitor                                                                           
C38        100nF                                     TopLayer    0402C                    20.6556      35.7352      180      Capacitor                                                                           
C37        100nF                                     TopLayer    0402C                    46.5931      37.0723      180      Capacitor                                                                           
C36        2.2uF                                     TopLayer    CASE-A                   40.3660      36.8020      0        "Low ESR Ceramic Capacitor (X7R)"                                                   
C35        100nF                                     TopLayer    0402C                    41.1958      39.8708      270      Capacitor                                                                           
C34        100nF                                     TopLayer    0402C                    24.0046      40.0707      90       Capacitor                                                                           
C33        2.2uF                                     TopLayer    CASE-A                   19.6068      39.8708      180      "Low ESR Ceramic Capacitor (X7R)"                                                   
C32        100nF                                     TopLayer    0402C                    21.2060      53.2640      270      Capacitor                                                                           
C31        100nF                                     TopLayer    0402C                    19.8067      53.2640      270      Capacitor                                                                           
C30        100nF                                     TopLayer    0402C                    43.3947      56.6623      270      Capacitor                                                                           
C3         1µF_X5R_0603                              TopLayer    0603C                    51.5420      87.0940      90       "0603  X5R 1µF"                                                                     
C29        100nF                                     TopLayer    0402C                    41.9954      56.6623      270      Capacitor                                                                           
C28        1uF                                       TopLayer    0603C                    39.6000      59.7000      90       Capacitor                                                                           
C27        6.8pF                                     TopLayer    0603C                    42.6000      59.5000      0        Capacitor                                                                           
C26        100nF                                     TopLayer    0402C                    27.0000      60.3000      0        Capacitor                                                                           
C25        100nF                                     TopLayer    0402C                    15.6089      60.4603      270      Capacitor                                                                           
C24        100nF                                     TopLayer    0402C                    34.7780      60.3986      0        Capacitor                                                                           
C23        1uF                                       TopLayer    CASE-A                   23.8000      62.9000      90       "Polarized Capacitor (Radial)"                                                      
C22        1uF                                       TopLayer    CASE-A                   17.6079      61.6597      90       "Polarized Capacitor (Radial)"                                                      
C21        100nF                                     TopLayer    0402C                    21.8000      63.7000      270      Capacitor                                                                           
C20        1µF_X5R_0603                              TopLayer    0603C                    19.4000      66.9000      270      "0603  X5R 1µF"                                                                     
C2         100nF                                     TopLayer    0402C                    45.7635      87.2845      90       Capacitor                                                                           
C19        100nF                                     TopLayer    0402C                    17.8000      66.7000      270      Capacitor                                                                           
C18        100nF                                     TopLayer    0402C                    11.0000      66.3000      270      Capacitor                                                                           
C17        1µF_X5R_0603                              TopLayer    0603C                    9.4000       66.7000      90       "0603  X5R 1µF"                                                                     
C16        6.8pF                                     TopLayer    0603C                    42.2000      67.5000      0        Capacitor                                                                           
C15        20pF                                      TopLayer    0603C                    34.6764      66.9772      180      Capacitor                                                                           
C14        20pF                                      TopLayer    0603C                    27.0564      66.9772      0        Capacitor                                                                           
C13        10nF_X7R_0603                             TopLayer    0603C                    10.8000      69.3000      0        "0603  X7R 10NF"                                                                    
C12        100nF                                     TopLayer    0402C                    36.0000      72.1000      270      Capacitor                                                                           
C11        100nF                                     TopLayer    0402C                    23.6000      71.9000      90       Capacitor                                                                           
C10        100nF                                     TopLayer    0402C                    24.4808      75.4202      270      Capacitor                                                                           
C1         1µF_X5R_0603                              TopLayer    0603C                    43.9990      87.1210      90       "0603  X5R 1µF"                                                                     
B2         SW-PUSH-CMS                               TopLayer    SW4SMD                   44.9496      31.7828      0        "Non-Open Push-Button 0.1A 24V"                                                     
B1         SW-PUSH-CMS                               TopLayer    SW4SMD                   21.0504      31.7628      180      "Non-Open Push-Button 0.1A 24V"                                                     
